{"text_format":"2","workbook":"xlsx","n_sheets":14,"sheets":["Main","list","OPCDA声明","L01","L19","新风机","吊顶空调","风机盘管","水风幕机","排风机","断电保存","集水井","扶梯","环境换算"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":3,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":7,"n_cols":4,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
["日期","版本号","编制记录","编制人"]
[null,1,"初始化建立","戴锦豪"]
[20220210,1.1000000000000001,"调整涉及累计时间程序，适应断电保存功能","潘平"]
[null,null,"增加空调、风机、集水井、扶梯、风机盘管断电保存变量声明部分，程序部分"]
[null,null,"增加吊顶空调专用模块程序部分"]
[null,null,"增加影院空调程序部分"]

{"sheet":"list","index":1,"n_rows":501,"n_cols":20,"rows_kept":501,"cut":false,"hidden":false,"merged":[[0,17,0,18],[0,1,0,2],[0,3,0,5],[0,6,0,7],[0,8,0,10],[0,12,0,14]]}
["序号","总线编号",null,"设备缩写",null,null,"设备编号",null,"功能名",null,null,null,"接线备注",null,null,null,"序号","设备索引"]
[1,"总线01","L01","<空调系统>>",null,null,"地下三层","B3","<电控箱功能>",null,null,null,"功能名","端子编号","线色备注",null,1,"AC24V电源","AC24V"]
[2,"总线02","L02","F新风机组","FAU","Fresh air unit","地下二层","B2","运行状态","R","Run",{"$nulls":5},2,"DC24V电源","DC24V"]
[3,"总线03","L03","P新风机组","PAU","术语备选","地下一层","B1","故障状态","F","Fault",{"$nulls":5},3,"8路数字量输入模块","IOM.0801R"]
[4,"总线04","L04","M新风机组","MAU","术语备选","夹层","BM","自动状态","A","Auto",{"$nulls":5},4,"16路数字量输入模块","IOM.1601R"]
[5,"总线05","L05","全热交换机组","HEU","Heat exchange unit","一层","01","启停控制","C","Control",{"$nulls":5},5,"8路数字量输出模块","IOM.0801D"]
[6,"总线06","L06","风机盘管","FCU","Fan Coil Units","二层","02","主泵运行状态","R1",{"$nulls":6},6,"16路数字量输出模块","IOM.1601D"]
[7,"总线07","L07","空调机组","AHU","Air handling unit","三层","03","主泵故障状态","F1",{"$nulls":6},7,"4路模拟量输入模块","IOM.0401U"]
[8,"总线08","L08","<送排风系统>>",null,null,"四层","04","主泵启停控制","C1",{"$nulls":6},8,"8路模拟量输入模块","IOM.0801U"]
[9,"总线09","L09","送风机","SAF","Supply fan","五层","05","备泵运行状态","R2",{"$nulls":6},9,"4路模拟量输出模块","IOM.0401A"]
[10,"···","···","排风机","EAF","Air exhaust fan",null,"···","备泵故障状态","F2",{"$nulls":6},10,"8路数字量输入模块","IOM.0801R OV"]
[11,"总线XX","LXX","排烟机","ESF","Somke exhaust fan","屋面","RF","备泵启停控制","C2",{"$nulls":6},11,"16路数字量输入模块","IOM.1601R OV"]
[12,null,null,"双速风机","EMF","Multipurpose exhaust fan",null,null,"变频器运行","VR","VFD run",{"$nulls":5},12,"8路数字量输出模块","IOM.0801D OV"]
[13,null,null,"<冷热源系统>",{"$nulls":4},"变频器故障","VF","VFD fault",{"$nulls":5},13,"16路数字量输出模块","IOM.1601D OV"]
[14,null,null,"冷水机组","CHR","CHILLER",null,null,"变频器启停","VC","VFD control",{"$nulls":5},14,"16路数字量输出模块","IOM.0401U OV"]
[15,null,null,"风冷热泵机组","CHR","按冷机缩写命名",null,null,"变频器频率控制","VFC","VFD frequency control",{"$nulls":5},15,"16路数字量输入输出模块","IOM.1601RD","暂未制作"]
[16,null,null,"水源热泵机组","CHR","按冷机缩写命名",null,null,"变频器频率反馈","VFB","VFD frequency feedback",{"$nulls":5},16,"8路模拟量输入模块","IOM.0801U ES"]
[17,null,null,"地源热泵机组","CHR","按冷机缩写命名",null,null,"高速运行状态","R1",{"$nulls":6},17,"模块在线状态中间变量","中间变量"]
[18,null,null,"冷冻水泵","CHP","Chilled water pump",null,null,"高速故障状态","F1",{"$nulls":6},18,"吊顶空调机组中间变量","AHU"]
[19,null,null,"冷却水泵","CLP","Cooling water pump",null,null,"高速启停控制","C1",{"$nulls":6},19,"风机盘管中间变量","FCU"]
[20,null,null,"蝶阀","BFV","Butterfly valve",null,null,"低速运行状态","R2",{"$nulls":6},20,"智能照明中间变量","LCB"]
[21,null,null,"旁通阀","BPV","Bypass valve",null,null,"低速故障状态","F2",{"$nulls":6},21]
[22,null,null,"锅炉","BLR","Boiler",null,null,"低速启停控制","C2",{"$nulls":6},22]
[23,null,null,"冷却塔","CLT","Cooling water tower",null,null,"<风路功能>",{"$nulls":7},23]
[24,null,null,"冷冻水回路","CHS","Chilled water system",null,null,"风机压差","FPS","Fan Differential Pressure Switch",{"$nulls":5},24]
[25,null,null,"冷却水回路","CLS","Cooling water system",null,null,"初效滤网压差","IPS","initial effect Differential Pressure Switch",{"$nulls":5},25]
[26,null,null,"一次侧热水回路","PHS","Primary hot water system",null,null,"中效滤网压差","MPS","Medium effect Differential Pressure Switch",{"$nulls":5},26]
[27,null,null,"二次侧热水回路","SHS","Secondary hot water system",null,null,"高效滤网压差","HPS","High effect Differential Pressure Switch",{"$nulls":5},27]
[28,null,null,"锅炉","BLR","Boiler",null,null,"低温断路开关","AFS","Antifreeze switch",{"$nulls":5},28]
[29,null,null,"热水循环泵","BFP","Boiler feed water pump",null,null,"送风温度","ST","Supply air Temperature",{"$nulls":5},29]
[30,null,null,"板式换热器","HEX","Heat exchanger",null,null,"回风温度","RT","Return air Temperature",{"$nulls":5},30]
[31,null,null,"<给排水系统>",{"$nulls":4},"排风温度","ET","Exhaust air Temperature"]
[32,null,null,"潜污泵井","SWP","Submersible sewage pump/sump ",null,null,"新风温度","FT","Fresh air Temperature"]
[33,null,null,"生活水泵","LWP","Life Water pump",null,null,"送风湿度","SH","Supply air Humidity"]
[34,null,null,"消防水泵","FWP","Fire water pump",null,null,"回风湿度","RH","Return air Humidity"]
[35,null,null,"生活水箱","LWT","Life water tank",null,null,"排风湿度","EH","Exhaust air Humidity"]
[36,null,null,"消防水箱","SWT","Fire water tank",null,null,"新风湿度","FH","Fresh air Humidity"]
[37,null,null,"其它水箱","OWT","Other water tank",null,null,"露点温度","DPT","Dew point temperature"]
[38,null,null,"<照明系统>",{"$nulls":4},"送风阀开","SDO","Supply air Damper open"]
[39,null,null,"照明控制箱","LCB","Lighting control box",null,null,"送风阀关","SDS","Supply air Damper shut"]
[40,null,null,"照明调光箱","LDB","Lighting dimming zone",null,null,"回风阀开","RDO","Return air Damper open"]
[41,null,null,"照明控制区域","LCZ","Lighting control zone",null,null,"回风阀关","RDS","Return air Damper shut"]
[42,null,null,"智能控制面板","LCP","Smart lighting panel",null,null,"排风阀开","EDO","Exhaust air Damper open"]
[43,null,null,"<其它系统>",{"$nulls":4},"排风阀关","EDS","Exhaust air Damper shut"]
[44,null,null,"扶梯","LET","level Escalator",null,null,"新风阀开","FDOB","Fresh air Damper open"]
[45,null,null,"垂直客梯","PET","Passenger elevator",null,null,"新风阀关","FDSB","Fresh air Damper shut"]
[46,null,null,"垂直货梯","CET","Cargo elevator",null,null,"送风阀控制","SDC","Supply air Damper regulation control"]
[47,null,null,"隔油池","OSP","oil separator",null,null,"送风阀反馈","SDB","Supply air Damper regulation feedback"]
[48,null,null,"高压综合主开关柜","HVM","High voltage main switchgear",null,null,"回风阀控制","RDC","Return air Damper regulation control"]
[49,null,null,"高压综合备开关柜","HVS","High voltage standby switchgear",null,null,"回风阀反馈","RDB","Return air Damper regulation feedback"]
[50,null,null,"低压综合主配电柜","LVM","Low voltage main switchgear",null,null,"排风阀控制","EDC","Exhaust air Damper regulation control"]
[51,null,null,"低压综合备配电柜","LVS","Low voltage standby switchgear",null,null,"排风阀反馈","EDB","Exhaust air Damper regulation feedback"]
[52,null,null,"电表","EM","electricity meter",null,null,"新风阀控制","FDC","Fresh air Damper regulation control"]
[53,null,null,"水表","WM","water meter",null,null,"新风阀反馈","FDB","Fresh air Damper regulation feedback"]
[54,null,null,"热表","HM","heat meter",null,null,"加湿器开控制","HFO","Humidifier open"]
[55,null,null,"<环境监测系统>",{"$nulls":4},"加湿器关控制","HFS","Humidifier shut"]
[56,null,null,"室内环境状态","IES","Indoor environmental state",null,null,"加湿器控制","HFC","Humidifier control"]
[57,null,null,"室外环境状态","OES","Outdoor environmental state",null,null,"水风幕阀控制","FMC"]
[58,null,null,"<吾悦特殊机组>",{"$nulls":4},"<水路功能>"]
[59,null,null,"吊顶式空调机组","AHU","Fresh air unit",null,null,"水阀控制","WVC","Water Valve control"]
[60,null,null,"<系统基础>>",{"$nulls":4},"水阀开","WVO","Water Valve open"]
[61,null,null,"控制箱","BOX",null,null,null,"水阀关","WVS","Water Valve shut"]
[62,null,null,"控制器","DEV","Device",null,null,"水阀反馈","WVB","Water Valve Feedback"]
[63,null,null,"命令","CMD",null,null,null,"水流开关","FS","Flow switch"]
[64,null,null,"风幕机","FMJ",null,null,null,"超高液位","SHL","Super high level"]
[65,null,null,"水幕机","SMJ",null,null,null,"高液位","HL","High level"]
[66,{"$nulls":7},"低液位","LL","Low level"]
[67,{"$nulls":7},"超低液位","SLL","Super low level"]
[68,{"$nulls":7},"供水温度","ST","Supply water temperature"]
[69,{"$nulls":7},"回水温度","RT","Return water temperature"]
[70,{"$nulls":7},"供水压力","SP","Supply water Pressure"]
[71,{"$nulls":7},"回水压力","RP","Return water Pressure"]
[72,{"$nulls":7},"供水流量","SF","Supply water flow"]
[73,{"$nulls":7},"回水流量","RF","Return water flow"]
[74,{"$nulls":7},"<照明功能>"]
[75,{"$nulls":7},"人体感应开关","MIS","Mobile induction switch"]
[76,{"$nulls":7},"照度读值","IS","illumination sensor"]
[77,{"$nulls":7},"面板按键01","B01","Button1"]
[78,{"$nulls":7},"面板按键02","B02","Button2"]
[79,{"$nulls":7},"面板按键03","B03","Button3"]
[80,{"$nulls":7},"面板按键04","B04","Button4"]
[81,{"$nulls":7},"面板按键05","B05","Button5"]
[82,{"$nulls":7},"面板按键06","B06","Button6"]
[83,{"$nulls":7},"回路开关1","C01","Control"]
[84,{"$nulls":7},"回路开关2","C02","Control"]
[85,{"$nulls":7},"回路开关3","C03","Control"]
[86,{"$nulls":7},"回路开关4","C04","Control"]
[87,{"$nulls":7},"回路开关5","C05","Control"]
[88,{"$nulls":7},"回路开关6","C06","Control"]
[89,{"$nulls":7},"回路开关7","C07","Control"]
[90,{"$nulls":7},"回路开关8","C08","Control"]
[91,{"$nulls":7},"回路开关9","C09","Control"]
[92,{"$nulls":7},"回路开关10","C10","Control"]
[93,{"$nulls":7},"回路开关11","C11","Control"]
[94,{"$nulls":7},"回路开关12","C12","Control"]
[95,{"$nulls":7},"回路开关13","C13","Control"]
[96,{"$nulls":7},"回路开关14","C14","Control"]
[97,{"$nulls":7},"回路开关15","C15","Control"]
[98,{"$nulls":7},"回路开关16","C16","Control"]
[99,{"$nulls":7},"回路开关17","C17","Control"]
[100,{"$nulls":7},"回路开关18","C18","Control"]
[101,{"$nulls":7},"回路开关19","C19","Control"]
[102,{"$nulls":7},"回路开关20","C20","Control"]
[103,{"$nulls":7},"回路调节1","D01","Dimming"]
[104,{"$nulls":7},"回路调节2","D02","Dimming"]
[105,{"$nulls":7},"回路调节3","D03","Dimming"]
[106,{"$nulls":7},"回路调节4","D04","Dimming"]
[107,{"$nulls":7},"回路调节5","D05","Dimming"]
[108,{"$nulls":7},"回路调节6","D06","Dimming"]
[109,{"$nulls":7},"回路调节7","D07","Dimming"]
[110,{"$nulls":7},"回路调节8","D08","Dimming"]
[111,{"$nulls":7},"<电梯功能>"]
[112,{"$nulls":7},"上行状态","US","Upward state"]
[113,{"$nulls":7},"下行状态","DS","Downward state"]
[114,{"$nulls":7},"<环境功能>"]
[115,{"$nulls":7},"照度状态","I","Illumination"]
[116,{"$nulls":7},"温度状态","T","Temperature"]
[117,{"$nulls":7},"湿度状态","H","Humidity"]
[118,{"$nulls":7},"露点温度状态","DEP","Dew point temperature"]
[119,{"$nulls":7},"一氧化碳浓度状态","CO"]
[120,{"$nulls":7},"二氧化碳浓度状态","CO2"]
[121,{"$nulls":7},"甲烷浓度状态","CH4"]
[122,{"$nulls":7},"氧气浓度状态","O2"]
[123,{"$nulls":7},"氨气浓度状态","NH4"]
[124,{"$nulls":7},"<冷机功能>"]
[125,{"$nulls":7},"控制模式","CM","Control mode"]
[126,{"$nulls":7},"工况模式"]
[127,{"$nulls":7},"电流百分比"]
[128,{"$nulls":7},"<锅炉功能>"]
[129,{"$nulls":7},"大火","HF","High fire"]
[130,{"$nulls":7},"中火","MF","Middle fire"]
[131,{"$nulls":7},"小火","LF","Low fire"]
[132,{"$nulls":7},"<吾悦特殊功能>"]
[133,{"$nulls":7},"电磁阀开启状态","EVR","Electromagnetic valve run"]
[134,{"$nulls":7},"电磁阀自动状态","EVA","Electromagnetic valve auto"]
[135,{"$nulls":7},"电磁阀开关控制","EVC","Electromagnetic valve control"]
[136,{"$nulls":7},"<中间变量>>"]
[137,{"$nulls":7},"模块地址状态","DS","Device Status"]
[138,{"$nulls":7},"模块在线比例","OR","Online Ratio"]
[139,{"$nulls":7},"设定温度值","TSET","Temperature Set"]
[140,{"$nulls":7},"季节模式","SM","Season Mode"]
[141,{"$nulls":7},"水阀反馈换算值","WVBS","Water Vavle Feedback Switch"]
[142,{"$nulls":7},"水阀手动控制","WVMC","Water Vavle Manual Control"]
[143,{"$nulls":7},"水阀手动控制值","WVMV","Water Vavle Manual Value"]
[144,{"$nulls":7},"回风温度换算值","RTS","Return Temperature Switch"]
[145,{"$nulls":7},"运行时间累积重置","RST","Runtime Reset"]
[146,{"$nulls":7},"运行时间累积重置值","RSTV","Runtime Reset Value"]
[147,{"$nulls":7},"运行时间累积值","RH","Runtime Hour"]
[148]
[149,{"$nulls":7},"隔离开关1","ISO1","Isolation Switch1"]
[150,{"$nulls":7},"隔离开关2","ISO2","Isolation Switch2"]
[151,{"$nulls":7},"P调节参数","VP","Value Proportion "]
[152,{"$nulls":7},"I调节参数","VI","Value Integration"]
[153,{"$nulls":7},"设备状态代码","SN","Status Number"]
[154,{"$nulls":7},"水阀控制转换值","WVCS","Water Vavle Control Switch"]
[155,{"$nulls":7},"室内温度转换值","TS","Temperature Switch"]
[156,{"$nulls":7},"程序控制","PC","Program Control"]
[157,{"$nulls":7},"新云模式","CM"]
[158,{"$nulls":7},"运行模式","RM"]
[159,{"$nulls":7},"温度换算值","TS"]
[160,{"$nulls":7},"电磁阀手动控制","EVMC"]
[161,{"$nulls":7},"电磁阀手动控制值","EVMV"]
[162,{"$nulls":7},"心跳值","DHV","Device Heart Vavle"]
[163,{"$nulls":7},"照度状态换算值","IS","Illumination Switch"]
[164,{"$nulls":7},"温度状态换算值","TS","Temperature Switch"]
[165,{"$nulls":7},"湿度状态换算值","HS","Humidity Switch"]
[166,{"$nulls":7},"新风阀开控制","FDOC"]
[167,{"$nulls":7},"新风阀关控制","FDSC"]
[168,{"$nulls":7},"送风温度换算值","STS"]
[169,{"$nulls":7},"变频手动控制值","VFMV"]
[170,{"$nulls":7},"低温断路报警隔离","ISO3"]
[171,{"$nulls":7},"变频器频率控制值","VFCS"]
[172,{"$nulls":7},"变频器频率反馈值","VFBS"]
[173,{"$nulls":7},"联动模式","LM"]
[174,{"$nulls":7},"全天候模式","DM"]
[175,{"$nulls":7},"CO2设定值","CO2SET"]
[176,{"$nulls":7},"定时控制","TC"]
[177,{"$nulls":7},"定时模式","TM"]
[178,{"$nulls":7},"一氧化碳浓度换算值","COS"]
[179,{"$nulls":7},"CO设定值","COSET"]
[180,{"$nulls":7},"二氧化碳浓度换算值","CO2S"]
[181]
[182,{"$nulls":7},"运行时间累积重置1","RST1"]
[183,{"$nulls":7},"运行时间累积重置值1","RSTV1"]
[184,{"$nulls":7},"运行时间累积值1","RH1"]
[185,{"$nulls":7},"运行时间累积重置2","RST2"]
[186,{"$nulls":7},"运行时间累积重置值2","RSTV2"]
[187,{"$nulls":7},"运行时间累积值2","RH2"]
[188]
[189]
[190]
[191]
[192]
[193]
[194]
[195]
[196]
[197]
[198]
[199]
[200]
[201]
[202]
[203]
[204]
[205]
[206]
[207]
[208]
[209]
[210]
[211]
[212]
[213]
[214]
[215]
[216]
[217]
[218]
[219]
[220]
[221]
[222]
[223]
[224]
[225]
[226]
[227]
[228]
[229]
[230]
[231]
[232]
[233]
[234]
[235]
[236]
[237]
[238]
[239]
[240]
[241]
[242]
[243]
[244]
[245]
[246]
[247]
[248]
[249]
[250]
[251]
[252]
[253]
[254]
[255]
[256]
[257]
[258]
[259]
[260]
[261]
[262]
[263]
[264]
[265]
[266]
[267]
[268]
[269]
[270]
[271]
[272]
[273]
[274]
[275]
[276]
[277]
[278]
[279]
[280]
[281]
[282]
[283]
[284]
[285]
[286]
[287]
[288]
[289]
[290]
[291]
[292]
[293]
[294]
[295]
[296]
[297]
[298]
[299]
[300]
[301]
[302]
[303]
[304]
[305]
[306]
[307]
[308]
[309]
[310]
[311]
[312]
[313]
[314]
[315]
[316]
[317]
[318]
[319]
[320]
[321]
[322]
[323]
[324]
[325]
[326]
[327]
[328]
[329]
[330]
[331]
[332]
[333]
[334]
[335]
[336]
[337]
[338]
[339]
[340]
[341]
[342]
[343]
[344]
[345]
[346]
[347]
[348]
[349]
[350]
[351]
[352]
[353]
[354]
[355]
[356]
[357]
[358]
[359]
[360]
[361]
[362]
[363]
[364]
[365]
[366]
[367]
[368]
[369]
[370]
[371]
[372]
[373]
[374]
[375]
[376]
[377]
[378]
[379]
[380]
[381]
[382]
[383]
[384]
[385]
[386]
[387]
[388]
[389]
[390]
[391]
[392]
[393]
[394]
[395]
[396]
[397]
[398]
[399]
[400]
[401]
[402]
[403]
[404]
[405]
[406]
[407]
[408]
[409]
[410]
[411]
[412]
[413]
[414]
[415]
[416]
[417]
[418]
[419]
[420]
[421]
[422]
[423]
[424]
[425]
[426]
[427]
[428]
[429]
[430]
[431]
[432]
[433]
[434]
[435]
[436]
[437]
[438]
[439]
[440]
[441]
[442]
[443]
[444]
[445]
[446]
[447]
[448]
[449]
[450]
[451]
[452]
[453]
[454]
[455]
[456]
[457]
[458]
[459]
[460]
[461]
[462]
[463]
[464]
[465]
[466]
[467]
[468]
[469]
[470]
[471]
[472]
[473]
[474]
[475]
[476]
[477]
[478]
[479]
[480]
[481]
[482]
[483]
[484]
[485]
[486]
[487]
[488]
[489]
[490]
[491]
[492]
[493]
[494]
[495]
[496]
[497]
[498]
[499]
[500]

{"sheet":"OPCDA声明","index":2,"n_rows":512,"n_cols":11,"rows_kept":512,"cut":false,"hidden":false,"merged":[]}
["中间变量"]
["100.0",{"$f":"IF((IF(OR(C2=\"INT\",C2=\"WORD\",C2=\"BOOL\"),MOD(A2,2),MOD(A2,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"INT","命令","L","00000","运行模式","总线程序-运行模式",{"$f":"E2&VLOOKUP(D2,list!$D$3:$F$501,2,FALSE)&F2&\"_\"&VLOOKUP(G2,list!$I$2:$K$502,2,FALSE)","v":"LCMD00000_RM"},{"$f":"I2&\" \"&\"AT%M\"&A2&\" \"&\":\"&C2&\";\"&\" \"&\"(*\"&H2&\"*)\"","v":"LCMD00000_RM AT%M100.0 :INT; (*总线程序-运行模式*)"},{"$f":"REPLACE(REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2))),SEARCH(\":\",REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2))))))","v":"LCMD00000_RM            AT%M100.0      :INT; (*总线程序-运行模式*)"}]
[{"$f":"IF(OR(C2=\"REAL\",C2=\"DWORD\",C2=\"DINT\"),(IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),A2+4+MOD(A2,4),A2+4)),(IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),A2+4+MOD(A2,4),A2+2)))&\".0\"","v":"102.0"},{"$f":"IF((IF(OR(C3=\"INT\",C3=\"WORD\",C3=\"BOOL\"),MOD(A3,2),MOD(A3,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","控制箱","L","H01","模块地址状态",{"$f":"D3&F3&\"-\"&IF(E3=\"R\",\"新云平台\"&G3,G3)","v":"控制箱H01-模块地址状态"},{"$f":"E3&VLOOKUP(D3,list!$D$3:$F$501,2,FALSE)&F3&\"_\"&VLOOKUP(G3,list!$I$2:$K$502,2,FALSE)","v":"LBOXH01_DS"},{"$f":"I3&\" \"&\"AT%M\"&A3&\" \"&\":\"&C3&\";\"&\" \"&\"(*\"&H3&\"*)\"","v":"LBOXH01_DS AT%M102.0 :BOOL; (*控制箱H01-模块地址状态*)"},"LBOXH01_DS              AT%M102.0      :BOOL; (*控制箱H01-模块地址状态*)"]
[{"$f":"IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),(IF(OR(C4=\"REAL\",C4=\"DWORD\",C4=\"DINT\"),A3+4+MOD(A3,4),A3+4)),(IF(OR(C4=\"REAL\",C4=\"DWORD\",C4=\"DINT\"),A3+4+MOD(A3,4),A3+2)))&\".0\"","v":"104.0"},"验证通过","BOOL","控制箱","L","H02","模块地址状态",{"$f":"D4&F4&\"-\"&IF(E4=\"R\",\"新云平台\"&G4,G4)","v":"控制箱H02-模块地址状态"},{"$f":"E4&VLOOKUP(D4,list!$D$3:$F$501,2,FALSE)&F4&\"_\"&VLOOKUP(G4,list!$I$2:$K$502,2,FALSE)","v":"LBOXH02_DS"},"LBOXH02_DS AT%M104.0 :BOOL; (*控制箱H02-模块地址状态*)","LBOXH02_DS              AT%M104.0      :BOOL; (*控制箱H02-模块地址状态*)"]
["106.0","验证通过","BOOL","控制箱","L","H03","模块地址状态","控制箱H03-模块地址状态",{"$f":"E5&VLOOKUP(D5,list!$D$3:$F$501,2,FALSE)&F5&\"_\"&VLOOKUP(G5,list!$I$2:$K$502,2,FALSE)","v":"LBOXH03_DS"},{"$f":"I5&\" \"&\"AT%M\"&A5&\" \"&\":\"&C5&\";\"&\" \"&\"(*\"&H5&\"*)\"","v":"LBOXH03_DS AT%M106.0 :BOOL; (*控制箱H03-模块地址状态*)"},"LBOXH03_DS              AT%M106.0      :BOOL; (*控制箱H03-模块地址状态*)"]
["108.0","验证通过","BOOL","控制箱","L","H04","模块地址状态","控制箱H04-模块地址状态",{"$f":"E6&VLOOKUP(D6,list!$D$3:$F$501,2,FALSE)&F6&\"_\"&VLOOKUP(G6,list!$I$2:$K$502,2,FALSE)","v":"LBOXH04_DS"},"LBOXH04_DS AT%M108.0 :BOOL; (*控制箱H04-模块地址状态*)","LBOXH04_DS              AT%M108.0      :BOOL; (*控制箱H04-模块地址状态*)"]
["110.0","验证通过","BOOL","控制箱","L","H05","模块地址状态","控制箱H05-模块地址状态",{"$f":"E7&VLOOKUP(D7,list!$D$3:$F$501,2,FALSE)&F7&\"_\"&VLOOKUP(G7,list!$I$2:$K$502,2,FALSE)","v":"LBOXH05_DS"},"LBOXH05_DS AT%M110.0 :BOOL; (*控制箱H05-模块地址状态*)","LBOXH05_DS              AT%M110.0      :BOOL; (*控制箱H05-模块地址状态*)"]
["112.0","验证通过","BOOL","控制箱","L","H06","模块地址状态","控制箱H06-模块地址状态",{"$f":"E8&VLOOKUP(D8,list!$D$3:$F$501,2,FALSE)&F8&\"_\"&VLOOKUP(G8,list!$I$2:$K$502,2,FALSE)","v":"LBOXH06_DS"},"LBOXH06_DS AT%M112.0 :BOOL; (*控制箱H06-模块地址状态*)","LBOXH06_DS              AT%M112.0      :BOOL; (*控制箱H06-模块地址状态*)"]
["114.0","验证通过","BOOL","控制箱","L","H07","模块地址状态","控制箱H07-模块地址状态",{"$f":"E9&VLOOKUP(D9,list!$D$3:$F$501,2,FALSE)&F9&\"_\"&VLOOKUP(G9,list!$I$2:$K$502,2,FALSE)","v":"LBOXH07_DS"},{"$f":"I9&\" \"&\"AT%M\"&A9&\" \"&\":\"&C9&\";\"&\" \"&\"(*\"&H9&\"*)\"","v":"LBOXH07_DS AT%M114.0 :BOOL; (*控制箱H07-模块地址状态*)"},"LBOXH07_DS              AT%M114.0      :BOOL; (*控制箱H07-模块地址状态*)"]
["116.0","验证通过","BOOL","控制箱","L","H08","模块地址状态","控制箱H08-模块地址状态",{"$f":"E10&VLOOKUP(D10,list!$D$3:$F$501,2,FALSE)&F10&\"_\"&VLOOKUP(G10,list!$I$2:$K$502,2,FALSE)","v":"LBOXH08_DS"},"LBOXH08_DS AT%M116.0 :BOOL; (*控制箱H08-模块地址状态*)","LBOXH08_DS              AT%M116.0      :BOOL; (*控制箱H08-模块地址状态*)"]
["118.0","验证通过","BOOL","控制箱","L","H09","模块地址状态","控制箱H09-模块地址状态",{"$f":"E11&VLOOKUP(D11,list!$D$3:$F$501,2,FALSE)&F11&\"_\"&VLOOKUP(G11,list!$I$2:$K$502,2,FALSE)","v":"LBOXH09_DS"},"LBOXH09_DS AT%M118.0 :BOOL; (*控制箱H09-模块地址状态*)","LBOXH09_DS              AT%M118.0      :BOOL; (*控制箱H09-模块地址状态*)"]
["120.0","验证通过","BOOL","控制箱","L","H10","模块地址状态","控制箱H10-模块地址状态",{"$f":"E12&VLOOKUP(D12,list!$D$3:$F$501,2,FALSE)&F12&\"_\"&VLOOKUP(G12,list!$I$2:$K$502,2,FALSE)","v":"LBOXH10_DS"},"LBOXH10_DS AT%M120.0 :BOOL; (*控制箱H10-模块地址状态*)","LBOXH10_DS              AT%M120.0      :BOOL; (*控制箱H10-模块地址状态*)"]
["124.0","验证通过","REAL","控制箱","L","H00","模块在线比例","控制箱H00-模块在线比例",{"$f":"E13&VLOOKUP(D13,list!$D$3:$F$501,2,FALSE)&F13&\"_\"&VLOOKUP(G13,list!$I$2:$K$502,2,FALSE)","v":"LBOXH00_OR"},"LBOXH00_OR AT%M124.0 :REAL; (*控制箱H00-模块在线比例*)","LBOXH00_OR              AT%M124.0      :REAL; (*控制箱H00-模块在线比例*)"]
["128.0","验证通过","REAL","控制箱","L","H01","模块在线比例","控制箱H01-模块在线比例",{"$f":"E14&VLOOKUP(D14,list!$D$3:$F$501,2,FALSE)&F14&\"_\"&VLOOKUP(G14,list!$I$2:$K$502,2,FALSE)","v":"LBOXH01_OR"},"LBOXH01_OR AT%M128.0 :REAL; (*控制箱H01-模块在线比例*)","LBOXH01_OR              AT%M128.0      :REAL; (*控制箱H01-模块在线比例*)"]
["132.0","验证通过","REAL","控制箱","L","H02","模块在线比例","控制箱H02-模块在线比例",{"$f":"E15&VLOOKUP(D15,list!$D$3:$F$501,2,FALSE)&F15&\"_\"&VLOOKUP(G15,list!$I$2:$K$502,2,FALSE)","v":"LBOXH02_OR"},"LBOXH02_OR AT%M132.0 :REAL; (*控制箱H02-模块在线比例*)","LBOXH02_OR              AT%M132.0      :REAL; (*控制箱H02-模块在线比例*)"]
["136.0","验证通过","REAL","控制箱","L","H03","模块在线比例","控制箱H03-模块在线比例",{"$f":"E16&VLOOKUP(D16,list!$D$3:$F$501,2,FALSE)&F16&\"_\"&VLOOKUP(G16,list!$I$2:$K$502,2,FALSE)","v":"LBOXH03_OR"},"LBOXH03_OR AT%M136.0 :REAL; (*控制箱H03-模块在线比例*)","LBOXH03_OR              AT%M136.0      :REAL; (*控制箱H03-模块在线比例*)"]
["140.0","验证通过","REAL","控制箱","L","H04","模块在线比例","控制箱H04-模块在线比例",{"$f":"E17&VLOOKUP(D17,list!$D$3:$F$501,2,FALSE)&F17&\"_\"&VLOOKUP(G17,list!$I$2:$K$502,2,FALSE)","v":"LBOXH04_OR"},"LBOXH04_OR AT%M140.0 :REAL; (*控制箱H04-模块在线比例*)","LBOXH04_OR              AT%M140.0      :REAL; (*控制箱H04-模块在线比例*)"]
["144.0","验证通过","REAL","控制箱","L","H05","模块在线比例","控制箱H05-模块在线比例",{"$f":"E18&VLOOKUP(D18,list!$D$3:$F$501,2,FALSE)&F18&\"_\"&VLOOKUP(G18,list!$I$2:$K$502,2,FALSE)","v":"LBOXH05_OR"},"LBOXH05_OR AT%M144.0 :REAL; (*控制箱H05-模块在线比例*)","LBOXH05_OR              AT%M144.0      :REAL; (*控制箱H05-模块在线比例*)"]
["148.0","验证通过","REAL","控制箱","L","H06","模块在线比例","控制箱H06-模块在线比例",{"$f":"E19&VLOOKUP(D19,list!$D$3:$F$501,2,FALSE)&F19&\"_\"&VLOOKUP(G19,list!$I$2:$K$502,2,FALSE)","v":"LBOXH06_OR"},"LBOXH06_OR AT%M148.0 :REAL; (*控制箱H06-模块在线比例*)","LBOXH06_OR              AT%M148.0      :REAL; (*控制箱H06-模块在线比例*)"]
["152.0","验证通过","REAL","控制箱","L","H07","模块在线比例","控制箱H07-模块在线比例",{"$f":"E20&VLOOKUP(D20,list!$D$3:$F$501,2,FALSE)&F20&\"_\"&VLOOKUP(G20,list!$I$2:$K$502,2,FALSE)","v":"LBOXH07_OR"},"LBOXH07_OR AT%M152.0 :REAL; (*控制箱H07-模块在线比例*)","LBOXH07_OR              AT%M152.0      :REAL; (*控制箱H07-模块在线比例*)"]
["156.0","验证通过","REAL","控制箱","L","H08","模块在线比例","控制箱H08-模块在线比例",{"$f":"E21&VLOOKUP(D21,list!$D$3:$F$501,2,FALSE)&F21&\"_\"&VLOOKUP(G21,list!$I$2:$K$502,2,FALSE)","v":"LBOXH08_OR"},"LBOXH08_OR AT%M156.0 :REAL; (*控制箱H08-模块在线比例*)","LBOXH08_OR              AT%M156.0      :REAL; (*控制箱H08-模块在线比例*)"]
["160.0","验证通过","REAL","控制箱","L","H09","模块在线比例","控制箱H09-模块在线比例",{"$f":"E22&VLOOKUP(D22,list!$D$3:$F$501,2,FALSE)&F22&\"_\"&VLOOKUP(G22,list!$I$2:$K$502,2,FALSE)","v":"LBOXH09_OR"},"LBOXH09_OR AT%M160.0 :REAL; (*控制箱H09-模块在线比例*)","LBOXH09_OR              AT%M160.0      :REAL; (*控制箱H09-模块在线比例*)"]
["164.0","验证通过","REAL","控制箱","L","H10","模块在线比例","控制箱H10-模块在线比例",{"$f":"E23&VLOOKUP(D23,list!$D$3:$F$501,2,FALSE)&F23&\"_\"&VLOOKUP(G23,list!$I$2:$K$502,2,FALSE)","v":"LBOXH10_OR"},"LBOXH10_OR AT%M164.0 :REAL; (*控制箱H10-模块在线比例*)","LBOXH10_OR              AT%M164.0      :REAL; (*控制箱H10-模块在线比例*)"]
["AHU"]
[{"$f":"IF(OR(C23=\"REAL\",C23=\"DWORD\",C23=\"DINT\"),(IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),A23+4+MOD(A23,4),A23+4)),(IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),A23+4+MOD(A23,4),A23+2)))&\".0\"","v":"168.0"},{"$f":"IF((IF(OR(C25=\"INT\",C25=\"WORD\",C25=\"BOOL\"),MOD(A25,2),MOD(A25,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H01","设定温度值",{"$f":"D25&F25&\"-\"&IF(E25=\"R\",\"新云平台\"&G25,G25)","v":"空调机组01H01-新云平台设定温度值"},{"$f":"E25&VLOOKUP(D25,list!$D$3:$F$501,2,FALSE)&F25&\"_\"&VLOOKUP(G25,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H01_TSET"},{"$f":"I25&\" \"&\"AT%M\"&A25&\" \"&\":\"&C25&\";\"&\" \"&\"(*\"&H25&\"*)\"","v":"RAHU01H01_TSET AT%M168.0 :REAL; (*空调机组01H01-新云平台设定温度值*)"},"RAHU01H01_TSET          AT%M168.0      :REAL; (*空调机组01H01-新云平台设定温度值*)"]
[{"$f":"IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),(IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),A25+4+MOD(A25,4),A25+4)),(IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),A25+4+MOD(A25,4),A25+2)))&\".0\"","v":"172.0"},"验证通过","INT","空调机组","R",{"$f":"F25","v":"01H01"},"季节模式","空调机组01H01-新云平台季节模式",{"$f":"E26&VLOOKUP(D26,list!$D$3:$F$501,2,FALSE)&F26&\"_\"&VLOOKUP(G26,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H01_SM"},"RAHU01H01_SM AT%M172.0 :INT; (*空调机组01H01-新云平台季节模式*)","RAHU01H01_SM            AT%M172.0      :INT; (*空调机组01H01-新云平台季节模式*)"]
[{"$f":"IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),(IF(OR(C27=\"REAL\",C27=\"DWORD\",C27=\"DINT\"),A26+4+MOD(A26,4),A26+4)),(IF(OR(C27=\"REAL\",C27=\"DWORD\",C27=\"DINT\"),A26+4+MOD(A26,4),A26+2)))&\".0\"","v":"174.0"},"验证通过","BOOL","空调机组","R",{"$f":"F26","v":"01H01"},"程序控制","空调机组01H01-新云平台程序控制",{"$f":"E27&VLOOKUP(D27,list!$D$3:$F$501,2,FALSE)&F27&\"_\"&VLOOKUP(G27,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H01_PC"},"RAHU01H01_PC AT%M174.0 :BOOL; (*空调机组01H01-新云平台程序控制*)","RAHU01H01_PC            AT%M174.0      :BOOL; (*空调机组01H01-新云平台程序控制*)"]
["180.0","验证通过","REAL","空调机组","L","01H01","设定温度值","空调机组01H01-设定温度值",{"$f":"E28&VLOOKUP(D28,list!$D$3:$F$501,2,FALSE)&F28&\"_\"&VLOOKUP(G28,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_TSET"},"LAHU01H01_TSET AT%M180.0 :REAL; (*空调机组01H01-设定温度值*)","LAHU01H01_TSET          AT%M180.0      :REAL; (*空调机组01H01-设定温度值*)"]
["184.0","验证通过","INT","空调机组","L","01H01","季节模式","空调机组01H01-季节模式",{"$f":"E29&VLOOKUP(D29,list!$D$3:$F$501,2,FALSE)&F29&\"_\"&VLOOKUP(G29,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_SM"},"LAHU01H01_SM AT%M184.0 :INT; (*空调机组01H01-季节模式*)","LAHU01H01_SM            AT%M184.0      :INT; (*空调机组01H01-季节模式*)"]
["188.0","验证通过","REAL","空调机组","L","01H01","水阀反馈换算值","空调机组01H01-水阀反馈换算值",{"$f":"E30&VLOOKUP(D30,list!$D$3:$F$501,2,FALSE)&F30&\"_\"&VLOOKUP(G30,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_WVBS"},"LAHU01H01_WVBS AT%M188.0 :REAL; (*空调机组01H01-水阀反馈换算值*)","LAHU01H01_WVBS          AT%M188.0      :REAL; (*空调机组01H01-水阀反馈换算值*)"]
["192.0","验证通过","BOOL","空调机组","L","01H01","水阀手动控制","空调机组01H01-水阀手动控制",{"$f":"E31&VLOOKUP(D31,list!$D$3:$F$501,2,FALSE)&F31&\"_\"&VLOOKUP(G31,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_WVMC"},"LAHU01H01_WVMC AT%M192.0 :BOOL; (*空调机组01H01-水阀手动控制*)","LAHU01H01_WVMC          AT%M192.0      :BOOL; (*空调机组01H01-水阀手动控制*)"]
["196.0","验证通过","REAL","空调机组","L","01H01","水阀手动控制值","空调机组01H01-水阀手动控制值",{"$f":"E32&VLOOKUP(D32,list!$D$3:$F$501,2,FALSE)&F32&\"_\"&VLOOKUP(G32,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_WVMV"},"LAHU01H01_WVMV AT%M196.0 :REAL; (*空调机组01H01-水阀手动控制值*)","LAHU01H01_WVMV          AT%M196.0      :REAL; (*空调机组01H01-水阀手动控制值*)"]
["200.0","验证通过","REAL","空调机组","L","01H01","回风温度换算值","空调机组01H01-回风温度换算值",{"$f":"E33&VLOOKUP(D33,list!$D$3:$F$501,2,FALSE)&F33&\"_\"&VLOOKUP(G33,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_RTS"},"LAHU01H01_RTS AT%M200.0 :REAL; (*空调机组01H01-回风温度换算值*)","LAHU01H01_RTS           AT%M200.0      :REAL; (*空调机组01H01-回风温度换算值*)"]
["204.0","验证通过","BOOL","空调机组","L","01H01","运行时间累积重置","空调机组01H01-运行时间累积重置",{"$f":"E34&VLOOKUP(D34,list!$D$3:$F$501,2,FALSE)&F34&\"_\"&VLOOKUP(G34,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_RST"},"LAHU01H01_RST AT%M204.0 :BOOL; (*空调机组01H01-运行时间累积重置*)","LAHU01H01_RST           AT%M204.0      :BOOL; (*空调机组01H01-运行时间累积重置*)"]
["208.0","验证通过","REAL","空调机组","L","01H01","运行时间累积重置值","空调机组01H01-运行时间累积重置值",{"$f":"E35&VLOOKUP(D35,list!$D$3:$F$501,2,FALSE)&F35&\"_\"&VLOOKUP(G35,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_RSTV"},"LAHU01H01_RSTV AT%M208.0 :REAL; (*空调机组01H01-运行时间累积重置值*)","LAHU01H01_RSTV          AT%M208.0      :REAL; (*空调机组01H01-运行时间累积重置值*)"]
["212.0","验证通过","BOOL","空调机组","L","01H01","隔离开关1","空调机组01H01-隔离开关1",{"$f":"E36&VLOOKUP(D36,list!$D$3:$F$501,2,FALSE)&F36&\"_\"&VLOOKUP(G36,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_ISO1"},"LAHU01H01_ISO1 AT%M212.0 :BOOL; (*空调机组01H01-隔离开关1*)","LAHU01H01_ISO1          AT%M212.0      :BOOL; (*空调机组01H01-隔离开关1*)"]
["214.0","验证通过","BOOL","空调机组","L","01H01","隔离开关2","空调机组01H01-隔离开关2",{"$f":"E37&VLOOKUP(D37,list!$D$3:$F$501,2,FALSE)&F37&\"_\"&VLOOKUP(G37,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_ISO2"},"LAHU01H01_ISO2 AT%M214.0 :BOOL; (*空调机组01H01-隔离开关2*)","LAHU01H01_ISO2          AT%M214.0      :BOOL; (*空调机组01H01-隔离开关2*)"]
["220.0","验证通过","REAL","空调机组","L","01H01","P调节参数","空调机组01H01-P调节参数",{"$f":"E38&VLOOKUP(D38,list!$D$3:$F$501,2,FALSE)&F38&\"_\"&VLOOKUP(G38,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_VP"},"LAHU01H01_VP AT%M220.0 :REAL; (*空调机组01H01-P调节参数*)","LAHU01H01_VP            AT%M220.0      :REAL; (*空调机组01H01-P调节参数*)"]
["224.0","验证通过","REAL","空调机组","L","01H01","I调节参数","空调机组01H01-I调节参数",{"$f":"E39&VLOOKUP(D39,list!$D$3:$F$501,2,FALSE)&F39&\"_\"&VLOOKUP(G39,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_VI"},"LAHU01H01_VI AT%M224.0 :REAL; (*空调机组01H01-I调节参数*)","LAHU01H01_VI            AT%M224.0      :REAL; (*空调机组01H01-I调节参数*)"]
["228.0","验证通过","REAL","空调机组","L","01H01","运行时间累积值","空调机组01H01-运行时间累积值",{"$f":"E40&VLOOKUP(D40,list!$D$3:$F$501,2,FALSE)&F40&\"_\"&VLOOKUP(G40,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_RH"},"LAHU01H01_RH AT%M228.0 :REAL; (*空调机组01H01-运行时间累积值*)","LAHU01H01_RH            AT%M228.0      :REAL; (*空调机组01H01-运行时间累积值*)"]
["232.0","验证通过","INT","空调机组","L","01H01","设备状态代码","空调机组01H01-设备状态代码",{"$f":"E41&VLOOKUP(D41,list!$D$3:$F$501,2,FALSE)&F41&\"_\"&VLOOKUP(G41,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_SN"},"LAHU01H01_SN AT%M232.0 :INT; (*空调机组01H01-设备状态代码*)","LAHU01H01_SN            AT%M232.0      :INT; (*空调机组01H01-设备状态代码*)"]
["234.0","验证通过","INT","空调机组","L","01H01","水阀控制转换值","空调机组01H01-水阀控制转换值",{"$f":"E42&VLOOKUP(D42,list!$D$3:$F$501,2,FALSE)&F42&\"_\"&VLOOKUP(G42,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_WVCS"},"LAHU01H01_WVCS AT%M234.0 :INT; (*空调机组01H01-水阀控制转换值*)","LAHU01H01_WVCS          AT%M234.0      :INT; (*空调机组01H01-水阀控制转换值*)"]
["236.0","验证通过","BOOL","空调机组","L","01H01","程序控制","空调机组01H01-程序控制",{"$f":"E43&VLOOKUP(D43,list!$D$3:$F$501,2,FALSE)&F43&\"_\"&VLOOKUP(G43,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H01_PC"},"LAHU01H01_PC AT%M236.0 :BOOL; (*空调机组01H01-程序控制*)","LAHU01H01_PC            AT%M236.0      :BOOL; (*空调机组01H01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C43=\"REAL\",C43=\"DWORD\",C43=\"DINT\"),(IF(OR(C45=\"REAL\",C45=\"DWORD\",C45=\"DINT\"),A43+4+MOD(A43,4),A43+4)),(IF(OR(C45=\"REAL\",C45=\"DWORD\",C45=\"DINT\"),A43+4+MOD(A43,4),A43+2)))&\".0\"","v":"240.0"},{"$f":"IF((IF(OR(C45=\"INT\",C45=\"WORD\",C45=\"BOOL\"),MOD(A45,2),MOD(A45,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H02","设定温度值",{"$f":"D45&F45&\"-\"&IF(E45=\"R\",\"新云平台\"&G45,G45)","v":"空调机组01H02-新云平台设定温度值"},{"$f":"E45&VLOOKUP(D45,list!$D$3:$F$501,2,FALSE)&F45&\"_\"&VLOOKUP(G45,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H02_TSET"},{"$f":"I45&\" \"&\"AT%M\"&A45&\" \"&\":\"&C45&\";\"&\" \"&\"(*\"&H45&\"*)\"","v":"RAHU01H02_TSET AT%M240.0 :REAL; (*空调机组01H02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J45,SEARCH(\"AT%\",J45),,REPT(\" \",25-SEARCH(\"AT%\",J45))),SEARCH(\":\",REPLACE(J45,SEARCH(\"AT%\",J45),,REPT(\" \",25-SEARCH(\"AT%\",J45)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J45,SEARCH(\"AT%\",J45),,REPT(\" \",25-SEARCH(\"AT%\",J45))))))","v":"RAHU01H02_TSET          AT%M240.0      :REAL; (*空调机组01H02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C45=\"REAL\",C45=\"DWORD\",C45=\"DINT\"),(IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),A45+4+MOD(A45,4),A45+4)),(IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),A45+4+MOD(A45,4),A45+2)))&\".0\"","v":"244.0"},"验证通过","INT","空调机组","R",{"$f":"F45","v":"01H02"},"季节模式","空调机组01H02-新云平台季节模式",{"$f":"E46&VLOOKUP(D46,list!$D$3:$F$501,2,FALSE)&F46&\"_\"&VLOOKUP(G46,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H02_SM"},"RAHU01H02_SM AT%M244.0 :INT; (*空调机组01H02-新云平台季节模式*)","RAHU01H02_SM            AT%M244.0      :INT; (*空调机组01H02-新云平台季节模式*)"]
["246.0","验证通过","BOOL","空调机组","R","01H02","程序控制","空调机组01H02-新云平台程序控制",{"$f":"E47&VLOOKUP(D47,list!$D$3:$F$501,2,FALSE)&F47&\"_\"&VLOOKUP(G47,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H02_PC"},"RAHU01H02_PC AT%M246.0 :BOOL; (*空调机组01H02-新云平台程序控制*)","RAHU01H02_PC            AT%M246.0      :BOOL; (*空调机组01H02-新云平台程序控制*)"]
["252.0","验证通过","REAL","空调机组","L","01H02","设定温度值","空调机组01H02-设定温度值",{"$f":"E48&VLOOKUP(D48,list!$D$3:$F$501,2,FALSE)&F48&\"_\"&VLOOKUP(G48,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_TSET"},"LAHU01H02_TSET AT%M252.0 :REAL; (*空调机组01H02-设定温度值*)","LAHU01H02_TSET          AT%M252.0      :REAL; (*空调机组01H02-设定温度值*)"]
["256.0","验证通过","INT","空调机组","L","01H02","季节模式","空调机组01H02-季节模式",{"$f":"E49&VLOOKUP(D49,list!$D$3:$F$501,2,FALSE)&F49&\"_\"&VLOOKUP(G49,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_SM"},"LAHU01H02_SM AT%M256.0 :INT; (*空调机组01H02-季节模式*)","LAHU01H02_SM            AT%M256.0      :INT; (*空调机组01H02-季节模式*)"]
["260.0","验证通过","REAL","空调机组","L","01H02","水阀反馈换算值","空调机组01H02-水阀反馈换算值",{"$f":"E50&VLOOKUP(D50,list!$D$3:$F$501,2,FALSE)&F50&\"_\"&VLOOKUP(G50,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_WVBS"},"LAHU01H02_WVBS AT%M260.0 :REAL; (*空调机组01H02-水阀反馈换算值*)","LAHU01H02_WVBS          AT%M260.0      :REAL; (*空调机组01H02-水阀反馈换算值*)"]
["264.0","验证通过","BOOL","空调机组","L","01H02","水阀手动控制","空调机组01H02-水阀手动控制",{"$f":"E51&VLOOKUP(D51,list!$D$3:$F$501,2,FALSE)&F51&\"_\"&VLOOKUP(G51,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_WVMC"},"LAHU01H02_WVMC AT%M264.0 :BOOL; (*空调机组01H02-水阀手动控制*)","LAHU01H02_WVMC          AT%M264.0      :BOOL; (*空调机组01H02-水阀手动控制*)"]
["268.0","验证通过","REAL","空调机组","L","01H02","水阀手动控制值","空调机组01H02-水阀手动控制值",{"$f":"E52&VLOOKUP(D52,list!$D$3:$F$501,2,FALSE)&F52&\"_\"&VLOOKUP(G52,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_WVMV"},"LAHU01H02_WVMV AT%M268.0 :REAL; (*空调机组01H02-水阀手动控制值*)","LAHU01H02_WVMV          AT%M268.0      :REAL; (*空调机组01H02-水阀手动控制值*)"]
["272.0","验证通过","REAL","空调机组","L","01H02","回风温度换算值","空调机组01H02-回风温度换算值",{"$f":"E53&VLOOKUP(D53,list!$D$3:$F$501,2,FALSE)&F53&\"_\"&VLOOKUP(G53,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_RTS"},"LAHU01H02_RTS AT%M272.0 :REAL; (*空调机组01H02-回风温度换算值*)","LAHU01H02_RTS           AT%M272.0      :REAL; (*空调机组01H02-回风温度换算值*)"]
["276.0","验证通过","BOOL","空调机组","L","01H02","运行时间累积重置","空调机组01H02-运行时间累积重置",{"$f":"E54&VLOOKUP(D54,list!$D$3:$F$501,2,FALSE)&F54&\"_\"&VLOOKUP(G54,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_RST"},"LAHU01H02_RST AT%M276.0 :BOOL; (*空调机组01H02-运行时间累积重置*)","LAHU01H02_RST           AT%M276.0      :BOOL; (*空调机组01H02-运行时间累积重置*)"]
["280.0","验证通过","REAL","空调机组","L","01H02","运行时间累积重置值","空调机组01H02-运行时间累积重置值",{"$f":"E55&VLOOKUP(D55,list!$D$3:$F$501,2,FALSE)&F55&\"_\"&VLOOKUP(G55,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_RSTV"},"LAHU01H02_RSTV AT%M280.0 :REAL; (*空调机组01H02-运行时间累积重置值*)","LAHU01H02_RSTV          AT%M280.0      :REAL; (*空调机组01H02-运行时间累积重置值*)"]
["284.0","验证通过","BOOL","空调机组","L","01H02","隔离开关1","空调机组01H02-隔离开关1",{"$f":"E56&VLOOKUP(D56,list!$D$3:$F$501,2,FALSE)&F56&\"_\"&VLOOKUP(G56,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_ISO1"},"LAHU01H02_ISO1 AT%M284.0 :BOOL; (*空调机组01H02-隔离开关1*)","LAHU01H02_ISO1          AT%M284.0      :BOOL; (*空调机组01H02-隔离开关1*)"]
["286.0","验证通过","BOOL","空调机组","L","01H02","隔离开关2","空调机组01H02-隔离开关2",{"$f":"E57&VLOOKUP(D57,list!$D$3:$F$501,2,FALSE)&F57&\"_\"&VLOOKUP(G57,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_ISO2"},"LAHU01H02_ISO2 AT%M286.0 :BOOL; (*空调机组01H02-隔离开关2*)","LAHU01H02_ISO2          AT%M286.0      :BOOL; (*空调机组01H02-隔离开关2*)"]
["292.0","验证通过","REAL","空调机组","L","01H02","P调节参数","空调机组01H02-P调节参数",{"$f":"E58&VLOOKUP(D58,list!$D$3:$F$501,2,FALSE)&F58&\"_\"&VLOOKUP(G58,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_VP"},"LAHU01H02_VP AT%M292.0 :REAL; (*空调机组01H02-P调节参数*)","LAHU01H02_VP            AT%M292.0      :REAL; (*空调机组01H02-P调节参数*)"]
["296.0","验证通过","REAL","空调机组","L","01H02","I调节参数","空调机组01H02-I调节参数",{"$f":"E59&VLOOKUP(D59,list!$D$3:$F$501,2,FALSE)&F59&\"_\"&VLOOKUP(G59,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_VI"},"LAHU01H02_VI AT%M296.0 :REAL; (*空调机组01H02-I调节参数*)","LAHU01H02_VI            AT%M296.0      :REAL; (*空调机组01H02-I调节参数*)"]
["300.0","验证通过","REAL","空调机组","L","01H02","运行时间累积值","空调机组01H02-运行时间累积值",{"$f":"E60&VLOOKUP(D60,list!$D$3:$F$501,2,FALSE)&F60&\"_\"&VLOOKUP(G60,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_RH"},"LAHU01H02_RH AT%M300.0 :REAL; (*空调机组01H02-运行时间累积值*)","LAHU01H02_RH            AT%M300.0      :REAL; (*空调机组01H02-运行时间累积值*)"]
["304.0","验证通过","INT","空调机组","L","01H02","设备状态代码","空调机组01H02-设备状态代码",{"$f":"E61&VLOOKUP(D61,list!$D$3:$F$501,2,FALSE)&F61&\"_\"&VLOOKUP(G61,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_SN"},"LAHU01H02_SN AT%M304.0 :INT; (*空调机组01H02-设备状态代码*)","LAHU01H02_SN            AT%M304.0      :INT; (*空调机组01H02-设备状态代码*)"]
["306.0","验证通过","INT","空调机组","L","01H02","水阀控制转换值","空调机组01H02-水阀控制转换值",{"$f":"E62&VLOOKUP(D62,list!$D$3:$F$501,2,FALSE)&F62&\"_\"&VLOOKUP(G62,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_WVCS"},"LAHU01H02_WVCS AT%M306.0 :INT; (*空调机组01H02-水阀控制转换值*)","LAHU01H02_WVCS          AT%M306.0      :INT; (*空调机组01H02-水阀控制转换值*)"]
["308.0","验证通过","BOOL","空调机组","L","01H02","程序控制","空调机组01H02-程序控制",{"$f":"E63&VLOOKUP(D63,list!$D$3:$F$501,2,FALSE)&F63&\"_\"&VLOOKUP(G63,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H02_PC"},"LAHU01H02_PC AT%M308.0 :BOOL; (*空调机组01H02-程序控制*)","LAHU01H02_PC            AT%M308.0      :BOOL; (*空调机组01H02-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C63=\"REAL\",C63=\"DWORD\",C63=\"DINT\"),(IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),A63+4+MOD(A63,4),A63+4)),(IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),A63+4+MOD(A63,4),A63+2)))&\".0\"","v":"312.0"},{"$f":"IF((IF(OR(C65=\"INT\",C65=\"WORD\",C65=\"BOOL\"),MOD(A65,2),MOD(A65,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H03","设定温度值",{"$f":"D65&F65&\"-\"&IF(E65=\"R\",\"新云平台\"&G65,G65)","v":"空调机组01H03-新云平台设定温度值"},{"$f":"E65&VLOOKUP(D65,list!$D$3:$F$501,2,FALSE)&F65&\"_\"&VLOOKUP(G65,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H03_TSET"},{"$f":"I65&\" \"&\"AT%M\"&A65&\" \"&\":\"&C65&\";\"&\" \"&\"(*\"&H65&\"*)\"","v":"RAHU01H03_TSET AT%M312.0 :REAL; (*空调机组01H03-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J65,SEARCH(\"AT%\",J65),,REPT(\" \",25-SEARCH(\"AT%\",J65))),SEARCH(\":\",REPLACE(J65,SEARCH(\"AT%\",J65),,REPT(\" \",25-SEARCH(\"AT%\",J65)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J65,SEARCH(\"AT%\",J65),,REPT(\" \",25-SEARCH(\"AT%\",J65))))))","v":"RAHU01H03_TSET          AT%M312.0      :REAL; (*空调机组01H03-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),(IF(OR(C66=\"REAL\",C66=\"DWORD\",C66=\"DINT\"),A65+4+MOD(A65,4),A65+4)),(IF(OR(C66=\"REAL\",C66=\"DWORD\",C66=\"DINT\"),A65+4+MOD(A65,4),A65+2)))&\".0\"","v":"316.0"},"验证通过","INT","空调机组","R",{"$f":"F65","v":"01H03"},"季节模式","空调机组01H03-新云平台季节模式",{"$f":"E66&VLOOKUP(D66,list!$D$3:$F$501,2,FALSE)&F66&\"_\"&VLOOKUP(G66,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H03_SM"},"RAHU01H03_SM AT%M316.0 :INT; (*空调机组01H03-新云平台季节模式*)","RAHU01H03_SM            AT%M316.0      :INT; (*空调机组01H03-新云平台季节模式*)"]
["318.0","验证通过","BOOL","空调机组","R","01H03","程序控制","空调机组01H03-新云平台程序控制",{"$f":"E67&VLOOKUP(D67,list!$D$3:$F$501,2,FALSE)&F67&\"_\"&VLOOKUP(G67,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H03_PC"},"RAHU01H03_PC AT%M318.0 :BOOL; (*空调机组01H03-新云平台程序控制*)","RAHU01H03_PC            AT%M318.0      :BOOL; (*空调机组01H03-新云平台程序控制*)"]
["324.0","验证通过","REAL","空调机组","L","01H03","设定温度值","空调机组01H03-设定温度值",{"$f":"E68&VLOOKUP(D68,list!$D$3:$F$501,2,FALSE)&F68&\"_\"&VLOOKUP(G68,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_TSET"},"LAHU01H03_TSET AT%M324.0 :REAL; (*空调机组01H03-设定温度值*)","LAHU01H03_TSET          AT%M324.0      :REAL; (*空调机组01H03-设定温度值*)"]
["328.0","验证通过","INT","空调机组","L","01H03","季节模式","空调机组01H03-季节模式",{"$f":"E69&VLOOKUP(D69,list!$D$3:$F$501,2,FALSE)&F69&\"_\"&VLOOKUP(G69,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_SM"},"LAHU01H03_SM AT%M328.0 :INT; (*空调机组01H03-季节模式*)","LAHU01H03_SM            AT%M328.0      :INT; (*空调机组01H03-季节模式*)"]
["332.0","验证通过","REAL","空调机组","L","01H03","水阀反馈换算值","空调机组01H03-水阀反馈换算值",{"$f":"E70&VLOOKUP(D70,list!$D$3:$F$501,2,FALSE)&F70&\"_\"&VLOOKUP(G70,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_WVBS"},"LAHU01H03_WVBS AT%M332.0 :REAL; (*空调机组01H03-水阀反馈换算值*)","LAHU01H03_WVBS          AT%M332.0      :REAL; (*空调机组01H03-水阀反馈换算值*)"]
["336.0","验证通过","BOOL","空调机组","L","01H03","水阀手动控制","空调机组01H03-水阀手动控制",{"$f":"E71&VLOOKUP(D71,list!$D$3:$F$501,2,FALSE)&F71&\"_\"&VLOOKUP(G71,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_WVMC"},"LAHU01H03_WVMC AT%M336.0 :BOOL; (*空调机组01H03-水阀手动控制*)","LAHU01H03_WVMC          AT%M336.0      :BOOL; (*空调机组01H03-水阀手动控制*)"]
["340.0","验证通过","REAL","空调机组","L","01H03","水阀手动控制值","空调机组01H03-水阀手动控制值",{"$f":"E72&VLOOKUP(D72,list!$D$3:$F$501,2,FALSE)&F72&\"_\"&VLOOKUP(G72,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_WVMV"},"LAHU01H03_WVMV AT%M340.0 :REAL; (*空调机组01H03-水阀手动控制值*)","LAHU01H03_WVMV          AT%M340.0      :REAL; (*空调机组01H03-水阀手动控制值*)"]
["344.0","验证通过","REAL","空调机组","L","01H03","回风温度换算值","空调机组01H03-回风温度换算值",{"$f":"E73&VLOOKUP(D73,list!$D$3:$F$501,2,FALSE)&F73&\"_\"&VLOOKUP(G73,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_RTS"},"LAHU01H03_RTS AT%M344.0 :REAL; (*空调机组01H03-回风温度换算值*)","LAHU01H03_RTS           AT%M344.0      :REAL; (*空调机组01H03-回风温度换算值*)"]
["348.0","验证通过","BOOL","空调机组","L","01H03","运行时间累积重置","空调机组01H03-运行时间累积重置",{"$f":"E74&VLOOKUP(D74,list!$D$3:$F$501,2,FALSE)&F74&\"_\"&VLOOKUP(G74,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_RST"},"LAHU01H03_RST AT%M348.0 :BOOL; (*空调机组01H03-运行时间累积重置*)","LAHU01H03_RST           AT%M348.0      :BOOL; (*空调机组01H03-运行时间累积重置*)"]
["352.0","验证通过","REAL","空调机组","L","01H03","运行时间累积重置值","空调机组01H03-运行时间累积重置值",{"$f":"E75&VLOOKUP(D75,list!$D$3:$F$501,2,FALSE)&F75&\"_\"&VLOOKUP(G75,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_RSTV"},"LAHU01H03_RSTV AT%M352.0 :REAL; (*空调机组01H03-运行时间累积重置值*)","LAHU01H03_RSTV          AT%M352.0      :REAL; (*空调机组01H03-运行时间累积重置值*)"]
["356.0","验证通过","BOOL","空调机组","L","01H03","隔离开关1","空调机组01H03-隔离开关1",{"$f":"E76&VLOOKUP(D76,list!$D$3:$F$501,2,FALSE)&F76&\"_\"&VLOOKUP(G76,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_ISO1"},"LAHU01H03_ISO1 AT%M356.0 :BOOL; (*空调机组01H03-隔离开关1*)","LAHU01H03_ISO1          AT%M356.0      :BOOL; (*空调机组01H03-隔离开关1*)"]
["358.0","验证通过","BOOL","空调机组","L","01H03","隔离开关2","空调机组01H03-隔离开关2",{"$f":"E77&VLOOKUP(D77,list!$D$3:$F$501,2,FALSE)&F77&\"_\"&VLOOKUP(G77,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_ISO2"},"LAHU01H03_ISO2 AT%M358.0 :BOOL; (*空调机组01H03-隔离开关2*)","LAHU01H03_ISO2          AT%M358.0      :BOOL; (*空调机组01H03-隔离开关2*)"]
["364.0","验证通过","REAL","空调机组","L","01H03","P调节参数","空调机组01H03-P调节参数",{"$f":"E78&VLOOKUP(D78,list!$D$3:$F$501,2,FALSE)&F78&\"_\"&VLOOKUP(G78,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_VP"},"LAHU01H03_VP AT%M364.0 :REAL; (*空调机组01H03-P调节参数*)","LAHU01H03_VP            AT%M364.0      :REAL; (*空调机组01H03-P调节参数*)"]
["368.0","验证通过","REAL","空调机组","L","01H03","I调节参数","空调机组01H03-I调节参数",{"$f":"E79&VLOOKUP(D79,list!$D$3:$F$501,2,FALSE)&F79&\"_\"&VLOOKUP(G79,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_VI"},"LAHU01H03_VI AT%M368.0 :REAL; (*空调机组01H03-I调节参数*)","LAHU01H03_VI            AT%M368.0      :REAL; (*空调机组01H03-I调节参数*)"]
["372.0","验证通过","REAL","空调机组","L","01H03","运行时间累积值","空调机组01H03-运行时间累积值",{"$f":"E80&VLOOKUP(D80,list!$D$3:$F$501,2,FALSE)&F80&\"_\"&VLOOKUP(G80,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_RH"},"LAHU01H03_RH AT%M372.0 :REAL; (*空调机组01H03-运行时间累积值*)","LAHU01H03_RH            AT%M372.0      :REAL; (*空调机组01H03-运行时间累积值*)"]
["376.0","验证通过","INT","空调机组","L","01H03","设备状态代码","空调机组01H03-设备状态代码",{"$f":"E81&VLOOKUP(D81,list!$D$3:$F$501,2,FALSE)&F81&\"_\"&VLOOKUP(G81,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_SN"},"LAHU01H03_SN AT%M376.0 :INT; (*空调机组01H03-设备状态代码*)","LAHU01H03_SN            AT%M376.0      :INT; (*空调机组01H03-设备状态代码*)"]
["378.0","验证通过","INT","空调机组","L","01H03","水阀控制转换值","空调机组01H03-水阀控制转换值",{"$f":"E82&VLOOKUP(D82,list!$D$3:$F$501,2,FALSE)&F82&\"_\"&VLOOKUP(G82,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_WVCS"},"LAHU01H03_WVCS AT%M378.0 :INT; (*空调机组01H03-水阀控制转换值*)","LAHU01H03_WVCS          AT%M378.0      :INT; (*空调机组01H03-水阀控制转换值*)"]
["380.0","验证通过","BOOL","空调机组","L","01H03","程序控制","空调机组01H03-程序控制",{"$f":"E83&VLOOKUP(D83,list!$D$3:$F$501,2,FALSE)&F83&\"_\"&VLOOKUP(G83,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H03_PC"},"LAHU01H03_PC AT%M380.0 :BOOL; (*空调机组01H03-程序控制*)","LAHU01H03_PC            AT%M380.0      :BOOL; (*空调机组01H03-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C83=\"REAL\",C83=\"DWORD\",C83=\"DINT\"),(IF(OR(C85=\"REAL\",C85=\"DWORD\",C85=\"DINT\"),A83+4+MOD(A83,4),A83+4)),(IF(OR(C85=\"REAL\",C85=\"DWORD\",C85=\"DINT\"),A83+4+MOD(A83,4),A83+2)))&\".0\"","v":"384.0"},{"$f":"IF((IF(OR(C85=\"INT\",C85=\"WORD\",C85=\"BOOL\"),MOD(A85,2),MOD(A85,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H04","设定温度值",{"$f":"D85&F85&\"-\"&IF(E85=\"R\",\"新云平台\"&G85,G85)","v":"空调机组01H04-新云平台设定温度值"},{"$f":"E85&VLOOKUP(D85,list!$D$3:$F$501,2,FALSE)&F85&\"_\"&VLOOKUP(G85,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H04_TSET"},{"$f":"I85&\" \"&\"AT%M\"&A85&\" \"&\":\"&C85&\";\"&\" \"&\"(*\"&H85&\"*)\"","v":"RAHU01H04_TSET AT%M384.0 :REAL; (*空调机组01H04-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J85,SEARCH(\"AT%\",J85),,REPT(\" \",25-SEARCH(\"AT%\",J85))),SEARCH(\":\",REPLACE(J85,SEARCH(\"AT%\",J85),,REPT(\" \",25-SEARCH(\"AT%\",J85)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J85,SEARCH(\"AT%\",J85),,REPT(\" \",25-SEARCH(\"AT%\",J85))))))","v":"RAHU01H04_TSET          AT%M384.0      :REAL; (*空调机组01H04-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C85=\"REAL\",C85=\"DWORD\",C85=\"DINT\"),(IF(OR(C86=\"REAL\",C86=\"DWORD\",C86=\"DINT\"),A85+4+MOD(A85,4),A85+4)),(IF(OR(C86=\"REAL\",C86=\"DWORD\",C86=\"DINT\"),A85+4+MOD(A85,4),A85+2)))&\".0\"","v":"388.0"},"验证通过","INT","空调机组","R",{"$f":"F85","v":"01H04"},"季节模式","空调机组01H04-新云平台季节模式",{"$f":"E86&VLOOKUP(D86,list!$D$3:$F$501,2,FALSE)&F86&\"_\"&VLOOKUP(G86,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H04_SM"},"RAHU01H04_SM AT%M388.0 :INT; (*空调机组01H04-新云平台季节模式*)","RAHU01H04_SM            AT%M388.0      :INT; (*空调机组01H04-新云平台季节模式*)"]
["390.0","验证通过","BOOL","空调机组","R","01H04","程序控制","空调机组01H04-新云平台程序控制",{"$f":"E87&VLOOKUP(D87,list!$D$3:$F$501,2,FALSE)&F87&\"_\"&VLOOKUP(G87,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H04_PC"},"RAHU01H04_PC AT%M390.0 :BOOL; (*空调机组01H04-新云平台程序控制*)","RAHU01H04_PC            AT%M390.0      :BOOL; (*空调机组01H04-新云平台程序控制*)"]
["396.0","验证通过","REAL","空调机组","L","01H04","设定温度值","空调机组01H04-设定温度值",{"$f":"E88&VLOOKUP(D88,list!$D$3:$F$501,2,FALSE)&F88&\"_\"&VLOOKUP(G88,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_TSET"},"LAHU01H04_TSET AT%M396.0 :REAL; (*空调机组01H04-设定温度值*)","LAHU01H04_TSET          AT%M396.0      :REAL; (*空调机组01H04-设定温度值*)"]
["400.0","验证通过","INT","空调机组","L","01H04","季节模式","空调机组01H04-季节模式",{"$f":"E89&VLOOKUP(D89,list!$D$3:$F$501,2,FALSE)&F89&\"_\"&VLOOKUP(G89,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_SM"},"LAHU01H04_SM AT%M400.0 :INT; (*空调机组01H04-季节模式*)","LAHU01H04_SM            AT%M400.0      :INT; (*空调机组01H04-季节模式*)"]
["404.0","验证通过","REAL","空调机组","L","01H04","水阀反馈换算值","空调机组01H04-水阀反馈换算值",{"$f":"E90&VLOOKUP(D90,list!$D$3:$F$501,2,FALSE)&F90&\"_\"&VLOOKUP(G90,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_WVBS"},"LAHU01H04_WVBS AT%M404.0 :REAL; (*空调机组01H04-水阀反馈换算值*)","LAHU01H04_WVBS          AT%M404.0      :REAL; (*空调机组01H04-水阀反馈换算值*)"]
["408.0","验证通过","BOOL","空调机组","L","01H04","水阀手动控制","空调机组01H04-水阀手动控制",{"$f":"E91&VLOOKUP(D91,list!$D$3:$F$501,2,FALSE)&F91&\"_\"&VLOOKUP(G91,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_WVMC"},"LAHU01H04_WVMC AT%M408.0 :BOOL; (*空调机组01H04-水阀手动控制*)","LAHU01H04_WVMC          AT%M408.0      :BOOL; (*空调机组01H04-水阀手动控制*)"]
["412.0","验证通过","REAL","空调机组","L","01H04","水阀手动控制值","空调机组01H04-水阀手动控制值",{"$f":"E92&VLOOKUP(D92,list!$D$3:$F$501,2,FALSE)&F92&\"_\"&VLOOKUP(G92,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_WVMV"},"LAHU01H04_WVMV AT%M412.0 :REAL; (*空调机组01H04-水阀手动控制值*)","LAHU01H04_WVMV          AT%M412.0      :REAL; (*空调机组01H04-水阀手动控制值*)"]
["416.0","验证通过","REAL","空调机组","L","01H04","回风温度换算值","空调机组01H04-回风温度换算值",{"$f":"E93&VLOOKUP(D93,list!$D$3:$F$501,2,FALSE)&F93&\"_\"&VLOOKUP(G93,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_RTS"},"LAHU01H04_RTS AT%M416.0 :REAL; (*空调机组01H04-回风温度换算值*)","LAHU01H04_RTS           AT%M416.0      :REAL; (*空调机组01H04-回风温度换算值*)"]
["420.0","验证通过","BOOL","空调机组","L","01H04","运行时间累积重置","空调机组01H04-运行时间累积重置",{"$f":"E94&VLOOKUP(D94,list!$D$3:$F$501,2,FALSE)&F94&\"_\"&VLOOKUP(G94,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_RST"},"LAHU01H04_RST AT%M420.0 :BOOL; (*空调机组01H04-运行时间累积重置*)","LAHU01H04_RST           AT%M420.0      :BOOL; (*空调机组01H04-运行时间累积重置*)"]
["424.0","验证通过","REAL","空调机组","L","01H04","运行时间累积重置值","空调机组01H04-运行时间累积重置值",{"$f":"E95&VLOOKUP(D95,list!$D$3:$F$501,2,FALSE)&F95&\"_\"&VLOOKUP(G95,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_RSTV"},"LAHU01H04_RSTV AT%M424.0 :REAL; (*空调机组01H04-运行时间累积重置值*)","LAHU01H04_RSTV          AT%M424.0      :REAL; (*空调机组01H04-运行时间累积重置值*)"]
["428.0","验证通过","BOOL","空调机组","L","01H04","隔离开关1","空调机组01H04-隔离开关1",{"$f":"E96&VLOOKUP(D96,list!$D$3:$F$501,2,FALSE)&F96&\"_\"&VLOOKUP(G96,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_ISO1"},"LAHU01H04_ISO1 AT%M428.0 :BOOL; (*空调机组01H04-隔离开关1*)","LAHU01H04_ISO1          AT%M428.0      :BOOL; (*空调机组01H04-隔离开关1*)"]
["430.0","验证通过","BOOL","空调机组","L","01H04","隔离开关2","空调机组01H04-隔离开关2",{"$f":"E97&VLOOKUP(D97,list!$D$3:$F$501,2,FALSE)&F97&\"_\"&VLOOKUP(G97,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_ISO2"},"LAHU01H04_ISO2 AT%M430.0 :BOOL; (*空调机组01H04-隔离开关2*)","LAHU01H04_ISO2          AT%M430.0      :BOOL; (*空调机组01H04-隔离开关2*)"]
["436.0","验证通过","REAL","空调机组","L","01H04","P调节参数","空调机组01H04-P调节参数",{"$f":"E98&VLOOKUP(D98,list!$D$3:$F$501,2,FALSE)&F98&\"_\"&VLOOKUP(G98,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_VP"},"LAHU01H04_VP AT%M436.0 :REAL; (*空调机组01H04-P调节参数*)","LAHU01H04_VP            AT%M436.0      :REAL; (*空调机组01H04-P调节参数*)"]
["440.0","验证通过","REAL","空调机组","L","01H04","I调节参数","空调机组01H04-I调节参数",{"$f":"E99&VLOOKUP(D99,list!$D$3:$F$501,2,FALSE)&F99&\"_\"&VLOOKUP(G99,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_VI"},"LAHU01H04_VI AT%M440.0 :REAL; (*空调机组01H04-I调节参数*)","LAHU01H04_VI            AT%M440.0      :REAL; (*空调机组01H04-I调节参数*)"]
["444.0","验证通过","REAL","空调机组","L","01H04","运行时间累积值","空调机组01H04-运行时间累积值",{"$f":"E100&VLOOKUP(D100,list!$D$3:$F$501,2,FALSE)&F100&\"_\"&VLOOKUP(G100,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_RH"},"LAHU01H04_RH AT%M444.0 :REAL; (*空调机组01H04-运行时间累积值*)","LAHU01H04_RH            AT%M444.0      :REAL; (*空调机组01H04-运行时间累积值*)"]
["448.0","验证通过","INT","空调机组","L","01H04","设备状态代码","空调机组01H04-设备状态代码",{"$f":"E101&VLOOKUP(D101,list!$D$3:$F$501,2,FALSE)&F101&\"_\"&VLOOKUP(G101,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_SN"},"LAHU01H04_SN AT%M448.0 :INT; (*空调机组01H04-设备状态代码*)","LAHU01H04_SN            AT%M448.0      :INT; (*空调机组01H04-设备状态代码*)"]
["450.0","验证通过","INT","空调机组","L","01H04","水阀控制转换值","空调机组01H04-水阀控制转换值",{"$f":"E102&VLOOKUP(D102,list!$D$3:$F$501,2,FALSE)&F102&\"_\"&VLOOKUP(G102,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_WVCS"},"LAHU01H04_WVCS AT%M450.0 :INT; (*空调机组01H04-水阀控制转换值*)","LAHU01H04_WVCS          AT%M450.0      :INT; (*空调机组01H04-水阀控制转换值*)"]
["452.0","验证通过","BOOL","空调机组","L","01H04","程序控制","空调机组01H04-程序控制",{"$f":"E103&VLOOKUP(D103,list!$D$3:$F$501,2,FALSE)&F103&\"_\"&VLOOKUP(G103,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H04_PC"},"LAHU01H04_PC AT%M452.0 :BOOL; (*空调机组01H04-程序控制*)","LAHU01H04_PC            AT%M452.0      :BOOL; (*空调机组01H04-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C103=\"REAL\",C103=\"DWORD\",C103=\"DINT\"),(IF(OR(C105=\"REAL\",C105=\"DWORD\",C105=\"DINT\"),A103+4+MOD(A103,4),A103+4)),(IF(OR(C105=\"REAL\",C105=\"DWORD\",C105=\"DINT\"),A103+4+MOD(A103,4),A103+2)))&\".0\"","v":"456.0"},{"$f":"IF((IF(OR(C105=\"INT\",C105=\"WORD\",C105=\"BOOL\"),MOD(A105,2),MOD(A105,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H05","设定温度值",{"$f":"D105&F105&\"-\"&IF(E105=\"R\",\"新云平台\"&G105,G105)","v":"空调机组01H05-新云平台设定温度值"},{"$f":"E105&VLOOKUP(D105,list!$D$3:$F$501,2,FALSE)&F105&\"_\"&VLOOKUP(G105,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H05_TSET"},{"$f":"I105&\" \"&\"AT%M\"&A105&\" \"&\":\"&C105&\";\"&\" \"&\"(*\"&H105&\"*)\"","v":"RAHU01H05_TSET AT%M456.0 :REAL; (*空调机组01H05-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J105,SEARCH(\"AT%\",J105),,REPT(\" \",25-SEARCH(\"AT%\",J105))),SEARCH(\":\",REPLACE(J105,SEARCH(\"AT%\",J105),,REPT(\" \",25-SEARCH(\"AT%\",J105)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J105,SEARCH(\"AT%\",J105),,REPT(\" \",25-SEARCH(\"AT%\",J105))))))","v":"RAHU01H05_TSET          AT%M456.0      :REAL; (*空调机组01H05-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C105=\"REAL\",C105=\"DWORD\",C105=\"DINT\"),(IF(OR(C106=\"REAL\",C106=\"DWORD\",C106=\"DINT\"),A105+4+MOD(A105,4),A105+4)),(IF(OR(C106=\"REAL\",C106=\"DWORD\",C106=\"DINT\"),A105+4+MOD(A105,4),A105+2)))&\".0\"","v":"460.0"},"验证通过","INT","空调机组","R",{"$f":"F105","v":"01H05"},"季节模式","空调机组01H05-新云平台季节模式",{"$f":"E106&VLOOKUP(D106,list!$D$3:$F$501,2,FALSE)&F106&\"_\"&VLOOKUP(G106,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H05_SM"},"RAHU01H05_SM AT%M460.0 :INT; (*空调机组01H05-新云平台季节模式*)","RAHU01H05_SM            AT%M460.0      :INT; (*空调机组01H05-新云平台季节模式*)"]
["462.0","验证通过","BOOL","空调机组","R","01H05","程序控制","空调机组01H05-新云平台程序控制",{"$f":"E107&VLOOKUP(D107,list!$D$3:$F$501,2,FALSE)&F107&\"_\"&VLOOKUP(G107,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H05_PC"},"RAHU01H05_PC AT%M462.0 :BOOL; (*空调机组01H05-新云平台程序控制*)","RAHU01H05_PC            AT%M462.0      :BOOL; (*空调机组01H05-新云平台程序控制*)"]
["468.0","验证通过","REAL","空调机组","L","01H05","设定温度值","空调机组01H05-设定温度值",{"$f":"E108&VLOOKUP(D108,list!$D$3:$F$501,2,FALSE)&F108&\"_\"&VLOOKUP(G108,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_TSET"},"LAHU01H05_TSET AT%M468.0 :REAL; (*空调机组01H05-设定温度值*)","LAHU01H05_TSET          AT%M468.0      :REAL; (*空调机组01H05-设定温度值*)"]
["472.0","验证通过","INT","空调机组","L","01H05","季节模式","空调机组01H05-季节模式",{"$f":"E109&VLOOKUP(D109,list!$D$3:$F$501,2,FALSE)&F109&\"_\"&VLOOKUP(G109,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_SM"},"LAHU01H05_SM AT%M472.0 :INT; (*空调机组01H05-季节模式*)","LAHU01H05_SM            AT%M472.0      :INT; (*空调机组01H05-季节模式*)"]
["476.0","验证通过","REAL","空调机组","L","01H05","水阀反馈换算值","空调机组01H05-水阀反馈换算值",{"$f":"E110&VLOOKUP(D110,list!$D$3:$F$501,2,FALSE)&F110&\"_\"&VLOOKUP(G110,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_WVBS"},"LAHU01H05_WVBS AT%M476.0 :REAL; (*空调机组01H05-水阀反馈换算值*)","LAHU01H05_WVBS          AT%M476.0      :REAL; (*空调机组01H05-水阀反馈换算值*)"]
["480.0","验证通过","BOOL","空调机组","L","01H05","水阀手动控制","空调机组01H05-水阀手动控制",{"$f":"E111&VLOOKUP(D111,list!$D$3:$F$501,2,FALSE)&F111&\"_\"&VLOOKUP(G111,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_WVMC"},"LAHU01H05_WVMC AT%M480.0 :BOOL; (*空调机组01H05-水阀手动控制*)","LAHU01H05_WVMC          AT%M480.0      :BOOL; (*空调机组01H05-水阀手动控制*)"]
["484.0","验证通过","REAL","空调机组","L","01H05","水阀手动控制值","空调机组01H05-水阀手动控制值",{"$f":"E112&VLOOKUP(D112,list!$D$3:$F$501,2,FALSE)&F112&\"_\"&VLOOKUP(G112,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_WVMV"},"LAHU01H05_WVMV AT%M484.0 :REAL; (*空调机组01H05-水阀手动控制值*)","LAHU01H05_WVMV          AT%M484.0      :REAL; (*空调机组01H05-水阀手动控制值*)"]
["488.0","验证通过","REAL","空调机组","L","01H05","回风温度换算值","空调机组01H05-回风温度换算值",{"$f":"E113&VLOOKUP(D113,list!$D$3:$F$501,2,FALSE)&F113&\"_\"&VLOOKUP(G113,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_RTS"},"LAHU01H05_RTS AT%M488.0 :REAL; (*空调机组01H05-回风温度换算值*)","LAHU01H05_RTS           AT%M488.0      :REAL; (*空调机组01H05-回风温度换算值*)"]
["492.0","验证通过","BOOL","空调机组","L","01H05","运行时间累积重置","空调机组01H05-运行时间累积重置",{"$f":"E114&VLOOKUP(D114,list!$D$3:$F$501,2,FALSE)&F114&\"_\"&VLOOKUP(G114,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_RST"},"LAHU01H05_RST AT%M492.0 :BOOL; (*空调机组01H05-运行时间累积重置*)","LAHU01H05_RST           AT%M492.0      :BOOL; (*空调机组01H05-运行时间累积重置*)"]
["496.0","验证通过","REAL","空调机组","L","01H05","运行时间累积重置值","空调机组01H05-运行时间累积重置值",{"$f":"E115&VLOOKUP(D115,list!$D$3:$F$501,2,FALSE)&F115&\"_\"&VLOOKUP(G115,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_RSTV"},"LAHU01H05_RSTV AT%M496.0 :REAL; (*空调机组01H05-运行时间累积重置值*)","LAHU01H05_RSTV          AT%M496.0      :REAL; (*空调机组01H05-运行时间累积重置值*)"]
["500.0","验证通过","BOOL","空调机组","L","01H05","隔离开关1","空调机组01H05-隔离开关1",{"$f":"E116&VLOOKUP(D116,list!$D$3:$F$501,2,FALSE)&F116&\"_\"&VLOOKUP(G116,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_ISO1"},"LAHU01H05_ISO1 AT%M500.0 :BOOL; (*空调机组01H05-隔离开关1*)","LAHU01H05_ISO1          AT%M500.0      :BOOL; (*空调机组01H05-隔离开关1*)"]
["502.0","验证通过","BOOL","空调机组","L","01H05","隔离开关2","空调机组01H05-隔离开关2",{"$f":"E117&VLOOKUP(D117,list!$D$3:$F$501,2,FALSE)&F117&\"_\"&VLOOKUP(G117,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_ISO2"},"LAHU01H05_ISO2 AT%M502.0 :BOOL; (*空调机组01H05-隔离开关2*)","LAHU01H05_ISO2          AT%M502.0      :BOOL; (*空调机组01H05-隔离开关2*)"]
["508.0","验证通过","REAL","空调机组","L","01H05","P调节参数","空调机组01H05-P调节参数",{"$f":"E118&VLOOKUP(D118,list!$D$3:$F$501,2,FALSE)&F118&\"_\"&VLOOKUP(G118,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_VP"},"LAHU01H05_VP AT%M508.0 :REAL; (*空调机组01H05-P调节参数*)","LAHU01H05_VP            AT%M508.0      :REAL; (*空调机组01H05-P调节参数*)"]
["512.0","验证通过","REAL","空调机组","L","01H05","I调节参数","空调机组01H05-I调节参数",{"$f":"E119&VLOOKUP(D119,list!$D$3:$F$501,2,FALSE)&F119&\"_\"&VLOOKUP(G119,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_VI"},"LAHU01H05_VI AT%M512.0 :REAL; (*空调机组01H05-I调节参数*)","LAHU01H05_VI            AT%M512.0      :REAL; (*空调机组01H05-I调节参数*)"]
["516.0","验证通过","REAL","空调机组","L","01H05","运行时间累积值","空调机组01H05-运行时间累积值",{"$f":"E120&VLOOKUP(D120,list!$D$3:$F$501,2,FALSE)&F120&\"_\"&VLOOKUP(G120,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_RH"},"LAHU01H05_RH AT%M516.0 :REAL; (*空调机组01H05-运行时间累积值*)","LAHU01H05_RH            AT%M516.0      :REAL; (*空调机组01H05-运行时间累积值*)"]
["520.0","验证通过","INT","空调机组","L","01H05","设备状态代码","空调机组01H05-设备状态代码",{"$f":"E121&VLOOKUP(D121,list!$D$3:$F$501,2,FALSE)&F121&\"_\"&VLOOKUP(G121,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_SN"},"LAHU01H05_SN AT%M520.0 :INT; (*空调机组01H05-设备状态代码*)","LAHU01H05_SN            AT%M520.0      :INT; (*空调机组01H05-设备状态代码*)"]
["522.0","验证通过","INT","空调机组","L","01H05","水阀控制转换值","空调机组01H05-水阀控制转换值",{"$f":"E122&VLOOKUP(D122,list!$D$3:$F$501,2,FALSE)&F122&\"_\"&VLOOKUP(G122,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_WVCS"},"LAHU01H05_WVCS AT%M522.0 :INT; (*空调机组01H05-水阀控制转换值*)","LAHU01H05_WVCS          AT%M522.0      :INT; (*空调机组01H05-水阀控制转换值*)"]
["524.0","验证通过","BOOL","空调机组","L","01H05","程序控制","空调机组01H05-程序控制",{"$f":"E123&VLOOKUP(D123,list!$D$3:$F$501,2,FALSE)&F123&\"_\"&VLOOKUP(G123,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H05_PC"},"LAHU01H05_PC AT%M524.0 :BOOL; (*空调机组01H05-程序控制*)","LAHU01H05_PC            AT%M524.0      :BOOL; (*空调机组01H05-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C123=\"REAL\",C123=\"DWORD\",C123=\"DINT\"),(IF(OR(C125=\"REAL\",C125=\"DWORD\",C125=\"DINT\"),A123+4+MOD(A123,4),A123+4)),(IF(OR(C125=\"REAL\",C125=\"DWORD\",C125=\"DINT\"),A123+4+MOD(A123,4),A123+2)))&\".0\"","v":"528.0"},{"$f":"IF((IF(OR(C125=\"INT\",C125=\"WORD\",C125=\"BOOL\"),MOD(A125,2),MOD(A125,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H06","设定温度值",{"$f":"D125&F125&\"-\"&IF(E125=\"R\",\"新云平台\"&G125,G125)","v":"空调机组01H06-新云平台设定温度值"},{"$f":"E125&VLOOKUP(D125,list!$D$3:$F$501,2,FALSE)&F125&\"_\"&VLOOKUP(G125,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H06_TSET"},{"$f":"I125&\" \"&\"AT%M\"&A125&\" \"&\":\"&C125&\";\"&\" \"&\"(*\"&H125&\"*)\"","v":"RAHU01H06_TSET AT%M528.0 :REAL; (*空调机组01H06-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J125,SEARCH(\"AT%\",J125),,REPT(\" \",25-SEARCH(\"AT%\",J125))),SEARCH(\":\",REPLACE(J125,SEARCH(\"AT%\",J125),,REPT(\" \",25-SEARCH(\"AT%\",J125)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J125,SEARCH(\"AT%\",J125),,REPT(\" \",25-SEARCH(\"AT%\",J125))))))","v":"RAHU01H06_TSET          AT%M528.0      :REAL; (*空调机组01H06-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C125=\"REAL\",C125=\"DWORD\",C125=\"DINT\"),(IF(OR(C126=\"REAL\",C126=\"DWORD\",C126=\"DINT\"),A125+4+MOD(A125,4),A125+4)),(IF(OR(C126=\"REAL\",C126=\"DWORD\",C126=\"DINT\"),A125+4+MOD(A125,4),A125+2)))&\".0\"","v":"532.0"},"验证通过","INT","空调机组","R",{"$f":"F125","v":"01H06"},"季节模式","空调机组01H06-新云平台季节模式",{"$f":"E126&VLOOKUP(D126,list!$D$3:$F$501,2,FALSE)&F126&\"_\"&VLOOKUP(G126,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H06_SM"},"RAHU01H06_SM AT%M532.0 :INT; (*空调机组01H06-新云平台季节模式*)","RAHU01H06_SM            AT%M532.0      :INT; (*空调机组01H06-新云平台季节模式*)"]
["534.0","验证通过","BOOL","空调机组","R","01H06","程序控制","空调机组01H06-新云平台程序控制",{"$f":"E127&VLOOKUP(D127,list!$D$3:$F$501,2,FALSE)&F127&\"_\"&VLOOKUP(G127,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H06_PC"},"RAHU01H06_PC AT%M534.0 :BOOL; (*空调机组01H06-新云平台程序控制*)","RAHU01H06_PC            AT%M534.0      :BOOL; (*空调机组01H06-新云平台程序控制*)"]
["540.0","验证通过","REAL","空调机组","L","01H06","设定温度值","空调机组01H06-设定温度值",{"$f":"E128&VLOOKUP(D128,list!$D$3:$F$501,2,FALSE)&F128&\"_\"&VLOOKUP(G128,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_TSET"},"LAHU01H06_TSET AT%M540.0 :REAL; (*空调机组01H06-设定温度值*)","LAHU01H06_TSET          AT%M540.0      :REAL; (*空调机组01H06-设定温度值*)"]
["544.0","验证通过","INT","空调机组","L","01H06","季节模式","空调机组01H06-季节模式",{"$f":"E129&VLOOKUP(D129,list!$D$3:$F$501,2,FALSE)&F129&\"_\"&VLOOKUP(G129,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_SM"},"LAHU01H06_SM AT%M544.0 :INT; (*空调机组01H06-季节模式*)","LAHU01H06_SM            AT%M544.0      :INT; (*空调机组01H06-季节模式*)"]
["548.0","验证通过","REAL","空调机组","L","01H06","水阀反馈换算值","空调机组01H06-水阀反馈换算值",{"$f":"E130&VLOOKUP(D130,list!$D$3:$F$501,2,FALSE)&F130&\"_\"&VLOOKUP(G130,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVBS"},"LAHU01H06_WVBS AT%M548.0 :REAL; (*空调机组01H06-水阀反馈换算值*)","LAHU01H06_WVBS          AT%M548.0      :REAL; (*空调机组01H06-水阀反馈换算值*)"]
["552.0","验证通过","BOOL","空调机组","L","01H06","水阀手动控制","空调机组01H06-水阀手动控制",{"$f":"E131&VLOOKUP(D131,list!$D$3:$F$501,2,FALSE)&F131&\"_\"&VLOOKUP(G131,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVMC"},"LAHU01H06_WVMC AT%M552.0 :BOOL; (*空调机组01H06-水阀手动控制*)","LAHU01H06_WVMC          AT%M552.0      :BOOL; (*空调机组01H06-水阀手动控制*)"]
["556.0","验证通过","REAL","空调机组","L","01H06","水阀手动控制值","空调机组01H06-水阀手动控制值",{"$f":"E132&VLOOKUP(D132,list!$D$3:$F$501,2,FALSE)&F132&\"_\"&VLOOKUP(G132,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVMV"},"LAHU01H06_WVMV AT%M556.0 :REAL; (*空调机组01H06-水阀手动控制值*)","LAHU01H06_WVMV          AT%M556.0      :REAL; (*空调机组01H06-水阀手动控制值*)"]
["560.0","验证通过","REAL","空调机组","L","01H06","回风温度换算值","空调机组01H06-回风温度换算值",{"$f":"E133&VLOOKUP(D133,list!$D$3:$F$501,2,FALSE)&F133&\"_\"&VLOOKUP(G133,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RTS"},"LAHU01H06_RTS AT%M560.0 :REAL; (*空调机组01H06-回风温度换算值*)","LAHU01H06_RTS           AT%M560.0      :REAL; (*空调机组01H06-回风温度换算值*)"]
["564.0","验证通过","BOOL","空调机组","L","01H06","运行时间累积重置","空调机组01H06-运行时间累积重置",{"$f":"E134&VLOOKUP(D134,list!$D$3:$F$501,2,FALSE)&F134&\"_\"&VLOOKUP(G134,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RST"},"LAHU01H06_RST AT%M564.0 :BOOL; (*空调机组01H06-运行时间累积重置*)","LAHU01H06_RST           AT%M564.0      :BOOL; (*空调机组01H06-运行时间累积重置*)"]
["568.0","验证通过","REAL","空调机组","L","01H06","运行时间累积重置值","空调机组01H06-运行时间累积重置值",{"$f":"E135&VLOOKUP(D135,list!$D$3:$F$501,2,FALSE)&F135&\"_\"&VLOOKUP(G135,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RSTV"},"LAHU01H06_RSTV AT%M568.0 :REAL; (*空调机组01H06-运行时间累积重置值*)","LAHU01H06_RSTV          AT%M568.0      :REAL; (*空调机组01H06-运行时间累积重置值*)"]
["572.0","验证通过","BOOL","空调机组","L","01H06","隔离开关1","空调机组01H06-隔离开关1",{"$f":"E136&VLOOKUP(D136,list!$D$3:$F$501,2,FALSE)&F136&\"_\"&VLOOKUP(G136,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_ISO1"},"LAHU01H06_ISO1 AT%M572.0 :BOOL; (*空调机组01H06-隔离开关1*)","LAHU01H06_ISO1          AT%M572.0      :BOOL; (*空调机组01H06-隔离开关1*)"]
["574.0","验证通过","BOOL","空调机组","L","01H06","隔离开关2","空调机组01H06-隔离开关2",{"$f":"E137&VLOOKUP(D137,list!$D$3:$F$501,2,FALSE)&F137&\"_\"&VLOOKUP(G137,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_ISO2"},"LAHU01H06_ISO2 AT%M574.0 :BOOL; (*空调机组01H06-隔离开关2*)","LAHU01H06_ISO2          AT%M574.0      :BOOL; (*空调机组01H06-隔离开关2*)"]
["580.0","验证通过","REAL","空调机组","L","01H06","P调节参数","空调机组01H06-P调节参数",{"$f":"E138&VLOOKUP(D138,list!$D$3:$F$501,2,FALSE)&F138&\"_\"&VLOOKUP(G138,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_VP"},"LAHU01H06_VP AT%M580.0 :REAL; (*空调机组01H06-P调节参数*)","LAHU01H06_VP            AT%M580.0      :REAL; (*空调机组01H06-P调节参数*)"]
["584.0","验证通过","REAL","空调机组","L","01H06","I调节参数","空调机组01H06-I调节参数",{"$f":"E139&VLOOKUP(D139,list!$D$3:$F$501,2,FALSE)&F139&\"_\"&VLOOKUP(G139,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_VI"},"LAHU01H06_VI AT%M584.0 :REAL; (*空调机组01H06-I调节参数*)","LAHU01H06_VI            AT%M584.0      :REAL; (*空调机组01H06-I调节参数*)"]
["588.0","验证通过","REAL","空调机组","L","01H06","运行时间累积值","空调机组01H06-运行时间累积值",{"$f":"E140&VLOOKUP(D140,list!$D$3:$F$501,2,FALSE)&F140&\"_\"&VLOOKUP(G140,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RH"},"LAHU01H06_RH AT%M588.0 :REAL; (*空调机组01H06-运行时间累积值*)","LAHU01H06_RH            AT%M588.0      :REAL; (*空调机组01H06-运行时间累积值*)"]
["592.0","验证通过","INT","空调机组","L","01H06","设备状态代码","空调机组01H06-设备状态代码",{"$f":"E141&VLOOKUP(D141,list!$D$3:$F$501,2,FALSE)&F141&\"_\"&VLOOKUP(G141,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_SN"},"LAHU01H06_SN AT%M592.0 :INT; (*空调机组01H06-设备状态代码*)","LAHU01H06_SN            AT%M592.0      :INT; (*空调机组01H06-设备状态代码*)"]
["594.0","验证通过","INT","空调机组","L","01H06","水阀控制转换值","空调机组01H06-水阀控制转换值",{"$f":"E142&VLOOKUP(D142,list!$D$3:$F$501,2,FALSE)&F142&\"_\"&VLOOKUP(G142,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVCS"},"LAHU01H06_WVCS AT%M594.0 :INT; (*空调机组01H06-水阀控制转换值*)","LAHU01H06_WVCS          AT%M594.0      :INT; (*空调机组01H06-水阀控制转换值*)"]
["596.0","验证通过","BOOL","空调机组","L","01H06","程序控制","空调机组01H06-程序控制",{"$f":"E143&VLOOKUP(D143,list!$D$3:$F$501,2,FALSE)&F143&\"_\"&VLOOKUP(G143,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_PC"},"LAHU01H06_PC AT%M596.0 :BOOL; (*空调机组01H06-程序控制*)","LAHU01H06_PC            AT%M596.0      :BOOL; (*空调机组01H06-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C143=\"REAL\",C143=\"DWORD\",C143=\"DINT\"),(IF(OR(C145=\"REAL\",C145=\"DWORD\",C145=\"DINT\"),A143+4+MOD(A143,4),A143+4)),(IF(OR(C145=\"REAL\",C145=\"DWORD\",C145=\"DINT\"),A143+4+MOD(A143,4),A143+2)))&\".0\"","v":"600.0"},{"$f":"IF((IF(OR(C145=\"INT\",C145=\"WORD\",C145=\"BOOL\"),MOD(A145,2),MOD(A145,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H07","设定温度值",{"$f":"D145&F145&\"-\"&IF(E145=\"R\",\"新云平台\"&G145,G145)","v":"空调机组01H07-新云平台设定温度值"},{"$f":"E145&VLOOKUP(D145,list!$D$3:$F$501,2,FALSE)&F145&\"_\"&VLOOKUP(G145,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_TSET"},{"$f":"I145&\" \"&\"AT%M\"&A145&\" \"&\":\"&C145&\";\"&\" \"&\"(*\"&H145&\"*)\"","v":"RAHU01H07_TSET AT%M600.0 :REAL; (*空调机组01H07-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J145,SEARCH(\"AT%\",J145),,REPT(\" \",25-SEARCH(\"AT%\",J145))),SEARCH(\":\",REPLACE(J145,SEARCH(\"AT%\",J145),,REPT(\" \",25-SEARCH(\"AT%\",J145)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J145,SEARCH(\"AT%\",J145),,REPT(\" \",25-SEARCH(\"AT%\",J145))))))","v":"RAHU01H07_TSET          AT%M600.0      :REAL; (*空调机组01H07-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C145=\"REAL\",C145=\"DWORD\",C145=\"DINT\"),(IF(OR(C146=\"REAL\",C146=\"DWORD\",C146=\"DINT\"),A145+4+MOD(A145,4),A145+4)),(IF(OR(C146=\"REAL\",C146=\"DWORD\",C146=\"DINT\"),A145+4+MOD(A145,4),A145+2)))&\".0\"","v":"604.0"},"验证通过","INT","空调机组","R",{"$f":"F145","v":"01H07"},"季节模式","空调机组01H07-新云平台季节模式",{"$f":"E146&VLOOKUP(D146,list!$D$3:$F$501,2,FALSE)&F146&\"_\"&VLOOKUP(G146,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_SM"},"RAHU01H07_SM AT%M604.0 :INT; (*空调机组01H07-新云平台季节模式*)","RAHU01H07_SM            AT%M604.0      :INT; (*空调机组01H07-新云平台季节模式*)"]
["606.0","验证通过","BOOL","空调机组","R","01H07","程序控制","空调机组01H07-新云平台程序控制",{"$f":"E147&VLOOKUP(D147,list!$D$3:$F$501,2,FALSE)&F147&\"_\"&VLOOKUP(G147,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_PC"},"RAHU01H07_PC AT%M606.0 :BOOL; (*空调机组01H07-新云平台程序控制*)","RAHU01H07_PC            AT%M606.0      :BOOL; (*空调机组01H07-新云平台程序控制*)"]
["612.0","验证通过","REAL","空调机组","L","01H07","设定温度值","空调机组01H07-设定温度值",{"$f":"E148&VLOOKUP(D148,list!$D$3:$F$501,2,FALSE)&F148&\"_\"&VLOOKUP(G148,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_TSET"},"LAHU01H07_TSET AT%M612.0 :REAL; (*空调机组01H07-设定温度值*)","LAHU01H07_TSET          AT%M612.0      :REAL; (*空调机组01H07-设定温度值*)"]
["616.0","验证通过","INT","空调机组","L","01H07","季节模式","空调机组01H07-季节模式",{"$f":"E149&VLOOKUP(D149,list!$D$3:$F$501,2,FALSE)&F149&\"_\"&VLOOKUP(G149,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_SM"},"LAHU01H07_SM AT%M616.0 :INT; (*空调机组01H07-季节模式*)","LAHU01H07_SM            AT%M616.0      :INT; (*空调机组01H07-季节模式*)"]
["620.0","验证通过","REAL","空调机组","L","01H07","水阀反馈换算值","空调机组01H07-水阀反馈换算值",{"$f":"E150&VLOOKUP(D150,list!$D$3:$F$501,2,FALSE)&F150&\"_\"&VLOOKUP(G150,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVBS"},"LAHU01H07_WVBS AT%M620.0 :REAL; (*空调机组01H07-水阀反馈换算值*)","LAHU01H07_WVBS          AT%M620.0      :REAL; (*空调机组01H07-水阀反馈换算值*)"]
["624.0","验证通过","BOOL","空调机组","L","01H07","水阀手动控制","空调机组01H07-水阀手动控制",{"$f":"E151&VLOOKUP(D151,list!$D$3:$F$501,2,FALSE)&F151&\"_\"&VLOOKUP(G151,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVMC"},"LAHU01H07_WVMC AT%M624.0 :BOOL; (*空调机组01H07-水阀手动控制*)","LAHU01H07_WVMC          AT%M624.0      :BOOL; (*空调机组01H07-水阀手动控制*)"]
["628.0","验证通过","REAL","空调机组","L","01H07","水阀手动控制值","空调机组01H07-水阀手动控制值",{"$f":"E152&VLOOKUP(D152,list!$D$3:$F$501,2,FALSE)&F152&\"_\"&VLOOKUP(G152,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVMV"},"LAHU01H07_WVMV AT%M628.0 :REAL; (*空调机组01H07-水阀手动控制值*)","LAHU01H07_WVMV          AT%M628.0      :REAL; (*空调机组01H07-水阀手动控制值*)"]
["632.0","验证通过","REAL","空调机组","L","01H07","回风温度换算值","空调机组01H07-回风温度换算值",{"$f":"E153&VLOOKUP(D153,list!$D$3:$F$501,2,FALSE)&F153&\"_\"&VLOOKUP(G153,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RTS"},"LAHU01H07_RTS AT%M632.0 :REAL; (*空调机组01H07-回风温度换算值*)","LAHU01H07_RTS           AT%M632.0      :REAL; (*空调机组01H07-回风温度换算值*)"]
["636.0","验证通过","BOOL","空调机组","L","01H07","运行时间累积重置","空调机组01H07-运行时间累积重置",{"$f":"E154&VLOOKUP(D154,list!$D$3:$F$501,2,FALSE)&F154&\"_\"&VLOOKUP(G154,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RST"},"LAHU01H07_RST AT%M636.0 :BOOL; (*空调机组01H07-运行时间累积重置*)","LAHU01H07_RST           AT%M636.0      :BOOL; (*空调机组01H07-运行时间累积重置*)"]
["640.0","验证通过","REAL","空调机组","L","01H07","运行时间累积重置值","空调机组01H07-运行时间累积重置值",{"$f":"E155&VLOOKUP(D155,list!$D$3:$F$501,2,FALSE)&F155&\"_\"&VLOOKUP(G155,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RSTV"},"LAHU01H07_RSTV AT%M640.0 :REAL; (*空调机组01H07-运行时间累积重置值*)","LAHU01H07_RSTV          AT%M640.0      :REAL; (*空调机组01H07-运行时间累积重置值*)"]
["644.0","验证通过","BOOL","空调机组","L","01H07","隔离开关1","空调机组01H07-隔离开关1",{"$f":"E156&VLOOKUP(D156,list!$D$3:$F$501,2,FALSE)&F156&\"_\"&VLOOKUP(G156,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_ISO1"},"LAHU01H07_ISO1 AT%M644.0 :BOOL; (*空调机组01H07-隔离开关1*)","LAHU01H07_ISO1          AT%M644.0      :BOOL; (*空调机组01H07-隔离开关1*)"]
["646.0","验证通过","BOOL","空调机组","L","01H07","隔离开关2","空调机组01H07-隔离开关2",{"$f":"E157&VLOOKUP(D157,list!$D$3:$F$501,2,FALSE)&F157&\"_\"&VLOOKUP(G157,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_ISO2"},"LAHU01H07_ISO2 AT%M646.0 :BOOL; (*空调机组01H07-隔离开关2*)","LAHU01H07_ISO2          AT%M646.0      :BOOL; (*空调机组01H07-隔离开关2*)"]
["652.0","验证通过","REAL","空调机组","L","01H07","P调节参数","空调机组01H07-P调节参数",{"$f":"E158&VLOOKUP(D158,list!$D$3:$F$501,2,FALSE)&F158&\"_\"&VLOOKUP(G158,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_VP"},"LAHU01H07_VP AT%M652.0 :REAL; (*空调机组01H07-P调节参数*)","LAHU01H07_VP            AT%M652.0      :REAL; (*空调机组01H07-P调节参数*)"]
["656.0","验证通过","REAL","空调机组","L","01H07","I调节参数","空调机组01H07-I调节参数",{"$f":"E159&VLOOKUP(D159,list!$D$3:$F$501,2,FALSE)&F159&\"_\"&VLOOKUP(G159,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_VI"},"LAHU01H07_VI AT%M656.0 :REAL; (*空调机组01H07-I调节参数*)","LAHU01H07_VI            AT%M656.0      :REAL; (*空调机组01H07-I调节参数*)"]
["660.0","验证通过","REAL","空调机组","L","01H07","运行时间累积值","空调机组01H07-运行时间累积值",{"$f":"E160&VLOOKUP(D160,list!$D$3:$F$501,2,FALSE)&F160&\"_\"&VLOOKUP(G160,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RH"},"LAHU01H07_RH AT%M660.0 :REAL; (*空调机组01H07-运行时间累积值*)","LAHU01H07_RH            AT%M660.0      :REAL; (*空调机组01H07-运行时间累积值*)"]
["664.0","验证通过","INT","空调机组","L","01H07","设备状态代码","空调机组01H07-设备状态代码",{"$f":"E161&VLOOKUP(D161,list!$D$3:$F$501,2,FALSE)&F161&\"_\"&VLOOKUP(G161,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_SN"},"LAHU01H07_SN AT%M664.0 :INT; (*空调机组01H07-设备状态代码*)","LAHU01H07_SN            AT%M664.0      :INT; (*空调机组01H07-设备状态代码*)"]
["666.0","验证通过","INT","空调机组","L","01H07","水阀控制转换值","空调机组01H07-水阀控制转换值",{"$f":"E162&VLOOKUP(D162,list!$D$3:$F$501,2,FALSE)&F162&\"_\"&VLOOKUP(G162,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVCS"},"LAHU01H07_WVCS AT%M666.0 :INT; (*空调机组01H07-水阀控制转换值*)","LAHU01H07_WVCS          AT%M666.0      :INT; (*空调机组01H07-水阀控制转换值*)"]
["668.0","验证通过","BOOL","空调机组","L","01H07","程序控制","空调机组01H07-程序控制",{"$f":"E163&VLOOKUP(D163,list!$D$3:$F$501,2,FALSE)&F163&\"_\"&VLOOKUP(G163,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_PC"},"LAHU01H07_PC AT%M668.0 :BOOL; (*空调机组01H07-程序控制*)","LAHU01H07_PC            AT%M668.0      :BOOL; (*空调机组01H07-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C163=\"REAL\",C163=\"DWORD\",C163=\"DINT\"),(IF(OR(C165=\"REAL\",C165=\"DWORD\",C165=\"DINT\"),A163+4+MOD(A163,4),A163+4)),(IF(OR(C165=\"REAL\",C165=\"DWORD\",C165=\"DINT\"),A163+4+MOD(A163,4),A163+2)))&\".0\"","v":"672.0"},{"$f":"IF((IF(OR(C165=\"INT\",C165=\"WORD\",C165=\"BOOL\"),MOD(A165,2),MOD(A165,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H08","设定温度值",{"$f":"D165&F165&\"-\"&IF(E165=\"R\",\"新云平台\"&G165,G165)","v":"空调机组01H08-新云平台设定温度值"},{"$f":"E165&VLOOKUP(D165,list!$D$3:$F$501,2,FALSE)&F165&\"_\"&VLOOKUP(G165,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_TSET"},{"$f":"I165&\" \"&\"AT%M\"&A165&\" \"&\":\"&C165&\";\"&\" \"&\"(*\"&H165&\"*)\"","v":"RAHU01H08_TSET AT%M672.0 :REAL; (*空调机组01H08-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J165,SEARCH(\"AT%\",J165),,REPT(\" \",25-SEARCH(\"AT%\",J165))),SEARCH(\":\",REPLACE(J165,SEARCH(\"AT%\",J165),,REPT(\" \",25-SEARCH(\"AT%\",J165)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J165,SEARCH(\"AT%\",J165),,REPT(\" \",25-SEARCH(\"AT%\",J165))))))","v":"RAHU01H08_TSET          AT%M672.0      :REAL; (*空调机组01H08-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C165=\"REAL\",C165=\"DWORD\",C165=\"DINT\"),(IF(OR(C166=\"REAL\",C166=\"DWORD\",C166=\"DINT\"),A165+4+MOD(A165,4),A165+4)),(IF(OR(C166=\"REAL\",C166=\"DWORD\",C166=\"DINT\"),A165+4+MOD(A165,4),A165+2)))&\".0\"","v":"676.0"},"验证通过","INT","空调机组","R",{"$f":"F165","v":"01H08"},"季节模式","空调机组01H08-新云平台季节模式",{"$f":"E166&VLOOKUP(D166,list!$D$3:$F$501,2,FALSE)&F166&\"_\"&VLOOKUP(G166,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_SM"},"RAHU01H08_SM AT%M676.0 :INT; (*空调机组01H08-新云平台季节模式*)","RAHU01H08_SM            AT%M676.0      :INT; (*空调机组01H08-新云平台季节模式*)"]
["678.0","验证通过","BOOL","空调机组","R","01H08","程序控制","空调机组01H08-新云平台程序控制",{"$f":"E167&VLOOKUP(D167,list!$D$3:$F$501,2,FALSE)&F167&\"_\"&VLOOKUP(G167,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_PC"},"RAHU01H08_PC AT%M678.0 :BOOL; (*空调机组01H08-新云平台程序控制*)","RAHU01H08_PC            AT%M678.0      :BOOL; (*空调机组01H08-新云平台程序控制*)"]
["684.0","验证通过","REAL","空调机组","L","01H08","设定温度值","空调机组01H08-设定温度值",{"$f":"E168&VLOOKUP(D168,list!$D$3:$F$501,2,FALSE)&F168&\"_\"&VLOOKUP(G168,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_TSET"},"LAHU01H08_TSET AT%M684.0 :REAL; (*空调机组01H08-设定温度值*)","LAHU01H08_TSET          AT%M684.0      :REAL; (*空调机组01H08-设定温度值*)"]
["688.0","验证通过","INT","空调机组","L","01H08","季节模式","空调机组01H08-季节模式",{"$f":"E169&VLOOKUP(D169,list!$D$3:$F$501,2,FALSE)&F169&\"_\"&VLOOKUP(G169,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_SM"},"LAHU01H08_SM AT%M688.0 :INT; (*空调机组01H08-季节模式*)","LAHU01H08_SM            AT%M688.0      :INT; (*空调机组01H08-季节模式*)"]
["692.0","验证通过","REAL","空调机组","L","01H08","水阀反馈换算值","空调机组01H08-水阀反馈换算值",{"$f":"E170&VLOOKUP(D170,list!$D$3:$F$501,2,FALSE)&F170&\"_\"&VLOOKUP(G170,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVBS"},"LAHU01H08_WVBS AT%M692.0 :REAL; (*空调机组01H08-水阀反馈换算值*)","LAHU01H08_WVBS          AT%M692.0      :REAL; (*空调机组01H08-水阀反馈换算值*)"]
["696.0","验证通过","BOOL","空调机组","L","01H08","水阀手动控制","空调机组01H08-水阀手动控制",{"$f":"E171&VLOOKUP(D171,list!$D$3:$F$501,2,FALSE)&F171&\"_\"&VLOOKUP(G171,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVMC"},"LAHU01H08_WVMC AT%M696.0 :BOOL; (*空调机组01H08-水阀手动控制*)","LAHU01H08_WVMC          AT%M696.0      :BOOL; (*空调机组01H08-水阀手动控制*)"]
["700.0","验证通过","REAL","空调机组","L","01H08","水阀手动控制值","空调机组01H08-水阀手动控制值",{"$f":"E172&VLOOKUP(D172,list!$D$3:$F$501,2,FALSE)&F172&\"_\"&VLOOKUP(G172,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVMV"},"LAHU01H08_WVMV AT%M700.0 :REAL; (*空调机组01H08-水阀手动控制值*)","LAHU01H08_WVMV          AT%M700.0      :REAL; (*空调机组01H08-水阀手动控制值*)"]
["704.0","验证通过","REAL","空调机组","L","01H08","回风温度换算值","空调机组01H08-回风温度换算值",{"$f":"E173&VLOOKUP(D173,list!$D$3:$F$501,2,FALSE)&F173&\"_\"&VLOOKUP(G173,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RTS"},"LAHU01H08_RTS AT%M704.0 :REAL; (*空调机组01H08-回风温度换算值*)","LAHU01H08_RTS           AT%M704.0      :REAL; (*空调机组01H08-回风温度换算值*)"]
["708.0","验证通过","BOOL","空调机组","L","01H08","运行时间累积重置","空调机组01H08-运行时间累积重置",{"$f":"E174&VLOOKUP(D174,list!$D$3:$F$501,2,FALSE)&F174&\"_\"&VLOOKUP(G174,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RST"},"LAHU01H08_RST AT%M708.0 :BOOL; (*空调机组01H08-运行时间累积重置*)","LAHU01H08_RST           AT%M708.0      :BOOL; (*空调机组01H08-运行时间累积重置*)"]
["712.0","验证通过","REAL","空调机组","L","01H08","运行时间累积重置值","空调机组01H08-运行时间累积重置值",{"$f":"E175&VLOOKUP(D175,list!$D$3:$F$501,2,FALSE)&F175&\"_\"&VLOOKUP(G175,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RSTV"},"LAHU01H08_RSTV AT%M712.0 :REAL; (*空调机组01H08-运行时间累积重置值*)","LAHU01H08_RSTV          AT%M712.0      :REAL; (*空调机组01H08-运行时间累积重置值*)"]
["716.0","验证通过","BOOL","空调机组","L","01H08","隔离开关1","空调机组01H08-隔离开关1",{"$f":"E176&VLOOKUP(D176,list!$D$3:$F$501,2,FALSE)&F176&\"_\"&VLOOKUP(G176,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_ISO1"},"LAHU01H08_ISO1 AT%M716.0 :BOOL; (*空调机组01H08-隔离开关1*)","LAHU01H08_ISO1          AT%M716.0      :BOOL; (*空调机组01H08-隔离开关1*)"]
["718.0","验证通过","BOOL","空调机组","L","01H08","隔离开关2","空调机组01H08-隔离开关2",{"$f":"E177&VLOOKUP(D177,list!$D$3:$F$501,2,FALSE)&F177&\"_\"&VLOOKUP(G177,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_ISO2"},"LAHU01H08_ISO2 AT%M718.0 :BOOL; (*空调机组01H08-隔离开关2*)","LAHU01H08_ISO2          AT%M718.0      :BOOL; (*空调机组01H08-隔离开关2*)"]
["724.0","验证通过","REAL","空调机组","L","01H08","P调节参数","空调机组01H08-P调节参数",{"$f":"E178&VLOOKUP(D178,list!$D$3:$F$501,2,FALSE)&F178&\"_\"&VLOOKUP(G178,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_VP"},"LAHU01H08_VP AT%M724.0 :REAL; (*空调机组01H08-P调节参数*)","LAHU01H08_VP            AT%M724.0      :REAL; (*空调机组01H08-P调节参数*)"]
["728.0","验证通过","REAL","空调机组","L","01H08","I调节参数","空调机组01H08-I调节参数",{"$f":"E179&VLOOKUP(D179,list!$D$3:$F$501,2,FALSE)&F179&\"_\"&VLOOKUP(G179,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_VI"},"LAHU01H08_VI AT%M728.0 :REAL; (*空调机组01H08-I调节参数*)","LAHU01H08_VI            AT%M728.0      :REAL; (*空调机组01H08-I调节参数*)"]
["732.0","验证通过","REAL","空调机组","L","01H08","运行时间累积值","空调机组01H08-运行时间累积值",{"$f":"E180&VLOOKUP(D180,list!$D$3:$F$501,2,FALSE)&F180&\"_\"&VLOOKUP(G180,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RH"},"LAHU01H08_RH AT%M732.0 :REAL; (*空调机组01H08-运行时间累积值*)","LAHU01H08_RH            AT%M732.0      :REAL; (*空调机组01H08-运行时间累积值*)"]
["736.0","验证通过","INT","空调机组","L","01H08","设备状态代码","空调机组01H08-设备状态代码",{"$f":"E181&VLOOKUP(D181,list!$D$3:$F$501,2,FALSE)&F181&\"_\"&VLOOKUP(G181,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_SN"},"LAHU01H08_SN AT%M736.0 :INT; (*空调机组01H08-设备状态代码*)","LAHU01H08_SN            AT%M736.0      :INT; (*空调机组01H08-设备状态代码*)"]
["738.0","验证通过","INT","空调机组","L","01H08","水阀控制转换值","空调机组01H08-水阀控制转换值",{"$f":"E182&VLOOKUP(D182,list!$D$3:$F$501,2,FALSE)&F182&\"_\"&VLOOKUP(G182,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVCS"},"LAHU01H08_WVCS AT%M738.0 :INT; (*空调机组01H08-水阀控制转换值*)","LAHU01H08_WVCS          AT%M738.0      :INT; (*空调机组01H08-水阀控制转换值*)"]
["740.0","验证通过","BOOL","空调机组","L","01H08","程序控制","空调机组01H08-程序控制",{"$f":"E183&VLOOKUP(D183,list!$D$3:$F$501,2,FALSE)&F183&\"_\"&VLOOKUP(G183,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_PC"},"LAHU01H08_PC AT%M740.0 :BOOL; (*空调机组01H08-程序控制*)","LAHU01H08_PC            AT%M740.0      :BOOL; (*空调机组01H08-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C183=\"REAL\",C183=\"DWORD\",C183=\"DINT\"),(IF(OR(C185=\"REAL\",C185=\"DWORD\",C185=\"DINT\"),A183+4+MOD(A183,4),A183+4)),(IF(OR(C185=\"REAL\",C185=\"DWORD\",C185=\"DINT\"),A183+4+MOD(A183,4),A183+2)))&\".0\"","v":"744.0"},{"$f":"IF((IF(OR(C185=\"INT\",C185=\"WORD\",C185=\"BOOL\"),MOD(A185,2),MOD(A185,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H09","设定温度值",{"$f":"D185&F185&\"-\"&IF(E185=\"R\",\"新云平台\"&G185,G185)","v":"空调机组01H09-新云平台设定温度值"},{"$f":"E185&VLOOKUP(D185,list!$D$3:$F$501,2,FALSE)&F185&\"_\"&VLOOKUP(G185,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H09_TSET"},{"$f":"I185&\" \"&\"AT%M\"&A185&\" \"&\":\"&C185&\";\"&\" \"&\"(*\"&H185&\"*)\"","v":"RAHU01H09_TSET AT%M744.0 :REAL; (*空调机组01H09-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J185,SEARCH(\"AT%\",J185),,REPT(\" \",25-SEARCH(\"AT%\",J185))),SEARCH(\":\",REPLACE(J185,SEARCH(\"AT%\",J185),,REPT(\" \",25-SEARCH(\"AT%\",J185)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J185,SEARCH(\"AT%\",J185),,REPT(\" \",25-SEARCH(\"AT%\",J185))))))","v":"RAHU01H09_TSET          AT%M744.0      :REAL; (*空调机组01H09-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C185=\"REAL\",C185=\"DWORD\",C185=\"DINT\"),(IF(OR(C186=\"REAL\",C186=\"DWORD\",C186=\"DINT\"),A185+4+MOD(A185,4),A185+4)),(IF(OR(C186=\"REAL\",C186=\"DWORD\",C186=\"DINT\"),A185+4+MOD(A185,4),A185+2)))&\".0\"","v":"748.0"},"验证通过","INT","空调机组","R",{"$f":"F185","v":"01H09"},"季节模式","空调机组01H09-新云平台季节模式",{"$f":"E186&VLOOKUP(D186,list!$D$3:$F$501,2,FALSE)&F186&\"_\"&VLOOKUP(G186,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H09_SM"},"RAHU01H09_SM AT%M748.0 :INT; (*空调机组01H09-新云平台季节模式*)","RAHU01H09_SM            AT%M748.0      :INT; (*空调机组01H09-新云平台季节模式*)"]
["750.0","验证通过","BOOL","空调机组","R","01H09","程序控制","空调机组01H09-新云平台程序控制",{"$f":"E187&VLOOKUP(D187,list!$D$3:$F$501,2,FALSE)&F187&\"_\"&VLOOKUP(G187,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H09_PC"},"RAHU01H09_PC AT%M750.0 :BOOL; (*空调机组01H09-新云平台程序控制*)","RAHU01H09_PC            AT%M750.0      :BOOL; (*空调机组01H09-新云平台程序控制*)"]
["756.0","验证通过","REAL","空调机组","L","01H09","设定温度值","空调机组01H09-设定温度值",{"$f":"E188&VLOOKUP(D188,list!$D$3:$F$501,2,FALSE)&F188&\"_\"&VLOOKUP(G188,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_TSET"},"LAHU01H09_TSET AT%M756.0 :REAL; (*空调机组01H09-设定温度值*)","LAHU01H09_TSET          AT%M756.0      :REAL; (*空调机组01H09-设定温度值*)"]
["760.0","验证通过","INT","空调机组","L","01H09","季节模式","空调机组01H09-季节模式",{"$f":"E189&VLOOKUP(D189,list!$D$3:$F$501,2,FALSE)&F189&\"_\"&VLOOKUP(G189,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_SM"},"LAHU01H09_SM AT%M760.0 :INT; (*空调机组01H09-季节模式*)","LAHU01H09_SM            AT%M760.0      :INT; (*空调机组01H09-季节模式*)"]
["764.0","验证通过","REAL","空调机组","L","01H09","水阀反馈换算值","空调机组01H09-水阀反馈换算值",{"$f":"E190&VLOOKUP(D190,list!$D$3:$F$501,2,FALSE)&F190&\"_\"&VLOOKUP(G190,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVBS"},"LAHU01H09_WVBS AT%M764.0 :REAL; (*空调机组01H09-水阀反馈换算值*)","LAHU01H09_WVBS          AT%M764.0      :REAL; (*空调机组01H09-水阀反馈换算值*)"]
["768.0","验证通过","BOOL","空调机组","L","01H09","水阀手动控制","空调机组01H09-水阀手动控制",{"$f":"E191&VLOOKUP(D191,list!$D$3:$F$501,2,FALSE)&F191&\"_\"&VLOOKUP(G191,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVMC"},"LAHU01H09_WVMC AT%M768.0 :BOOL; (*空调机组01H09-水阀手动控制*)","LAHU01H09_WVMC          AT%M768.0      :BOOL; (*空调机组01H09-水阀手动控制*)"]
["772.0","验证通过","REAL","空调机组","L","01H09","水阀手动控制值","空调机组01H09-水阀手动控制值",{"$f":"E192&VLOOKUP(D192,list!$D$3:$F$501,2,FALSE)&F192&\"_\"&VLOOKUP(G192,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVMV"},"LAHU01H09_WVMV AT%M772.0 :REAL; (*空调机组01H09-水阀手动控制值*)","LAHU01H09_WVMV          AT%M772.0      :REAL; (*空调机组01H09-水阀手动控制值*)"]
["776.0","验证通过","REAL","空调机组","L","01H09","回风温度换算值","空调机组01H09-回风温度换算值",{"$f":"E193&VLOOKUP(D193,list!$D$3:$F$501,2,FALSE)&F193&\"_\"&VLOOKUP(G193,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RTS"},"LAHU01H09_RTS AT%M776.0 :REAL; (*空调机组01H09-回风温度换算值*)","LAHU01H09_RTS           AT%M776.0      :REAL; (*空调机组01H09-回风温度换算值*)"]
["780.0","验证通过","BOOL","空调机组","L","01H09","运行时间累积重置","空调机组01H09-运行时间累积重置",{"$f":"E194&VLOOKUP(D194,list!$D$3:$F$501,2,FALSE)&F194&\"_\"&VLOOKUP(G194,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RST"},"LAHU01H09_RST AT%M780.0 :BOOL; (*空调机组01H09-运行时间累积重置*)","LAHU01H09_RST           AT%M780.0      :BOOL; (*空调机组01H09-运行时间累积重置*)"]
["784.0","验证通过","REAL","空调机组","L","01H09","运行时间累积重置值","空调机组01H09-运行时间累积重置值",{"$f":"E195&VLOOKUP(D195,list!$D$3:$F$501,2,FALSE)&F195&\"_\"&VLOOKUP(G195,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RSTV"},"LAHU01H09_RSTV AT%M784.0 :REAL; (*空调机组01H09-运行时间累积重置值*)","LAHU01H09_RSTV          AT%M784.0      :REAL; (*空调机组01H09-运行时间累积重置值*)"]
["788.0","验证通过","BOOL","空调机组","L","01H09","隔离开关1","空调机组01H09-隔离开关1",{"$f":"E196&VLOOKUP(D196,list!$D$3:$F$501,2,FALSE)&F196&\"_\"&VLOOKUP(G196,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_ISO1"},"LAHU01H09_ISO1 AT%M788.0 :BOOL; (*空调机组01H09-隔离开关1*)","LAHU01H09_ISO1          AT%M788.0      :BOOL; (*空调机组01H09-隔离开关1*)"]
["790.0","验证通过","BOOL","空调机组","L","01H09","隔离开关2","空调机组01H09-隔离开关2",{"$f":"E197&VLOOKUP(D197,list!$D$3:$F$501,2,FALSE)&F197&\"_\"&VLOOKUP(G197,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_ISO2"},"LAHU01H09_ISO2 AT%M790.0 :BOOL; (*空调机组01H09-隔离开关2*)","LAHU01H09_ISO2          AT%M790.0      :BOOL; (*空调机组01H09-隔离开关2*)"]
["796.0","验证通过","REAL","空调机组","L","01H09","P调节参数","空调机组01H09-P调节参数",{"$f":"E198&VLOOKUP(D198,list!$D$3:$F$501,2,FALSE)&F198&\"_\"&VLOOKUP(G198,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_VP"},"LAHU01H09_VP AT%M796.0 :REAL; (*空调机组01H09-P调节参数*)","LAHU01H09_VP            AT%M796.0      :REAL; (*空调机组01H09-P调节参数*)"]
["800.0","验证通过","REAL","空调机组","L","01H09","I调节参数","空调机组01H09-I调节参数",{"$f":"E199&VLOOKUP(D199,list!$D$3:$F$501,2,FALSE)&F199&\"_\"&VLOOKUP(G199,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_VI"},"LAHU01H09_VI AT%M800.0 :REAL; (*空调机组01H09-I调节参数*)","LAHU01H09_VI            AT%M800.0      :REAL; (*空调机组01H09-I调节参数*)"]
["804.0","验证通过","REAL","空调机组","L","01H09","运行时间累积值","空调机组01H09-运行时间累积值",{"$f":"E200&VLOOKUP(D200,list!$D$3:$F$501,2,FALSE)&F200&\"_\"&VLOOKUP(G200,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RH"},"LAHU01H09_RH AT%M804.0 :REAL; (*空调机组01H09-运行时间累积值*)","LAHU01H09_RH            AT%M804.0      :REAL; (*空调机组01H09-运行时间累积值*)"]
["808.0","验证通过","INT","空调机组","L","01H09","设备状态代码","空调机组01H09-设备状态代码",{"$f":"E201&VLOOKUP(D201,list!$D$3:$F$501,2,FALSE)&F201&\"_\"&VLOOKUP(G201,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_SN"},"LAHU01H09_SN AT%M808.0 :INT; (*空调机组01H09-设备状态代码*)","LAHU01H09_SN            AT%M808.0      :INT; (*空调机组01H09-设备状态代码*)"]
["810.0","验证通过","INT","空调机组","L","01H09","水阀控制转换值","空调机组01H09-水阀控制转换值",{"$f":"E202&VLOOKUP(D202,list!$D$3:$F$501,2,FALSE)&F202&\"_\"&VLOOKUP(G202,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVCS"},"LAHU01H09_WVCS AT%M810.0 :INT; (*空调机组01H09-水阀控制转换值*)","LAHU01H09_WVCS          AT%M810.0      :INT; (*空调机组01H09-水阀控制转换值*)"]
["812.0","验证通过","BOOL","空调机组","L","01H09","程序控制","空调机组01H09-程序控制",{"$f":"E203&VLOOKUP(D203,list!$D$3:$F$501,2,FALSE)&F203&\"_\"&VLOOKUP(G203,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_PC"},"LAHU01H09_PC AT%M812.0 :BOOL; (*空调机组01H09-程序控制*)","LAHU01H09_PC            AT%M812.0      :BOOL; (*空调机组01H09-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C203=\"REAL\",C203=\"DWORD\",C203=\"DINT\"),(IF(OR(C205=\"REAL\",C205=\"DWORD\",C205=\"DINT\"),A203+4+MOD(A203,4),A203+4)),(IF(OR(C205=\"REAL\",C205=\"DWORD\",C205=\"DINT\"),A203+4+MOD(A203,4),A203+2)))&\".0\"","v":"816.0"},{"$f":"IF((IF(OR(C205=\"INT\",C205=\"WORD\",C205=\"BOOL\"),MOD(A205,2),MOD(A205,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H10","设定温度值",{"$f":"D205&F205&\"-\"&IF(E205=\"R\",\"新云平台\"&G205,G205)","v":"空调机组01H10-新云平台设定温度值"},{"$f":"E205&VLOOKUP(D205,list!$D$3:$F$501,2,FALSE)&F205&\"_\"&VLOOKUP(G205,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H10_TSET"},{"$f":"I205&\" \"&\"AT%M\"&A205&\" \"&\":\"&C205&\";\"&\" \"&\"(*\"&H205&\"*)\"","v":"RAHU01H10_TSET AT%M816.0 :REAL; (*空调机组01H10-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J205,SEARCH(\"AT%\",J205),,REPT(\" \",25-SEARCH(\"AT%\",J205))),SEARCH(\":\",REPLACE(J205,SEARCH(\"AT%\",J205),,REPT(\" \",25-SEARCH(\"AT%\",J205)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J205,SEARCH(\"AT%\",J205),,REPT(\" \",25-SEARCH(\"AT%\",J205))))))","v":"RAHU01H10_TSET          AT%M816.0      :REAL; (*空调机组01H10-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C205=\"REAL\",C205=\"DWORD\",C205=\"DINT\"),(IF(OR(C206=\"REAL\",C206=\"DWORD\",C206=\"DINT\"),A205+4+MOD(A205,4),A205+4)),(IF(OR(C206=\"REAL\",C206=\"DWORD\",C206=\"DINT\"),A205+4+MOD(A205,4),A205+2)))&\".0\"","v":"820.0"},"验证通过","INT","空调机组","R",{"$f":"F205","v":"01H10"},"季节模式","空调机组01H10-新云平台季节模式",{"$f":"E206&VLOOKUP(D206,list!$D$3:$F$501,2,FALSE)&F206&\"_\"&VLOOKUP(G206,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H10_SM"},"RAHU01H10_SM AT%M820.0 :INT; (*空调机组01H10-新云平台季节模式*)","RAHU01H10_SM            AT%M820.0      :INT; (*空调机组01H10-新云平台季节模式*)"]
["822.0","验证通过","BOOL","空调机组","R","01H10","程序控制","空调机组01H10-新云平台程序控制",{"$f":"E207&VLOOKUP(D207,list!$D$3:$F$501,2,FALSE)&F207&\"_\"&VLOOKUP(G207,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H10_PC"},"RAHU01H10_PC AT%M822.0 :BOOL; (*空调机组01H10-新云平台程序控制*)","RAHU01H10_PC            AT%M822.0      :BOOL; (*空调机组01H10-新云平台程序控制*)"]
["828.0","验证通过","REAL","空调机组","L","01H10","设定温度值","空调机组01H10-设定温度值",{"$f":"E208&VLOOKUP(D208,list!$D$3:$F$501,2,FALSE)&F208&\"_\"&VLOOKUP(G208,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_TSET"},"LAHU01H10_TSET AT%M828.0 :REAL; (*空调机组01H10-设定温度值*)","LAHU01H10_TSET          AT%M828.0      :REAL; (*空调机组01H10-设定温度值*)"]
["832.0","验证通过","INT","空调机组","L","01H10","季节模式","空调机组01H10-季节模式",{"$f":"E209&VLOOKUP(D209,list!$D$3:$F$501,2,FALSE)&F209&\"_\"&VLOOKUP(G209,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_SM"},"LAHU01H10_SM AT%M832.0 :INT; (*空调机组01H10-季节模式*)","LAHU01H10_SM            AT%M832.0      :INT; (*空调机组01H10-季节模式*)"]
["836.0","验证通过","REAL","空调机组","L","01H10","水阀反馈换算值","空调机组01H10-水阀反馈换算值",{"$f":"E210&VLOOKUP(D210,list!$D$3:$F$501,2,FALSE)&F210&\"_\"&VLOOKUP(G210,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVBS"},"LAHU01H10_WVBS AT%M836.0 :REAL; (*空调机组01H10-水阀反馈换算值*)","LAHU01H10_WVBS          AT%M836.0      :REAL; (*空调机组01H10-水阀反馈换算值*)"]
["840.0","验证通过","BOOL","空调机组","L","01H10","水阀手动控制","空调机组01H10-水阀手动控制",{"$f":"E211&VLOOKUP(D211,list!$D$3:$F$501,2,FALSE)&F211&\"_\"&VLOOKUP(G211,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVMC"},"LAHU01H10_WVMC AT%M840.0 :BOOL; (*空调机组01H10-水阀手动控制*)","LAHU01H10_WVMC          AT%M840.0      :BOOL; (*空调机组01H10-水阀手动控制*)"]
["844.0","验证通过","REAL","空调机组","L","01H10","水阀手动控制值","空调机组01H10-水阀手动控制值",{"$f":"E212&VLOOKUP(D212,list!$D$3:$F$501,2,FALSE)&F212&\"_\"&VLOOKUP(G212,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVMV"},"LAHU01H10_WVMV AT%M844.0 :REAL; (*空调机组01H10-水阀手动控制值*)","LAHU01H10_WVMV          AT%M844.0      :REAL; (*空调机组01H10-水阀手动控制值*)"]
["848.0","验证通过","REAL","空调机组","L","01H10","回风温度换算值","空调机组01H10-回风温度换算值",{"$f":"E213&VLOOKUP(D213,list!$D$3:$F$501,2,FALSE)&F213&\"_\"&VLOOKUP(G213,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RTS"},"LAHU01H10_RTS AT%M848.0 :REAL; (*空调机组01H10-回风温度换算值*)","LAHU01H10_RTS           AT%M848.0      :REAL; (*空调机组01H10-回风温度换算值*)"]
["852.0","验证通过","BOOL","空调机组","L","01H10","运行时间累积重置","空调机组01H10-运行时间累积重置",{"$f":"E214&VLOOKUP(D214,list!$D$3:$F$501,2,FALSE)&F214&\"_\"&VLOOKUP(G214,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RST"},"LAHU01H10_RST AT%M852.0 :BOOL; (*空调机组01H10-运行时间累积重置*)","LAHU01H10_RST           AT%M852.0      :BOOL; (*空调机组01H10-运行时间累积重置*)"]
["856.0","验证通过","REAL","空调机组","L","01H10","运行时间累积重置值","空调机组01H10-运行时间累积重置值",{"$f":"E215&VLOOKUP(D215,list!$D$3:$F$501,2,FALSE)&F215&\"_\"&VLOOKUP(G215,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RSTV"},"LAHU01H10_RSTV AT%M856.0 :REAL; (*空调机组01H10-运行时间累积重置值*)","LAHU01H10_RSTV          AT%M856.0      :REAL; (*空调机组01H10-运行时间累积重置值*)"]
["860.0","验证通过","BOOL","空调机组","L","01H10","隔离开关1","空调机组01H10-隔离开关1",{"$f":"E216&VLOOKUP(D216,list!$D$3:$F$501,2,FALSE)&F216&\"_\"&VLOOKUP(G216,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_ISO1"},"LAHU01H10_ISO1 AT%M860.0 :BOOL; (*空调机组01H10-隔离开关1*)","LAHU01H10_ISO1          AT%M860.0      :BOOL; (*空调机组01H10-隔离开关1*)"]
["862.0","验证通过","BOOL","空调机组","L","01H10","隔离开关2","空调机组01H10-隔离开关2",{"$f":"E217&VLOOKUP(D217,list!$D$3:$F$501,2,FALSE)&F217&\"_\"&VLOOKUP(G217,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_ISO2"},"LAHU01H10_ISO2 AT%M862.0 :BOOL; (*空调机组01H10-隔离开关2*)","LAHU01H10_ISO2          AT%M862.0      :BOOL; (*空调机组01H10-隔离开关2*)"]
["868.0","验证通过","REAL","空调机组","L","01H10","P调节参数","空调机组01H10-P调节参数",{"$f":"E218&VLOOKUP(D218,list!$D$3:$F$501,2,FALSE)&F218&\"_\"&VLOOKUP(G218,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_VP"},"LAHU01H10_VP AT%M868.0 :REAL; (*空调机组01H10-P调节参数*)","LAHU01H10_VP            AT%M868.0      :REAL; (*空调机组01H10-P调节参数*)"]
["872.0","验证通过","REAL","空调机组","L","01H10","I调节参数","空调机组01H10-I调节参数",{"$f":"E219&VLOOKUP(D219,list!$D$3:$F$501,2,FALSE)&F219&\"_\"&VLOOKUP(G219,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_VI"},"LAHU01H10_VI AT%M872.0 :REAL; (*空调机组01H10-I调节参数*)","LAHU01H10_VI            AT%M872.0      :REAL; (*空调机组01H10-I调节参数*)"]
["876.0","验证通过","REAL","空调机组","L","01H10","运行时间累积值","空调机组01H10-运行时间累积值",{"$f":"E220&VLOOKUP(D220,list!$D$3:$F$501,2,FALSE)&F220&\"_\"&VLOOKUP(G220,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RH"},"LAHU01H10_RH AT%M876.0 :REAL; (*空调机组01H10-运行时间累积值*)","LAHU01H10_RH            AT%M876.0      :REAL; (*空调机组01H10-运行时间累积值*)"]
["880.0","验证通过","INT","空调机组","L","01H10","设备状态代码","空调机组01H10-设备状态代码",{"$f":"E221&VLOOKUP(D221,list!$D$3:$F$501,2,FALSE)&F221&\"_\"&VLOOKUP(G221,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_SN"},"LAHU01H10_SN AT%M880.0 :INT; (*空调机组01H10-设备状态代码*)","LAHU01H10_SN            AT%M880.0      :INT; (*空调机组01H10-设备状态代码*)"]
["882.0","验证通过","INT","空调机组","L","01H10","水阀控制转换值","空调机组01H10-水阀控制转换值",{"$f":"E222&VLOOKUP(D222,list!$D$3:$F$501,2,FALSE)&F222&\"_\"&VLOOKUP(G222,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVCS"},"LAHU01H10_WVCS AT%M882.0 :INT; (*空调机组01H10-水阀控制转换值*)","LAHU01H10_WVCS          AT%M882.0      :INT; (*空调机组01H10-水阀控制转换值*)"]
["884.0","验证通过","BOOL","空调机组","L","01H10","程序控制","空调机组01H10-程序控制",{"$f":"E223&VLOOKUP(D223,list!$D$3:$F$501,2,FALSE)&F223&\"_\"&VLOOKUP(G223,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_PC"},"LAHU01H10_PC AT%M884.0 :BOOL; (*空调机组01H10-程序控制*)","LAHU01H10_PC            AT%M884.0      :BOOL; (*空调机组01H10-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C223=\"REAL\",C223=\"DWORD\",C223=\"DINT\"),(IF(OR(C225=\"REAL\",C225=\"DWORD\",C225=\"DINT\"),A223+4+MOD(A223,4),A223+4)),(IF(OR(C225=\"REAL\",C225=\"DWORD\",C225=\"DINT\"),A223+4+MOD(A223,4),A223+2)))&\".0\"","v":"888.0"},{"$f":"IF((IF(OR(C225=\"INT\",C225=\"WORD\",C225=\"BOOL\"),MOD(A225,2),MOD(A225,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H01","设定温度值",{"$f":"D225&F225&\"-\"&IF(E225=\"R\",\"新云平台\"&G225,G225)","v":"空调机组02H01-新云平台设定温度值"},{"$f":"E225&VLOOKUP(D225,list!$D$3:$F$501,2,FALSE)&F225&\"_\"&VLOOKUP(G225,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H01_TSET"},{"$f":"I225&\" \"&\"AT%M\"&A225&\" \"&\":\"&C225&\";\"&\" \"&\"(*\"&H225&\"*)\"","v":"RAHU02H01_TSET AT%M888.0 :REAL; (*空调机组02H01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J225,SEARCH(\"AT%\",J225),,REPT(\" \",25-SEARCH(\"AT%\",J225))),SEARCH(\":\",REPLACE(J225,SEARCH(\"AT%\",J225),,REPT(\" \",25-SEARCH(\"AT%\",J225)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J225,SEARCH(\"AT%\",J225),,REPT(\" \",25-SEARCH(\"AT%\",J225))))))","v":"RAHU02H01_TSET          AT%M888.0      :REAL; (*空调机组02H01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C225=\"REAL\",C225=\"DWORD\",C225=\"DINT\"),(IF(OR(C226=\"REAL\",C226=\"DWORD\",C226=\"DINT\"),A225+4+MOD(A225,4),A225+4)),(IF(OR(C226=\"REAL\",C226=\"DWORD\",C226=\"DINT\"),A225+4+MOD(A225,4),A225+2)))&\".0\"","v":"892.0"},"验证通过","INT","空调机组","R",{"$f":"F225","v":"02H01"},"季节模式","空调机组02H01-新云平台季节模式",{"$f":"E226&VLOOKUP(D226,list!$D$3:$F$501,2,FALSE)&F226&\"_\"&VLOOKUP(G226,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H01_SM"},"RAHU02H01_SM AT%M892.0 :INT; (*空调机组02H01-新云平台季节模式*)","RAHU02H01_SM            AT%M892.0      :INT; (*空调机组02H01-新云平台季节模式*)"]
["894.0","验证通过","BOOL","空调机组","R","02H01","程序控制","空调机组02H01-新云平台程序控制",{"$f":"E227&VLOOKUP(D227,list!$D$3:$F$501,2,FALSE)&F227&\"_\"&VLOOKUP(G227,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H01_PC"},"RAHU02H01_PC AT%M894.0 :BOOL; (*空调机组02H01-新云平台程序控制*)","RAHU02H01_PC            AT%M894.0      :BOOL; (*空调机组02H01-新云平台程序控制*)"]
["900.0","验证通过","REAL","空调机组","L","02H01","设定温度值","空调机组02H01-设定温度值",{"$f":"E228&VLOOKUP(D228,list!$D$3:$F$501,2,FALSE)&F228&\"_\"&VLOOKUP(G228,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_TSET"},"LAHU02H01_TSET AT%M900.0 :REAL; (*空调机组02H01-设定温度值*)","LAHU02H01_TSET          AT%M900.0      :REAL; (*空调机组02H01-设定温度值*)"]
["904.0","验证通过","INT","空调机组","L","02H01","季节模式","空调机组02H01-季节模式",{"$f":"E229&VLOOKUP(D229,list!$D$3:$F$501,2,FALSE)&F229&\"_\"&VLOOKUP(G229,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_SM"},"LAHU02H01_SM AT%M904.0 :INT; (*空调机组02H01-季节模式*)","LAHU02H01_SM            AT%M904.0      :INT; (*空调机组02H01-季节模式*)"]
["908.0","验证通过","REAL","空调机组","L","02H01","水阀反馈换算值","空调机组02H01-水阀反馈换算值",{"$f":"E230&VLOOKUP(D230,list!$D$3:$F$501,2,FALSE)&F230&\"_\"&VLOOKUP(G230,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_WVBS"},"LAHU02H01_WVBS AT%M908.0 :REAL; (*空调机组02H01-水阀反馈换算值*)","LAHU02H01_WVBS          AT%M908.0      :REAL; (*空调机组02H01-水阀反馈换算值*)"]
["912.0","验证通过","BOOL","空调机组","L","02H01","水阀手动控制","空调机组02H01-水阀手动控制",{"$f":"E231&VLOOKUP(D231,list!$D$3:$F$501,2,FALSE)&F231&\"_\"&VLOOKUP(G231,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_WVMC"},"LAHU02H01_WVMC AT%M912.0 :BOOL; (*空调机组02H01-水阀手动控制*)","LAHU02H01_WVMC          AT%M912.0      :BOOL; (*空调机组02H01-水阀手动控制*)"]
["916.0","验证通过","REAL","空调机组","L","02H01","水阀手动控制值","空调机组02H01-水阀手动控制值",{"$f":"E232&VLOOKUP(D232,list!$D$3:$F$501,2,FALSE)&F232&\"_\"&VLOOKUP(G232,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_WVMV"},"LAHU02H01_WVMV AT%M916.0 :REAL; (*空调机组02H01-水阀手动控制值*)","LAHU02H01_WVMV          AT%M916.0      :REAL; (*空调机组02H01-水阀手动控制值*)"]
["920.0","验证通过","REAL","空调机组","L","02H01","回风温度换算值","空调机组02H01-回风温度换算值",{"$f":"E233&VLOOKUP(D233,list!$D$3:$F$501,2,FALSE)&F233&\"_\"&VLOOKUP(G233,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_RTS"},"LAHU02H01_RTS AT%M920.0 :REAL; (*空调机组02H01-回风温度换算值*)","LAHU02H01_RTS           AT%M920.0      :REAL; (*空调机组02H01-回风温度换算值*)"]
["924.0","验证通过","BOOL","空调机组","L","02H01","运行时间累积重置","空调机组02H01-运行时间累积重置",{"$f":"E234&VLOOKUP(D234,list!$D$3:$F$501,2,FALSE)&F234&\"_\"&VLOOKUP(G234,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_RST"},"LAHU02H01_RST AT%M924.0 :BOOL; (*空调机组02H01-运行时间累积重置*)","LAHU02H01_RST           AT%M924.0      :BOOL; (*空调机组02H01-运行时间累积重置*)"]
["928.0","验证通过","REAL","空调机组","L","02H01","运行时间累积重置值","空调机组02H01-运行时间累积重置值",{"$f":"E235&VLOOKUP(D235,list!$D$3:$F$501,2,FALSE)&F235&\"_\"&VLOOKUP(G235,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_RSTV"},"LAHU02H01_RSTV AT%M928.0 :REAL; (*空调机组02H01-运行时间累积重置值*)","LAHU02H01_RSTV          AT%M928.0      :REAL; (*空调机组02H01-运行时间累积重置值*)"]
["932.0","验证通过","BOOL","空调机组","L","02H01","隔离开关1","空调机组02H01-隔离开关1",{"$f":"E236&VLOOKUP(D236,list!$D$3:$F$501,2,FALSE)&F236&\"_\"&VLOOKUP(G236,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_ISO1"},"LAHU02H01_ISO1 AT%M932.0 :BOOL; (*空调机组02H01-隔离开关1*)","LAHU02H01_ISO1          AT%M932.0      :BOOL; (*空调机组02H01-隔离开关1*)"]
["934.0","验证通过","BOOL","空调机组","L","02H01","隔离开关2","空调机组02H01-隔离开关2",{"$f":"E237&VLOOKUP(D237,list!$D$3:$F$501,2,FALSE)&F237&\"_\"&VLOOKUP(G237,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_ISO2"},"LAHU02H01_ISO2 AT%M934.0 :BOOL; (*空调机组02H01-隔离开关2*)","LAHU02H01_ISO2          AT%M934.0      :BOOL; (*空调机组02H01-隔离开关2*)"]
["940.0","验证通过","REAL","空调机组","L","02H01","P调节参数","空调机组02H01-P调节参数",{"$f":"E238&VLOOKUP(D238,list!$D$3:$F$501,2,FALSE)&F238&\"_\"&VLOOKUP(G238,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_VP"},"LAHU02H01_VP AT%M940.0 :REAL; (*空调机组02H01-P调节参数*)","LAHU02H01_VP            AT%M940.0      :REAL; (*空调机组02H01-P调节参数*)"]
["944.0","验证通过","REAL","空调机组","L","02H01","I调节参数","空调机组02H01-I调节参数",{"$f":"E239&VLOOKUP(D239,list!$D$3:$F$501,2,FALSE)&F239&\"_\"&VLOOKUP(G239,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_VI"},"LAHU02H01_VI AT%M944.0 :REAL; (*空调机组02H01-I调节参数*)","LAHU02H01_VI            AT%M944.0      :REAL; (*空调机组02H01-I调节参数*)"]
["948.0","验证通过","REAL","空调机组","L","02H01","运行时间累积值","空调机组02H01-运行时间累积值",{"$f":"E240&VLOOKUP(D240,list!$D$3:$F$501,2,FALSE)&F240&\"_\"&VLOOKUP(G240,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_RH"},"LAHU02H01_RH AT%M948.0 :REAL; (*空调机组02H01-运行时间累积值*)","LAHU02H01_RH            AT%M948.0      :REAL; (*空调机组02H01-运行时间累积值*)"]
["952.0","验证通过","INT","空调机组","L","02H01","设备状态代码","空调机组02H01-设备状态代码",{"$f":"E241&VLOOKUP(D241,list!$D$3:$F$501,2,FALSE)&F241&\"_\"&VLOOKUP(G241,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_SN"},"LAHU02H01_SN AT%M952.0 :INT; (*空调机组02H01-设备状态代码*)","LAHU02H01_SN            AT%M952.0      :INT; (*空调机组02H01-设备状态代码*)"]
["954.0","验证通过","INT","空调机组","L","02H01","水阀控制转换值","空调机组02H01-水阀控制转换值",{"$f":"E242&VLOOKUP(D242,list!$D$3:$F$501,2,FALSE)&F242&\"_\"&VLOOKUP(G242,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_WVCS"},"LAHU02H01_WVCS AT%M954.0 :INT; (*空调机组02H01-水阀控制转换值*)","LAHU02H01_WVCS          AT%M954.0      :INT; (*空调机组02H01-水阀控制转换值*)"]
["956.0","验证通过","BOOL","空调机组","L","02H01","程序控制","空调机组02H01-程序控制",{"$f":"E243&VLOOKUP(D243,list!$D$3:$F$501,2,FALSE)&F243&\"_\"&VLOOKUP(G243,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H01_PC"},"LAHU02H01_PC AT%M956.0 :BOOL; (*空调机组02H01-程序控制*)","LAHU02H01_PC            AT%M956.0      :BOOL; (*空调机组02H01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C243=\"REAL\",C243=\"DWORD\",C243=\"DINT\"),(IF(OR(C245=\"REAL\",C245=\"DWORD\",C245=\"DINT\"),A243+4+MOD(A243,4),A243+4)),(IF(OR(C245=\"REAL\",C245=\"DWORD\",C245=\"DINT\"),A243+4+MOD(A243,4),A243+2)))&\".0\"","v":"960.0"},{"$f":"IF((IF(OR(C245=\"INT\",C245=\"WORD\",C245=\"BOOL\"),MOD(A245,2),MOD(A245,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H02","设定温度值",{"$f":"D245&F245&\"-\"&IF(E245=\"R\",\"新云平台\"&G245,G245)","v":"空调机组02H02-新云平台设定温度值"},{"$f":"E245&VLOOKUP(D245,list!$D$3:$F$501,2,FALSE)&F245&\"_\"&VLOOKUP(G245,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H02_TSET"},{"$f":"I245&\" \"&\"AT%M\"&A245&\" \"&\":\"&C245&\";\"&\" \"&\"(*\"&H245&\"*)\"","v":"RAHU02H02_TSET AT%M960.0 :REAL; (*空调机组02H02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J245,SEARCH(\"AT%\",J245),,REPT(\" \",25-SEARCH(\"AT%\",J245))),SEARCH(\":\",REPLACE(J245,SEARCH(\"AT%\",J245),,REPT(\" \",25-SEARCH(\"AT%\",J245)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J245,SEARCH(\"AT%\",J245),,REPT(\" \",25-SEARCH(\"AT%\",J245))))))","v":"RAHU02H02_TSET          AT%M960.0      :REAL; (*空调机组02H02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C245=\"REAL\",C245=\"DWORD\",C245=\"DINT\"),(IF(OR(C246=\"REAL\",C246=\"DWORD\",C246=\"DINT\"),A245+4+MOD(A245,4),A245+4)),(IF(OR(C246=\"REAL\",C246=\"DWORD\",C246=\"DINT\"),A245+4+MOD(A245,4),A245+2)))&\".0\"","v":"964.0"},"验证通过","INT","空调机组","R",{"$f":"F245","v":"02H02"},"季节模式","空调机组02H02-新云平台季节模式",{"$f":"E246&VLOOKUP(D246,list!$D$3:$F$501,2,FALSE)&F246&\"_\"&VLOOKUP(G246,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H02_SM"},"RAHU02H02_SM AT%M964.0 :INT; (*空调机组02H02-新云平台季节模式*)","RAHU02H02_SM            AT%M964.0      :INT; (*空调机组02H02-新云平台季节模式*)"]
["966.0","验证通过","BOOL","空调机组","R","02H02","程序控制","空调机组02H02-新云平台程序控制",{"$f":"E247&VLOOKUP(D247,list!$D$3:$F$501,2,FALSE)&F247&\"_\"&VLOOKUP(G247,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H02_PC"},"RAHU02H02_PC AT%M966.0 :BOOL; (*空调机组02H02-新云平台程序控制*)","RAHU02H02_PC            AT%M966.0      :BOOL; (*空调机组02H02-新云平台程序控制*)"]
["972.0","验证通过","REAL","空调机组","L","02H02","设定温度值","空调机组02H02-设定温度值",{"$f":"E248&VLOOKUP(D248,list!$D$3:$F$501,2,FALSE)&F248&\"_\"&VLOOKUP(G248,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_TSET"},"LAHU02H02_TSET AT%M972.0 :REAL; (*空调机组02H02-设定温度值*)","LAHU02H02_TSET          AT%M972.0      :REAL; (*空调机组02H02-设定温度值*)"]
["976.0","验证通过","INT","空调机组","L","02H02","季节模式","空调机组02H02-季节模式",{"$f":"E249&VLOOKUP(D249,list!$D$3:$F$501,2,FALSE)&F249&\"_\"&VLOOKUP(G249,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_SM"},"LAHU02H02_SM AT%M976.0 :INT; (*空调机组02H02-季节模式*)","LAHU02H02_SM            AT%M976.0      :INT; (*空调机组02H02-季节模式*)"]
["980.0","验证通过","REAL","空调机组","L","02H02","水阀反馈换算值","空调机组02H02-水阀反馈换算值",{"$f":"E250&VLOOKUP(D250,list!$D$3:$F$501,2,FALSE)&F250&\"_\"&VLOOKUP(G250,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_WVBS"},"LAHU02H02_WVBS AT%M980.0 :REAL; (*空调机组02H02-水阀反馈换算值*)","LAHU02H02_WVBS          AT%M980.0      :REAL; (*空调机组02H02-水阀反馈换算值*)"]
["984.0","验证通过","BOOL","空调机组","L","02H02","水阀手动控制","空调机组02H02-水阀手动控制",{"$f":"E251&VLOOKUP(D251,list!$D$3:$F$501,2,FALSE)&F251&\"_\"&VLOOKUP(G251,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_WVMC"},"LAHU02H02_WVMC AT%M984.0 :BOOL; (*空调机组02H02-水阀手动控制*)","LAHU02H02_WVMC          AT%M984.0      :BOOL; (*空调机组02H02-水阀手动控制*)"]
["988.0","验证通过","REAL","空调机组","L","02H02","水阀手动控制值","空调机组02H02-水阀手动控制值",{"$f":"E252&VLOOKUP(D252,list!$D$3:$F$501,2,FALSE)&F252&\"_\"&VLOOKUP(G252,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_WVMV"},"LAHU02H02_WVMV AT%M988.0 :REAL; (*空调机组02H02-水阀手动控制值*)","LAHU02H02_WVMV          AT%M988.0      :REAL; (*空调机组02H02-水阀手动控制值*)"]
["992.0","验证通过","REAL","空调机组","L","02H02","回风温度换算值","空调机组02H02-回风温度换算值",{"$f":"E253&VLOOKUP(D253,list!$D$3:$F$501,2,FALSE)&F253&\"_\"&VLOOKUP(G253,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_RTS"},"LAHU02H02_RTS AT%M992.0 :REAL; (*空调机组02H02-回风温度换算值*)","LAHU02H02_RTS           AT%M992.0      :REAL; (*空调机组02H02-回风温度换算值*)"]
["996.0","验证通过","BOOL","空调机组","L","02H02","运行时间累积重置","空调机组02H02-运行时间累积重置",{"$f":"E254&VLOOKUP(D254,list!$D$3:$F$501,2,FALSE)&F254&\"_\"&VLOOKUP(G254,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_RST"},"LAHU02H02_RST AT%M996.0 :BOOL; (*空调机组02H02-运行时间累积重置*)","LAHU02H02_RST           AT%M996.0      :BOOL; (*空调机组02H02-运行时间累积重置*)"]
["1000.0","验证通过","REAL","空调机组","L","02H02","运行时间累积重置值","空调机组02H02-运行时间累积重置值",{"$f":"E255&VLOOKUP(D255,list!$D$3:$F$501,2,FALSE)&F255&\"_\"&VLOOKUP(G255,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_RSTV"},"LAHU02H02_RSTV AT%M1000.0 :REAL; (*空调机组02H02-运行时间累积重置值*)","LAHU02H02_RSTV          AT%M1000.0     :REAL; (*空调机组02H02-运行时间累积重置值*)"]
["1004.0","验证通过","BOOL","空调机组","L","02H02","隔离开关1","空调机组02H02-隔离开关1",{"$f":"E256&VLOOKUP(D256,list!$D$3:$F$501,2,FALSE)&F256&\"_\"&VLOOKUP(G256,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_ISO1"},"LAHU02H02_ISO1 AT%M1004.0 :BOOL; (*空调机组02H02-隔离开关1*)","LAHU02H02_ISO1          AT%M1004.0     :BOOL; (*空调机组02H02-隔离开关1*)"]
["1006.0","验证通过","BOOL","空调机组","L","02H02","隔离开关2","空调机组02H02-隔离开关2",{"$f":"E257&VLOOKUP(D257,list!$D$3:$F$501,2,FALSE)&F257&\"_\"&VLOOKUP(G257,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_ISO2"},"LAHU02H02_ISO2 AT%M1006.0 :BOOL; (*空调机组02H02-隔离开关2*)","LAHU02H02_ISO2          AT%M1006.0     :BOOL; (*空调机组02H02-隔离开关2*)"]
["1012.0","验证通过","REAL","空调机组","L","02H02","P调节参数","空调机组02H02-P调节参数",{"$f":"E258&VLOOKUP(D258,list!$D$3:$F$501,2,FALSE)&F258&\"_\"&VLOOKUP(G258,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_VP"},"LAHU02H02_VP AT%M1012.0 :REAL; (*空调机组02H02-P调节参数*)","LAHU02H02_VP            AT%M1012.0     :REAL; (*空调机组02H02-P调节参数*)"]
["1016.0","验证通过","REAL","空调机组","L","02H02","I调节参数","空调机组02H02-I调节参数",{"$f":"E259&VLOOKUP(D259,list!$D$3:$F$501,2,FALSE)&F259&\"_\"&VLOOKUP(G259,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_VI"},"LAHU02H02_VI AT%M1016.0 :REAL; (*空调机组02H02-I调节参数*)","LAHU02H02_VI            AT%M1016.0     :REAL; (*空调机组02H02-I调节参数*)"]
["1020.0","验证通过","REAL","空调机组","L","02H02","运行时间累积值","空调机组02H02-运行时间累积值",{"$f":"E260&VLOOKUP(D260,list!$D$3:$F$501,2,FALSE)&F260&\"_\"&VLOOKUP(G260,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_RH"},"LAHU02H02_RH AT%M1020.0 :REAL; (*空调机组02H02-运行时间累积值*)","LAHU02H02_RH            AT%M1020.0     :REAL; (*空调机组02H02-运行时间累积值*)"]
["1024.0","验证通过","INT","空调机组","L","02H02","设备状态代码","空调机组02H02-设备状态代码",{"$f":"E261&VLOOKUP(D261,list!$D$3:$F$501,2,FALSE)&F261&\"_\"&VLOOKUP(G261,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_SN"},"LAHU02H02_SN AT%M1024.0 :INT; (*空调机组02H02-设备状态代码*)","LAHU02H02_SN            AT%M1024.0     :INT; (*空调机组02H02-设备状态代码*)"]
["1026.0","验证通过","INT","空调机组","L","02H02","水阀控制转换值","空调机组02H02-水阀控制转换值",{"$f":"E262&VLOOKUP(D262,list!$D$3:$F$501,2,FALSE)&F262&\"_\"&VLOOKUP(G262,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_WVCS"},"LAHU02H02_WVCS AT%M1026.0 :INT; (*空调机组02H02-水阀控制转换值*)","LAHU02H02_WVCS          AT%M1026.0     :INT; (*空调机组02H02-水阀控制转换值*)"]
["1028.0","验证通过","BOOL","空调机组","L","02H02","程序控制","空调机组02H02-程序控制",{"$f":"E263&VLOOKUP(D263,list!$D$3:$F$501,2,FALSE)&F263&\"_\"&VLOOKUP(G263,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H02_PC"},"LAHU02H02_PC AT%M1028.0 :BOOL; (*空调机组02H02-程序控制*)","LAHU02H02_PC            AT%M1028.0     :BOOL; (*空调机组02H02-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C263=\"REAL\",C263=\"DWORD\",C263=\"DINT\"),(IF(OR(C265=\"REAL\",C265=\"DWORD\",C265=\"DINT\"),A263+4+MOD(A263,4),A263+4)),(IF(OR(C265=\"REAL\",C265=\"DWORD\",C265=\"DINT\"),A263+4+MOD(A263,4),A263+2)))&\".0\"","v":"1032.0"},{"$f":"IF((IF(OR(C265=\"INT\",C265=\"WORD\",C265=\"BOOL\"),MOD(A265,2),MOD(A265,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H03","设定温度值",{"$f":"D265&F265&\"-\"&IF(E265=\"R\",\"新云平台\"&G265,G265)","v":"空调机组02H03-新云平台设定温度值"},{"$f":"E265&VLOOKUP(D265,list!$D$3:$F$501,2,FALSE)&F265&\"_\"&VLOOKUP(G265,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H03_TSET"},{"$f":"I265&\" \"&\"AT%M\"&A265&\" \"&\":\"&C265&\";\"&\" \"&\"(*\"&H265&\"*)\"","v":"RAHU02H03_TSET AT%M1032.0 :REAL; (*空调机组02H03-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J265,SEARCH(\"AT%\",J265),,REPT(\" \",25-SEARCH(\"AT%\",J265))),SEARCH(\":\",REPLACE(J265,SEARCH(\"AT%\",J265),,REPT(\" \",25-SEARCH(\"AT%\",J265)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J265,SEARCH(\"AT%\",J265),,REPT(\" \",25-SEARCH(\"AT%\",J265))))))","v":"RAHU02H03_TSET          AT%M1032.0     :REAL; (*空调机组02H03-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C265=\"REAL\",C265=\"DWORD\",C265=\"DINT\"),(IF(OR(C266=\"REAL\",C266=\"DWORD\",C266=\"DINT\"),A265+4+MOD(A265,4),A265+4)),(IF(OR(C266=\"REAL\",C266=\"DWORD\",C266=\"DINT\"),A265+4+MOD(A265,4),A265+2)))&\".0\"","v":"1036.0"},"验证通过","INT","空调机组","R",{"$f":"F265","v":"02H03"},"季节模式","空调机组02H03-新云平台季节模式",{"$f":"E266&VLOOKUP(D266,list!$D$3:$F$501,2,FALSE)&F266&\"_\"&VLOOKUP(G266,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H03_SM"},"RAHU02H03_SM AT%M1036.0 :INT; (*空调机组02H03-新云平台季节模式*)","RAHU02H03_SM            AT%M1036.0     :INT; (*空调机组02H03-新云平台季节模式*)"]
["1038.0","验证通过","BOOL","空调机组","R","02H03","程序控制","空调机组02H03-新云平台程序控制",{"$f":"E267&VLOOKUP(D267,list!$D$3:$F$501,2,FALSE)&F267&\"_\"&VLOOKUP(G267,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H03_PC"},"RAHU02H03_PC AT%M1038.0 :BOOL; (*空调机组02H03-新云平台程序控制*)","RAHU02H03_PC            AT%M1038.0     :BOOL; (*空调机组02H03-新云平台程序控制*)"]
["1044.0","验证通过","REAL","空调机组","L","02H03","设定温度值","空调机组02H03-设定温度值",{"$f":"E268&VLOOKUP(D268,list!$D$3:$F$501,2,FALSE)&F268&\"_\"&VLOOKUP(G268,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_TSET"},"LAHU02H03_TSET AT%M1044.0 :REAL; (*空调机组02H03-设定温度值*)","LAHU02H03_TSET          AT%M1044.0     :REAL; (*空调机组02H03-设定温度值*)"]
["1048.0","验证通过","INT","空调机组","L","02H03","季节模式","空调机组02H03-季节模式",{"$f":"E269&VLOOKUP(D269,list!$D$3:$F$501,2,FALSE)&F269&\"_\"&VLOOKUP(G269,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_SM"},"LAHU02H03_SM AT%M1048.0 :INT; (*空调机组02H03-季节模式*)","LAHU02H03_SM            AT%M1048.0     :INT; (*空调机组02H03-季节模式*)"]
["1052.0","验证通过","REAL","空调机组","L","02H03","水阀反馈换算值","空调机组02H03-水阀反馈换算值",{"$f":"E270&VLOOKUP(D270,list!$D$3:$F$501,2,FALSE)&F270&\"_\"&VLOOKUP(G270,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_WVBS"},"LAHU02H03_WVBS AT%M1052.0 :REAL; (*空调机组02H03-水阀反馈换算值*)","LAHU02H03_WVBS          AT%M1052.0     :REAL; (*空调机组02H03-水阀反馈换算值*)"]
["1056.0","验证通过","BOOL","空调机组","L","02H03","水阀手动控制","空调机组02H03-水阀手动控制",{"$f":"E271&VLOOKUP(D271,list!$D$3:$F$501,2,FALSE)&F271&\"_\"&VLOOKUP(G271,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_WVMC"},"LAHU02H03_WVMC AT%M1056.0 :BOOL; (*空调机组02H03-水阀手动控制*)","LAHU02H03_WVMC          AT%M1056.0     :BOOL; (*空调机组02H03-水阀手动控制*)"]
["1060.0","验证通过","REAL","空调机组","L","02H03","水阀手动控制值","空调机组02H03-水阀手动控制值",{"$f":"E272&VLOOKUP(D272,list!$D$3:$F$501,2,FALSE)&F272&\"_\"&VLOOKUP(G272,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_WVMV"},"LAHU02H03_WVMV AT%M1060.0 :REAL; (*空调机组02H03-水阀手动控制值*)","LAHU02H03_WVMV          AT%M1060.0     :REAL; (*空调机组02H03-水阀手动控制值*)"]
["1064.0","验证通过","REAL","空调机组","L","02H03","回风温度换算值","空调机组02H03-回风温度换算值",{"$f":"E273&VLOOKUP(D273,list!$D$3:$F$501,2,FALSE)&F273&\"_\"&VLOOKUP(G273,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_RTS"},"LAHU02H03_RTS AT%M1064.0 :REAL; (*空调机组02H03-回风温度换算值*)","LAHU02H03_RTS           AT%M1064.0     :REAL; (*空调机组02H03-回风温度换算值*)"]
["1068.0","验证通过","BOOL","空调机组","L","02H03","运行时间累积重置","空调机组02H03-运行时间累积重置",{"$f":"E274&VLOOKUP(D274,list!$D$3:$F$501,2,FALSE)&F274&\"_\"&VLOOKUP(G274,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_RST"},"LAHU02H03_RST AT%M1068.0 :BOOL; (*空调机组02H03-运行时间累积重置*)","LAHU02H03_RST           AT%M1068.0     :BOOL; (*空调机组02H03-运行时间累积重置*)"]
["1072.0","验证通过","REAL","空调机组","L","02H03","运行时间累积重置值","空调机组02H03-运行时间累积重置值",{"$f":"E275&VLOOKUP(D275,list!$D$3:$F$501,2,FALSE)&F275&\"_\"&VLOOKUP(G275,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_RSTV"},"LAHU02H03_RSTV AT%M1072.0 :REAL; (*空调机组02H03-运行时间累积重置值*)","LAHU02H03_RSTV          AT%M1072.0     :REAL; (*空调机组02H03-运行时间累积重置值*)"]
["1076.0","验证通过","BOOL","空调机组","L","02H03","隔离开关1","空调机组02H03-隔离开关1",{"$f":"E276&VLOOKUP(D276,list!$D$3:$F$501,2,FALSE)&F276&\"_\"&VLOOKUP(G276,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_ISO1"},"LAHU02H03_ISO1 AT%M1076.0 :BOOL; (*空调机组02H03-隔离开关1*)","LAHU02H03_ISO1          AT%M1076.0     :BOOL; (*空调机组02H03-隔离开关1*)"]
["1078.0","验证通过","BOOL","空调机组","L","02H03","隔离开关2","空调机组02H03-隔离开关2",{"$f":"E277&VLOOKUP(D277,list!$D$3:$F$501,2,FALSE)&F277&\"_\"&VLOOKUP(G277,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_ISO2"},"LAHU02H03_ISO2 AT%M1078.0 :BOOL; (*空调机组02H03-隔离开关2*)","LAHU02H03_ISO2          AT%M1078.0     :BOOL; (*空调机组02H03-隔离开关2*)"]
["1084.0","验证通过","REAL","空调机组","L","02H03","P调节参数","空调机组02H03-P调节参数",{"$f":"E278&VLOOKUP(D278,list!$D$3:$F$501,2,FALSE)&F278&\"_\"&VLOOKUP(G278,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_VP"},"LAHU02H03_VP AT%M1084.0 :REAL; (*空调机组02H03-P调节参数*)","LAHU02H03_VP            AT%M1084.0     :REAL; (*空调机组02H03-P调节参数*)"]
["1088.0","验证通过","REAL","空调机组","L","02H03","I调节参数","空调机组02H03-I调节参数",{"$f":"E279&VLOOKUP(D279,list!$D$3:$F$501,2,FALSE)&F279&\"_\"&VLOOKUP(G279,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_VI"},"LAHU02H03_VI AT%M1088.0 :REAL; (*空调机组02H03-I调节参数*)","LAHU02H03_VI            AT%M1088.0     :REAL; (*空调机组02H03-I调节参数*)"]
["1092.0","验证通过","REAL","空调机组","L","02H03","运行时间累积值","空调机组02H03-运行时间累积值",{"$f":"E280&VLOOKUP(D280,list!$D$3:$F$501,2,FALSE)&F280&\"_\"&VLOOKUP(G280,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_RH"},"LAHU02H03_RH AT%M1092.0 :REAL; (*空调机组02H03-运行时间累积值*)","LAHU02H03_RH            AT%M1092.0     :REAL; (*空调机组02H03-运行时间累积值*)"]
["1096.0","验证通过","INT","空调机组","L","02H03","设备状态代码","空调机组02H03-设备状态代码",{"$f":"E281&VLOOKUP(D281,list!$D$3:$F$501,2,FALSE)&F281&\"_\"&VLOOKUP(G281,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_SN"},"LAHU02H03_SN AT%M1096.0 :INT; (*空调机组02H03-设备状态代码*)","LAHU02H03_SN            AT%M1096.0     :INT; (*空调机组02H03-设备状态代码*)"]
["1098.0","验证通过","INT","空调机组","L","02H03","水阀控制转换值","空调机组02H03-水阀控制转换值",{"$f":"E282&VLOOKUP(D282,list!$D$3:$F$501,2,FALSE)&F282&\"_\"&VLOOKUP(G282,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_WVCS"},"LAHU02H03_WVCS AT%M1098.0 :INT; (*空调机组02H03-水阀控制转换值*)","LAHU02H03_WVCS          AT%M1098.0     :INT; (*空调机组02H03-水阀控制转换值*)"]
["1100.0","验证通过","BOOL","空调机组","L","02H03","程序控制","空调机组02H03-程序控制",{"$f":"E283&VLOOKUP(D283,list!$D$3:$F$501,2,FALSE)&F283&\"_\"&VLOOKUP(G283,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H03_PC"},"LAHU02H03_PC AT%M1100.0 :BOOL; (*空调机组02H03-程序控制*)","LAHU02H03_PC            AT%M1100.0     :BOOL; (*空调机组02H03-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C283=\"REAL\",C283=\"DWORD\",C283=\"DINT\"),(IF(OR(C285=\"REAL\",C285=\"DWORD\",C285=\"DINT\"),A283+4+MOD(A283,4),A283+4)),(IF(OR(C285=\"REAL\",C285=\"DWORD\",C285=\"DINT\"),A283+4+MOD(A283,4),A283+2)))&\".0\"","v":"1104.0"},{"$f":"IF((IF(OR(C285=\"INT\",C285=\"WORD\",C285=\"BOOL\"),MOD(A285,2),MOD(A285,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H04","设定温度值",{"$f":"D285&F285&\"-\"&IF(E285=\"R\",\"新云平台\"&G285,G285)","v":"空调机组02H04-新云平台设定温度值"},{"$f":"E285&VLOOKUP(D285,list!$D$3:$F$501,2,FALSE)&F285&\"_\"&VLOOKUP(G285,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H04_TSET"},{"$f":"I285&\" \"&\"AT%M\"&A285&\" \"&\":\"&C285&\";\"&\" \"&\"(*\"&H285&\"*)\"","v":"RAHU02H04_TSET AT%M1104.0 :REAL; (*空调机组02H04-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J285,SEARCH(\"AT%\",J285),,REPT(\" \",25-SEARCH(\"AT%\",J285))),SEARCH(\":\",REPLACE(J285,SEARCH(\"AT%\",J285),,REPT(\" \",25-SEARCH(\"AT%\",J285)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J285,SEARCH(\"AT%\",J285),,REPT(\" \",25-SEARCH(\"AT%\",J285))))))","v":"RAHU02H04_TSET          AT%M1104.0     :REAL; (*空调机组02H04-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C285=\"REAL\",C285=\"DWORD\",C285=\"DINT\"),(IF(OR(C286=\"REAL\",C286=\"DWORD\",C286=\"DINT\"),A285+4+MOD(A285,4),A285+4)),(IF(OR(C286=\"REAL\",C286=\"DWORD\",C286=\"DINT\"),A285+4+MOD(A285,4),A285+2)))&\".0\"","v":"1108.0"},"验证通过","INT","空调机组","R",{"$f":"F285","v":"02H04"},"季节模式","空调机组02H04-新云平台季节模式",{"$f":"E286&VLOOKUP(D286,list!$D$3:$F$501,2,FALSE)&F286&\"_\"&VLOOKUP(G286,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H04_SM"},"RAHU02H04_SM AT%M1108.0 :INT; (*空调机组02H04-新云平台季节模式*)","RAHU02H04_SM            AT%M1108.0     :INT; (*空调机组02H04-新云平台季节模式*)"]
["1110.0","验证通过","BOOL","空调机组","R","02H04","程序控制","空调机组02H04-新云平台程序控制",{"$f":"E287&VLOOKUP(D287,list!$D$3:$F$501,2,FALSE)&F287&\"_\"&VLOOKUP(G287,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H04_PC"},"RAHU02H04_PC AT%M1110.0 :BOOL; (*空调机组02H04-新云平台程序控制*)","RAHU02H04_PC            AT%M1110.0     :BOOL; (*空调机组02H04-新云平台程序控制*)"]
["1116.0","验证通过","REAL","空调机组","L","02H04","设定温度值","空调机组02H04-设定温度值",{"$f":"E288&VLOOKUP(D288,list!$D$3:$F$501,2,FALSE)&F288&\"_\"&VLOOKUP(G288,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_TSET"},"LAHU02H04_TSET AT%M1116.0 :REAL; (*空调机组02H04-设定温度值*)","LAHU02H04_TSET          AT%M1116.0     :REAL; (*空调机组02H04-设定温度值*)"]
["1120.0","验证通过","INT","空调机组","L","02H04","季节模式","空调机组02H04-季节模式",{"$f":"E289&VLOOKUP(D289,list!$D$3:$F$501,2,FALSE)&F289&\"_\"&VLOOKUP(G289,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_SM"},"LAHU02H04_SM AT%M1120.0 :INT; (*空调机组02H04-季节模式*)","LAHU02H04_SM            AT%M1120.0     :INT; (*空调机组02H04-季节模式*)"]
["1124.0","验证通过","REAL","空调机组","L","02H04","水阀反馈换算值","空调机组02H04-水阀反馈换算值",{"$f":"E290&VLOOKUP(D290,list!$D$3:$F$501,2,FALSE)&F290&\"_\"&VLOOKUP(G290,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_WVBS"},"LAHU02H04_WVBS AT%M1124.0 :REAL; (*空调机组02H04-水阀反馈换算值*)","LAHU02H04_WVBS          AT%M1124.0     :REAL; (*空调机组02H04-水阀反馈换算值*)"]
["1128.0","验证通过","BOOL","空调机组","L","02H04","水阀手动控制","空调机组02H04-水阀手动控制",{"$f":"E291&VLOOKUP(D291,list!$D$3:$F$501,2,FALSE)&F291&\"_\"&VLOOKUP(G291,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_WVMC"},"LAHU02H04_WVMC AT%M1128.0 :BOOL; (*空调机组02H04-水阀手动控制*)","LAHU02H04_WVMC          AT%M1128.0     :BOOL; (*空调机组02H04-水阀手动控制*)"]
["1132.0","验证通过","REAL","空调机组","L","02H04","水阀手动控制值","空调机组02H04-水阀手动控制值",{"$f":"E292&VLOOKUP(D292,list!$D$3:$F$501,2,FALSE)&F292&\"_\"&VLOOKUP(G292,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_WVMV"},"LAHU02H04_WVMV AT%M1132.0 :REAL; (*空调机组02H04-水阀手动控制值*)","LAHU02H04_WVMV          AT%M1132.0     :REAL; (*空调机组02H04-水阀手动控制值*)"]
["1136.0","验证通过","REAL","空调机组","L","02H04","回风温度换算值","空调机组02H04-回风温度换算值",{"$f":"E293&VLOOKUP(D293,list!$D$3:$F$501,2,FALSE)&F293&\"_\"&VLOOKUP(G293,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_RTS"},"LAHU02H04_RTS AT%M1136.0 :REAL; (*空调机组02H04-回风温度换算值*)","LAHU02H04_RTS           AT%M1136.0     :REAL; (*空调机组02H04-回风温度换算值*)"]
["1140.0","验证通过","BOOL","空调机组","L","02H04","运行时间累积重置","空调机组02H04-运行时间累积重置",{"$f":"E294&VLOOKUP(D294,list!$D$3:$F$501,2,FALSE)&F294&\"_\"&VLOOKUP(G294,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_RST"},"LAHU02H04_RST AT%M1140.0 :BOOL; (*空调机组02H04-运行时间累积重置*)","LAHU02H04_RST           AT%M1140.0     :BOOL; (*空调机组02H04-运行时间累积重置*)"]
["1144.0","验证通过","REAL","空调机组","L","02H04","运行时间累积重置值","空调机组02H04-运行时间累积重置值",{"$f":"E295&VLOOKUP(D295,list!$D$3:$F$501,2,FALSE)&F295&\"_\"&VLOOKUP(G295,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_RSTV"},"LAHU02H04_RSTV AT%M1144.0 :REAL; (*空调机组02H04-运行时间累积重置值*)","LAHU02H04_RSTV          AT%M1144.0     :REAL; (*空调机组02H04-运行时间累积重置值*)"]
["1148.0","验证通过","BOOL","空调机组","L","02H04","隔离开关1","空调机组02H04-隔离开关1",{"$f":"E296&VLOOKUP(D296,list!$D$3:$F$501,2,FALSE)&F296&\"_\"&VLOOKUP(G296,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_ISO1"},"LAHU02H04_ISO1 AT%M1148.0 :BOOL; (*空调机组02H04-隔离开关1*)","LAHU02H04_ISO1          AT%M1148.0     :BOOL; (*空调机组02H04-隔离开关1*)"]
["1150.0","验证通过","BOOL","空调机组","L","02H04","隔离开关2","空调机组02H04-隔离开关2",{"$f":"E297&VLOOKUP(D297,list!$D$3:$F$501,2,FALSE)&F297&\"_\"&VLOOKUP(G297,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_ISO2"},"LAHU02H04_ISO2 AT%M1150.0 :BOOL; (*空调机组02H04-隔离开关2*)","LAHU02H04_ISO2          AT%M1150.0     :BOOL; (*空调机组02H04-隔离开关2*)"]
["1156.0","验证通过","REAL","空调机组","L","02H04","P调节参数","空调机组02H04-P调节参数",{"$f":"E298&VLOOKUP(D298,list!$D$3:$F$501,2,FALSE)&F298&\"_\"&VLOOKUP(G298,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_VP"},"LAHU02H04_VP AT%M1156.0 :REAL; (*空调机组02H04-P调节参数*)","LAHU02H04_VP            AT%M1156.0     :REAL; (*空调机组02H04-P调节参数*)"]
["1160.0","验证通过","REAL","空调机组","L","02H04","I调节参数","空调机组02H04-I调节参数",{"$f":"E299&VLOOKUP(D299,list!$D$3:$F$501,2,FALSE)&F299&\"_\"&VLOOKUP(G299,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_VI"},"LAHU02H04_VI AT%M1160.0 :REAL; (*空调机组02H04-I调节参数*)","LAHU02H04_VI            AT%M1160.0     :REAL; (*空调机组02H04-I调节参数*)"]
["1164.0","验证通过","REAL","空调机组","L","02H04","运行时间累积值","空调机组02H04-运行时间累积值",{"$f":"E300&VLOOKUP(D300,list!$D$3:$F$501,2,FALSE)&F300&\"_\"&VLOOKUP(G300,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_RH"},"LAHU02H04_RH AT%M1164.0 :REAL; (*空调机组02H04-运行时间累积值*)","LAHU02H04_RH            AT%M1164.0     :REAL; (*空调机组02H04-运行时间累积值*)"]
["1168.0","验证通过","INT","空调机组","L","02H04","设备状态代码","空调机组02H04-设备状态代码",{"$f":"E301&VLOOKUP(D301,list!$D$3:$F$501,2,FALSE)&F301&\"_\"&VLOOKUP(G301,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_SN"},"LAHU02H04_SN AT%M1168.0 :INT; (*空调机组02H04-设备状态代码*)","LAHU02H04_SN            AT%M1168.0     :INT; (*空调机组02H04-设备状态代码*)"]
["1170.0","验证通过","INT","空调机组","L","02H04","水阀控制转换值","空调机组02H04-水阀控制转换值",{"$f":"E302&VLOOKUP(D302,list!$D$3:$F$501,2,FALSE)&F302&\"_\"&VLOOKUP(G302,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_WVCS"},"LAHU02H04_WVCS AT%M1170.0 :INT; (*空调机组02H04-水阀控制转换值*)","LAHU02H04_WVCS          AT%M1170.0     :INT; (*空调机组02H04-水阀控制转换值*)"]
["1172.0","验证通过","BOOL","空调机组","L","02H04","程序控制","空调机组02H04-程序控制",{"$f":"E303&VLOOKUP(D303,list!$D$3:$F$501,2,FALSE)&F303&\"_\"&VLOOKUP(G303,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H04_PC"},"LAHU02H04_PC AT%M1172.0 :BOOL; (*空调机组02H04-程序控制*)","LAHU02H04_PC            AT%M1172.0     :BOOL; (*空调机组02H04-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C303=\"REAL\",C303=\"DWORD\",C303=\"DINT\"),(IF(OR(C305=\"REAL\",C305=\"DWORD\",C305=\"DINT\"),A303+4+MOD(A303,4),A303+4)),(IF(OR(C305=\"REAL\",C305=\"DWORD\",C305=\"DINT\"),A303+4+MOD(A303,4),A303+2)))&\".0\"","v":"1176.0"},{"$f":"IF((IF(OR(C305=\"INT\",C305=\"WORD\",C305=\"BOOL\"),MOD(A305,2),MOD(A305,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H05","设定温度值",{"$f":"D305&F305&\"-\"&IF(E305=\"R\",\"新云平台\"&G305,G305)","v":"空调机组02H05-新云平台设定温度值"},{"$f":"E305&VLOOKUP(D305,list!$D$3:$F$501,2,FALSE)&F305&\"_\"&VLOOKUP(G305,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H05_TSET"},{"$f":"I305&\" \"&\"AT%M\"&A305&\" \"&\":\"&C305&\";\"&\" \"&\"(*\"&H305&\"*)\"","v":"RAHU02H05_TSET AT%M1176.0 :REAL; (*空调机组02H05-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J305,SEARCH(\"AT%\",J305),,REPT(\" \",25-SEARCH(\"AT%\",J305))),SEARCH(\":\",REPLACE(J305,SEARCH(\"AT%\",J305),,REPT(\" \",25-SEARCH(\"AT%\",J305)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J305,SEARCH(\"AT%\",J305),,REPT(\" \",25-SEARCH(\"AT%\",J305))))))","v":"RAHU02H05_TSET          AT%M1176.0     :REAL; (*空调机组02H05-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C305=\"REAL\",C305=\"DWORD\",C305=\"DINT\"),(IF(OR(C306=\"REAL\",C306=\"DWORD\",C306=\"DINT\"),A305+4+MOD(A305,4),A305+4)),(IF(OR(C306=\"REAL\",C306=\"DWORD\",C306=\"DINT\"),A305+4+MOD(A305,4),A305+2)))&\".0\"","v":"1180.0"},"验证通过","INT","空调机组","R",{"$f":"F305","v":"02H05"},"季节模式","空调机组02H05-新云平台季节模式",{"$f":"E306&VLOOKUP(D306,list!$D$3:$F$501,2,FALSE)&F306&\"_\"&VLOOKUP(G306,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H05_SM"},"RAHU02H05_SM AT%M1180.0 :INT; (*空调机组02H05-新云平台季节模式*)","RAHU02H05_SM            AT%M1180.0     :INT; (*空调机组02H05-新云平台季节模式*)"]
["1182.0","验证通过","BOOL","空调机组","R","02H05","程序控制","空调机组02H05-新云平台程序控制",{"$f":"E307&VLOOKUP(D307,list!$D$3:$F$501,2,FALSE)&F307&\"_\"&VLOOKUP(G307,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H05_PC"},"RAHU02H05_PC AT%M1182.0 :BOOL; (*空调机组02H05-新云平台程序控制*)","RAHU02H05_PC            AT%M1182.0     :BOOL; (*空调机组02H05-新云平台程序控制*)"]
["1188.0","验证通过","REAL","空调机组","L","02H05","设定温度值","空调机组02H05-设定温度值",{"$f":"E308&VLOOKUP(D308,list!$D$3:$F$501,2,FALSE)&F308&\"_\"&VLOOKUP(G308,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_TSET"},"LAHU02H05_TSET AT%M1188.0 :REAL; (*空调机组02H05-设定温度值*)","LAHU02H05_TSET          AT%M1188.0     :REAL; (*空调机组02H05-设定温度值*)"]
["1192.0","验证通过","INT","空调机组","L","02H05","季节模式","空调机组02H05-季节模式",{"$f":"E309&VLOOKUP(D309,list!$D$3:$F$501,2,FALSE)&F309&\"_\"&VLOOKUP(G309,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_SM"},"LAHU02H05_SM AT%M1192.0 :INT; (*空调机组02H05-季节模式*)","LAHU02H05_SM            AT%M1192.0     :INT; (*空调机组02H05-季节模式*)"]
["1196.0","验证通过","REAL","空调机组","L","02H05","水阀反馈换算值","空调机组02H05-水阀反馈换算值",{"$f":"E310&VLOOKUP(D310,list!$D$3:$F$501,2,FALSE)&F310&\"_\"&VLOOKUP(G310,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_WVBS"},"LAHU02H05_WVBS AT%M1196.0 :REAL; (*空调机组02H05-水阀反馈换算值*)","LAHU02H05_WVBS          AT%M1196.0     :REAL; (*空调机组02H05-水阀反馈换算值*)"]
["1200.0","验证通过","BOOL","空调机组","L","02H05","水阀手动控制","空调机组02H05-水阀手动控制",{"$f":"E311&VLOOKUP(D311,list!$D$3:$F$501,2,FALSE)&F311&\"_\"&VLOOKUP(G311,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_WVMC"},"LAHU02H05_WVMC AT%M1200.0 :BOOL; (*空调机组02H05-水阀手动控制*)","LAHU02H05_WVMC          AT%M1200.0     :BOOL; (*空调机组02H05-水阀手动控制*)"]
["1204.0","验证通过","REAL","空调机组","L","02H05","水阀手动控制值","空调机组02H05-水阀手动控制值",{"$f":"E312&VLOOKUP(D312,list!$D$3:$F$501,2,FALSE)&F312&\"_\"&VLOOKUP(G312,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_WVMV"},"LAHU02H05_WVMV AT%M1204.0 :REAL; (*空调机组02H05-水阀手动控制值*)","LAHU02H05_WVMV          AT%M1204.0     :REAL; (*空调机组02H05-水阀手动控制值*)"]
["1208.0","验证通过","REAL","空调机组","L","02H05","回风温度换算值","空调机组02H05-回风温度换算值",{"$f":"E313&VLOOKUP(D313,list!$D$3:$F$501,2,FALSE)&F313&\"_\"&VLOOKUP(G313,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_RTS"},"LAHU02H05_RTS AT%M1208.0 :REAL; (*空调机组02H05-回风温度换算值*)","LAHU02H05_RTS           AT%M1208.0     :REAL; (*空调机组02H05-回风温度换算值*)"]
["1212.0","验证通过","BOOL","空调机组","L","02H05","运行时间累积重置","空调机组02H05-运行时间累积重置",{"$f":"E314&VLOOKUP(D314,list!$D$3:$F$501,2,FALSE)&F314&\"_\"&VLOOKUP(G314,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_RST"},"LAHU02H05_RST AT%M1212.0 :BOOL; (*空调机组02H05-运行时间累积重置*)","LAHU02H05_RST           AT%M1212.0     :BOOL; (*空调机组02H05-运行时间累积重置*)"]
["1216.0","验证通过","REAL","空调机组","L","02H05","运行时间累积重置值","空调机组02H05-运行时间累积重置值",{"$f":"E315&VLOOKUP(D315,list!$D$3:$F$501,2,FALSE)&F315&\"_\"&VLOOKUP(G315,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_RSTV"},"LAHU02H05_RSTV AT%M1216.0 :REAL; (*空调机组02H05-运行时间累积重置值*)","LAHU02H05_RSTV          AT%M1216.0     :REAL; (*空调机组02H05-运行时间累积重置值*)"]
["1220.0","验证通过","BOOL","空调机组","L","02H05","隔离开关1","空调机组02H05-隔离开关1",{"$f":"E316&VLOOKUP(D316,list!$D$3:$F$501,2,FALSE)&F316&\"_\"&VLOOKUP(G316,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_ISO1"},"LAHU02H05_ISO1 AT%M1220.0 :BOOL; (*空调机组02H05-隔离开关1*)","LAHU02H05_ISO1          AT%M1220.0     :BOOL; (*空调机组02H05-隔离开关1*)"]
["1222.0","验证通过","BOOL","空调机组","L","02H05","隔离开关2","空调机组02H05-隔离开关2",{"$f":"E317&VLOOKUP(D317,list!$D$3:$F$501,2,FALSE)&F317&\"_\"&VLOOKUP(G317,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_ISO2"},"LAHU02H05_ISO2 AT%M1222.0 :BOOL; (*空调机组02H05-隔离开关2*)","LAHU02H05_ISO2          AT%M1222.0     :BOOL; (*空调机组02H05-隔离开关2*)"]
["1228.0","验证通过","REAL","空调机组","L","02H05","P调节参数","空调机组02H05-P调节参数",{"$f":"E318&VLOOKUP(D318,list!$D$3:$F$501,2,FALSE)&F318&\"_\"&VLOOKUP(G318,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_VP"},"LAHU02H05_VP AT%M1228.0 :REAL; (*空调机组02H05-P调节参数*)","LAHU02H05_VP            AT%M1228.0     :REAL; (*空调机组02H05-P调节参数*)"]
["1232.0","验证通过","REAL","空调机组","L","02H05","I调节参数","空调机组02H05-I调节参数",{"$f":"E319&VLOOKUP(D319,list!$D$3:$F$501,2,FALSE)&F319&\"_\"&VLOOKUP(G319,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_VI"},"LAHU02H05_VI AT%M1232.0 :REAL; (*空调机组02H05-I调节参数*)","LAHU02H05_VI            AT%M1232.0     :REAL; (*空调机组02H05-I调节参数*)"]
["1236.0","验证通过","REAL","空调机组","L","02H05","运行时间累积值","空调机组02H05-运行时间累积值",{"$f":"E320&VLOOKUP(D320,list!$D$3:$F$501,2,FALSE)&F320&\"_\"&VLOOKUP(G320,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_RH"},"LAHU02H05_RH AT%M1236.0 :REAL; (*空调机组02H05-运行时间累积值*)","LAHU02H05_RH            AT%M1236.0     :REAL; (*空调机组02H05-运行时间累积值*)"]
["1240.0","验证通过","INT","空调机组","L","02H05","设备状态代码","空调机组02H05-设备状态代码",{"$f":"E321&VLOOKUP(D321,list!$D$3:$F$501,2,FALSE)&F321&\"_\"&VLOOKUP(G321,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_SN"},"LAHU02H05_SN AT%M1240.0 :INT; (*空调机组02H05-设备状态代码*)","LAHU02H05_SN            AT%M1240.0     :INT; (*空调机组02H05-设备状态代码*)"]
["1242.0","验证通过","INT","空调机组","L","02H05","水阀控制转换值","空调机组02H05-水阀控制转换值",{"$f":"E322&VLOOKUP(D322,list!$D$3:$F$501,2,FALSE)&F322&\"_\"&VLOOKUP(G322,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_WVCS"},"LAHU02H05_WVCS AT%M1242.0 :INT; (*空调机组02H05-水阀控制转换值*)","LAHU02H05_WVCS          AT%M1242.0     :INT; (*空调机组02H05-水阀控制转换值*)"]
["1244.0","验证通过","BOOL","空调机组","L","02H05","程序控制","空调机组02H05-程序控制",{"$f":"E323&VLOOKUP(D323,list!$D$3:$F$501,2,FALSE)&F323&\"_\"&VLOOKUP(G323,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H05_PC"},"LAHU02H05_PC AT%M1244.0 :BOOL; (*空调机组02H05-程序控制*)","LAHU02H05_PC            AT%M1244.0     :BOOL; (*空调机组02H05-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C323=\"REAL\",C323=\"DWORD\",C323=\"DINT\"),(IF(OR(C325=\"REAL\",C325=\"DWORD\",C325=\"DINT\"),A323+4+MOD(A323,4),A323+4)),(IF(OR(C325=\"REAL\",C325=\"DWORD\",C325=\"DINT\"),A323+4+MOD(A323,4),A323+2)))&\".0\"","v":"1248.0"},{"$f":"IF((IF(OR(C325=\"INT\",C325=\"WORD\",C325=\"BOOL\"),MOD(A325,2),MOD(A325,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H06","设定温度值",{"$f":"D325&F325&\"-\"&IF(E325=\"R\",\"新云平台\"&G325,G325)","v":"空调机组02H06-新云平台设定温度值"},{"$f":"E325&VLOOKUP(D325,list!$D$3:$F$501,2,FALSE)&F325&\"_\"&VLOOKUP(G325,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H06_TSET"},{"$f":"I325&\" \"&\"AT%M\"&A325&\" \"&\":\"&C325&\";\"&\" \"&\"(*\"&H325&\"*)\"","v":"RAHU02H06_TSET AT%M1248.0 :REAL; (*空调机组02H06-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J325,SEARCH(\"AT%\",J325),,REPT(\" \",25-SEARCH(\"AT%\",J325))),SEARCH(\":\",REPLACE(J325,SEARCH(\"AT%\",J325),,REPT(\" \",25-SEARCH(\"AT%\",J325)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J325,SEARCH(\"AT%\",J325),,REPT(\" \",25-SEARCH(\"AT%\",J325))))))","v":"RAHU02H06_TSET          AT%M1248.0     :REAL; (*空调机组02H06-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C325=\"REAL\",C325=\"DWORD\",C325=\"DINT\"),(IF(OR(C326=\"REAL\",C326=\"DWORD\",C326=\"DINT\"),A325+4+MOD(A325,4),A325+4)),(IF(OR(C326=\"REAL\",C326=\"DWORD\",C326=\"DINT\"),A325+4+MOD(A325,4),A325+2)))&\".0\"","v":"1252.0"},"验证通过","INT","空调机组","R",{"$f":"F325","v":"02H06"},"季节模式","空调机组02H06-新云平台季节模式",{"$f":"E326&VLOOKUP(D326,list!$D$3:$F$501,2,FALSE)&F326&\"_\"&VLOOKUP(G326,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H06_SM"},"RAHU02H06_SM AT%M1252.0 :INT; (*空调机组02H06-新云平台季节模式*)","RAHU02H06_SM            AT%M1252.0     :INT; (*空调机组02H06-新云平台季节模式*)"]
["1254.0","验证通过","BOOL","空调机组","R","02H06","程序控制","空调机组02H06-新云平台程序控制",{"$f":"E327&VLOOKUP(D327,list!$D$3:$F$501,2,FALSE)&F327&\"_\"&VLOOKUP(G327,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H06_PC"},"RAHU02H06_PC AT%M1254.0 :BOOL; (*空调机组02H06-新云平台程序控制*)","RAHU02H06_PC            AT%M1254.0     :BOOL; (*空调机组02H06-新云平台程序控制*)"]
["1260.0","验证通过","REAL","空调机组","L","02H06","设定温度值","空调机组02H06-设定温度值",{"$f":"E328&VLOOKUP(D328,list!$D$3:$F$501,2,FALSE)&F328&\"_\"&VLOOKUP(G328,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_TSET"},"LAHU02H06_TSET AT%M1260.0 :REAL; (*空调机组02H06-设定温度值*)","LAHU02H06_TSET          AT%M1260.0     :REAL; (*空调机组02H06-设定温度值*)"]
["1264.0","验证通过","INT","空调机组","L","02H06","季节模式","空调机组02H06-季节模式",{"$f":"E329&VLOOKUP(D329,list!$D$3:$F$501,2,FALSE)&F329&\"_\"&VLOOKUP(G329,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_SM"},"LAHU02H06_SM AT%M1264.0 :INT; (*空调机组02H06-季节模式*)","LAHU02H06_SM            AT%M1264.0     :INT; (*空调机组02H06-季节模式*)"]
["1268.0","验证通过","REAL","空调机组","L","02H06","水阀反馈换算值","空调机组02H06-水阀反馈换算值",{"$f":"E330&VLOOKUP(D330,list!$D$3:$F$501,2,FALSE)&F330&\"_\"&VLOOKUP(G330,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_WVBS"},"LAHU02H06_WVBS AT%M1268.0 :REAL; (*空调机组02H06-水阀反馈换算值*)","LAHU02H06_WVBS          AT%M1268.0     :REAL; (*空调机组02H06-水阀反馈换算值*)"]
["1272.0","验证通过","BOOL","空调机组","L","02H06","水阀手动控制","空调机组02H06-水阀手动控制",{"$f":"E331&VLOOKUP(D331,list!$D$3:$F$501,2,FALSE)&F331&\"_\"&VLOOKUP(G331,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_WVMC"},"LAHU02H06_WVMC AT%M1272.0 :BOOL; (*空调机组02H06-水阀手动控制*)","LAHU02H06_WVMC          AT%M1272.0     :BOOL; (*空调机组02H06-水阀手动控制*)"]
["1276.0","验证通过","REAL","空调机组","L","02H06","水阀手动控制值","空调机组02H06-水阀手动控制值",{"$f":"E332&VLOOKUP(D332,list!$D$3:$F$501,2,FALSE)&F332&\"_\"&VLOOKUP(G332,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_WVMV"},"LAHU02H06_WVMV AT%M1276.0 :REAL; (*空调机组02H06-水阀手动控制值*)","LAHU02H06_WVMV          AT%M1276.0     :REAL; (*空调机组02H06-水阀手动控制值*)"]
["1280.0","验证通过","REAL","空调机组","L","02H06","回风温度换算值","空调机组02H06-回风温度换算值",{"$f":"E333&VLOOKUP(D333,list!$D$3:$F$501,2,FALSE)&F333&\"_\"&VLOOKUP(G333,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_RTS"},"LAHU02H06_RTS AT%M1280.0 :REAL; (*空调机组02H06-回风温度换算值*)","LAHU02H06_RTS           AT%M1280.0     :REAL; (*空调机组02H06-回风温度换算值*)"]
["1284.0","验证通过","BOOL","空调机组","L","02H06","运行时间累积重置","空调机组02H06-运行时间累积重置",{"$f":"E334&VLOOKUP(D334,list!$D$3:$F$501,2,FALSE)&F334&\"_\"&VLOOKUP(G334,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_RST"},"LAHU02H06_RST AT%M1284.0 :BOOL; (*空调机组02H06-运行时间累积重置*)","LAHU02H06_RST           AT%M1284.0     :BOOL; (*空调机组02H06-运行时间累积重置*)"]
["1288.0","验证通过","REAL","空调机组","L","02H06","运行时间累积重置值","空调机组02H06-运行时间累积重置值",{"$f":"E335&VLOOKUP(D335,list!$D$3:$F$501,2,FALSE)&F335&\"_\"&VLOOKUP(G335,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_RSTV"},"LAHU02H06_RSTV AT%M1288.0 :REAL; (*空调机组02H06-运行时间累积重置值*)","LAHU02H06_RSTV          AT%M1288.0     :REAL; (*空调机组02H06-运行时间累积重置值*)"]
["1292.0","验证通过","BOOL","空调机组","L","02H06","隔离开关1","空调机组02H06-隔离开关1",{"$f":"E336&VLOOKUP(D336,list!$D$3:$F$501,2,FALSE)&F336&\"_\"&VLOOKUP(G336,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_ISO1"},"LAHU02H06_ISO1 AT%M1292.0 :BOOL; (*空调机组02H06-隔离开关1*)","LAHU02H06_ISO1          AT%M1292.0     :BOOL; (*空调机组02H06-隔离开关1*)"]
["1294.0","验证通过","BOOL","空调机组","L","02H06","隔离开关2","空调机组02H06-隔离开关2",{"$f":"E337&VLOOKUP(D337,list!$D$3:$F$501,2,FALSE)&F337&\"_\"&VLOOKUP(G337,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_ISO2"},"LAHU02H06_ISO2 AT%M1294.0 :BOOL; (*空调机组02H06-隔离开关2*)","LAHU02H06_ISO2          AT%M1294.0     :BOOL; (*空调机组02H06-隔离开关2*)"]
["1300.0","验证通过","REAL","空调机组","L","02H06","P调节参数","空调机组02H06-P调节参数",{"$f":"E338&VLOOKUP(D338,list!$D$3:$F$501,2,FALSE)&F338&\"_\"&VLOOKUP(G338,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_VP"},"LAHU02H06_VP AT%M1300.0 :REAL; (*空调机组02H06-P调节参数*)","LAHU02H06_VP            AT%M1300.0     :REAL; (*空调机组02H06-P调节参数*)"]
["1304.0","验证通过","REAL","空调机组","L","02H06","I调节参数","空调机组02H06-I调节参数",{"$f":"E339&VLOOKUP(D339,list!$D$3:$F$501,2,FALSE)&F339&\"_\"&VLOOKUP(G339,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_VI"},"LAHU02H06_VI AT%M1304.0 :REAL; (*空调机组02H06-I调节参数*)","LAHU02H06_VI            AT%M1304.0     :REAL; (*空调机组02H06-I调节参数*)"]
["1308.0","验证通过","REAL","空调机组","L","02H06","运行时间累积值","空调机组02H06-运行时间累积值",{"$f":"E340&VLOOKUP(D340,list!$D$3:$F$501,2,FALSE)&F340&\"_\"&VLOOKUP(G340,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_RH"},"LAHU02H06_RH AT%M1308.0 :REAL; (*空调机组02H06-运行时间累积值*)","LAHU02H06_RH            AT%M1308.0     :REAL; (*空调机组02H06-运行时间累积值*)"]
["1312.0","验证通过","INT","空调机组","L","02H06","设备状态代码","空调机组02H06-设备状态代码",{"$f":"E341&VLOOKUP(D341,list!$D$3:$F$501,2,FALSE)&F341&\"_\"&VLOOKUP(G341,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_SN"},"LAHU02H06_SN AT%M1312.0 :INT; (*空调机组02H06-设备状态代码*)","LAHU02H06_SN            AT%M1312.0     :INT; (*空调机组02H06-设备状态代码*)"]
["1314.0","验证通过","INT","空调机组","L","02H06","水阀控制转换值","空调机组02H06-水阀控制转换值",{"$f":"E342&VLOOKUP(D342,list!$D$3:$F$501,2,FALSE)&F342&\"_\"&VLOOKUP(G342,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_WVCS"},"LAHU02H06_WVCS AT%M1314.0 :INT; (*空调机组02H06-水阀控制转换值*)","LAHU02H06_WVCS          AT%M1314.0     :INT; (*空调机组02H06-水阀控制转换值*)"]
["1316.0","验证通过","BOOL","空调机组","L","02H06","程序控制","空调机组02H06-程序控制",{"$f":"E343&VLOOKUP(D343,list!$D$3:$F$501,2,FALSE)&F343&\"_\"&VLOOKUP(G343,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H06_PC"},"LAHU02H06_PC AT%M1316.0 :BOOL; (*空调机组02H06-程序控制*)","LAHU02H06_PC            AT%M1316.0     :BOOL; (*空调机组02H06-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C343=\"REAL\",C343=\"DWORD\",C343=\"DINT\"),(IF(OR(C345=\"REAL\",C345=\"DWORD\",C345=\"DINT\"),A343+4+MOD(A343,4),A343+4)),(IF(OR(C345=\"REAL\",C345=\"DWORD\",C345=\"DINT\"),A343+4+MOD(A343,4),A343+2)))&\".0\"","v":"1320.0"},{"$f":"IF((IF(OR(C345=\"INT\",C345=\"WORD\",C345=\"BOOL\"),MOD(A345,2),MOD(A345,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H07","设定温度值",{"$f":"D345&F345&\"-\"&IF(E345=\"R\",\"新云平台\"&G345,G345)","v":"空调机组02H07-新云平台设定温度值"},{"$f":"E345&VLOOKUP(D345,list!$D$3:$F$501,2,FALSE)&F345&\"_\"&VLOOKUP(G345,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H07_TSET"},{"$f":"I345&\" \"&\"AT%M\"&A345&\" \"&\":\"&C345&\";\"&\" \"&\"(*\"&H345&\"*)\"","v":"RAHU02H07_TSET AT%M1320.0 :REAL; (*空调机组02H07-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J345,SEARCH(\"AT%\",J345),,REPT(\" \",25-SEARCH(\"AT%\",J345))),SEARCH(\":\",REPLACE(J345,SEARCH(\"AT%\",J345),,REPT(\" \",25-SEARCH(\"AT%\",J345)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J345,SEARCH(\"AT%\",J345),,REPT(\" \",25-SEARCH(\"AT%\",J345))))))","v":"RAHU02H07_TSET          AT%M1320.0     :REAL; (*空调机组02H07-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C345=\"REAL\",C345=\"DWORD\",C345=\"DINT\"),(IF(OR(C346=\"REAL\",C346=\"DWORD\",C346=\"DINT\"),A345+4+MOD(A345,4),A345+4)),(IF(OR(C346=\"REAL\",C346=\"DWORD\",C346=\"DINT\"),A345+4+MOD(A345,4),A345+2)))&\".0\"","v":"1324.0"},"验证通过","INT","空调机组","R",{"$f":"F345","v":"02H07"},"季节模式","空调机组02H07-新云平台季节模式",{"$f":"E346&VLOOKUP(D346,list!$D$3:$F$501,2,FALSE)&F346&\"_\"&VLOOKUP(G346,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H07_SM"},"RAHU02H07_SM AT%M1324.0 :INT; (*空调机组02H07-新云平台季节模式*)","RAHU02H07_SM            AT%M1324.0     :INT; (*空调机组02H07-新云平台季节模式*)"]
["1326.0","验证通过","BOOL","空调机组","R","02H07","程序控制","空调机组02H07-新云平台程序控制",{"$f":"E347&VLOOKUP(D347,list!$D$3:$F$501,2,FALSE)&F347&\"_\"&VLOOKUP(G347,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H07_PC"},"RAHU02H07_PC AT%M1326.0 :BOOL; (*空调机组02H07-新云平台程序控制*)","RAHU02H07_PC            AT%M1326.0     :BOOL; (*空调机组02H07-新云平台程序控制*)"]
["1332.0","验证通过","REAL","空调机组","L","02H07","设定温度值","空调机组02H07-设定温度值",{"$f":"E348&VLOOKUP(D348,list!$D$3:$F$501,2,FALSE)&F348&\"_\"&VLOOKUP(G348,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_TSET"},"LAHU02H07_TSET AT%M1332.0 :REAL; (*空调机组02H07-设定温度值*)","LAHU02H07_TSET          AT%M1332.0     :REAL; (*空调机组02H07-设定温度值*)"]
["1336.0","验证通过","INT","空调机组","L","02H07","季节模式","空调机组02H07-季节模式",{"$f":"E349&VLOOKUP(D349,list!$D$3:$F$501,2,FALSE)&F349&\"_\"&VLOOKUP(G349,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_SM"},"LAHU02H07_SM AT%M1336.0 :INT; (*空调机组02H07-季节模式*)","LAHU02H07_SM            AT%M1336.0     :INT; (*空调机组02H07-季节模式*)"]
["1340.0","验证通过","REAL","空调机组","L","02H07","水阀反馈换算值","空调机组02H07-水阀反馈换算值",{"$f":"E350&VLOOKUP(D350,list!$D$3:$F$501,2,FALSE)&F350&\"_\"&VLOOKUP(G350,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_WVBS"},"LAHU02H07_WVBS AT%M1340.0 :REAL; (*空调机组02H07-水阀反馈换算值*)","LAHU02H07_WVBS          AT%M1340.0     :REAL; (*空调机组02H07-水阀反馈换算值*)"]
["1344.0","验证通过","BOOL","空调机组","L","02H07","水阀手动控制","空调机组02H07-水阀手动控制",{"$f":"E351&VLOOKUP(D351,list!$D$3:$F$501,2,FALSE)&F351&\"_\"&VLOOKUP(G351,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_WVMC"},"LAHU02H07_WVMC AT%M1344.0 :BOOL; (*空调机组02H07-水阀手动控制*)","LAHU02H07_WVMC          AT%M1344.0     :BOOL; (*空调机组02H07-水阀手动控制*)"]
["1348.0","验证通过","REAL","空调机组","L","02H07","水阀手动控制值","空调机组02H07-水阀手动控制值",{"$f":"E352&VLOOKUP(D352,list!$D$3:$F$501,2,FALSE)&F352&\"_\"&VLOOKUP(G352,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_WVMV"},"LAHU02H07_WVMV AT%M1348.0 :REAL; (*空调机组02H07-水阀手动控制值*)","LAHU02H07_WVMV          AT%M1348.0     :REAL; (*空调机组02H07-水阀手动控制值*)"]
["1352.0","验证通过","REAL","空调机组","L","02H07","回风温度换算值","空调机组02H07-回风温度换算值",{"$f":"E353&VLOOKUP(D353,list!$D$3:$F$501,2,FALSE)&F353&\"_\"&VLOOKUP(G353,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_RTS"},"LAHU02H07_RTS AT%M1352.0 :REAL; (*空调机组02H07-回风温度换算值*)","LAHU02H07_RTS           AT%M1352.0     :REAL; (*空调机组02H07-回风温度换算值*)"]
["1356.0","验证通过","BOOL","空调机组","L","02H07","运行时间累积重置","空调机组02H07-运行时间累积重置",{"$f":"E354&VLOOKUP(D354,list!$D$3:$F$501,2,FALSE)&F354&\"_\"&VLOOKUP(G354,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_RST"},"LAHU02H07_RST AT%M1356.0 :BOOL; (*空调机组02H07-运行时间累积重置*)","LAHU02H07_RST           AT%M1356.0     :BOOL; (*空调机组02H07-运行时间累积重置*)"]
["1360.0","验证通过","REAL","空调机组","L","02H07","运行时间累积重置值","空调机组02H07-运行时间累积重置值",{"$f":"E355&VLOOKUP(D355,list!$D$3:$F$501,2,FALSE)&F355&\"_\"&VLOOKUP(G355,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_RSTV"},"LAHU02H07_RSTV AT%M1360.0 :REAL; (*空调机组02H07-运行时间累积重置值*)","LAHU02H07_RSTV          AT%M1360.0     :REAL; (*空调机组02H07-运行时间累积重置值*)"]
["1364.0","验证通过","BOOL","空调机组","L","02H07","隔离开关1","空调机组02H07-隔离开关1",{"$f":"E356&VLOOKUP(D356,list!$D$3:$F$501,2,FALSE)&F356&\"_\"&VLOOKUP(G356,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_ISO1"},"LAHU02H07_ISO1 AT%M1364.0 :BOOL; (*空调机组02H07-隔离开关1*)","LAHU02H07_ISO1          AT%M1364.0     :BOOL; (*空调机组02H07-隔离开关1*)"]
["1366.0","验证通过","BOOL","空调机组","L","02H07","隔离开关2","空调机组02H07-隔离开关2",{"$f":"E357&VLOOKUP(D357,list!$D$3:$F$501,2,FALSE)&F357&\"_\"&VLOOKUP(G357,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_ISO2"},"LAHU02H07_ISO2 AT%M1366.0 :BOOL; (*空调机组02H07-隔离开关2*)","LAHU02H07_ISO2          AT%M1366.0     :BOOL; (*空调机组02H07-隔离开关2*)"]
["1372.0","验证通过","REAL","空调机组","L","02H07","P调节参数","空调机组02H07-P调节参数",{"$f":"E358&VLOOKUP(D358,list!$D$3:$F$501,2,FALSE)&F358&\"_\"&VLOOKUP(G358,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_VP"},"LAHU02H07_VP AT%M1372.0 :REAL; (*空调机组02H07-P调节参数*)","LAHU02H07_VP            AT%M1372.0     :REAL; (*空调机组02H07-P调节参数*)"]
["1376.0","验证通过","REAL","空调机组","L","02H07","I调节参数","空调机组02H07-I调节参数",{"$f":"E359&VLOOKUP(D359,list!$D$3:$F$501,2,FALSE)&F359&\"_\"&VLOOKUP(G359,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_VI"},"LAHU02H07_VI AT%M1376.0 :REAL; (*空调机组02H07-I调节参数*)","LAHU02H07_VI            AT%M1376.0     :REAL; (*空调机组02H07-I调节参数*)"]
["1380.0","验证通过","REAL","空调机组","L","02H07","运行时间累积值","空调机组02H07-运行时间累积值",{"$f":"E360&VLOOKUP(D360,list!$D$3:$F$501,2,FALSE)&F360&\"_\"&VLOOKUP(G360,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_RH"},"LAHU02H07_RH AT%M1380.0 :REAL; (*空调机组02H07-运行时间累积值*)","LAHU02H07_RH            AT%M1380.0     :REAL; (*空调机组02H07-运行时间累积值*)"]
["1384.0","验证通过","INT","空调机组","L","02H07","设备状态代码","空调机组02H07-设备状态代码",{"$f":"E361&VLOOKUP(D361,list!$D$3:$F$501,2,FALSE)&F361&\"_\"&VLOOKUP(G361,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_SN"},"LAHU02H07_SN AT%M1384.0 :INT; (*空调机组02H07-设备状态代码*)","LAHU02H07_SN            AT%M1384.0     :INT; (*空调机组02H07-设备状态代码*)"]
["1386.0","验证通过","INT","空调机组","L","02H07","水阀控制转换值","空调机组02H07-水阀控制转换值",{"$f":"E362&VLOOKUP(D362,list!$D$3:$F$501,2,FALSE)&F362&\"_\"&VLOOKUP(G362,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_WVCS"},"LAHU02H07_WVCS AT%M1386.0 :INT; (*空调机组02H07-水阀控制转换值*)","LAHU02H07_WVCS          AT%M1386.0     :INT; (*空调机组02H07-水阀控制转换值*)"]
["1388.0","验证通过","BOOL","空调机组","L","02H07","程序控制","空调机组02H07-程序控制",{"$f":"E363&VLOOKUP(D363,list!$D$3:$F$501,2,FALSE)&F363&\"_\"&VLOOKUP(G363,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H07_PC"},"LAHU02H07_PC AT%M1388.0 :BOOL; (*空调机组02H07-程序控制*)","LAHU02H07_PC            AT%M1388.0     :BOOL; (*空调机组02H07-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C363=\"REAL\",C363=\"DWORD\",C363=\"DINT\"),(IF(OR(C365=\"REAL\",C365=\"DWORD\",C365=\"DINT\"),A363+4+MOD(A363,4),A363+4)),(IF(OR(C365=\"REAL\",C365=\"DWORD\",C365=\"DINT\"),A363+4+MOD(A363,4),A363+2)))&\".0\"","v":"1392.0"},{"$f":"IF((IF(OR(C365=\"INT\",C365=\"WORD\",C365=\"BOOL\"),MOD(A365,2),MOD(A365,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02H08","设定温度值",{"$f":"D365&F365&\"-\"&IF(E365=\"R\",\"新云平台\"&G365,G365)","v":"空调机组02H08-新云平台设定温度值"},{"$f":"E365&VLOOKUP(D365,list!$D$3:$F$501,2,FALSE)&F365&\"_\"&VLOOKUP(G365,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H08_TSET"},{"$f":"I365&\" \"&\"AT%M\"&A365&\" \"&\":\"&C365&\";\"&\" \"&\"(*\"&H365&\"*)\"","v":"RAHU02H08_TSET AT%M1392.0 :REAL; (*空调机组02H08-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J365,SEARCH(\"AT%\",J365),,REPT(\" \",25-SEARCH(\"AT%\",J365))),SEARCH(\":\",REPLACE(J365,SEARCH(\"AT%\",J365),,REPT(\" \",25-SEARCH(\"AT%\",J365)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J365,SEARCH(\"AT%\",J365),,REPT(\" \",25-SEARCH(\"AT%\",J365))))))","v":"RAHU02H08_TSET          AT%M1392.0     :REAL; (*空调机组02H08-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C365=\"REAL\",C365=\"DWORD\",C365=\"DINT\"),(IF(OR(C366=\"REAL\",C366=\"DWORD\",C366=\"DINT\"),A365+4+MOD(A365,4),A365+4)),(IF(OR(C366=\"REAL\",C366=\"DWORD\",C366=\"DINT\"),A365+4+MOD(A365,4),A365+2)))&\".0\"","v":"1396.0"},"验证通过","INT","空调机组","R",{"$f":"F365","v":"02H08"},"季节模式","空调机组02H08-新云平台季节模式",{"$f":"E366&VLOOKUP(D366,list!$D$3:$F$501,2,FALSE)&F366&\"_\"&VLOOKUP(G366,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H08_SM"},"RAHU02H08_SM AT%M1396.0 :INT; (*空调机组02H08-新云平台季节模式*)","RAHU02H08_SM            AT%M1396.0     :INT; (*空调机组02H08-新云平台季节模式*)"]
["1398.0","验证通过","BOOL","空调机组","R","02H08","程序控制","空调机组02H08-新云平台程序控制",{"$f":"E367&VLOOKUP(D367,list!$D$3:$F$501,2,FALSE)&F367&\"_\"&VLOOKUP(G367,list!$I$2:$K$502,2,FALSE)","v":"RAHU02H08_PC"},"RAHU02H08_PC AT%M1398.0 :BOOL; (*空调机组02H08-新云平台程序控制*)","RAHU02H08_PC            AT%M1398.0     :BOOL; (*空调机组02H08-新云平台程序控制*)"]
["1404.0","验证通过","REAL","空调机组","L","02H08","设定温度值","空调机组02H08-设定温度值",{"$f":"E368&VLOOKUP(D368,list!$D$3:$F$501,2,FALSE)&F368&\"_\"&VLOOKUP(G368,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_TSET"},"LAHU02H08_TSET AT%M1404.0 :REAL; (*空调机组02H08-设定温度值*)","LAHU02H08_TSET          AT%M1404.0     :REAL; (*空调机组02H08-设定温度值*)"]
["1408.0","验证通过","INT","空调机组","L","02H08","季节模式","空调机组02H08-季节模式",{"$f":"E369&VLOOKUP(D369,list!$D$3:$F$501,2,FALSE)&F369&\"_\"&VLOOKUP(G369,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_SM"},"LAHU02H08_SM AT%M1408.0 :INT; (*空调机组02H08-季节模式*)","LAHU02H08_SM            AT%M1408.0     :INT; (*空调机组02H08-季节模式*)"]
["1412.0","验证通过","REAL","空调机组","L","02H08","水阀反馈换算值","空调机组02H08-水阀反馈换算值",{"$f":"E370&VLOOKUP(D370,list!$D$3:$F$501,2,FALSE)&F370&\"_\"&VLOOKUP(G370,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_WVBS"},"LAHU02H08_WVBS AT%M1412.0 :REAL; (*空调机组02H08-水阀反馈换算值*)","LAHU02H08_WVBS          AT%M1412.0     :REAL; (*空调机组02H08-水阀反馈换算值*)"]
["1416.0","验证通过","BOOL","空调机组","L","02H08","水阀手动控制","空调机组02H08-水阀手动控制",{"$f":"E371&VLOOKUP(D371,list!$D$3:$F$501,2,FALSE)&F371&\"_\"&VLOOKUP(G371,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_WVMC"},"LAHU02H08_WVMC AT%M1416.0 :BOOL; (*空调机组02H08-水阀手动控制*)","LAHU02H08_WVMC          AT%M1416.0     :BOOL; (*空调机组02H08-水阀手动控制*)"]
["1420.0","验证通过","REAL","空调机组","L","02H08","水阀手动控制值","空调机组02H08-水阀手动控制值",{"$f":"E372&VLOOKUP(D372,list!$D$3:$F$501,2,FALSE)&F372&\"_\"&VLOOKUP(G372,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_WVMV"},"LAHU02H08_WVMV AT%M1420.0 :REAL; (*空调机组02H08-水阀手动控制值*)","LAHU02H08_WVMV          AT%M1420.0     :REAL; (*空调机组02H08-水阀手动控制值*)"]
["1424.0","验证通过","REAL","空调机组","L","02H08","回风温度换算值","空调机组02H08-回风温度换算值",{"$f":"E373&VLOOKUP(D373,list!$D$3:$F$501,2,FALSE)&F373&\"_\"&VLOOKUP(G373,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_RTS"},"LAHU02H08_RTS AT%M1424.0 :REAL; (*空调机组02H08-回风温度换算值*)","LAHU02H08_RTS           AT%M1424.0     :REAL; (*空调机组02H08-回风温度换算值*)"]
["1428.0","验证通过","BOOL","空调机组","L","02H08","运行时间累积重置","空调机组02H08-运行时间累积重置",{"$f":"E374&VLOOKUP(D374,list!$D$3:$F$501,2,FALSE)&F374&\"_\"&VLOOKUP(G374,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_RST"},"LAHU02H08_RST AT%M1428.0 :BOOL; (*空调机组02H08-运行时间累积重置*)","LAHU02H08_RST           AT%M1428.0     :BOOL; (*空调机组02H08-运行时间累积重置*)"]
["1432.0","验证通过","REAL","空调机组","L","02H08","运行时间累积重置值","空调机组02H08-运行时间累积重置值",{"$f":"E375&VLOOKUP(D375,list!$D$3:$F$501,2,FALSE)&F375&\"_\"&VLOOKUP(G375,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_RSTV"},"LAHU02H08_RSTV AT%M1432.0 :REAL; (*空调机组02H08-运行时间累积重置值*)","LAHU02H08_RSTV          AT%M1432.0     :REAL; (*空调机组02H08-运行时间累积重置值*)"]
["1436.0","验证通过","BOOL","空调机组","L","02H08","隔离开关1","空调机组02H08-隔离开关1",{"$f":"E376&VLOOKUP(D376,list!$D$3:$F$501,2,FALSE)&F376&\"_\"&VLOOKUP(G376,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_ISO1"},"LAHU02H08_ISO1 AT%M1436.0 :BOOL; (*空调机组02H08-隔离开关1*)","LAHU02H08_ISO1          AT%M1436.0     :BOOL; (*空调机组02H08-隔离开关1*)"]
["1438.0","验证通过","BOOL","空调机组","L","02H08","隔离开关2","空调机组02H08-隔离开关2",{"$f":"E377&VLOOKUP(D377,list!$D$3:$F$501,2,FALSE)&F377&\"_\"&VLOOKUP(G377,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_ISO2"},"LAHU02H08_ISO2 AT%M1438.0 :BOOL; (*空调机组02H08-隔离开关2*)","LAHU02H08_ISO2          AT%M1438.0     :BOOL; (*空调机组02H08-隔离开关2*)"]
["1444.0","验证通过","REAL","空调机组","L","02H08","P调节参数","空调机组02H08-P调节参数",{"$f":"E378&VLOOKUP(D378,list!$D$3:$F$501,2,FALSE)&F378&\"_\"&VLOOKUP(G378,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_VP"},"LAHU02H08_VP AT%M1444.0 :REAL; (*空调机组02H08-P调节参数*)","LAHU02H08_VP            AT%M1444.0     :REAL; (*空调机组02H08-P调节参数*)"]
["1448.0","验证通过","REAL","空调机组","L","02H08","I调节参数","空调机组02H08-I调节参数",{"$f":"E379&VLOOKUP(D379,list!$D$3:$F$501,2,FALSE)&F379&\"_\"&VLOOKUP(G379,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_VI"},"LAHU02H08_VI AT%M1448.0 :REAL; (*空调机组02H08-I调节参数*)","LAHU02H08_VI            AT%M1448.0     :REAL; (*空调机组02H08-I调节参数*)"]
["1452.0","验证通过","REAL","空调机组","L","02H08","运行时间累积值","空调机组02H08-运行时间累积值",{"$f":"E380&VLOOKUP(D380,list!$D$3:$F$501,2,FALSE)&F380&\"_\"&VLOOKUP(G380,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_RH"},"LAHU02H08_RH AT%M1452.0 :REAL; (*空调机组02H08-运行时间累积值*)","LAHU02H08_RH            AT%M1452.0     :REAL; (*空调机组02H08-运行时间累积值*)"]
["1456.0","验证通过","INT","空调机组","L","02H08","设备状态代码","空调机组02H08-设备状态代码",{"$f":"E381&VLOOKUP(D381,list!$D$3:$F$501,2,FALSE)&F381&\"_\"&VLOOKUP(G381,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_SN"},"LAHU02H08_SN AT%M1456.0 :INT; (*空调机组02H08-设备状态代码*)","LAHU02H08_SN            AT%M1456.0     :INT; (*空调机组02H08-设备状态代码*)"]
["1458.0","验证通过","INT","空调机组","L","02H08","水阀控制转换值","空调机组02H08-水阀控制转换值",{"$f":"E382&VLOOKUP(D382,list!$D$3:$F$501,2,FALSE)&F382&\"_\"&VLOOKUP(G382,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_WVCS"},"LAHU02H08_WVCS AT%M1458.0 :INT; (*空调机组02H08-水阀控制转换值*)","LAHU02H08_WVCS          AT%M1458.0     :INT; (*空调机组02H08-水阀控制转换值*)"]
["1460.0","验证通过","BOOL","空调机组","L","02H08","程序控制","空调机组02H08-程序控制",{"$f":"E383&VLOOKUP(D383,list!$D$3:$F$501,2,FALSE)&F383&\"_\"&VLOOKUP(G383,list!$I$2:$K$502,2,FALSE)","v":"LAHU02H08_PC"},"LAHU02H08_PC AT%M1460.0 :BOOL; (*空调机组02H08-程序控制*)","LAHU02H08_PC            AT%M1460.0     :BOOL; (*空调机组02H08-程序控制*)"]
["FCU"]
[{"$f":"IF(OR(C383=\"REAL\",C383=\"DWORD\",C383=\"DINT\"),(IF(OR(C385=\"REAL\",C385=\"DWORD\",C385=\"DINT\"),A383+4+MOD(A383,4),A383+4)),(IF(OR(C385=\"REAL\",C385=\"DWORD\",C385=\"DINT\"),A383+4+MOD(A383,4),A383+2)))&\".0\"","v":"1464.0"},{"$f":"IF((IF(OR(C385=\"INT\",C385=\"WORD\",C385=\"BOOL\"),MOD(A385,2),MOD(A385,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","01H01","设定温度值",{"$f":"D385&F385&\"-\"&IF(E385=\"R\",\"新云平台\"&G385,G385)","v":"风机盘管01H01-新云平台设定温度值"},{"$f":"E385&VLOOKUP(D385,list!$D$3:$F$501,2,FALSE)&F385&\"_\"&VLOOKUP(G385,list!$I$2:$K$502,2,FALSE)","v":"RFCU01H01_TSET"},{"$f":"I385&\" \"&\"AT%M\"&A385&\" \"&\":\"&C385&\";\"&\" \"&\"(*\"&H385&\"*)\"","v":"RFCU01H01_TSET AT%M1464.0 :REAL; (*风机盘管01H01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J385,SEARCH(\"AT%\",J385),,REPT(\" \",25-SEARCH(\"AT%\",J385))),SEARCH(\":\",REPLACE(J385,SEARCH(\"AT%\",J385),,REPT(\" \",25-SEARCH(\"AT%\",J385)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J385,SEARCH(\"AT%\",J385),,REPT(\" \",25-SEARCH(\"AT%\",J385))))))","v":"RFCU01H01_TSET          AT%M1464.0     :REAL; (*风机盘管01H01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C385=\"REAL\",C385=\"DWORD\",C385=\"DINT\"),(IF(OR(C386=\"REAL\",C386=\"DWORD\",C386=\"DINT\"),A385+4+MOD(A385,4),A385+4)),(IF(OR(C386=\"REAL\",C386=\"DWORD\",C386=\"DINT\"),A385+4+MOD(A385,4),A385+2)))&\".0\"","v":"1468.0"},"验证通过","INT","风机盘管","R",{"$f":"F385","v":"01H01"},"季节模式","风机盘管01H01-新云平台季节模式",{"$f":"E386&VLOOKUP(D386,list!$D$3:$F$501,2,FALSE)&F386&\"_\"&VLOOKUP(G386,list!$I$2:$K$502,2,FALSE)","v":"RFCU01H01_SM"},"RFCU01H01_SM AT%M1468.0 :INT; (*风机盘管01H01-新云平台季节模式*)","RFCU01H01_SM            AT%M1468.0     :INT; (*风机盘管01H01-新云平台季节模式*)"]
[{"$f":"IF(OR(C386=\"REAL\",C386=\"DWORD\",C386=\"DINT\"),(IF(OR(C387=\"REAL\",C387=\"DWORD\",C387=\"DINT\"),A386+4+MOD(A386,4),A386+4)),(IF(OR(C387=\"REAL\",C387=\"DWORD\",C387=\"DINT\"),A386+4+MOD(A386,4),A386+2)))&\".0\"","v":"1470.0"},"验证通过","BOOL","风机盘管","R","01H01","程序控制","风机盘管01H01-新云平台程序控制",{"$f":"E387&VLOOKUP(D387,list!$D$3:$F$501,2,FALSE)&F387&\"_\"&VLOOKUP(G387,list!$I$2:$K$502,2,FALSE)","v":"RFCU01H01_PC"},"RFCU01H01_PC AT%M1470.0 :BOOL; (*风机盘管01H01-新云平台程序控制*)","RFCU01H01_PC            AT%M1470.0     :BOOL; (*风机盘管01H01-新云平台程序控制*)"]
["1476.0","验证通过","REAL","风机盘管","L","01H01","设定温度值","风机盘管01H01-设定温度值",{"$f":"E388&VLOOKUP(D388,list!$D$3:$F$501,2,FALSE)&F388&\"_\"&VLOOKUP(G388,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_TSET"},"LFCU01H01_TSET AT%M1476.0 :REAL; (*风机盘管01H01-设定温度值*)","LFCU01H01_TSET          AT%M1476.0     :REAL; (*风机盘管01H01-设定温度值*)"]
["1480.0","验证通过","INT","风机盘管","L","01H01","季节模式","风机盘管01H01-季节模式",{"$f":"E389&VLOOKUP(D389,list!$D$3:$F$501,2,FALSE)&F389&\"_\"&VLOOKUP(G389,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_SM"},"LFCU01H01_SM AT%M1480.0 :INT; (*风机盘管01H01-季节模式*)","LFCU01H01_SM            AT%M1480.0     :INT; (*风机盘管01H01-季节模式*)"]
["1484.0","验证通过","REAL","风机盘管","L","01H01","温度换算值","风机盘管01H01-温度换算值",{"$f":"E390&VLOOKUP(D390,list!$D$3:$F$501,2,FALSE)&F390&\"_\"&VLOOKUP(G390,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_TS"},"LFCU01H01_TS AT%M1484.0 :REAL; (*风机盘管01H01-温度换算值*)","LFCU01H01_TS            AT%M1484.0     :REAL; (*风机盘管01H01-温度换算值*)"]
["1488.0","验证通过","BOOL","风机盘管","L","01H01","电磁阀手动控制","风机盘管01H01-电磁阀手动控制",{"$f":"E391&VLOOKUP(D391,list!$D$3:$F$501,2,FALSE)&F391&\"_\"&VLOOKUP(G391,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_EVMC"},"LFCU01H01_EVMC AT%M1488.0 :BOOL; (*风机盘管01H01-电磁阀手动控制*)","LFCU01H01_EVMC          AT%M1488.0     :BOOL; (*风机盘管01H01-电磁阀手动控制*)"]
["1490.0","验证通过","BOOL","风机盘管","L","01H01","电磁阀手动控制值","风机盘管01H01-电磁阀手动控制值",{"$f":"E392&VLOOKUP(D392,list!$D$3:$F$501,2,FALSE)&F392&\"_\"&VLOOKUP(G392,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_EVMV"},"LFCU01H01_EVMV AT%M1490.0 :BOOL; (*风机盘管01H01-电磁阀手动控制值*)","LFCU01H01_EVMV          AT%M1490.0     :BOOL; (*风机盘管01H01-电磁阀手动控制值*)"]
["1496.0","验证通过","REAL","风机盘管","L","01H01","回风温度换算值","风机盘管01H01-回风温度换算值",{"$f":"E393&VLOOKUP(D393,list!$D$3:$F$501,2,FALSE)&F393&\"_\"&VLOOKUP(G393,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RTS"},"LFCU01H01_RTS AT%M1496.0 :REAL; (*风机盘管01H01-回风温度换算值*)","LFCU01H01_RTS           AT%M1496.0     :REAL; (*风机盘管01H01-回风温度换算值*)"]
["1500.0","验证通过","BOOL","风机盘管","L","01H01","运行时间累积重置","风机盘管01H01-运行时间累积重置",{"$f":"E394&VLOOKUP(D394,list!$D$3:$F$501,2,FALSE)&F394&\"_\"&VLOOKUP(G394,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RST"},"LFCU01H01_RST AT%M1500.0 :BOOL; (*风机盘管01H01-运行时间累积重置*)","LFCU01H01_RST           AT%M1500.0     :BOOL; (*风机盘管01H01-运行时间累积重置*)"]
["1504.0","验证通过","REAL","风机盘管","L","01H01","运行时间累积重置值","风机盘管01H01-运行时间累积重置值",{"$f":"E395&VLOOKUP(D395,list!$D$3:$F$501,2,FALSE)&F395&\"_\"&VLOOKUP(G395,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RSTV"},"LFCU01H01_RSTV AT%M1504.0 :REAL; (*风机盘管01H01-运行时间累积重置值*)","LFCU01H01_RSTV          AT%M1504.0     :REAL; (*风机盘管01H01-运行时间累积重置值*)"]
["1508.0","验证通过","BOOL","风机盘管","L","01H01","隔离开关1","风机盘管01H01-隔离开关1",{"$f":"E396&VLOOKUP(D396,list!$D$3:$F$501,2,FALSE)&F396&\"_\"&VLOOKUP(G396,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_ISO1"},"LFCU01H01_ISO1 AT%M1508.0 :BOOL; (*风机盘管01H01-隔离开关1*)","LFCU01H01_ISO1          AT%M1508.0     :BOOL; (*风机盘管01H01-隔离开关1*)"]
["1512.0","验证通过","REAL","风机盘管","L","01H01","运行时间累积值","风机盘管01H01-运行时间累积值",{"$f":"E397&VLOOKUP(D397,list!$D$3:$F$501,2,FALSE)&F397&\"_\"&VLOOKUP(G397,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RH"},"LFCU01H01_RH AT%M1512.0 :REAL; (*风机盘管01H01-运行时间累积值*)","LFCU01H01_RH            AT%M1512.0     :REAL; (*风机盘管01H01-运行时间累积值*)"]
["1516.0","验证通过","INT","风机盘管","L","01H01","设备状态代码","风机盘管01H01-设备状态代码",{"$f":"E398&VLOOKUP(D398,list!$D$3:$F$501,2,FALSE)&F398&\"_\"&VLOOKUP(G398,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_SN"},"LFCU01H01_SN AT%M1516.0 :INT; (*风机盘管01H01-设备状态代码*)","LFCU01H01_SN            AT%M1516.0     :INT; (*风机盘管01H01-设备状态代码*)"]
["1518.0","验证通过","INT","风机盘管","L","01H01","水阀控制转换值","风机盘管01H01-水阀控制转换值",{"$f":"E399&VLOOKUP(D399,list!$D$3:$F$501,2,FALSE)&F399&\"_\"&VLOOKUP(G399,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_WVCS"},"LFCU01H01_WVCS AT%M1518.0 :INT; (*风机盘管01H01-水阀控制转换值*)","LFCU01H01_WVCS          AT%M1518.0     :INT; (*风机盘管01H01-水阀控制转换值*)"]
["1520.0","验证通过","BOOL","风机盘管","L","01H01","程序控制","风机盘管01H01-程序控制",{"$f":"E400&VLOOKUP(D400,list!$D$3:$F$501,2,FALSE)&F400&\"_\"&VLOOKUP(G400,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_PC"},"LFCU01H01_PC AT%M1520.0 :BOOL; (*风机盘管01H01-程序控制*)","LFCU01H01_PC            AT%M1520.0     :BOOL; (*风机盘管01H01-程序控制*)"]
["PAU"]
[{"$f":"IF(OR(C400=\"REAL\",C400=\"DWORD\",C400=\"DINT\"),(IF(OR(C402=\"REAL\",C402=\"DWORD\",C402=\"DINT\"),A400+4+MOD(A400,4),A400+4)),(IF(OR(C402=\"REAL\",C402=\"DWORD\",C402=\"DINT\"),A400+4+MOD(A400,4),A400+2)))&\".0\"","v":"1524.0"},{"$f":"IF((IF(OR(C402=\"INT\",C402=\"WORD\",C402=\"BOOL\"),MOD(A402,2),MOD(A402,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","01A01","设定温度值","P新风机组01A01-新云平台设定温度值",{"$f":"E402&VLOOKUP(D402,list!$D$3:$F$501,2,FALSE)&F402&\"_\"&VLOOKUP(G402,list!$I$2:$K$502,2,FALSE)","v":"RPAU01A01_TSET"},"RPAU01A01_TSET AT%M1524.0 :REAL; (*P新风机组01A01-新云平台设定温度值*)",{"$f":"REPLACE(REPLACE(J402,SEARCH(\"AT%\",J402),,REPT(\" \",25-SEARCH(\"AT%\",J402))),SEARCH(\":\",REPLACE(J402,SEARCH(\"AT%\",J402),,REPT(\" \",25-SEARCH(\"AT%\",J402)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J402,SEARCH(\"AT%\",J402),,REPT(\" \",25-SEARCH(\"AT%\",J402))))))","v":"RPAU01A01_TSET          AT%M1524.0     :REAL; (*P新风机组01A01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C402=\"REAL\",C402=\"DWORD\",C402=\"DINT\"),(IF(OR(C403=\"REAL\",C403=\"DWORD\",C403=\"DINT\"),A402+4+MOD(A402,4),A402+4)),(IF(OR(C403=\"REAL\",C403=\"DWORD\",C403=\"DINT\"),A402+4+MOD(A402,4),A402+2)))&\".0\"","v":"1528.0"},"验证通过","INT","P新风机组","R",{"$f":"F402","v":"01A01"},"季节模式","P新风机组01A01-新云平台季节模式",{"$f":"E403&VLOOKUP(D403,list!$D$3:$F$501,2,FALSE)&F403&\"_\"&VLOOKUP(G403,list!$I$2:$K$502,2,FALSE)","v":"RPAU01A01_SM"},"RPAU01A01_SM AT%M1528.0 :INT; (*P新风机组01A01-新云平台季节模式*)",{"$f":"REPLACE(REPLACE(J403,SEARCH(\"AT%\",J403),,REPT(\" \",25-SEARCH(\"AT%\",J403))),SEARCH(\":\",REPLACE(J403,SEARCH(\"AT%\",J403),,REPT(\" \",25-SEARCH(\"AT%\",J403)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J403,SEARCH(\"AT%\",J403),,REPT(\" \",25-SEARCH(\"AT%\",J403))))))","v":"RPAU01A01_SM            AT%M1528.0     :INT; (*P新风机组01A01-新云平台季节模式*)"}]
[{"$f":"IF(OR(C403=\"REAL\",C403=\"DWORD\",C403=\"DINT\"),(IF(OR(C404=\"REAL\",C404=\"DWORD\",C404=\"DINT\"),A403+4+MOD(A403,4),A403+4)),(IF(OR(C404=\"REAL\",C404=\"DWORD\",C404=\"DINT\"),A403+4+MOD(A403,4),A403+2)))&\".0\"","v":"1530.0"},"验证通过","BOOL","P新风机组","R","01A01","程序控制","P新风机组01A01-新云平台程序控制",{"$f":"E404&VLOOKUP(D404,list!$D$3:$F$501,2,FALSE)&F404&\"_\"&VLOOKUP(G404,list!$I$2:$K$502,2,FALSE)","v":"RPAU01A01_PC"},"RPAU01A01_PC AT%M1530.0 :BOOL; (*P新风机组01A01-新云平台程序控制*)",{"$f":"REPLACE(REPLACE(J404,SEARCH(\"AT%\",J404),,REPT(\" \",25-SEARCH(\"AT%\",J404))),SEARCH(\":\",REPLACE(J404,SEARCH(\"AT%\",J404),,REPT(\" \",25-SEARCH(\"AT%\",J404)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J404,SEARCH(\"AT%\",J404),,REPT(\" \",25-SEARCH(\"AT%\",J404))))))","v":"RPAU01A01_PC            AT%M1530.0     :BOOL; (*P新风机组01A01-新云平台程序控制*)"}]
["1536.0","验证通过","REAL","P新风机组","L","01A01","设定温度值","P新风机组01A01-设定温度值",{"$f":"E405&VLOOKUP(D405,list!$D$3:$F$501,2,FALSE)&F405&\"_\"&VLOOKUP(G405,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_TSET"},"LPAU01A01_TSET AT%M1536.0 :REAL; (*P新风机组01A01-设定温度值*)",{"$f":"REPLACE(REPLACE(J405,SEARCH(\"AT%\",J405),,REPT(\" \",25-SEARCH(\"AT%\",J405))),SEARCH(\":\",REPLACE(J405,SEARCH(\"AT%\",J405),,REPT(\" \",25-SEARCH(\"AT%\",J405)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J405,SEARCH(\"AT%\",J405),,REPT(\" \",25-SEARCH(\"AT%\",J405))))))","v":"LPAU01A01_TSET          AT%M1536.0     :REAL; (*P新风机组01A01-设定温度值*)"}]
["1540.0","验证通过","INT","P新风机组","L","01A01","季节模式","P新风机组01A01-季节模式",{"$f":"E406&VLOOKUP(D406,list!$D$3:$F$501,2,FALSE)&F406&\"_\"&VLOOKUP(G406,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_SM"},"LPAU01A01_SM AT%M1540.0 :INT; (*P新风机组01A01-季节模式*)",{"$f":"REPLACE(REPLACE(J406,SEARCH(\"AT%\",J406),,REPT(\" \",25-SEARCH(\"AT%\",J406))),SEARCH(\":\",REPLACE(J406,SEARCH(\"AT%\",J406),,REPT(\" \",25-SEARCH(\"AT%\",J406)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J406,SEARCH(\"AT%\",J406),,REPT(\" \",25-SEARCH(\"AT%\",J406))))))","v":"LPAU01A01_SM            AT%M1540.0     :INT; (*P新风机组01A01-季节模式*)"}]
["1544.0","验证通过","REAL","P新风机组","L","01A01","水阀反馈换算值","P新风机组01A01-水阀反馈换算值",{"$f":"E407&VLOOKUP(D407,list!$D$3:$F$501,2,FALSE)&F407&\"_\"&VLOOKUP(G407,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_WVBS"},"LPAU01A01_WVBS AT%M1544.0 :REAL; (*P新风机组01A01-水阀反馈换算值*)","LPAU01A01_WVBS          AT%M1544.0     :REAL; (*P新风机组01A01-水阀反馈换算值*)"]
["1548.0","验证通过","BOOL","P新风机组","L","01A01","水阀手动控制","P新风机组01A01-水阀手动控制",{"$f":"E408&VLOOKUP(D408,list!$D$3:$F$501,2,FALSE)&F408&\"_\"&VLOOKUP(G408,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_WVMC"},"LPAU01A01_WVMC AT%M1548.0 :BOOL; (*P新风机组01A01-水阀手动控制*)","LPAU01A01_WVMC          AT%M1548.0     :BOOL; (*P新风机组01A01-水阀手动控制*)"]
["1552.0","验证通过","REAL","P新风机组","L","01A01","水阀手动控制值","P新风机组01A01-水阀手动控制值",{"$f":"E409&VLOOKUP(D409,list!$D$3:$F$501,2,FALSE)&F409&\"_\"&VLOOKUP(G409,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_WVMV"},"LPAU01A01_WVMV AT%M1552.0 :REAL; (*P新风机组01A01-水阀手动控制值*)","LPAU01A01_WVMV          AT%M1552.0     :REAL; (*P新风机组01A01-水阀手动控制值*)"]
["1556.0","验证通过","REAL","P新风机组","L","01A01","送风温度换算值","P新风机组01A01-送风温度换算值",{"$f":"E410&VLOOKUP(D410,list!$D$3:$F$501,2,FALSE)&F410&\"_\"&VLOOKUP(G410,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_STS"},"LPAU01A01_STS AT%M1556.0 :REAL; (*P新风机组01A01-送风温度换算值*)","LPAU01A01_STS           AT%M1556.0     :REAL; (*P新风机组01A01-送风温度换算值*)"]
["1560.0","验证通过","BOOL","P新风机组","L","01A01","运行时间累积重置","P新风机组01A01-运行时间累积重置",{"$f":"E411&VLOOKUP(D411,list!$D$3:$F$501,2,FALSE)&F411&\"_\"&VLOOKUP(G411,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_RST"},"LPAU01A01_RST AT%M1560.0 :BOOL; (*P新风机组01A01-运行时间累积重置*)","LPAU01A01_RST           AT%M1560.0     :BOOL; (*P新风机组01A01-运行时间累积重置*)"]
["1564.0","验证通过","REAL","P新风机组","L","01A01","运行时间累积重置值","P新风机组01A01-运行时间累积重置值",{"$f":"E412&VLOOKUP(D412,list!$D$3:$F$501,2,FALSE)&F412&\"_\"&VLOOKUP(G412,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_RSTV"},"LPAU01A01_RSTV AT%M1564.0 :REAL; (*P新风机组01A01-运行时间累积重置值*)","LPAU01A01_RSTV          AT%M1564.0     :REAL; (*P新风机组01A01-运行时间累积重置值*)"]
["1568.0","验证通过","BOOL","P新风机组","L","01A01","隔离开关1","P新风机组01A01-隔离开关1",{"$f":"E413&VLOOKUP(D413,list!$D$3:$F$501,2,FALSE)&F413&\"_\"&VLOOKUP(G413,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_ISO1"},"LPAU01A01_ISO1 AT%M1568.0 :BOOL; (*P新风机组01A01-隔离开关1*)","LPAU01A01_ISO1          AT%M1568.0     :BOOL; (*P新风机组01A01-隔离开关1*)"]
["1570.0","验证通过","BOOL","P新风机组","L","01A01","隔离开关2","P新风机组01A01-隔离开关2",{"$f":"E414&VLOOKUP(D414,list!$D$3:$F$501,2,FALSE)&F414&\"_\"&VLOOKUP(G414,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_ISO2"},"LPAU01A01_ISO2 AT%M1570.0 :BOOL; (*P新风机组01A01-隔离开关2*)","LPAU01A01_ISO2          AT%M1570.0     :BOOL; (*P新风机组01A01-隔离开关2*)"]
["1576.0","验证通过","REAL","P新风机组","L","01A01","P调节参数","P新风机组01A01-P调节参数",{"$f":"E415&VLOOKUP(D415,list!$D$3:$F$501,2,FALSE)&F415&\"_\"&VLOOKUP(G415,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_VP"},"LPAU01A01_VP AT%M1576.0 :REAL; (*P新风机组01A01-P调节参数*)","LPAU01A01_VP            AT%M1576.0     :REAL; (*P新风机组01A01-P调节参数*)"]
["1580.0","验证通过","REAL","P新风机组","L","01A01","I调节参数","P新风机组01A01-I调节参数",{"$f":"E416&VLOOKUP(D416,list!$D$3:$F$501,2,FALSE)&F416&\"_\"&VLOOKUP(G416,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_VI"},"LPAU01A01_VI AT%M1580.0 :REAL; (*P新风机组01A01-I调节参数*)","LPAU01A01_VI            AT%M1580.0     :REAL; (*P新风机组01A01-I调节参数*)"]
["1584.0","验证通过","REAL","P新风机组","L","01A01","运行时间累积值","P新风机组01A01-运行时间累积值",{"$f":"E417&VLOOKUP(D417,list!$D$3:$F$501,2,FALSE)&F417&\"_\"&VLOOKUP(G417,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_RH"},"LPAU01A01_RH AT%M1584.0 :REAL; (*P新风机组01A01-运行时间累积值*)","LPAU01A01_RH            AT%M1584.0     :REAL; (*P新风机组01A01-运行时间累积值*)"]
[{"$f":"IF(OR(C417=\"REAL\",C417=\"DWORD\",C417=\"DINT\"),(IF(OR(C418=\"REAL\",C418=\"DWORD\",C418=\"DINT\"),A417+4+MOD(A417,4),A417+4)),(IF(OR(C418=\"REAL\",C418=\"DWORD\",C418=\"DINT\"),A417+4+MOD(A417,4),A417+2)))&\".0\"","v":"1588.0"},{"$f":"IF((IF(OR(C418=\"INT\",C418=\"WORD\",C418=\"BOOL\"),MOD(A418,2),MOD(A418,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"INT","P新风机组","L","01A01","设备状态代码","P新风机组01A01-设备状态代码",{"$f":"E418&VLOOKUP(D418,list!$D$3:$F$501,2,FALSE)&F418&\"_\"&VLOOKUP(G418,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_SN"},"LPAU01A01_SN AT%M1588.0 :INT; (*P新风机组01A01-设备状态代码*)","LPAU01A01_SN            AT%M1588.0     :INT; (*P新风机组01A01-设备状态代码*)"]
["1590.0","验证通过","INT","P新风机组","L","01A01","水阀控制转换值","P新风机组01A01-水阀控制转换值",{"$f":"E419&VLOOKUP(D419,list!$D$3:$F$501,2,FALSE)&F419&\"_\"&VLOOKUP(G419,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_WVCS"},"LPAU01A01_WVCS AT%M1590.0 :INT; (*P新风机组01A01-水阀控制转换值*)","LPAU01A01_WVCS          AT%M1590.0     :INT; (*P新风机组01A01-水阀控制转换值*)"]
["1592.0","验证通过","BOOL","P新风机组","L","01A01","程序控制","P新风机组01A01-程序控制",{"$f":"E420&VLOOKUP(D420,list!$D$3:$F$501,2,FALSE)&F420&\"_\"&VLOOKUP(G420,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_PC"},"LPAU01A01_PC AT%M1592.0 :BOOL; (*P新风机组01A01-程序控制*)","LPAU01A01_PC            AT%M1592.0     :BOOL; (*P新风机组01A01-程序控制*)"]
["1594.0","验证通过","INT","P新风机组","L","01A01","变频手动控制值","P新风机组01A01-变频手动控制值",{"$f":"E421&VLOOKUP(D421,list!$D$3:$F$501,2,FALSE)&F421&\"_\"&VLOOKUP(G421,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_VFMV"},"LPAU01A01_VFMV AT%M1594.0 :INT; (*P新风机组01A01-变频手动控制值*)","LPAU01A01_VFMV          AT%M1594.0     :INT; (*P新风机组01A01-变频手动控制值*)"]
["1596.0","验证通过","BOOL","P新风机组","L","01A01","低温断路报警隔离","P新风机组01A01-低温断路报警隔离",{"$f":"E422&VLOOKUP(D422,list!$D$3:$F$501,2,FALSE)&F422&\"_\"&VLOOKUP(G422,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_ISO3"},"LPAU01A01_ISO3 AT%M1596.0 :BOOL; (*P新风机组01A01-低温断路报警隔离*)","LPAU01A01_ISO3          AT%M1596.0     :BOOL; (*P新风机组01A01-低温断路报警隔离*)"]
["1598.0","验证通过","INT","P新风机组","L","01A01","变频器频率控制值","P新风机组01A01-变频器频率控制值",{"$f":"E423&VLOOKUP(D423,list!$D$3:$F$501,2,FALSE)&F423&\"_\"&VLOOKUP(G423,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_VFCS"},"LPAU01A01_VFCS AT%M1598.0 :INT; (*P新风机组01A01-变频器频率控制值*)","LPAU01A01_VFCS          AT%M1598.0     :INT; (*P新风机组01A01-变频器频率控制值*)"]
["1600.0","验证通过","INT","P新风机组","L","01A01","变频器频率反馈值","P新风机组01A01-变频器频率反馈值",{"$f":"E424&VLOOKUP(D424,list!$D$3:$F$501,2,FALSE)&F424&\"_\"&VLOOKUP(G424,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_VFBS"},"LPAU01A01_VFBS AT%M1600.0 :INT; (*P新风机组01A01-变频器频率反馈值*)","LPAU01A01_VFBS          AT%M1600.0     :INT; (*P新风机组01A01-变频器频率反馈值*)"]
["1602.0","验证通过","BOOL","P新风机组","L","01A01","联动模式","P新风机组01A01-联动模式",{"$f":"E425&VLOOKUP(D425,list!$D$3:$F$501,2,FALSE)&F425&\"_\"&VLOOKUP(G425,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_LM"},"LPAU01A01_LM AT%M1602.0 :BOOL; (*P新风机组01A01-联动模式*)","LPAU01A01_LM            AT%M1602.0     :BOOL; (*P新风机组01A01-联动模式*)"]
["1604.0","验证通过","BOOL","P新风机组","L","01A01","全天候模式","P新风机组01A01-全天候模式",{"$f":"E426&VLOOKUP(D426,list!$D$3:$F$501,2,FALSE)&F426&\"_\"&VLOOKUP(G426,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_DM"},"LPAU01A01_DM AT%M1604.0 :BOOL; (*P新风机组01A01-全天候模式*)","LPAU01A01_DM            AT%M1604.0     :BOOL; (*P新风机组01A01-全天候模式*)"]
["1608.0","验证通过","REAL","P新风机组","L","01A01","CO2设定值","P新风机组01A01-CO2设定值",{"$f":"E427&VLOOKUP(D427,list!$D$3:$F$501,2,FALSE)&F427&\"_\"&VLOOKUP(G427,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_CO2SET"},"LPAU01A01_CO2SET AT%M1608.0 :REAL; (*P新风机组01A01-CO2设定值*)","LPAU01A01_CO2SET        AT%M1608.0     :REAL; (*P新风机组01A01-CO2设定值*)"]
["1612.0","验证通过","BOOL","P新风机组","L","01A01","定时控制","P新风机组01A01-定时控制",{"$f":"E428&VLOOKUP(D428,list!$D$3:$F$501,2,FALSE)&F428&\"_\"&VLOOKUP(G428,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_TC"},"LPAU01A01_TC AT%M1612.0 :BOOL; (*P新风机组01A01-定时控制*)","LPAU01A01_TC            AT%M1612.0     :BOOL; (*P新风机组01A01-定时控制*)"]
["1614.0","验证通过","BOOL","P新风机组","L","01A01","定时模式","P新风机组01A01-定时模式",{"$f":"E429&VLOOKUP(D429,list!$D$3:$F$501,2,FALSE)&F429&\"_\"&VLOOKUP(G429,list!$I$2:$K$502,2,FALSE)","v":"LPAU01A01_TM"},"LPAU01A01_TM AT%M1614.0 :BOOL; (*P新风机组01A01-定时模式*)","LPAU01A01_TM            AT%M1614.0     :BOOL; (*P新风机组01A01-定时模式*)"]
["CO"]
[{"$f":"IF(OR(C429=\"REAL\",C429=\"DWORD\",C429=\"DINT\"),(IF(OR(C431=\"REAL\",C431=\"DWORD\",C431=\"DINT\"),A429+4+MOD(A429,4),A429+4)),(IF(OR(C431=\"REAL\",C431=\"DWORD\",C431=\"DINT\"),A429+4+MOD(A429,4),A429+2)))&\".0\"","v":"1620.0"},{"$f":"IF((IF(OR(C431=\"INT\",C431=\"WORD\",C431=\"BOOL\"),MOD(A431,2),MOD(A431,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","室内环境状态","L","01A01","一氧化碳浓度换算值",{"$f":"D431&F431&\"-\"&IF(E431=\"R\",\"新云平台\"&G431,G431)","v":"室内环境状态01A01-一氧化碳浓度换算值"},{"$f":"E431&VLOOKUP(D431,list!$D$3:$F$501,2,FALSE)&F431&\"_\"&VLOOKUP(G431,list!$I$2:$K$502,2,FALSE)","v":"LIES01A01_COS"},"LIES01A01_COS AT%M1620.0 :REAL; (*室内环境状态01A01-一氧化碳浓度换算值*)","LIES01A01_COS           AT%M1620.0     :REAL; (*室内环境状态01A01-一氧化碳浓度换算值*)"]
["EAF"]
[{"$f":"IF(OR(C431=\"REAL\",C431=\"DWORD\",C431=\"DINT\"),(IF(OR(C433=\"REAL\",C433=\"DWORD\",C433=\"DINT\"),A431+4+MOD(A431,4),A431+4)),(IF(OR(C433=\"REAL\",C433=\"DWORD\",C433=\"DINT\"),A431+4+MOD(A431,4),A431+2)))&\".0\"","v":"1624.0"},{"$f":"IF((IF(OR(C433=\"INT\",C433=\"WORD\",C433=\"BOOL\"),MOD(A433,2),MOD(A433,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","01A01","启停控制",{"$f":"D433&F433&\"-\"&IF(E433=\"R\",\"新云平台\"&G433,G433)","v":"排风机01A01-新云平台启停控制"},{"$f":"E433&VLOOKUP(D433,[1]list!$D$3:$F$501,2,FALSE)&F433&\"_\"&VLOOKUP(G433,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF01A01_C"},{"$f":"I433&\" \"&\"AT%M\"&A433&\" \"&\":\"&C433&\";\"&\" \"&\"(*\"&H433&\"*)\"","v":"REAF01A01_C AT%M1624.0 :BOOL; (*排风机01A01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J433,SEARCH(\"AT%\",J433),,REPT(\" \",25-SEARCH(\"AT%\",J433))),SEARCH(\":\",REPLACE(J433,SEARCH(\"AT%\",J433),,REPT(\" \",25-SEARCH(\"AT%\",J433)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J433,SEARCH(\"AT%\",J433),,REPT(\" \",25-SEARCH(\"AT%\",J433))))))","v":"REAF01A01_C             AT%M1624.0     :BOOL; (*排风机01A01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C433=\"REAL\",C433=\"DWORD\",C433=\"DINT\"),(IF(OR(C434=\"REAL\",C434=\"DWORD\",C434=\"DINT\"),A433+4+MOD(A433,4),A433+4)),(IF(OR(C434=\"REAL\",C434=\"DWORD\",C434=\"DINT\"),A433+4+MOD(A433,4),A433+2)))&\".0\"","v":"1626.0"},"验证通过","BOOL","排风机","L","01A01","运行时间累积重置","排风机01A01-运行时间累积重置",{"$f":"E434&VLOOKUP(D434,[1]list!$D$3:$F$501,2,FALSE)&F434&\"_\"&VLOOKUP(G434,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_RST"},"LEAF01A01_RST AT%M1626.0 :BOOL; (*排风机01A01-运行时间累积重置*)","LEAF01A01_RST           AT%M1626.0     :BOOL; (*排风机01A01-运行时间累积重置*)"]
["1632.0","验证通过","REAL","排风机","L","01A01","运行时间累积重置值","排风机01A01-运行时间累积重置值",{"$f":"E435&VLOOKUP(D435,[1]list!$D$3:$F$501,2,FALSE)&F435&\"_\"&VLOOKUP(G435,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_RSTV"},"LEAF01A01_RSTV AT%M1632.0 :REAL; (*排风机01A01-运行时间累积重置值*)","LEAF01A01_RSTV          AT%M1632.0     :REAL; (*排风机01A01-运行时间累积重置值*)"]
["1636.0","验证通过","REAL","排风机","L","01A01","运行时间累积值","排风机01A01-运行时间累积值",{"$f":"E436&VLOOKUP(D436,[1]list!$D$3:$F$501,2,FALSE)&F436&\"_\"&VLOOKUP(G436,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_RH"},"LEAF01A01_RH AT%M1636.0 :REAL; (*排风机01A01-运行时间累积值*)","LEAF01A01_RH            AT%M1636.0     :REAL; (*排风机01A01-运行时间累积值*)"]
["1640.0","验证通过","BOOL","排风机","L","01A01","定时模式","排风机01A01-定时模式",{"$f":"E437&VLOOKUP(D437,[1]list!$D$3:$F$501,2,FALSE)&F437&\"_\"&VLOOKUP(G437,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_TM"},"LEAF01A01_TM AT%M1640.0 :BOOL; (*排风机01A01-定时模式*)","LEAF01A01_TM            AT%M1640.0     :BOOL; (*排风机01A01-定时模式*)"]
["1642.0","验证通过","BOOL","排风机","L","01A01","定时控制","排风机01A01-定时控制",{"$f":"E438&VLOOKUP(D438,[1]list!$D$3:$F$501,2,FALSE)&F438&\"_\"&VLOOKUP(G438,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_TC"},"LEAF01A01_TC AT%M1642.0 :BOOL; (*排风机01A01-定时控制*)","LEAF01A01_TC            AT%M1642.0     :BOOL; (*排风机01A01-定时控制*)"]
["1644.0","验证通过","BOOL","排风机","L","01A01","全天候模式","排风机01A01-全天候模式",{"$f":"E439&VLOOKUP(D439,[1]list!$D$3:$F$501,2,FALSE)&F439&\"_\"&VLOOKUP(G439,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_DM"},"LEAF01A01_DM AT%M1644.0 :BOOL; (*排风机01A01-全天候模式*)","LEAF01A01_DM            AT%M1644.0     :BOOL; (*排风机01A01-全天候模式*)"]
["1648.0","验证通过","REAL","排风机","L","01A01","CO设定值","排风机01A01-CO设定值",{"$f":"E440&VLOOKUP(D440,[1]list!$D$3:$F$501,2,FALSE)&F440&\"_\"&VLOOKUP(G440,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_COSET"},"LEAF01A01_COSET AT%M1648.0 :REAL; (*排风机01A01-CO设定值*)","LEAF01A01_COSET         AT%M1648.0     :REAL; (*排风机01A01-CO设定值*)"]
["1652.0","验证通过","REAL","排烟机","L","01A01","设定温度值","排烟机01A01-设定温度值",{"$f":"E441&VLOOKUP(D441,[1]list!$D$3:$F$501,2,FALSE)&F441&\"_\"&VLOOKUP(G441,[1]list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_TSET"},"LESF01A01_TSET AT%M1652.0 :REAL; (*排烟机01A01-设定温度值*)","LESF01A01_TSET          AT%M1652.0     :REAL; (*排烟机01A01-设定温度值*)"]
["FMJ"]
[{"$f":"IF(OR(C441=\"REAL\",C441=\"DWORD\",C441=\"DINT\"),(IF(OR(C443=\"REAL\",C443=\"DWORD\",C443=\"DINT\"),A441+4+MOD(A441,4),A441+4)),(IF(OR(C443=\"REAL\",C443=\"DWORD\",C443=\"DINT\"),A441+4+MOD(A441,4),A441+2)))&\".0\"","v":"1656.0"},{"$f":"IF((IF(OR(C443=\"INT\",C443=\"WORD\",C443=\"BOOL\"),MOD(A443,2),MOD(A443,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","风幕机","R","01A01","启停控制",{"$f":"D443&F443&\"-\"&IF(E443=\"R\",\"新云平台\"&G443,G443)","v":"风幕机01A01-新云平台启停控制"},{"$f":"E443&VLOOKUP(D443,list!$D$3:$F$501,2,FALSE)&F443&\"_\"&VLOOKUP(G443,list!$I$2:$K$502,2,FALSE)","v":"RFMJ01A01_C"},{"$f":"I443&\" \"&\"AT%M\"&A443&\" \"&\":\"&C443&\";\"&\" \"&\"(*\"&H443&\"*)\"","v":"RFMJ01A01_C AT%M1656.0 :BOOL; (*风幕机01A01-新云平台启停控制*)"},"RFMJ01A01_C             AT%M1656.0     :BOOL; (*风幕机01A01-新云平台启停控制*)"]
[{"$f":"IF(OR(C443=\"REAL\",C443=\"DWORD\",C443=\"DINT\"),(IF(OR(C444=\"REAL\",C444=\"DWORD\",C444=\"DINT\"),A443+4+MOD(A443,4),A443+4)),(IF(OR(C444=\"REAL\",C444=\"DWORD\",C444=\"DINT\"),A443+4+MOD(A443,4),A443+2)))&\".0\"","v":"1658.0"},"验证通过","BOOL","风幕机","L","01A01","定时模式","风幕机01A01-定时模式",{"$f":"E444&VLOOKUP(D444,list!$D$3:$F$501,2,FALSE)&F444&\"_\"&VLOOKUP(G444,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_TM"},"LFMJ01A01_TM AT%M1658.0 :BOOL; (*风幕机01A01-定时模式*)","LFMJ01A01_TM            AT%M1658.0     :BOOL; (*风幕机01A01-定时模式*)"]
["1660.0","验证通过","BOOL","风幕机","L","01A01","定时控制","风幕机01A01-定时控制",{"$f":"E445&VLOOKUP(D445,list!$D$3:$F$501,2,FALSE)&F445&\"_\"&VLOOKUP(G445,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_TC"},"LFMJ01A01_TC AT%M1660.0 :BOOL; (*风幕机01A01-定时控制*)","LFMJ01A01_TC            AT%M1660.0     :BOOL; (*风幕机01A01-定时控制*)"]
["1662.0","验证通过","BOOL","风幕机","L","01A01","运行时间累积重置",{"$f":"D446&F446&\"-\"&IF(E446=\"R\",\"新云平台\"&G446,G446)","v":"风幕机01A01-运行时间累积重置"},{"$f":"E446&VLOOKUP(D446,list!$D$3:$F$501,2,FALSE)&F446&\"_\"&VLOOKUP(G446,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_RST"},"LFMJ01A01_RST AT%M1662.0 :BOOL; (*风幕机01A01-运行时间累积重置*)",{"$f":"REPLACE(REPLACE(J446,SEARCH(\"AT%\",J446),,REPT(\" \",25-SEARCH(\"AT%\",J446))),SEARCH(\":\",REPLACE(J446,SEARCH(\"AT%\",J446),,REPT(\" \",25-SEARCH(\"AT%\",J446)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J446,SEARCH(\"AT%\",J446),,REPT(\" \",25-SEARCH(\"AT%\",J446))))))","v":"LFMJ01A01_RST           AT%M1662.0     :BOOL; (*风幕机01A01-运行时间累积重置*)"}]
["1668.0","验证通过","REAL","风幕机","L","01A01","运行时间累积重置值","风幕机01A01-运行时间累积重置值",{"$f":"E447&VLOOKUP(D447,list!$D$3:$F$501,2,FALSE)&F447&\"_\"&VLOOKUP(G447,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_RSTV"},"LFMJ01A01_RSTV AT%M1668.0 :REAL; (*风幕机01A01-运行时间累积重置值*)","LFMJ01A01_RSTV          AT%M1668.0     :REAL; (*风幕机01A01-运行时间累积重置值*)"]
["1672.0","验证通过","REAL","风幕机","L","01A01","运行时间累积值","风幕机01A01-运行时间累积值",{"$f":"E448&VLOOKUP(D448,list!$D$3:$F$501,2,FALSE)&F448&\"_\"&VLOOKUP(G448,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_RH"},"LFMJ01A01_RH AT%M1672.0 :REAL; (*风幕机01A01-运行时间累积值*)","LFMJ01A01_RH            AT%M1672.0     :REAL; (*风幕机01A01-运行时间累积值*)"]
["LET"]
[{"$f":"IF(OR(C448=\"REAL\",C448=\"DWORD\",C448=\"DINT\"),(IF(OR(C450=\"REAL\",C450=\"DWORD\",C450=\"DINT\"),A448+4+MOD(A448,4),A448+4)),(IF(OR(C450=\"REAL\",C450=\"DWORD\",C450=\"DINT\"),A448+4+MOD(A448,4),A448+2)))&\".0\"","v":"1676.0"},{"$f":"IF((IF(OR(C450=\"INT\",C450=\"WORD\",C450=\"BOOL\"),MOD(A450,2),MOD(A450,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","扶梯","L","01A01","运行状态","扶梯01A01-运行状态",{"$f":"E450&VLOOKUP(D450,list!$D$3:$F$501,2,FALSE)&F450&\"_\"&VLOOKUP(G450,list!$I$2:$K$502,2,FALSE)","v":"LLET01A01_R"},{"$f":"I450&\" \"&\"AT%M\"&A450&\" \"&\":\"&C450&\";\"&\" \"&\"(*\"&H450&\"*)\"","v":"LLET01A01_R AT%M1676.0 :BOOL; (*扶梯01A01-运行状态*)"},"LLET01A01_R             AT%M1676.0     :BOOL; (*扶梯01A01-运行状态*)"]
[{"$f":"IF(OR(C450=\"REAL\",C450=\"DWORD\",C450=\"DINT\"),(IF(OR(C451=\"REAL\",C451=\"DWORD\",C451=\"DINT\"),A450+4+MOD(A450,4),A450+4)),(IF(OR(C451=\"REAL\",C451=\"DWORD\",C451=\"DINT\"),A450+4+MOD(A450,4),A450+2)))&\".0\"","v":"1678.0"},"验证通过","BOOL","扶梯","L","01A01","运行时间累积重置","扶梯01A01-运行时间累积重置",{"$f":"E451&VLOOKUP(D451,list!$D$3:$F$501,2,FALSE)&F451&\"_\"&VLOOKUP(G451,list!$I$2:$K$502,2,FALSE)","v":"LLET01A01_RST"},"LLET01A01_RST AT%M1678.0 :BOOL; (*扶梯01A01-运行时间累积重置*)","LLET01A01_RST           AT%M1678.0     :BOOL; (*扶梯01A01-运行时间累积重置*)"]
["1684.0","验证通过","REAL","扶梯","L","01A01","运行时间累积重置值","扶梯01A01-运行时间累积重置值",{"$f":"E452&VLOOKUP(D452,list!$D$3:$F$501,2,FALSE)&F452&\"_\"&VLOOKUP(G452,list!$I$2:$K$502,2,FALSE)","v":"LLET01A01_RSTV"},"LLET01A01_RSTV AT%M1684.0 :REAL; (*扶梯01A01-运行时间累积重置值*)","LLET01A01_RSTV          AT%M1684.0     :REAL; (*扶梯01A01-运行时间累积重置值*)"]
["1688.0","验证通过","REAL","扶梯","L","01A01","运行时间累积值","扶梯01A01-运行时间累积值",{"$f":"E453&VLOOKUP(D453,list!$D$3:$F$501,2,FALSE)&F453&\"_\"&VLOOKUP(G453,list!$I$2:$K$502,2,FALSE)","v":"LLET01A01_RH"},"LLET01A01_RH AT%M1688.0 :REAL; (*扶梯01A01-运行时间累积值*)","LLET01A01_RH            AT%M1688.0     :REAL; (*扶梯01A01-运行时间累积值*)"]
["ESF"]
[{"$f":"IF(OR(C453=\"REAL\",C453=\"DWORD\",C453=\"DINT\"),(IF(OR(C455=\"REAL\",C455=\"DWORD\",C455=\"DINT\"),A453+4+MOD(A453,4),A453+4)),(IF(OR(C455=\"REAL\",C455=\"DWORD\",C455=\"DINT\"),A453+4+MOD(A453,4),A453+2)))&\".0\"","v":"1692.0"},{"$f":"IF((IF(OR(C455=\"INT\",C455=\"WORD\",C455=\"BOOL\"),MOD(A455,2),MOD(A455,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排烟机","R","01A01","启停控制",{"$f":"D455&F455&\"-\"&IF(E455=\"R\",\"新云平台\"&G455,G455)","v":"排烟机01A01-新云平台启停控制"},{"$f":"E455&VLOOKUP(D455,list!$D$3:$F$501,2,FALSE)&F455&\"_\"&VLOOKUP(G455,list!$I$2:$K$502,2,FALSE)","v":"RESF01A01_C"},{"$f":"I455&\" \"&\"AT%M\"&A455&\" \"&\":\"&C455&\";\"&\" \"&\"(*\"&H455&\"*)\"","v":"RESF01A01_C AT%M1692.0 :BOOL; (*排烟机01A01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J455,SEARCH(\"AT%\",J455),,REPT(\" \",25-SEARCH(\"AT%\",J455))),SEARCH(\":\",REPLACE(J455,SEARCH(\"AT%\",J455),,REPT(\" \",25-SEARCH(\"AT%\",J455)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J455,SEARCH(\"AT%\",J455),,REPT(\" \",25-SEARCH(\"AT%\",J455))))))","v":"RESF01A01_C             AT%M1692.0     :BOOL; (*排烟机01A01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C455=\"REAL\",C455=\"DWORD\",C455=\"DINT\"),(IF(OR(C456=\"REAL\",C456=\"DWORD\",C456=\"DINT\"),A455+4+MOD(A455,4),A455+4)),(IF(OR(C456=\"REAL\",C456=\"DWORD\",C456=\"DINT\"),A455+4+MOD(A455,4),A455+2)))&\".0\"","v":"1694.0"},"验证通过","BOOL","排烟机","L","01A01","运行时间累积重置","排烟机01A01-运行时间累积重置",{"$f":"E456&VLOOKUP(D456,list!$D$3:$F$501,2,FALSE)&F456&\"_\"&VLOOKUP(G456,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_RST"},"LESF01A01_RST AT%M1694.0 :BOOL; (*排烟机01A01-运行时间累积重置*)","LESF01A01_RST           AT%M1694.0     :BOOL; (*排烟机01A01-运行时间累积重置*)"]
["1700.0","验证通过","REAL","排烟机","L","01A01","运行时间累积重置值","排烟机01A01-运行时间累积重置值",{"$f":"E457&VLOOKUP(D457,list!$D$3:$F$501,2,FALSE)&F457&\"_\"&VLOOKUP(G457,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_RSTV"},"LESF01A01_RSTV AT%M1700.0 :REAL; (*排烟机01A01-运行时间累积重置值*)","LESF01A01_RSTV          AT%M1700.0     :REAL; (*排烟机01A01-运行时间累积重置值*)"]
["1704.0","验证通过","REAL","排烟机","L","01A01","运行时间累积值","排烟机01A01-运行时间累积值",{"$f":"E458&VLOOKUP(D458,list!$D$3:$F$501,2,FALSE)&F458&\"_\"&VLOOKUP(G458,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_RH"},"LESF01A01_RH AT%M1704.0 :REAL; (*排烟机01A01-运行时间累积值*)","LESF01A01_RH            AT%M1704.0     :REAL; (*排烟机01A01-运行时间累积值*)"]
["1708.0","验证通过","BOOL","排烟机","L","01A01","定时模式","排烟机01A01-定时模式",{"$f":"E459&VLOOKUP(D459,list!$D$3:$F$501,2,FALSE)&F459&\"_\"&VLOOKUP(G459,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_TM"},"LESF01A01_TM AT%M1708.0 :BOOL; (*排烟机01A01-定时模式*)","LESF01A01_TM            AT%M1708.0     :BOOL; (*排烟机01A01-定时模式*)"]
["1710.0","验证通过","BOOL","排烟机","L","01A01","定时控制","排烟机01A01-定时控制",{"$f":"E460&VLOOKUP(D460,list!$D$3:$F$501,2,FALSE)&F460&\"_\"&VLOOKUP(G460,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_TC"},"LESF01A01_TC AT%M1710.0 :BOOL; (*排烟机01A01-定时控制*)","LESF01A01_TC            AT%M1710.0     :BOOL; (*排烟机01A01-定时控制*)"]
["1712.0","验证通过","BOOL","排烟机","L","01A01","全天候模式","排烟机01A01-全天候模式",{"$f":"E461&VLOOKUP(D461,list!$D$3:$F$501,2,FALSE)&F461&\"_\"&VLOOKUP(G461,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_DM"},"LESF01A01_DM AT%M1712.0 :BOOL; (*排烟机01A01-全天候模式*)","LESF01A01_DM            AT%M1712.0     :BOOL; (*排烟机01A01-全天候模式*)"]
["1716.0","验证通过","REAL","排烟机","L","01A01","CO2设定值","排烟机01A01-CO2设定值",{"$f":"E462&VLOOKUP(D462,list!$D$3:$F$501,2,FALSE)&F462&\"_\"&VLOOKUP(G462,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_CO2SET"},"LESF01A01_CO2SET AT%M1716.0 :REAL; (*排烟机01A01-CO2设定值*)","LESF01A01_CO2SET        AT%M1716.0     :REAL; (*排烟机01A01-CO2设定值*)"]
[{"$f":"IF(OR(C462=\"REAL\",C462=\"DWORD\",C462=\"DINT\"),(IF(OR(C463=\"REAL\",C463=\"DWORD\",C463=\"DINT\"),A462+4+MOD(A462,4),A462+4)),(IF(OR(C463=\"REAL\",C463=\"DWORD\",C463=\"DINT\"),A462+4+MOD(A462,4),A462+2)))&\".0\"","v":"1720.0"},{"$f":"IF((IF(OR(C463=\"INT\",C463=\"WORD\",C463=\"BOOL\"),MOD(A463,2),MOD(A463,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","排烟机","L","01A01","设定温度值",{"$f":"D463&F463&\"-\"&IF(E463=\"R\",\"新云平台\"&G463,G463)","v":"排烟机01A01-设定温度值"},{"$f":"E463&VLOOKUP(D463,list!$D$3:$F$501,2,FALSE)&F463&\"_\"&VLOOKUP(G463,list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_TSET"},{"$f":"I463&\" \"&\"AT%M\"&A463&\" \"&\":\"&C463&\";\"&\" \"&\"(*\"&H463&\"*)\"","v":"LESF01A01_TSET AT%M1720.0 :REAL; (*排烟机01A01-设定温度值*)"},{"$f":"REPLACE(REPLACE(J463,SEARCH(\"AT%\",J463),,REPT(\" \",25-SEARCH(\"AT%\",J463))),SEARCH(\":\",REPLACE(J463,SEARCH(\"AT%\",J463),,REPT(\" \",25-SEARCH(\"AT%\",J463)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J463,SEARCH(\"AT%\",J463),,REPT(\" \",25-SEARCH(\"AT%\",J463))))))","v":"LESF01A01_TSET          AT%M1720.0     :REAL; (*排烟机01A01-设定温度值*)"}]
["SWP"]
[{"$f":"IF(OR(C463=\"REAL\",C463=\"DWORD\",C463=\"DINT\"),(IF(OR(C465=\"REAL\",C465=\"DWORD\",C465=\"DINT\"),A463+4+MOD(A463,4),A463+4)),(IF(OR(C465=\"REAL\",C465=\"DWORD\",C465=\"DINT\"),A463+4+MOD(A463,4),A463+2)))&\".0\"","v":"1724.0"},{"$f":"IF((IF(OR(C465=\"INT\",C465=\"WORD\",C465=\"BOOL\"),MOD(A465,2),MOD(A465,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","潜污泵井","L","01A01","运行时间累积重置1",{"$f":"D465&F465&\"-\"&IF(E465=\"R\",\"新云平台\"&G465,G465)","v":"潜污泵井01A01-运行时间累积重置1"},{"$f":"E465&VLOOKUP(D465,list!$D$3:$F$501,2,FALSE)&F465&\"_\"&VLOOKUP(G465,list!$I$2:$K$502,2,FALSE)","v":"LSWP01A01_RST1"},{"$f":"I465&\" \"&\"AT%M\"&A465&\" \"&\":\"&C465&\";\"&\" \"&\"(*\"&H465&\"*)\"","v":"LSWP01A01_RST1 AT%M1724.0 :BOOL; (*潜污泵井01A01-运行时间累积重置1*)"},{"$f":"REPLACE(REPLACE(J465,SEARCH(\"AT%\",J465),,REPT(\" \",25-SEARCH(\"AT%\",J465))),SEARCH(\":\",REPLACE(J465,SEARCH(\"AT%\",J465),,REPT(\" \",25-SEARCH(\"AT%\",J465)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J465,SEARCH(\"AT%\",J465),,REPT(\" \",25-SEARCH(\"AT%\",J465))))))","v":"LSWP01A01_RST1          AT%M1724.0     :BOOL; (*潜污泵井01A01-运行时间累积重置1*)"}]
[{"$f":"IF(OR(C465=\"REAL\",C465=\"DWORD\",C465=\"DINT\"),(IF(OR(C466=\"REAL\",C466=\"DWORD\",C466=\"DINT\"),A465+4+MOD(A465,4),A465+4)),(IF(OR(C466=\"REAL\",C466=\"DWORD\",C466=\"DINT\"),A465+4+MOD(A465,4),A465+2)))&\".0\"","v":"1728.0"},"验证通过","REAL","潜污泵井","L","01A01","运行时间累积重置值1","潜污泵井01A01-运行时间累积重置值1",{"$f":"E466&VLOOKUP(D466,list!$D$3:$F$501,2,FALSE)&F466&\"_\"&VLOOKUP(G466,list!$I$2:$K$502,2,FALSE)","v":"LSWP01A01_RSTV1"},"LSWP01A01_RSTV1 AT%M1728.0 :REAL; (*潜污泵井01A01-运行时间累积重置值1*)","LSWP01A01_RSTV1         AT%M1728.0     :REAL; (*潜污泵井01A01-运行时间累积重置值1*)"]
["1732.0","验证通过","REAL","潜污泵井","L","01A01","运行时间累积值1","潜污泵井01A01-运行时间累积值1",{"$f":"E467&VLOOKUP(D467,list!$D$3:$F$501,2,FALSE)&F467&\"_\"&VLOOKUP(G467,list!$I$2:$K$502,2,FALSE)","v":"LSWP01A01_RH1"},"LSWP01A01_RH1 AT%M1732.0 :REAL; (*潜污泵井01A01-运行时间累积值1*)","LSWP01A01_RH1           AT%M1732.0     :REAL; (*潜污泵井01A01-运行时间累积值1*)"]
["1736.0",{"$f":"IF((IF(OR(C468=\"INT\",C468=\"WORD\",C468=\"BOOL\"),MOD(A468,2),MOD(A468,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","潜污泵井","L","01A01","运行时间累积重置2",{"$f":"D468&F468&\"-\"&IF(E468=\"R\",\"新云平台\"&G468,G468)","v":"潜污泵井01A01-运行时间累积重置2"},{"$f":"E468&VLOOKUP(D468,list!$D$3:$F$501,2,FALSE)&F468&\"_\"&VLOOKUP(G468,list!$I$2:$K$502,2,FALSE)","v":"LSWP01A01_RST2"},{"$f":"I468&\" \"&\"AT%M\"&A468&\" \"&\":\"&C468&\";\"&\" \"&\"(*\"&H468&\"*)\"","v":"LSWP01A01_RST2 AT%M1736.0 :BOOL; (*潜污泵井01A01-运行时间累积重置2*)"},{"$f":"REPLACE(REPLACE(J468,SEARCH(\"AT%\",J468),,REPT(\" \",25-SEARCH(\"AT%\",J468))),SEARCH(\":\",REPLACE(J468,SEARCH(\"AT%\",J468),,REPT(\" \",25-SEARCH(\"AT%\",J468)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J468,SEARCH(\"AT%\",J468),,REPT(\" \",25-SEARCH(\"AT%\",J468))))))","v":"LSWP01A01_RST2          AT%M1736.0     :BOOL; (*潜污泵井01A01-运行时间累积重置2*)"}]
[{"$f":"IF(OR(C468=\"REAL\",C468=\"DWORD\",C468=\"DINT\"),(IF(OR(C469=\"REAL\",C469=\"DWORD\",C469=\"DINT\"),A468+4+MOD(A468,4),A468+4)),(IF(OR(C469=\"REAL\",C469=\"DWORD\",C469=\"DINT\"),A468+4+MOD(A468,4),A468+2)))&\".0\"","v":"1740.0"},"验证通过","REAL","潜污泵井","L","01A01","运行时间累积重置值2","潜污泵井01A01-运行时间累积重置值2",{"$f":"E469&VLOOKUP(D469,list!$D$3:$F$501,2,FALSE)&F469&\"_\"&VLOOKUP(G469,list!$I$2:$K$502,2,FALSE)","v":"LSWP01A01_RSTV2"},"LSWP01A01_RSTV2 AT%M1740.0 :REAL; (*潜污泵井01A01-运行时间累积重置值2*)","LSWP01A01_RSTV2         AT%M1740.0     :REAL; (*潜污泵井01A01-运行时间累积重置值2*)"]
["1744.0","验证通过","REAL","潜污泵井","L","01A01","运行时间累积值2","潜污泵井01A01-运行时间累积值2",{"$f":"E470&VLOOKUP(D470,list!$D$3:$F$501,2,FALSE)&F470&\"_\"&VLOOKUP(G470,list!$I$2:$K$502,2,FALSE)","v":"LSWP01A01_RH2"},"LSWP01A01_RH2 AT%M1744.0 :REAL; (*潜污泵井01A01-运行时间累积值2*)","LSWP01A01_RH2           AT%M1744.0     :REAL; (*潜污泵井01A01-运行时间累积值2*)"]
["AHU"]
[{"$f":"IF(OR(C470=\"REAL\",C470=\"DWORD\",C470=\"DINT\"),(IF(OR(C472=\"REAL\",C472=\"DWORD\",C472=\"DINT\"),A470+4+MOD(A470,4),A470+4)),(IF(OR(C472=\"REAL\",C472=\"DWORD\",C472=\"DINT\"),A470+4+MOD(A470,4),A470+2)))&\".0\"","v":"1748.0"},{"$f":"IF((IF(OR(C472=\"INT\",C472=\"WORD\",C472=\"BOOL\"),MOD(A472,2),MOD(A472,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","空调机组","R","YYA01","程序控制",{"$f":"D472&F472&\"-\"&IF(E472=\"R\",\"新云平台\"&G472,G472)","v":"空调机组YYA01-新云平台程序控制"},{"$f":"E472&VLOOKUP(D472,[2]list!$D$3:$F$501,2,FALSE)&F472&\"_\"&VLOOKUP(G472,[2]list!$I$2:$K$501,2,FALSE)","v":"RAHUYYA01_PC"},{"$f":"I472&\" \"&\"AT%M\"&A472&\" \"&\":\"&C472&\";\"&\" \"&\"(*\"&H472&\"*)\"","v":"RAHUYYA01_PC AT%M1748.0 :BOOL; (*空调机组YYA01-新云平台程序控制*)"},{"$f":"REPLACE(REPLACE(J472,SEARCH(\"AT%\",J472),,REPT(\" \",25-SEARCH(\"AT%\",J472))),SEARCH(\":\",REPLACE(J472,SEARCH(\"AT%\",J472),,REPT(\" \",25-SEARCH(\"AT%\",J472)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J472,SEARCH(\"AT%\",J472),,REPT(\" \",25-SEARCH(\"AT%\",J472))))))","v":"RAHUYYA01_PC            AT%M1748.0     :BOOL; (*空调机组YYA01-新云平台程序控制*)"}]
[{"$f":"IF(OR(C472=\"REAL\",C472=\"DWORD\",C472=\"DINT\"),(IF(OR(C473=\"REAL\",C473=\"DWORD\",C473=\"DINT\"),A472+4+MOD(A472,4),A472+4)),(IF(OR(C473=\"REAL\",C473=\"DWORD\",C473=\"DINT\"),A472+4+MOD(A472,4),A472+2)))&\".0\"","v":"1752.0"},"验证通过","REAL","空调机组","R",{"$f":"F472","v":"YYA01"},"设定温度值","空调机组YYA01-新云平台设定温度值",{"$f":"E473&VLOOKUP(D473,[2]list!$D$3:$F$501,2,FALSE)&F473&\"_\"&VLOOKUP(G473,[2]list!$I$2:$K$501,2,FALSE)","v":"RAHUYYA01_TSET"},"RAHUYYA01_TSET AT%M1752.0 :REAL; (*空调机组YYA01-新云平台设定温度值*)","RAHUYYA01_TSET          AT%M1752.0     :REAL; (*空调机组YYA01-新云平台设定温度值*)"]
[{"$f":"IF(OR(C473=\"REAL\",C473=\"DWORD\",C473=\"DINT\"),(IF(OR(C474=\"REAL\",C474=\"DWORD\",C474=\"DINT\"),A473+4+MOD(A473,4),A473+4)),(IF(OR(C474=\"REAL\",C474=\"DWORD\",C474=\"DINT\"),A473+4+MOD(A473,4),A473+2)))&\".0\"","v":"1756.0"},"验证通过","INT","空调机组","R","YYA01","季节模式","空调机组YYA01-新云平台季节模式",{"$f":"E474&VLOOKUP(D474,[2]list!$D$3:$F$501,2,FALSE)&F474&\"_\"&VLOOKUP(G474,[2]list!$I$2:$K$501,2,FALSE)","v":"RAHUYYA01_SM"},"RAHUYYA01_SM AT%M1756.0 :INT; (*空调机组YYA01-新云平台季节模式*)","RAHUYYA01_SM            AT%M1756.0     :INT; (*空调机组YYA01-新云平台季节模式*)"]
["1760.0","验证通过","REAL","空调机组","L","YYA01","水阀反馈换算值","空调机组YYA01-水阀反馈换算值",{"$f":"E475&VLOOKUP(D475,[2]list!$D$3:$F$501,2,FALSE)&F475&\"_\"&VLOOKUP(G475,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_WVBS"},"LAHUYYA01_WVBS AT%M1760.0 :REAL; (*空调机组YYA01-水阀反馈换算值*)","LAHUYYA01_WVBS          AT%M1760.0     :REAL; (*空调机组YYA01-水阀反馈换算值*)"]
["1764.0","验证通过","BOOL","空调机组","L","YYA01","水阀手动控制","空调机组YYA01-水阀手动控制",{"$f":"E476&VLOOKUP(D476,[2]list!$D$3:$F$501,2,FALSE)&F476&\"_\"&VLOOKUP(G476,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_WVMC"},"LAHUYYA01_WVMC AT%M1764.0 :BOOL; (*空调机组YYA01-水阀手动控制*)","LAHUYYA01_WVMC          AT%M1764.0     :BOOL; (*空调机组YYA01-水阀手动控制*)"]
["1768.0","验证通过","REAL","空调机组","L","YYA01","水阀手动控制值","空调机组YYA01-水阀手动控制值",{"$f":"E477&VLOOKUP(D477,[2]list!$D$3:$F$501,2,FALSE)&F477&\"_\"&VLOOKUP(G477,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_WVMV"},"LAHUYYA01_WVMV AT%M1768.0 :REAL; (*空调机组YYA01-水阀手动控制值*)","LAHUYYA01_WVMV          AT%M1768.0     :REAL; (*空调机组YYA01-水阀手动控制值*)"]
["1772.0","验证通过","REAL","空调机组","L",{"$f":"F476","v":"YYA01"},"二氧化碳换算值","空调机组YYA01-二氧化碳换算值",{"$f":"E478&VLOOKUP(D478,[2]list!$D$3:$F$501,2,FALSE)&F478&\"_\"&VLOOKUP(G478,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_CO2S"},"LAHUYYA01_CO2S AT%M1772.0 :REAL; (*空调机组YYA01-二氧化碳换算值*)","LAHUYYA01_CO2S          AT%M1772.0     :REAL; (*空调机组YYA01-二氧化碳换算值*)"]
["1776.0","验证通过","REAL","空调机组","L",{"$f":"F477","v":"YYA01"},"二氧化碳设定值","空调机组YYA01-二氧化碳设定值",{"$f":"E479&VLOOKUP(D479,[2]list!$D$3:$F$501,2,FALSE)&F479&\"_\"&VLOOKUP(G479,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_CO2SET"},"LAHUYYA01_CO2SET AT%M1776.0 :REAL; (*空调机组YYA01-二氧化碳设定值*)","LAHUYYA01_CO2SET        AT%M1776.0     :REAL; (*空调机组YYA01-二氧化碳设定值*)"]
["1780.0","验证通过","REAL","空调机组","L",{"$f":"F477","v":"YYA01"},"回风温度换算值","空调机组YYA01-回风温度换算值",{"$f":"E480&VLOOKUP(D480,[2]list!$D$3:$F$501,2,FALSE)&F480&\"_\"&VLOOKUP(G480,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_RTS"},"LAHUYYA01_RTS AT%M1780.0 :REAL; (*空调机组YYA01-回风温度换算值*)","LAHUYYA01_RTS           AT%M1780.0     :REAL; (*空调机组YYA01-回风温度换算值*)"]
["1784.0","验证通过","REAL","空调机组","L","YYA01","送风温度换算值","空调机组YYA01-送风温度换算值",{"$f":"E481&VLOOKUP(D481,[2]list!$D$3:$F$501,2,FALSE)&F481&\"_\"&VLOOKUP(G481,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_STS"},"LAHUYYA01_STS AT%M1784.0 :REAL; (*空调机组YYA01-送风温度换算值*)","LAHUYYA01_STS           AT%M1784.0     :REAL; (*空调机组YYA01-送风温度换算值*)"]
["1788.0","验证通过","BOOL","空调机组","L",{"$f":"F480","v":"YYA01"},"运行时间累积重置","空调机组YYA01-运行时间累积重置",{"$f":"E482&VLOOKUP(D482,[2]list!$D$3:$F$501,2,FALSE)&F482&\"_\"&VLOOKUP(G482,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_RST"},"LAHUYYA01_RST AT%M1788.0 :BOOL; (*空调机组YYA01-运行时间累积重置*)","LAHUYYA01_RST           AT%M1788.0     :BOOL; (*空调机组YYA01-运行时间累积重置*)"]
["1792.0","验证通过","REAL","空调机组","L","YYA01","运行时间累积重置值","空调机组YYA01-运行时间累积重置值",{"$f":"E483&VLOOKUP(D483,[2]list!$D$3:$F$501,2,FALSE)&F483&\"_\"&VLOOKUP(G483,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_RSTV"},"LAHUYYA01_RSTV AT%M1792.0 :REAL; (*空调机组YYA01-运行时间累积重置值*)","LAHUYYA01_RSTV          AT%M1792.0     :REAL; (*空调机组YYA01-运行时间累积重置值*)"]
["1796.0","验证通过","BOOL","空调机组","L","YYA01","隔离开关1","空调机组YYA01-隔离开关1",{"$f":"E484&VLOOKUP(D484,[2]list!$D$3:$F$501,2,FALSE)&F484&\"_\"&VLOOKUP(G484,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_ISO1"},"LAHUYYA01_ISO1 AT%M1796.0 :BOOL; (*空调机组YYA01-隔离开关1*)","LAHUYYA01_ISO1          AT%M1796.0     :BOOL; (*空调机组YYA01-隔离开关1*)"]
["1798.0","验证通过","BOOL","空调机组","L","YYA01","隔离开关2","空调机组YYA01-隔离开关2",{"$f":"E485&VLOOKUP(D485,[2]list!$D$3:$F$501,2,FALSE)&F485&\"_\"&VLOOKUP(G485,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_ISO2"},"LAHUYYA01_ISO2 AT%M1798.0 :BOOL; (*空调机组YYA01-隔离开关2*)","LAHUYYA01_ISO2          AT%M1798.0     :BOOL; (*空调机组YYA01-隔离开关2*)"]
["1804.0","验证通过","REAL","空调机组","L","YYA01","P调节参数","空调机组YYA01-P调节参数",{"$f":"E486&VLOOKUP(D486,[2]list!$D$3:$F$501,2,FALSE)&F486&\"_\"&VLOOKUP(G486,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_VP"},"LAHUYYA01_VP AT%M1804.0 :REAL; (*空调机组YYA01-P调节参数*)","LAHUYYA01_VP            AT%M1804.0     :REAL; (*空调机组YYA01-P调节参数*)"]
["1808.0","验证通过","REAL","空调机组","L","YYA01","I调节参数","空调机组YYA01-I调节参数",{"$f":"E487&VLOOKUP(D487,[2]list!$D$3:$F$501,2,FALSE)&F487&\"_\"&VLOOKUP(G487,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_VI"},"LAHUYYA01_VI AT%M1808.0 :REAL; (*空调机组YYA01-I调节参数*)","LAHUYYA01_VI            AT%M1808.0     :REAL; (*空调机组YYA01-I调节参数*)"]
["1812.0","验证通过","REAL","空调机组","L","YYA01","运行时间累积值","空调机组YYA01-运行时间累积值",{"$f":"E488&VLOOKUP(D488,[2]list!$D$3:$F$501,2,FALSE)&F488&\"_\"&VLOOKUP(G488,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_RH"},"LAHUYYA01_RH AT%M1812.0 :REAL; (*空调机组YYA01-运行时间累积值*)","LAHUYYA01_RH            AT%M1812.0     :REAL; (*空调机组YYA01-运行时间累积值*)"]
["1816.0","验证通过","INT","空调机组","L","YYA01","设备状态代码","空调机组YYA01-设备状态代码",{"$f":"E489&VLOOKUP(D489,[2]list!$D$3:$F$501,2,FALSE)&F489&\"_\"&VLOOKUP(G489,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_SN"},"LAHUYYA01_SN AT%M1816.0 :INT; (*空调机组YYA01-设备状态代码*)","LAHUYYA01_SN            AT%M1816.0     :INT; (*空调机组YYA01-设备状态代码*)"]
["1818.0","验证通过","INT","空调机组","L","YYA01","水阀控制转换值","空调机组YYA01-水阀控制转换值",{"$f":"E490&VLOOKUP(D490,[2]list!$D$3:$F$501,2,FALSE)&F490&\"_\"&VLOOKUP(G490,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_WVCS"},"LAHUYYA01_WVCS AT%M1818.0 :INT; (*空调机组YYA01-水阀控制转换值*)","LAHUYYA01_WVCS          AT%M1818.0     :INT; (*空调机组YYA01-水阀控制转换值*)"]
["1820.0","验证通过","BOOL","空调机组","L","YYA01","程序控制","空调机组YYA01-程序控制",{"$f":"E491&VLOOKUP(D491,[2]list!$D$3:$F$501,2,FALSE)&F491&\"_\"&VLOOKUP(G491,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_PC"},"LAHUYYA01_PC AT%M1820.0 :BOOL; (*空调机组YYA01-程序控制*)","LAHUYYA01_PC            AT%M1820.0     :BOOL; (*空调机组YYA01-程序控制*)"]
["1824.0","验证通过","REAL","空调机组","L","YYA01","设定温度值","空调机组YYA01-设定温度值",{"$f":"E492&VLOOKUP(D492,[2]list!$D$3:$F$501,2,FALSE)&F492&\"_\"&VLOOKUP(G492,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_TSET"},"LAHUYYA01_TSET AT%M1824.0 :REAL; (*空调机组YYA01-设定温度值*)","LAHUYYA01_TSET          AT%M1824.0     :REAL; (*空调机组YYA01-设定温度值*)"]
["1828.0","验证通过","INT","空调机组","L","YYA01","季节模式","空调机组YYA01-季节模式",{"$f":"E493&VLOOKUP(D493,[2]list!$D$3:$F$501,2,FALSE)&F493&\"_\"&VLOOKUP(G493,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_SM"},"LAHUYYA01_SM AT%M1828.0 :INT; (*空调机组YYA01-季节模式*)","LAHUYYA01_SM            AT%M1828.0     :INT; (*空调机组YYA01-季节模式*)"]
["1830.0","验证通过","INT","空调机组","L",{"$f":"F491","v":"YYA01"},"变频手动控制值","空调机组YYA01-变频手动控制值",{"$f":"E494&VLOOKUP(D494,[2]list!$D$3:$F$501,2,FALSE)&F494&\"_\"&VLOOKUP(G494,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_VFMV"},"LAHUYYA01_VFMV AT%M1830.0 :INT; (*空调机组YYA01-变频手动控制值*)","LAHUYYA01_VFMV          AT%M1830.0     :INT; (*空调机组YYA01-变频手动控制值*)"]
["1832.0","验证通过","BOOL","空调机组","L","YYA01","低温断路报警隔离","空调机组YYA01-低温断路报警隔离",{"$f":"E495&VLOOKUP(D495,[2]list!$D$3:$F$501,2,FALSE)&F495&\"_\"&VLOOKUP(G495,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_ISO3"},"LAHUYYA01_ISO3 AT%M1832.0 :BOOL; (*空调机组YYA01-低温断路报警隔离*)","LAHUYYA01_ISO3          AT%M1832.0     :BOOL; (*空调机组YYA01-低温断路报警隔离*)"]
["1834.0","验证通过","INT","空调机组","L","YYA01","变频器频率控制值","空调机组YYA01-变频器频率控制值",{"$f":"E496&VLOOKUP(D496,[2]list!$D$3:$F$501,2,FALSE)&F496&\"_\"&VLOOKUP(G496,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_VFCS"},"LAHUYYA01_VFCS AT%M1834.0 :INT; (*空调机组YYA01-变频器频率控制值*)","LAHUYYA01_VFCS          AT%M1834.0     :INT; (*空调机组YYA01-变频器频率控制值*)"]
["1836.0","验证通过","INT","空调机组","L","YYA01","变频器频率反馈值","空调机组YYA01-变频器频率反馈值",{"$f":"E497&VLOOKUP(D497,[2]list!$D$3:$F$501,2,FALSE)&F497&\"_\"&VLOOKUP(G497,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_VFBS"},"LAHUYYA01_VFBS AT%M1836.0 :INT; (*空调机组YYA01-变频器频率反馈值*)","LAHUYYA01_VFBS          AT%M1836.0     :INT; (*空调机组YYA01-变频器频率反馈值*)"]
["1838.0","验证通过","BOOL","空调机组","L","YYA01","联动模式","空调机组YYA01-联动模式",{"$f":"E498&VLOOKUP(D498,[2]list!$D$3:$F$501,2,FALSE)&F498&\"_\"&VLOOKUP(G498,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_LM"},"LAHUYYA01_LM AT%M1838.0 :BOOL; (*空调机组YYA01-联动模式*)","LAHUYYA01_LM            AT%M1838.0     :BOOL; (*空调机组YYA01-联动模式*)"]
["1840.0","验证通过","BOOL","空调机组","L","YYA01","风阀联动模式","空调机组YYA01-风阀联动模式",{"$f":"E499&VLOOKUP(D499,[2]list!$D$3:$F$501,2,FALSE)&F499&\"_\"&VLOOKUP(G499,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_FM"},"LAHUYYA01_FM AT%M1840.0 :BOOL; (*空调机组YYA01-风阀联动模式*)","LAHUYYA01_FM            AT%M1840.0     :BOOL; (*空调机组YYA01-风阀联动模式*)"]
["1842.0","验证通过","BOOL","空调机组","L",{"$f":"F498","v":"YYA01"},"定时控制","空调机组YYA01-定时控制",{"$f":"E500&VLOOKUP(D500,[2]list!$D$3:$F$501,2,FALSE)&F500&\"_\"&VLOOKUP(G500,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_TC"},"LAHUYYA01_TC AT%M1842.0 :BOOL; (*空调机组YYA01-定时控制*)","LAHUYYA01_TC            AT%M1842.0     :BOOL; (*空调机组YYA01-定时控制*)"]
["1844.0","验证通过","BOOL","空调机组","L","YYA01","定时模式","空调机组YYA01-定时模式",{"$f":"E501&VLOOKUP(D501,[2]list!$D$3:$F$501,2,FALSE)&F501&\"_\"&VLOOKUP(G501,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_TM"},"LAHUYYA01_TM AT%M1844.0 :BOOL; (*空调机组YYA01-定时模式*)","LAHUYYA01_TM            AT%M1844.0     :BOOL; (*空调机组YYA01-定时模式*)"]
["1846.0","验证通过","INT","空调机组","L","YYA01","回风阀控制换算值","空调机组YYA01-回风阀控制换算值",{"$f":"E502&VLOOKUP(D502,[2]list!$D$3:$F$501,2,FALSE)&F502&\"_\"&VLOOKUP(G502,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_RDCS"},"LAHUYYA01_RDCS AT%M1846.0 :INT; (*空调机组YYA01-回风阀控制换算值*)","LAHUYYA01_RDCS          AT%M1846.0     :INT; (*空调机组YYA01-回风阀控制换算值*)"]
["1848.0","验证通过","INT","空调机组","L","YYA01","新风阀控制换算值","空调机组YYA01-新风阀控制换算值",{"$f":"E503&VLOOKUP(D503,[2]list!$D$3:$F$501,2,FALSE)&F503&\"_\"&VLOOKUP(G503,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_FDCS"},"LAHUYYA01_FDCS AT%M1848.0 :INT; (*空调机组YYA01-新风阀控制换算值*)","LAHUYYA01_FDCS          AT%M1848.0     :INT; (*空调机组YYA01-新风阀控制换算值*)"]
["1852.0","验证通过","REAL","空调机组","L","YYA01","回风阀反馈换算值","空调机组YYA01-回风阀反馈换算值",{"$f":"E504&VLOOKUP(D504,[2]list!$D$3:$F$501,2,FALSE)&F504&\"_\"&VLOOKUP(G504,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_RDBS"},"LAHUYYA01_RDBS AT%M1852.0 :REAL; (*空调机组YYA01-回风阀反馈换算值*)","LAHUYYA01_RDBS          AT%M1852.0     :REAL; (*空调机组YYA01-回风阀反馈换算值*)"]
["1856.0","验证通过","REAL","空调机组","L","YYA01","新风阀反馈换算值","空调机组YYA01-新风阀反馈换算值",{"$f":"E505&VLOOKUP(D505,[2]list!$D$3:$F$501,2,FALSE)&F505&\"_\"&VLOOKUP(G505,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_FDBS"},"LAHUYYA01_FDBS AT%M1856.0 :REAL; (*空调机组YYA01-新风阀反馈换算值*)","LAHUYYA01_FDBS          AT%M1856.0     :REAL; (*空调机组YYA01-新风阀反馈换算值*)"]
["1860.0","验证通过","INT","空调机组","L","YYA01","回风阀手动控制值","空调机组YYA01-回风阀手动控制值",{"$f":"E506&VLOOKUP(D506,[2]list!$D$3:$F$501,2,FALSE)&F506&\"_\"&VLOOKUP(G506,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_RDMV"},"LAHUYYA01_RDMV AT%M1860.0 :INT; (*空调机组YYA01-回风阀手动控制值*)","LAHUYYA01_RDMV          AT%M1860.0     :INT; (*空调机组YYA01-回风阀手动控制值*)"]
["1862.0","验证通过","INT","空调机组","L","YYA01","新风阀手动控制值","空调机组YYA01-新风阀手动控制值",{"$f":"E507&VLOOKUP(D507,[2]list!$D$3:$F$501,2,FALSE)&F507&\"_\"&VLOOKUP(G507,[2]list!$I$2:$K$501,2,FALSE)","v":"LAHUYYA01_FDMV"},"LAHUYYA01_FDMV AT%M1862.0 :INT; (*空调机组YYA01-新风阀手动控制值*)","LAHUYYA01_FDMV          AT%M1862.0     :INT; (*空调机组YYA01-新风阀手动控制值*)"]
["SYS"]
["1500.0",{"$f":"IF((IF(OR(C509=\"INT\",C509=\"WORD\",C509=\"BOOL\"),MOD(A509,2),MOD(A509,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"INT","系统","/","/","闪存写入次数",{"$f":"D509&\"-\"&IF(E509=\"R\",\"新云平台\"&G509,G509)","v":"系统-闪存写入次数"},"SYS_WriteNum",{"$f":"I509&\" \"&\"AT%M\"&A509&\" \"&\":\"&C509&\";\"&\" \"&\"(*\"&H509&\"*)\"","v":"SYS_WriteNum AT%M1500.0 :INT; (*系统-闪存写入次数*)"},{"$f":"REPLACE(REPLACE(J509,SEARCH(\"AT%\",J509),,REPT(\" \",25-SEARCH(\"AT%\",J509))),SEARCH(\":\",REPLACE(J509,SEARCH(\"AT%\",J509),,REPT(\" \",25-SEARCH(\"AT%\",J509)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J509,SEARCH(\"AT%\",J509),,REPT(\" \",25-SEARCH(\"AT%\",J509))))))","v":"SYS_WriteNum            AT%M1500.0     :INT; (*系统-闪存写入次数*)"}]
[{"$f":"IF(OR(C509=\"REAL\",C509=\"DWORD\",C509=\"DINT\"),(IF(OR(C510=\"REAL\",C510=\"DWORD\",C510=\"DINT\"),A509+4+MOD(A509,4),A509+4)),(IF(OR(C510=\"REAL\",C510=\"DWORD\",C510=\"DINT\"),A509+4+MOD(A509,4),A509+2)))&\".0\"","v":"1502.0"},{"$f":"IF((IF(OR(C510=\"INT\",C510=\"WORD\",C510=\"BOOL\"),MOD(A510,2),MOD(A510,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","系统","/","/","闪存写入成功标记","系统-闪存写入成功标记","SYS_Write_Flag",{"$f":"I510&\" \"&\"AT%M\"&A510&\" \"&\":\"&C510&\";\"&\" \"&\"(*\"&H510&\"*)\"","v":"SYS_Write_Flag AT%M1502.0 :BOOL; (*系统-闪存写入成功标记*)"},{"$f":"REPLACE(REPLACE(J510,SEARCH(\"AT%\",J510),,REPT(\" \",25-SEARCH(\"AT%\",J510))),SEARCH(\":\",REPLACE(J510,SEARCH(\"AT%\",J510),,REPT(\" \",25-SEARCH(\"AT%\",J510)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J510,SEARCH(\"AT%\",J510),,REPT(\" \",25-SEARCH(\"AT%\",J510))))))","v":"SYS_Write_Flag          AT%M1502.0     :BOOL; (*系统-闪存写入成功标记*)"}]
[{"$f":"IF(OR(C510=\"REAL\",C510=\"DWORD\",C510=\"DINT\"),(IF(OR(C511=\"REAL\",C511=\"DWORD\",C511=\"DINT\"),A510+4+MOD(A510,4),A510+4)),(IF(OR(C511=\"REAL\",C511=\"DWORD\",C511=\"DINT\"),A510+4+MOD(A510,4),A510+2)))&\".0\"","v":"1504.0"},"验证通过","BOOL","系统","/","/","闪存读取成功标记","系统-闪存读取成功标记","SYS_Read_Flag","SYS_Read_Flag AT%M1504.0 :BOOL; (*系统-闪存读取成功标记*)","SYS_Read_Flag           AT%M1504.0     :BOOL; (*系统-闪存读取成功标记*)"]
[{"$f":"IF(OR(C511=\"REAL\",C511=\"DWORD\",C511=\"DINT\"),(IF(OR(C512=\"REAL\",C512=\"DWORD\",C512=\"DINT\"),A511+4+MOD(A511,4),A511+4)),(IF(OR(C512=\"REAL\",C512=\"DWORD\",C512=\"DINT\"),A511+4+MOD(A511,4),A511+2)))&\".0\"","v":"1506.0"},{"$f":"IF((IF(OR(C512=\"INT\",C512=\"WORD\",C512=\"BOOL\"),MOD(A512,2),MOD(A512,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"INT","系统","/","/","变化判断变量",{"$f":"D512&\"-\"&IF(E512=\"R\",\"新云平台\"&G512,G512)","v":"系统-变化判断变量"},"SYS_Judge_Num",{"$f":"I512&\" \"&\"AT%M\"&A512&\" \"&\":\"&C512&\";\"&\" \"&\"(*\"&H512&\"*)\"","v":"SYS_Judge_Num AT%M1506.0 :INT; (*系统-变化判断变量*)"},{"$f":"REPLACE(REPLACE(J512,SEARCH(\"AT%\",J512),,REPT(\" \",25-SEARCH(\"AT%\",J512))),SEARCH(\":\",REPLACE(J512,SEARCH(\"AT%\",J512),,REPT(\" \",25-SEARCH(\"AT%\",J512)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J512,SEARCH(\"AT%\",J512),,REPT(\" \",25-SEARCH(\"AT%\",J512))))))","v":"SYS_Judge_Num           AT%M1506.0     :INT; (*系统-变化判断变量*)"}]

{"sheet":"L01","index":3,"n_rows":1507,"n_cols":11,"rows_kept":1507,"cut":false,"hidden":false,"merged":[]}
["中间变量"]
["100.0",{"$f":"IF((IF(OR(C2=\"INT\",C2=\"WORD\",C2=\"BOOL\"),MOD(A2,2),MOD(A2,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"INT","命令","L","00000","运行模式","总线程序-运行模式",{"$f":"E2&VLOOKUP(D2,list!$D$3:$F$501,2,FALSE)&F2&\"_\"&VLOOKUP(G2,list!$I$2:$K$502,2,FALSE)","v":"LCMD00000_RM"},{"$f":"I2&\" \"&\"AT%M\"&A2&\" \"&\":\"&C2&\";\"&\" \"&\"(*\"&H2&\"*)\"","v":"LCMD00000_RM AT%M100.0 :INT; (*总线程序-运行模式*)"},{"$f":"REPLACE(REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2))),SEARCH(\":\",REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2))))))","v":"LCMD00000_RM            AT%M100.0      :INT; (*总线程序-运行模式*)"}]
[{"$f":"IF(OR(C2=\"REAL\",C2=\"DWORD\",C2=\"DINT\"),(IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),A2+4+MOD(A2,4),A2+4)),(IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),A2+4+MOD(A2,4),A2+2)))&\".0\"","v":"102.0"},{"$f":"IF((IF(OR(C3=\"INT\",C3=\"WORD\",C3=\"BOOL\"),MOD(A3,2),MOD(A3,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","控制箱","L","N01","模块地址状态",{"$f":"D3&F3&\"-\"&IF(E3=\"R\",\"新云平台\"&G3,G3)","v":"控制箱N01-模块地址状态"},{"$f":"E3&VLOOKUP(D3,list!$D$3:$F$501,2,FALSE)&F3&\"_\"&VLOOKUP(G3,list!$I$2:$K$502,2,FALSE)","v":"LBOXN01_DS"},{"$f":"I3&\" \"&\"AT%M\"&A3&\" \"&\":\"&C3&\";\"&\" \"&\"(*\"&H3&\"*)\"","v":"LBOXN01_DS AT%M102.0 :BOOL; (*控制箱N01-模块地址状态*)"},"LBOXN01_DS              AT%M102.0      :BOOL; (*控制箱N01-模块地址状态*)"]
[{"$f":"IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),(IF(OR(C4=\"REAL\",C4=\"DWORD\",C4=\"DINT\"),A3+4+MOD(A3,4),A3+4)),(IF(OR(C4=\"REAL\",C4=\"DWORD\",C4=\"DINT\"),A3+4+MOD(A3,4),A3+2)))&\".0\"","v":"104.0"},"验证通过","BOOL","控制箱","L","N02","模块地址状态",{"$f":"D4&F4&\"-\"&IF(E4=\"R\",\"新云平台\"&G4,G4)","v":"控制箱N02-模块地址状态"},{"$f":"E4&VLOOKUP(D4,list!$D$3:$F$501,2,FALSE)&F4&\"_\"&VLOOKUP(G4,list!$I$2:$K$502,2,FALSE)","v":"LBOXN02_DS"},"LBOXN02_DS AT%M104.0 :BOOL; (*控制箱N02-模块地址状态*)","LBOXN02_DS              AT%M104.0      :BOOL; (*控制箱N02-模块地址状态*)"]
["106.0","验证通过","BOOL","控制箱","L","N03","模块地址状态","控制箱N03-模块地址状态",{"$f":"E5&VLOOKUP(D5,list!$D$3:$F$501,2,FALSE)&F5&\"_\"&VLOOKUP(G5,list!$I$2:$K$502,2,FALSE)","v":"LBOXN03_DS"},"LBOXN03_DS AT%M106.0 :BOOL; (*控制箱N03-模块地址状态*)","LBOXN03_DS              AT%M106.0      :BOOL; (*控制箱N03-模块地址状态*)"]
["108.0","验证通过","BOOL","控制箱","L","N04","模块地址状态","控制箱N04-模块地址状态",{"$f":"E6&VLOOKUP(D6,list!$D$3:$F$501,2,FALSE)&F6&\"_\"&VLOOKUP(G6,list!$I$2:$K$502,2,FALSE)","v":"LBOXN04_DS"},"LBOXN04_DS AT%M108.0 :BOOL; (*控制箱N04-模块地址状态*)","LBOXN04_DS              AT%M108.0      :BOOL; (*控制箱N04-模块地址状态*)"]
["110.0","验证通过","BOOL","控制箱","L","N05","模块地址状态","控制箱N05-模块地址状态",{"$f":"E7&VLOOKUP(D7,list!$D$3:$F$501,2,FALSE)&F7&\"_\"&VLOOKUP(G7,list!$I$2:$K$502,2,FALSE)","v":"LBOXN05_DS"},"LBOXN05_DS AT%M110.0 :BOOL; (*控制箱N05-模块地址状态*)","LBOXN05_DS              AT%M110.0      :BOOL; (*控制箱N05-模块地址状态*)"]
["112.0","验证通过","BOOL","控制箱","L","N06","模块地址状态","控制箱N06-模块地址状态",{"$f":"E8&VLOOKUP(D8,list!$D$3:$F$501,2,FALSE)&F8&\"_\"&VLOOKUP(G8,list!$I$2:$K$502,2,FALSE)","v":"LBOXN06_DS"},"LBOXN06_DS AT%M112.0 :BOOL; (*控制箱N06-模块地址状态*)","LBOXN06_DS              AT%M112.0      :BOOL; (*控制箱N06-模块地址状态*)"]
["114.0","验证通过","BOOL","控制箱","L","N07","模块地址状态","控制箱N07-模块地址状态",{"$f":"E9&VLOOKUP(D9,list!$D$3:$F$501,2,FALSE)&F9&\"_\"&VLOOKUP(G9,list!$I$2:$K$502,2,FALSE)","v":"LBOXN07_DS"},"LBOXN07_DS AT%M114.0 :BOOL; (*控制箱N07-模块地址状态*)","LBOXN07_DS              AT%M114.0      :BOOL; (*控制箱N07-模块地址状态*)"]
["116.0","验证通过","BOOL","控制箱","L","N08","模块地址状态","控制箱N08-模块地址状态",{"$f":"E10&VLOOKUP(D10,list!$D$3:$F$501,2,FALSE)&F10&\"_\"&VLOOKUP(G10,list!$I$2:$K$502,2,FALSE)","v":"LBOXN08_DS"},"LBOXN08_DS AT%M116.0 :BOOL; (*控制箱N08-模块地址状态*)","LBOXN08_DS              AT%M116.0      :BOOL; (*控制箱N08-模块地址状态*)"]
["118.0","验证通过","BOOL","控制箱","L","N09","模块地址状态","控制箱N09-模块地址状态",{"$f":"E11&VLOOKUP(D11,list!$D$3:$F$501,2,FALSE)&F11&\"_\"&VLOOKUP(G11,list!$I$2:$K$502,2,FALSE)","v":"LBOXN09_DS"},"LBOXN09_DS AT%M118.0 :BOOL; (*控制箱N09-模块地址状态*)","LBOXN09_DS              AT%M118.0      :BOOL; (*控制箱N09-模块地址状态*)"]
["120.0","验证通过","BOOL","控制箱","L","N10","模块地址状态","控制箱N10-模块地址状态",{"$f":"E12&VLOOKUP(D12,list!$D$3:$F$501,2,FALSE)&F12&\"_\"&VLOOKUP(G12,list!$I$2:$K$502,2,FALSE)","v":"LBOXN10_DS"},"LBOXN10_DS AT%M120.0 :BOOL; (*控制箱N10-模块地址状态*)","LBOXN10_DS              AT%M120.0      :BOOL; (*控制箱N10-模块地址状态*)"]
["124.0","验证通过","REAL","控制箱","L","N00","模块在线比例","控制箱N00-模块在线比例",{"$f":"E13&VLOOKUP(D13,list!$D$3:$F$501,2,FALSE)&F13&\"_\"&VLOOKUP(G13,list!$I$2:$K$502,2,FALSE)","v":"LBOXN00_OR"},"LBOXN00_OR AT%M124.0 :REAL; (*控制箱N00-模块在线比例*)","LBOXN00_OR              AT%M124.0      :REAL; (*控制箱N00-模块在线比例*)"]
["128.0","验证通过","REAL","控制箱","L","N01","模块在线比例","控制箱N01-模块在线比例",{"$f":"E14&VLOOKUP(D14,list!$D$3:$F$501,2,FALSE)&F14&\"_\"&VLOOKUP(G14,list!$I$2:$K$502,2,FALSE)","v":"LBOXN01_OR"},"LBOXN01_OR AT%M128.0 :REAL; (*控制箱N01-模块在线比例*)","LBOXN01_OR              AT%M128.0      :REAL; (*控制箱N01-模块在线比例*)"]
["132.0","验证通过","REAL","控制箱","L","N02","模块在线比例","控制箱N02-模块在线比例",{"$f":"E15&VLOOKUP(D15,list!$D$3:$F$501,2,FALSE)&F15&\"_\"&VLOOKUP(G15,list!$I$2:$K$502,2,FALSE)","v":"LBOXN02_OR"},"LBOXN02_OR AT%M132.0 :REAL; (*控制箱N02-模块在线比例*)","LBOXN02_OR              AT%M132.0      :REAL; (*控制箱N02-模块在线比例*)"]
["136.0","验证通过","REAL","控制箱","L","N03","模块在线比例","控制箱N03-模块在线比例",{"$f":"E16&VLOOKUP(D16,list!$D$3:$F$501,2,FALSE)&F16&\"_\"&VLOOKUP(G16,list!$I$2:$K$502,2,FALSE)","v":"LBOXN03_OR"},"LBOXN03_OR AT%M136.0 :REAL; (*控制箱N03-模块在线比例*)","LBOXN03_OR              AT%M136.0      :REAL; (*控制箱N03-模块在线比例*)"]
["140.0","验证通过","REAL","控制箱","L","N04","模块在线比例","控制箱N04-模块在线比例",{"$f":"E17&VLOOKUP(D17,list!$D$3:$F$501,2,FALSE)&F17&\"_\"&VLOOKUP(G17,list!$I$2:$K$502,2,FALSE)","v":"LBOXN04_OR"},"LBOXN04_OR AT%M140.0 :REAL; (*控制箱N04-模块在线比例*)","LBOXN04_OR              AT%M140.0      :REAL; (*控制箱N04-模块在线比例*)"]
["144.0","验证通过","REAL","控制箱","L","N05","模块在线比例","控制箱N05-模块在线比例",{"$f":"E18&VLOOKUP(D18,list!$D$3:$F$501,2,FALSE)&F18&\"_\"&VLOOKUP(G18,list!$I$2:$K$502,2,FALSE)","v":"LBOXN05_OR"},"LBOXN05_OR AT%M144.0 :REAL; (*控制箱N05-模块在线比例*)","LBOXN05_OR              AT%M144.0      :REAL; (*控制箱N05-模块在线比例*)"]
["148.0","验证通过","REAL","控制箱","L","N06","模块在线比例","控制箱N06-模块在线比例",{"$f":"E19&VLOOKUP(D19,list!$D$3:$F$501,2,FALSE)&F19&\"_\"&VLOOKUP(G19,list!$I$2:$K$502,2,FALSE)","v":"LBOXN06_OR"},"LBOXN06_OR AT%M148.0 :REAL; (*控制箱N06-模块在线比例*)","LBOXN06_OR              AT%M148.0      :REAL; (*控制箱N06-模块在线比例*)"]
["152.0","验证通过","REAL","控制箱","L","N07","模块在线比例","控制箱N07-模块在线比例",{"$f":"E20&VLOOKUP(D20,list!$D$3:$F$501,2,FALSE)&F20&\"_\"&VLOOKUP(G20,list!$I$2:$K$502,2,FALSE)","v":"LBOXN07_OR"},"LBOXN07_OR AT%M152.0 :REAL; (*控制箱N07-模块在线比例*)","LBOXN07_OR              AT%M152.0      :REAL; (*控制箱N07-模块在线比例*)"]
["156.0","验证通过","REAL","控制箱","L","N08","模块在线比例","控制箱N08-模块在线比例",{"$f":"E21&VLOOKUP(D21,list!$D$3:$F$501,2,FALSE)&F21&\"_\"&VLOOKUP(G21,list!$I$2:$K$502,2,FALSE)","v":"LBOXN08_OR"},"LBOXN08_OR AT%M156.0 :REAL; (*控制箱N08-模块在线比例*)","LBOXN08_OR              AT%M156.0      :REAL; (*控制箱N08-模块在线比例*)"]
["160.0","验证通过","REAL","控制箱","L","N09","模块在线比例","控制箱N09-模块在线比例",{"$f":"E22&VLOOKUP(D22,list!$D$3:$F$501,2,FALSE)&F22&\"_\"&VLOOKUP(G22,list!$I$2:$K$502,2,FALSE)","v":"LBOXN09_OR"},"LBOXN09_OR AT%M160.0 :REAL; (*控制箱N09-模块在线比例*)","LBOXN09_OR              AT%M160.0      :REAL; (*控制箱N09-模块在线比例*)"]
["164.0","验证通过","REAL","控制箱","L","N10","模块在线比例","控制箱N10-模块在线比例",{"$f":"E23&VLOOKUP(D23,list!$D$3:$F$501,2,FALSE)&F23&\"_\"&VLOOKUP(G23,list!$I$2:$K$502,2,FALSE)","v":"LBOXN10_OR"},"LBOXN10_OR AT%M164.0 :REAL; (*控制箱N10-模块在线比例*)","LBOXN10_OR              AT%M164.0      :REAL; (*控制箱N10-模块在线比例*)"]
["AHU"]
[{"$f":"IF(OR(C23=\"REAL\",C23=\"DWORD\",C23=\"DINT\"),(IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),A23+4+MOD(A23,4),A23+4)),(IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),A23+4+MOD(A23,4),A23+2)))&\".0\"","v":"168.0"},{"$f":"IF((IF(OR(C25=\"INT\",C25=\"WORD\",C25=\"BOOL\"),MOD(A25,2),MOD(A25,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03F01","设定温度值",{"$f":"D25&F25&\"-\"&IF(E25=\"R\",\"新云平台\"&G25,G25)","v":"空调机组03F01-新云平台设定温度值"},{"$f":"E25&VLOOKUP(D25,list!$D$3:$F$501,2,FALSE)&F25&\"_\"&VLOOKUP(G25,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F01_TSET"},{"$f":"I25&\" \"&\"AT%M\"&A25&\" \"&\":\"&C25&\";\"&\" \"&\"(*\"&H25&\"*)\"","v":"RAHU03F01_TSET AT%M168.0 :REAL; (*空调机组03F01-新云平台设定温度值*)"},"RAHU03F01_TSET          AT%M168.0      :REAL; (*空调机组03F01-新云平台设定温度值*)"]
[{"$f":"IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),(IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),A25+4+MOD(A25,4),A25+4)),(IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),A25+4+MOD(A25,4),A25+2)))&\".0\"","v":"172.0"},"验证通过","INT","空调机组","R",{"$f":"F25","v":"03F01"},"季节模式","空调机组03F01-新云平台季节模式",{"$f":"E26&VLOOKUP(D26,list!$D$3:$F$501,2,FALSE)&F26&\"_\"&VLOOKUP(G26,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F01_SM"},"RAHU03F01_SM AT%M172.0 :INT; (*空调机组03F01-新云平台季节模式*)","RAHU03F01_SM            AT%M172.0      :INT; (*空调机组03F01-新云平台季节模式*)"]
[{"$f":"IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),(IF(OR(C27=\"REAL\",C27=\"DWORD\",C27=\"DINT\"),A26+4+MOD(A26,4),A26+4)),(IF(OR(C27=\"REAL\",C27=\"DWORD\",C27=\"DINT\"),A26+4+MOD(A26,4),A26+2)))&\".0\"","v":"174.0"},"验证通过","BOOL","空调机组","R",{"$f":"F26","v":"03F01"},"程序控制","空调机组03F01-新云平台程序控制",{"$f":"E27&VLOOKUP(D27,list!$D$3:$F$501,2,FALSE)&F27&\"_\"&VLOOKUP(G27,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F01_PC"},"RAHU03F01_PC AT%M174.0 :BOOL; (*空调机组03F01-新云平台程序控制*)","RAHU03F01_PC            AT%M174.0      :BOOL; (*空调机组03F01-新云平台程序控制*)"]
["180.0","验证通过","REAL","空调机组","L","03F01","设定温度值","空调机组03F01-设定温度值",{"$f":"E28&VLOOKUP(D28,list!$D$3:$F$501,2,FALSE)&F28&\"_\"&VLOOKUP(G28,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_TSET"},"LAHU03F01_TSET AT%M180.0 :REAL; (*空调机组03F01-设定温度值*)","LAHU03F01_TSET          AT%M180.0      :REAL; (*空调机组03F01-设定温度值*)"]
["184.0","验证通过","INT","空调机组","L","03F01","季节模式","空调机组03F01-季节模式",{"$f":"E29&VLOOKUP(D29,list!$D$3:$F$501,2,FALSE)&F29&\"_\"&VLOOKUP(G29,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_SM"},"LAHU03F01_SM AT%M184.0 :INT; (*空调机组03F01-季节模式*)","LAHU03F01_SM            AT%M184.0      :INT; (*空调机组03F01-季节模式*)"]
["188.0","验证通过","REAL","空调机组","L","03F01","水阀反馈换算值","空调机组03F01-水阀反馈换算值",{"$f":"E30&VLOOKUP(D30,list!$D$3:$F$501,2,FALSE)&F30&\"_\"&VLOOKUP(G30,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_WVBS"},"LAHU03F01_WVBS AT%M188.0 :REAL; (*空调机组03F01-水阀反馈换算值*)","LAHU03F01_WVBS          AT%M188.0      :REAL; (*空调机组03F01-水阀反馈换算值*)"]
["192.0","验证通过","BOOL","空调机组","L","03F01","水阀手动控制","空调机组03F01-水阀手动控制",{"$f":"E31&VLOOKUP(D31,list!$D$3:$F$501,2,FALSE)&F31&\"_\"&VLOOKUP(G31,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_WVMC"},"LAHU03F01_WVMC AT%M192.0 :BOOL; (*空调机组03F01-水阀手动控制*)","LAHU03F01_WVMC          AT%M192.0      :BOOL; (*空调机组03F01-水阀手动控制*)"]
["196.0","验证通过","REAL","空调机组","L","03F01","水阀手动控制值","空调机组03F01-水阀手动控制值",{"$f":"E32&VLOOKUP(D32,list!$D$3:$F$501,2,FALSE)&F32&\"_\"&VLOOKUP(G32,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_WVMV"},"LAHU03F01_WVMV AT%M196.0 :REAL; (*空调机组03F01-水阀手动控制值*)","LAHU03F01_WVMV          AT%M196.0      :REAL; (*空调机组03F01-水阀手动控制值*)"]
["200.0","验证通过","REAL","空调机组","L","03F01","回风温度换算值","空调机组03F01-回风温度换算值",{"$f":"E33&VLOOKUP(D33,list!$D$3:$F$501,2,FALSE)&F33&\"_\"&VLOOKUP(G33,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_RTS"},"LAHU03F01_RTS AT%M200.0 :REAL; (*空调机组03F01-回风温度换算值*)","LAHU03F01_RTS           AT%M200.0      :REAL; (*空调机组03F01-回风温度换算值*)"]
["204.0","验证通过","BOOL","空调机组","L","03F01","运行时间累积重置","空调机组03F01-运行时间累积重置",{"$f":"E34&VLOOKUP(D34,list!$D$3:$F$501,2,FALSE)&F34&\"_\"&VLOOKUP(G34,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_RST"},"LAHU03F01_RST AT%M204.0 :BOOL; (*空调机组03F01-运行时间累积重置*)","LAHU03F01_RST           AT%M204.0      :BOOL; (*空调机组03F01-运行时间累积重置*)"]
["208.0","验证通过","REAL","空调机组","L","03F01","运行时间累积重置值","空调机组03F01-运行时间累积重置值",{"$f":"E35&VLOOKUP(D35,list!$D$3:$F$501,2,FALSE)&F35&\"_\"&VLOOKUP(G35,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_RSTV"},"LAHU03F01_RSTV AT%M208.0 :REAL; (*空调机组03F01-运行时间累积重置值*)","LAHU03F01_RSTV          AT%M208.0      :REAL; (*空调机组03F01-运行时间累积重置值*)"]
["212.0","验证通过","BOOL","空调机组","L","03F01","隔离开关1","空调机组03F01-隔离开关1",{"$f":"E36&VLOOKUP(D36,list!$D$3:$F$501,2,FALSE)&F36&\"_\"&VLOOKUP(G36,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_ISO1"},"LAHU03F01_ISO1 AT%M212.0 :BOOL; (*空调机组03F01-隔离开关1*)","LAHU03F01_ISO1          AT%M212.0      :BOOL; (*空调机组03F01-隔离开关1*)"]
["214.0","验证通过","BOOL","空调机组","L","03F01","隔离开关2","空调机组03F01-隔离开关2",{"$f":"E37&VLOOKUP(D37,list!$D$3:$F$501,2,FALSE)&F37&\"_\"&VLOOKUP(G37,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_ISO2"},"LAHU03F01_ISO2 AT%M214.0 :BOOL; (*空调机组03F01-隔离开关2*)","LAHU03F01_ISO2          AT%M214.0      :BOOL; (*空调机组03F01-隔离开关2*)"]
["220.0","验证通过","REAL","空调机组","L","03F01","P调节参数","空调机组03F01-P调节参数",{"$f":"E38&VLOOKUP(D38,list!$D$3:$F$501,2,FALSE)&F38&\"_\"&VLOOKUP(G38,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_VP"},"LAHU03F01_VP AT%M220.0 :REAL; (*空调机组03F01-P调节参数*)","LAHU03F01_VP            AT%M220.0      :REAL; (*空调机组03F01-P调节参数*)"]
["224.0","验证通过","REAL","空调机组","L","03F01","I调节参数","空调机组03F01-I调节参数",{"$f":"E39&VLOOKUP(D39,list!$D$3:$F$501,2,FALSE)&F39&\"_\"&VLOOKUP(G39,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_VI"},"LAHU03F01_VI AT%M224.0 :REAL; (*空调机组03F01-I调节参数*)","LAHU03F01_VI            AT%M224.0      :REAL; (*空调机组03F01-I调节参数*)"]
["228.0","验证通过","REAL","空调机组","L","03F01","运行时间累积值","空调机组03F01-运行时间累积值",{"$f":"E40&VLOOKUP(D40,list!$D$3:$F$501,2,FALSE)&F40&\"_\"&VLOOKUP(G40,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_RH"},"LAHU03F01_RH AT%M228.0 :REAL; (*空调机组03F01-运行时间累积值*)","LAHU03F01_RH            AT%M228.0      :REAL; (*空调机组03F01-运行时间累积值*)"]
["232.0","验证通过","INT","空调机组","L","03F01","设备状态代码","空调机组03F01-设备状态代码",{"$f":"E41&VLOOKUP(D41,list!$D$3:$F$501,2,FALSE)&F41&\"_\"&VLOOKUP(G41,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_SN"},"LAHU03F01_SN AT%M232.0 :INT; (*空调机组03F01-设备状态代码*)","LAHU03F01_SN            AT%M232.0      :INT; (*空调机组03F01-设备状态代码*)"]
["234.0","验证通过","INT","空调机组","L","03F01","水阀控制转换值","空调机组03F01-水阀控制转换值",{"$f":"E42&VLOOKUP(D42,list!$D$3:$F$501,2,FALSE)&F42&\"_\"&VLOOKUP(G42,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_WVCS"},"LAHU03F01_WVCS AT%M234.0 :INT; (*空调机组03F01-水阀控制转换值*)","LAHU03F01_WVCS          AT%M234.0      :INT; (*空调机组03F01-水阀控制转换值*)"]
["236.0","验证通过","BOOL","空调机组","L","03F01","程序控制","空调机组03F01-程序控制",{"$f":"E43&VLOOKUP(D43,list!$D$3:$F$501,2,FALSE)&F43&\"_\"&VLOOKUP(G43,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F01_PC"},"LAHU03F01_PC AT%M236.0 :BOOL; (*空调机组03F01-程序控制*)","LAHU03F01_PC            AT%M236.0      :BOOL; (*空调机组03F01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C43=\"REAL\",C43=\"DWORD\",C43=\"DINT\"),(IF(OR(C45=\"REAL\",C45=\"DWORD\",C45=\"DINT\"),A43+4+MOD(A43,4),A43+4)),(IF(OR(C45=\"REAL\",C45=\"DWORD\",C45=\"DINT\"),A43+4+MOD(A43,4),A43+2)))&\".0\"","v":"240.0"},{"$f":"IF((IF(OR(C45=\"INT\",C45=\"WORD\",C45=\"BOOL\"),MOD(A45,2),MOD(A45,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03F02","设定温度值",{"$f":"D45&F45&\"-\"&IF(E45=\"R\",\"新云平台\"&G45,G45)","v":"空调机组03F02-新云平台设定温度值"},{"$f":"E45&VLOOKUP(D45,list!$D$3:$F$501,2,FALSE)&F45&\"_\"&VLOOKUP(G45,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F02_TSET"},{"$f":"I45&\" \"&\"AT%M\"&A45&\" \"&\":\"&C45&\";\"&\" \"&\"(*\"&H45&\"*)\"","v":"RAHU03F02_TSET AT%M240.0 :REAL; (*空调机组03F02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J45,SEARCH(\"AT%\",J45),,REPT(\" \",25-SEARCH(\"AT%\",J45))),SEARCH(\":\",REPLACE(J45,SEARCH(\"AT%\",J45),,REPT(\" \",25-SEARCH(\"AT%\",J45)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J45,SEARCH(\"AT%\",J45),,REPT(\" \",25-SEARCH(\"AT%\",J45))))))","v":"RAHU03F02_TSET          AT%M240.0      :REAL; (*空调机组03F02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C45=\"REAL\",C45=\"DWORD\",C45=\"DINT\"),(IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),A45+4+MOD(A45,4),A45+4)),(IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),A45+4+MOD(A45,4),A45+2)))&\".0\"","v":"244.0"},"验证通过","INT","空调机组","R",{"$f":"F45","v":"03F02"},"季节模式","空调机组03F02-新云平台季节模式",{"$f":"E46&VLOOKUP(D46,list!$D$3:$F$501,2,FALSE)&F46&\"_\"&VLOOKUP(G46,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F02_SM"},"RAHU03F02_SM AT%M244.0 :INT; (*空调机组03F02-新云平台季节模式*)","RAHU03F02_SM            AT%M244.0      :INT; (*空调机组03F02-新云平台季节模式*)"]
[{"$f":"IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),(IF(OR(C47=\"REAL\",C47=\"DWORD\",C47=\"DINT\"),A46+4+MOD(A46,4),A46+4)),(IF(OR(C47=\"REAL\",C47=\"DWORD\",C47=\"DINT\"),A46+4+MOD(A46,4),A46+2)))&\".0\"","v":"246.0"},"验证通过","BOOL","空调机组","R",{"$f":"F46","v":"03F02"},"程序控制","空调机组03F02-新云平台程序控制",{"$f":"E47&VLOOKUP(D47,list!$D$3:$F$501,2,FALSE)&F47&\"_\"&VLOOKUP(G47,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F02_PC"},"RAHU03F02_PC AT%M246.0 :BOOL; (*空调机组03F02-新云平台程序控制*)","RAHU03F02_PC            AT%M246.0      :BOOL; (*空调机组03F02-新云平台程序控制*)"]
["252.0","验证通过","REAL","空调机组","L","03F02","设定温度值","空调机组03F02-设定温度值",{"$f":"E48&VLOOKUP(D48,list!$D$3:$F$501,2,FALSE)&F48&\"_\"&VLOOKUP(G48,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_TSET"},"LAHU03F02_TSET AT%M252.0 :REAL; (*空调机组03F02-设定温度值*)","LAHU03F02_TSET          AT%M252.0      :REAL; (*空调机组03F02-设定温度值*)"]
["256.0","验证通过","INT","空调机组","L","03F02","季节模式","空调机组03F02-季节模式",{"$f":"E49&VLOOKUP(D49,list!$D$3:$F$501,2,FALSE)&F49&\"_\"&VLOOKUP(G49,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_SM"},"LAHU03F02_SM AT%M256.0 :INT; (*空调机组03F02-季节模式*)","LAHU03F02_SM            AT%M256.0      :INT; (*空调机组03F02-季节模式*)"]
["260.0","验证通过","REAL","空调机组","L","03F02","水阀反馈换算值","空调机组03F02-水阀反馈换算值",{"$f":"E50&VLOOKUP(D50,list!$D$3:$F$501,2,FALSE)&F50&\"_\"&VLOOKUP(G50,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_WVBS"},"LAHU03F02_WVBS AT%M260.0 :REAL; (*空调机组03F02-水阀反馈换算值*)","LAHU03F02_WVBS          AT%M260.0      :REAL; (*空调机组03F02-水阀反馈换算值*)"]
["264.0","验证通过","BOOL","空调机组","L","03F02","水阀手动控制","空调机组03F02-水阀手动控制",{"$f":"E51&VLOOKUP(D51,list!$D$3:$F$501,2,FALSE)&F51&\"_\"&VLOOKUP(G51,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_WVMC"},"LAHU03F02_WVMC AT%M264.0 :BOOL; (*空调机组03F02-水阀手动控制*)","LAHU03F02_WVMC          AT%M264.0      :BOOL; (*空调机组03F02-水阀手动控制*)"]
["268.0","验证通过","REAL","空调机组","L","03F02","水阀手动控制值","空调机组03F02-水阀手动控制值",{"$f":"E52&VLOOKUP(D52,list!$D$3:$F$501,2,FALSE)&F52&\"_\"&VLOOKUP(G52,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_WVMV"},"LAHU03F02_WVMV AT%M268.0 :REAL; (*空调机组03F02-水阀手动控制值*)","LAHU03F02_WVMV          AT%M268.0      :REAL; (*空调机组03F02-水阀手动控制值*)"]
["272.0","验证通过","REAL","空调机组","L","03F02","回风温度换算值","空调机组03F02-回风温度换算值",{"$f":"E53&VLOOKUP(D53,list!$D$3:$F$501,2,FALSE)&F53&\"_\"&VLOOKUP(G53,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_RTS"},"LAHU03F02_RTS AT%M272.0 :REAL; (*空调机组03F02-回风温度换算值*)","LAHU03F02_RTS           AT%M272.0      :REAL; (*空调机组03F02-回风温度换算值*)"]
["276.0","验证通过","BOOL","空调机组","L","03F02","运行时间累积重置","空调机组03F02-运行时间累积重置",{"$f":"E54&VLOOKUP(D54,list!$D$3:$F$501,2,FALSE)&F54&\"_\"&VLOOKUP(G54,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_RST"},"LAHU03F02_RST AT%M276.0 :BOOL; (*空调机组03F02-运行时间累积重置*)","LAHU03F02_RST           AT%M276.0      :BOOL; (*空调机组03F02-运行时间累积重置*)"]
["280.0","验证通过","REAL","空调机组","L","03F02","运行时间累积重置值","空调机组03F02-运行时间累积重置值",{"$f":"E55&VLOOKUP(D55,list!$D$3:$F$501,2,FALSE)&F55&\"_\"&VLOOKUP(G55,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_RSTV"},"LAHU03F02_RSTV AT%M280.0 :REAL; (*空调机组03F02-运行时间累积重置值*)","LAHU03F02_RSTV          AT%M280.0      :REAL; (*空调机组03F02-运行时间累积重置值*)"]
["284.0","验证通过","BOOL","空调机组","L","03F02","隔离开关1","空调机组03F02-隔离开关1",{"$f":"E56&VLOOKUP(D56,list!$D$3:$F$501,2,FALSE)&F56&\"_\"&VLOOKUP(G56,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_ISO1"},"LAHU03F02_ISO1 AT%M284.0 :BOOL; (*空调机组03F02-隔离开关1*)","LAHU03F02_ISO1          AT%M284.0      :BOOL; (*空调机组03F02-隔离开关1*)"]
["286.0","验证通过","BOOL","空调机组","L","03F02","隔离开关2","空调机组03F02-隔离开关2",{"$f":"E57&VLOOKUP(D57,list!$D$3:$F$501,2,FALSE)&F57&\"_\"&VLOOKUP(G57,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_ISO2"},"LAHU03F02_ISO2 AT%M286.0 :BOOL; (*空调机组03F02-隔离开关2*)","LAHU03F02_ISO2          AT%M286.0      :BOOL; (*空调机组03F02-隔离开关2*)"]
["292.0","验证通过","REAL","空调机组","L","03F02","P调节参数","空调机组03F02-P调节参数",{"$f":"E58&VLOOKUP(D58,list!$D$3:$F$501,2,FALSE)&F58&\"_\"&VLOOKUP(G58,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_VP"},"LAHU03F02_VP AT%M292.0 :REAL; (*空调机组03F02-P调节参数*)","LAHU03F02_VP            AT%M292.0      :REAL; (*空调机组03F02-P调节参数*)"]
["296.0","验证通过","REAL","空调机组","L","03F02","I调节参数","空调机组03F02-I调节参数",{"$f":"E59&VLOOKUP(D59,list!$D$3:$F$501,2,FALSE)&F59&\"_\"&VLOOKUP(G59,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_VI"},"LAHU03F02_VI AT%M296.0 :REAL; (*空调机组03F02-I调节参数*)","LAHU03F02_VI            AT%M296.0      :REAL; (*空调机组03F02-I调节参数*)"]
["300.0","验证通过","REAL","空调机组","L","03F02","运行时间累积值","空调机组03F02-运行时间累积值",{"$f":"E60&VLOOKUP(D60,list!$D$3:$F$501,2,FALSE)&F60&\"_\"&VLOOKUP(G60,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_RH"},"LAHU03F02_RH AT%M300.0 :REAL; (*空调机组03F02-运行时间累积值*)","LAHU03F02_RH            AT%M300.0      :REAL; (*空调机组03F02-运行时间累积值*)"]
["304.0","验证通过","INT","空调机组","L","03F02","设备状态代码","空调机组03F02-设备状态代码",{"$f":"E61&VLOOKUP(D61,list!$D$3:$F$501,2,FALSE)&F61&\"_\"&VLOOKUP(G61,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_SN"},"LAHU03F02_SN AT%M304.0 :INT; (*空调机组03F02-设备状态代码*)","LAHU03F02_SN            AT%M304.0      :INT; (*空调机组03F02-设备状态代码*)"]
["306.0","验证通过","INT","空调机组","L","03F02","水阀控制转换值","空调机组03F02-水阀控制转换值",{"$f":"E62&VLOOKUP(D62,list!$D$3:$F$501,2,FALSE)&F62&\"_\"&VLOOKUP(G62,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_WVCS"},"LAHU03F02_WVCS AT%M306.0 :INT; (*空调机组03F02-水阀控制转换值*)","LAHU03F02_WVCS          AT%M306.0      :INT; (*空调机组03F02-水阀控制转换值*)"]
["308.0","验证通过","BOOL","空调机组","L","03F02","程序控制","空调机组03F02-程序控制",{"$f":"E63&VLOOKUP(D63,list!$D$3:$F$501,2,FALSE)&F63&\"_\"&VLOOKUP(G63,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F02_PC"},"LAHU03F02_PC AT%M308.0 :BOOL; (*空调机组03F02-程序控制*)","LAHU03F02_PC            AT%M308.0      :BOOL; (*空调机组03F02-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C63=\"REAL\",C63=\"DWORD\",C63=\"DINT\"),(IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),A63+4+MOD(A63,4),A63+4)),(IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),A63+4+MOD(A63,4),A63+2)))&\".0\"","v":"312.0"},{"$f":"IF((IF(OR(C65=\"INT\",C65=\"WORD\",C65=\"BOOL\"),MOD(A65,2),MOD(A65,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03F03","设定温度值",{"$f":"D65&F65&\"-\"&IF(E65=\"R\",\"新云平台\"&G65,G65)","v":"空调机组03F03-新云平台设定温度值"},{"$f":"E65&VLOOKUP(D65,list!$D$3:$F$501,2,FALSE)&F65&\"_\"&VLOOKUP(G65,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F03_TSET"},{"$f":"I65&\" \"&\"AT%M\"&A65&\" \"&\":\"&C65&\";\"&\" \"&\"(*\"&H65&\"*)\"","v":"RAHU03F03_TSET AT%M312.0 :REAL; (*空调机组03F03-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J65,SEARCH(\"AT%\",J65),,REPT(\" \",25-SEARCH(\"AT%\",J65))),SEARCH(\":\",REPLACE(J65,SEARCH(\"AT%\",J65),,REPT(\" \",25-SEARCH(\"AT%\",J65)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J65,SEARCH(\"AT%\",J65),,REPT(\" \",25-SEARCH(\"AT%\",J65))))))","v":"RAHU03F03_TSET          AT%M312.0      :REAL; (*空调机组03F03-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),(IF(OR(C66=\"REAL\",C66=\"DWORD\",C66=\"DINT\"),A65+4+MOD(A65,4),A65+4)),(IF(OR(C66=\"REAL\",C66=\"DWORD\",C66=\"DINT\"),A65+4+MOD(A65,4),A65+2)))&\".0\"","v":"316.0"},"验证通过","INT","空调机组","R",{"$f":"F65","v":"03F03"},"季节模式","空调机组03F03-新云平台季节模式",{"$f":"E66&VLOOKUP(D66,list!$D$3:$F$501,2,FALSE)&F66&\"_\"&VLOOKUP(G66,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F03_SM"},"RAHU03F03_SM AT%M316.0 :INT; (*空调机组03F03-新云平台季节模式*)","RAHU03F03_SM            AT%M316.0      :INT; (*空调机组03F03-新云平台季节模式*)"]
[{"$f":"IF(OR(C66=\"REAL\",C66=\"DWORD\",C66=\"DINT\"),(IF(OR(C67=\"REAL\",C67=\"DWORD\",C67=\"DINT\"),A66+4+MOD(A66,4),A66+4)),(IF(OR(C67=\"REAL\",C67=\"DWORD\",C67=\"DINT\"),A66+4+MOD(A66,4),A66+2)))&\".0\"","v":"318.0"},"验证通过","BOOL","空调机组","R",{"$f":"F66","v":"03F03"},"程序控制","空调机组03F03-新云平台程序控制",{"$f":"E67&VLOOKUP(D67,list!$D$3:$F$501,2,FALSE)&F67&\"_\"&VLOOKUP(G67,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F03_PC"},"RAHU03F03_PC AT%M318.0 :BOOL; (*空调机组03F03-新云平台程序控制*)","RAHU03F03_PC            AT%M318.0      :BOOL; (*空调机组03F03-新云平台程序控制*)"]
["324.0","验证通过","REAL","空调机组","L","03F03","设定温度值","空调机组03F03-设定温度值",{"$f":"E68&VLOOKUP(D68,list!$D$3:$F$501,2,FALSE)&F68&\"_\"&VLOOKUP(G68,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_TSET"},"LAHU03F03_TSET AT%M324.0 :REAL; (*空调机组03F03-设定温度值*)","LAHU03F03_TSET          AT%M324.0      :REAL; (*空调机组03F03-设定温度值*)"]
["328.0","验证通过","INT","空调机组","L","03F03","季节模式","空调机组03F03-季节模式",{"$f":"E69&VLOOKUP(D69,list!$D$3:$F$501,2,FALSE)&F69&\"_\"&VLOOKUP(G69,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_SM"},"LAHU03F03_SM AT%M328.0 :INT; (*空调机组03F03-季节模式*)","LAHU03F03_SM            AT%M328.0      :INT; (*空调机组03F03-季节模式*)"]
["332.0","验证通过","REAL","空调机组","L","03F03","水阀反馈换算值","空调机组03F03-水阀反馈换算值",{"$f":"E70&VLOOKUP(D70,list!$D$3:$F$501,2,FALSE)&F70&\"_\"&VLOOKUP(G70,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_WVBS"},"LAHU03F03_WVBS AT%M332.0 :REAL; (*空调机组03F03-水阀反馈换算值*)","LAHU03F03_WVBS          AT%M332.0      :REAL; (*空调机组03F03-水阀反馈换算值*)"]
["336.0","验证通过","BOOL","空调机组","L","03F03","水阀手动控制","空调机组03F03-水阀手动控制",{"$f":"E71&VLOOKUP(D71,list!$D$3:$F$501,2,FALSE)&F71&\"_\"&VLOOKUP(G71,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_WVMC"},"LAHU03F03_WVMC AT%M336.0 :BOOL; (*空调机组03F03-水阀手动控制*)","LAHU03F03_WVMC          AT%M336.0      :BOOL; (*空调机组03F03-水阀手动控制*)"]
["340.0","验证通过","REAL","空调机组","L","03F03","水阀手动控制值","空调机组03F03-水阀手动控制值",{"$f":"E72&VLOOKUP(D72,list!$D$3:$F$501,2,FALSE)&F72&\"_\"&VLOOKUP(G72,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_WVMV"},"LAHU03F03_WVMV AT%M340.0 :REAL; (*空调机组03F03-水阀手动控制值*)","LAHU03F03_WVMV          AT%M340.0      :REAL; (*空调机组03F03-水阀手动控制值*)"]
["344.0","验证通过","REAL","空调机组","L","03F03","回风温度换算值","空调机组03F03-回风温度换算值",{"$f":"E73&VLOOKUP(D73,list!$D$3:$F$501,2,FALSE)&F73&\"_\"&VLOOKUP(G73,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_RTS"},"LAHU03F03_RTS AT%M344.0 :REAL; (*空调机组03F03-回风温度换算值*)","LAHU03F03_RTS           AT%M344.0      :REAL; (*空调机组03F03-回风温度换算值*)"]
["348.0","验证通过","BOOL","空调机组","L","03F03","运行时间累积重置","空调机组03F03-运行时间累积重置",{"$f":"E74&VLOOKUP(D74,list!$D$3:$F$501,2,FALSE)&F74&\"_\"&VLOOKUP(G74,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_RST"},"LAHU03F03_RST AT%M348.0 :BOOL; (*空调机组03F03-运行时间累积重置*)","LAHU03F03_RST           AT%M348.0      :BOOL; (*空调机组03F03-运行时间累积重置*)"]
["352.0","验证通过","REAL","空调机组","L","03F03","运行时间累积重置值","空调机组03F03-运行时间累积重置值",{"$f":"E75&VLOOKUP(D75,list!$D$3:$F$501,2,FALSE)&F75&\"_\"&VLOOKUP(G75,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_RSTV"},"LAHU03F03_RSTV AT%M352.0 :REAL; (*空调机组03F03-运行时间累积重置值*)","LAHU03F03_RSTV          AT%M352.0      :REAL; (*空调机组03F03-运行时间累积重置值*)"]
["356.0","验证通过","BOOL","空调机组","L","03F03","隔离开关1","空调机组03F03-隔离开关1",{"$f":"E76&VLOOKUP(D76,list!$D$3:$F$501,2,FALSE)&F76&\"_\"&VLOOKUP(G76,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_ISO1"},"LAHU03F03_ISO1 AT%M356.0 :BOOL; (*空调机组03F03-隔离开关1*)","LAHU03F03_ISO1          AT%M356.0      :BOOL; (*空调机组03F03-隔离开关1*)"]
["358.0","验证通过","BOOL","空调机组","L","03F03","隔离开关2","空调机组03F03-隔离开关2",{"$f":"E77&VLOOKUP(D77,list!$D$3:$F$501,2,FALSE)&F77&\"_\"&VLOOKUP(G77,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_ISO2"},"LAHU03F03_ISO2 AT%M358.0 :BOOL; (*空调机组03F03-隔离开关2*)","LAHU03F03_ISO2          AT%M358.0      :BOOL; (*空调机组03F03-隔离开关2*)"]
["364.0","验证通过","REAL","空调机组","L","03F03","P调节参数","空调机组03F03-P调节参数",{"$f":"E78&VLOOKUP(D78,list!$D$3:$F$501,2,FALSE)&F78&\"_\"&VLOOKUP(G78,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_VP"},"LAHU03F03_VP AT%M364.0 :REAL; (*空调机组03F03-P调节参数*)","LAHU03F03_VP            AT%M364.0      :REAL; (*空调机组03F03-P调节参数*)"]
["368.0","验证通过","REAL","空调机组","L","03F03","I调节参数","空调机组03F03-I调节参数",{"$f":"E79&VLOOKUP(D79,list!$D$3:$F$501,2,FALSE)&F79&\"_\"&VLOOKUP(G79,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_VI"},"LAHU03F03_VI AT%M368.0 :REAL; (*空调机组03F03-I调节参数*)","LAHU03F03_VI            AT%M368.0      :REAL; (*空调机组03F03-I调节参数*)"]
["372.0","验证通过","REAL","空调机组","L","03F03","运行时间累积值","空调机组03F03-运行时间累积值",{"$f":"E80&VLOOKUP(D80,list!$D$3:$F$501,2,FALSE)&F80&\"_\"&VLOOKUP(G80,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_RH"},"LAHU03F03_RH AT%M372.0 :REAL; (*空调机组03F03-运行时间累积值*)","LAHU03F03_RH            AT%M372.0      :REAL; (*空调机组03F03-运行时间累积值*)"]
["376.0","验证通过","INT","空调机组","L","03F03","设备状态代码","空调机组03F03-设备状态代码",{"$f":"E81&VLOOKUP(D81,list!$D$3:$F$501,2,FALSE)&F81&\"_\"&VLOOKUP(G81,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_SN"},"LAHU03F03_SN AT%M376.0 :INT; (*空调机组03F03-设备状态代码*)","LAHU03F03_SN            AT%M376.0      :INT; (*空调机组03F03-设备状态代码*)"]
["378.0","验证通过","INT","空调机组","L","03F03","水阀控制转换值","空调机组03F03-水阀控制转换值",{"$f":"E82&VLOOKUP(D82,list!$D$3:$F$501,2,FALSE)&F82&\"_\"&VLOOKUP(G82,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_WVCS"},"LAHU03F03_WVCS AT%M378.0 :INT; (*空调机组03F03-水阀控制转换值*)","LAHU03F03_WVCS          AT%M378.0      :INT; (*空调机组03F03-水阀控制转换值*)"]
["380.0","验证通过","BOOL","空调机组","L","03F03","程序控制","空调机组03F03-程序控制",{"$f":"E83&VLOOKUP(D83,list!$D$3:$F$501,2,FALSE)&F83&\"_\"&VLOOKUP(G83,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F03_PC"},"LAHU03F03_PC AT%M380.0 :BOOL; (*空调机组03F03-程序控制*)","LAHU03F03_PC            AT%M380.0      :BOOL; (*空调机组03F03-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C83=\"REAL\",C83=\"DWORD\",C83=\"DINT\"),(IF(OR(C85=\"REAL\",C85=\"DWORD\",C85=\"DINT\"),A83+4+MOD(A83,4),A83+4)),(IF(OR(C85=\"REAL\",C85=\"DWORD\",C85=\"DINT\"),A83+4+MOD(A83,4),A83+2)))&\".0\"","v":"384.0"},{"$f":"IF((IF(OR(C85=\"INT\",C85=\"WORD\",C85=\"BOOL\"),MOD(A85,2),MOD(A85,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03F04","设定温度值",{"$f":"D85&F85&\"-\"&IF(E85=\"R\",\"新云平台\"&G85,G85)","v":"空调机组03F04-新云平台设定温度值"},{"$f":"E85&VLOOKUP(D85,list!$D$3:$F$501,2,FALSE)&F85&\"_\"&VLOOKUP(G85,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F04_TSET"},{"$f":"I85&\" \"&\"AT%M\"&A85&\" \"&\":\"&C85&\";\"&\" \"&\"(*\"&H85&\"*)\"","v":"RAHU03F04_TSET AT%M384.0 :REAL; (*空调机组03F04-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J85,SEARCH(\"AT%\",J85),,REPT(\" \",25-SEARCH(\"AT%\",J85))),SEARCH(\":\",REPLACE(J85,SEARCH(\"AT%\",J85),,REPT(\" \",25-SEARCH(\"AT%\",J85)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J85,SEARCH(\"AT%\",J85),,REPT(\" \",25-SEARCH(\"AT%\",J85))))))","v":"RAHU03F04_TSET          AT%M384.0      :REAL; (*空调机组03F04-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C85=\"REAL\",C85=\"DWORD\",C85=\"DINT\"),(IF(OR(C86=\"REAL\",C86=\"DWORD\",C86=\"DINT\"),A85+4+MOD(A85,4),A85+4)),(IF(OR(C86=\"REAL\",C86=\"DWORD\",C86=\"DINT\"),A85+4+MOD(A85,4),A85+2)))&\".0\"","v":"388.0"},"验证通过","INT","空调机组","R",{"$f":"F85","v":"03F04"},"季节模式","空调机组03F04-新云平台季节模式",{"$f":"E86&VLOOKUP(D86,list!$D$3:$F$501,2,FALSE)&F86&\"_\"&VLOOKUP(G86,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F04_SM"},"RAHU03F04_SM AT%M388.0 :INT; (*空调机组03F04-新云平台季节模式*)","RAHU03F04_SM            AT%M388.0      :INT; (*空调机组03F04-新云平台季节模式*)"]
[{"$f":"IF(OR(C86=\"REAL\",C86=\"DWORD\",C86=\"DINT\"),(IF(OR(C87=\"REAL\",C87=\"DWORD\",C87=\"DINT\"),A86+4+MOD(A86,4),A86+4)),(IF(OR(C87=\"REAL\",C87=\"DWORD\",C87=\"DINT\"),A86+4+MOD(A86,4),A86+2)))&\".0\"","v":"390.0"},"验证通过","BOOL","空调机组","R",{"$f":"F86","v":"03F04"},"程序控制","空调机组03F04-新云平台程序控制",{"$f":"E87&VLOOKUP(D87,list!$D$3:$F$501,2,FALSE)&F87&\"_\"&VLOOKUP(G87,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F04_PC"},"RAHU03F04_PC AT%M390.0 :BOOL; (*空调机组03F04-新云平台程序控制*)","RAHU03F04_PC            AT%M390.0      :BOOL; (*空调机组03F04-新云平台程序控制*)"]
["396.0","验证通过","REAL","空调机组","L","03F04","设定温度值","空调机组03F04-设定温度值",{"$f":"E88&VLOOKUP(D88,list!$D$3:$F$501,2,FALSE)&F88&\"_\"&VLOOKUP(G88,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_TSET"},"LAHU03F04_TSET AT%M396.0 :REAL; (*空调机组03F04-设定温度值*)","LAHU03F04_TSET          AT%M396.0      :REAL; (*空调机组03F04-设定温度值*)"]
["400.0","验证通过","INT","空调机组","L","03F04","季节模式","空调机组03F04-季节模式",{"$f":"E89&VLOOKUP(D89,list!$D$3:$F$501,2,FALSE)&F89&\"_\"&VLOOKUP(G89,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_SM"},"LAHU03F04_SM AT%M400.0 :INT; (*空调机组03F04-季节模式*)","LAHU03F04_SM            AT%M400.0      :INT; (*空调机组03F04-季节模式*)"]
["404.0","验证通过","REAL","空调机组","L","03F04","水阀反馈换算值","空调机组03F04-水阀反馈换算值",{"$f":"E90&VLOOKUP(D90,list!$D$3:$F$501,2,FALSE)&F90&\"_\"&VLOOKUP(G90,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_WVBS"},"LAHU03F04_WVBS AT%M404.0 :REAL; (*空调机组03F04-水阀反馈换算值*)","LAHU03F04_WVBS          AT%M404.0      :REAL; (*空调机组03F04-水阀反馈换算值*)"]
["408.0","验证通过","BOOL","空调机组","L","03F04","水阀手动控制","空调机组03F04-水阀手动控制",{"$f":"E91&VLOOKUP(D91,list!$D$3:$F$501,2,FALSE)&F91&\"_\"&VLOOKUP(G91,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_WVMC"},"LAHU03F04_WVMC AT%M408.0 :BOOL; (*空调机组03F04-水阀手动控制*)","LAHU03F04_WVMC          AT%M408.0      :BOOL; (*空调机组03F04-水阀手动控制*)"]
["412.0","验证通过","REAL","空调机组","L","03F04","水阀手动控制值","空调机组03F04-水阀手动控制值",{"$f":"E92&VLOOKUP(D92,list!$D$3:$F$501,2,FALSE)&F92&\"_\"&VLOOKUP(G92,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_WVMV"},"LAHU03F04_WVMV AT%M412.0 :REAL; (*空调机组03F04-水阀手动控制值*)","LAHU03F04_WVMV          AT%M412.0      :REAL; (*空调机组03F04-水阀手动控制值*)"]
["416.0","验证通过","REAL","空调机组","L","03F04","回风温度换算值","空调机组03F04-回风温度换算值",{"$f":"E93&VLOOKUP(D93,list!$D$3:$F$501,2,FALSE)&F93&\"_\"&VLOOKUP(G93,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_RTS"},"LAHU03F04_RTS AT%M416.0 :REAL; (*空调机组03F04-回风温度换算值*)","LAHU03F04_RTS           AT%M416.0      :REAL; (*空调机组03F04-回风温度换算值*)"]
["420.0","验证通过","BOOL","空调机组","L","03F04","运行时间累积重置","空调机组03F04-运行时间累积重置",{"$f":"E94&VLOOKUP(D94,list!$D$3:$F$501,2,FALSE)&F94&\"_\"&VLOOKUP(G94,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_RST"},"LAHU03F04_RST AT%M420.0 :BOOL; (*空调机组03F04-运行时间累积重置*)","LAHU03F04_RST           AT%M420.0      :BOOL; (*空调机组03F04-运行时间累积重置*)"]
["424.0","验证通过","REAL","空调机组","L","03F04","运行时间累积重置值","空调机组03F04-运行时间累积重置值",{"$f":"E95&VLOOKUP(D95,list!$D$3:$F$501,2,FALSE)&F95&\"_\"&VLOOKUP(G95,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_RSTV"},"LAHU03F04_RSTV AT%M424.0 :REAL; (*空调机组03F04-运行时间累积重置值*)","LAHU03F04_RSTV          AT%M424.0      :REAL; (*空调机组03F04-运行时间累积重置值*)"]
["428.0","验证通过","BOOL","空调机组","L","03F04","隔离开关1","空调机组03F04-隔离开关1",{"$f":"E96&VLOOKUP(D96,list!$D$3:$F$501,2,FALSE)&F96&\"_\"&VLOOKUP(G96,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_ISO1"},"LAHU03F04_ISO1 AT%M428.0 :BOOL; (*空调机组03F04-隔离开关1*)","LAHU03F04_ISO1          AT%M428.0      :BOOL; (*空调机组03F04-隔离开关1*)"]
["430.0","验证通过","BOOL","空调机组","L","03F04","隔离开关2","空调机组03F04-隔离开关2",{"$f":"E97&VLOOKUP(D97,list!$D$3:$F$501,2,FALSE)&F97&\"_\"&VLOOKUP(G97,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_ISO2"},"LAHU03F04_ISO2 AT%M430.0 :BOOL; (*空调机组03F04-隔离开关2*)","LAHU03F04_ISO2          AT%M430.0      :BOOL; (*空调机组03F04-隔离开关2*)"]
["436.0","验证通过","REAL","空调机组","L","03F04","P调节参数","空调机组03F04-P调节参数",{"$f":"E98&VLOOKUP(D98,list!$D$3:$F$501,2,FALSE)&F98&\"_\"&VLOOKUP(G98,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_VP"},"LAHU03F04_VP AT%M436.0 :REAL; (*空调机组03F04-P调节参数*)","LAHU03F04_VP            AT%M436.0      :REAL; (*空调机组03F04-P调节参数*)"]
["440.0","验证通过","REAL","空调机组","L","03F04","I调节参数","空调机组03F04-I调节参数",{"$f":"E99&VLOOKUP(D99,list!$D$3:$F$501,2,FALSE)&F99&\"_\"&VLOOKUP(G99,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_VI"},"LAHU03F04_VI AT%M440.0 :REAL; (*空调机组03F04-I调节参数*)","LAHU03F04_VI            AT%M440.0      :REAL; (*空调机组03F04-I调节参数*)"]
["444.0","验证通过","REAL","空调机组","L","03F04","运行时间累积值","空调机组03F04-运行时间累积值",{"$f":"E100&VLOOKUP(D100,list!$D$3:$F$501,2,FALSE)&F100&\"_\"&VLOOKUP(G100,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_RH"},"LAHU03F04_RH AT%M444.0 :REAL; (*空调机组03F04-运行时间累积值*)","LAHU03F04_RH            AT%M444.0      :REAL; (*空调机组03F04-运行时间累积值*)"]
["448.0","验证通过","INT","空调机组","L","03F04","设备状态代码","空调机组03F04-设备状态代码",{"$f":"E101&VLOOKUP(D101,list!$D$3:$F$501,2,FALSE)&F101&\"_\"&VLOOKUP(G101,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_SN"},"LAHU03F04_SN AT%M448.0 :INT; (*空调机组03F04-设备状态代码*)","LAHU03F04_SN            AT%M448.0      :INT; (*空调机组03F04-设备状态代码*)"]
["450.0","验证通过","INT","空调机组","L","03F04","水阀控制转换值","空调机组03F04-水阀控制转换值",{"$f":"E102&VLOOKUP(D102,list!$D$3:$F$501,2,FALSE)&F102&\"_\"&VLOOKUP(G102,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_WVCS"},"LAHU03F04_WVCS AT%M450.0 :INT; (*空调机组03F04-水阀控制转换值*)","LAHU03F04_WVCS          AT%M450.0      :INT; (*空调机组03F04-水阀控制转换值*)"]
["452.0","验证通过","BOOL","空调机组","L","03F04","程序控制","空调机组03F04-程序控制",{"$f":"E103&VLOOKUP(D103,list!$D$3:$F$501,2,FALSE)&F103&\"_\"&VLOOKUP(G103,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F04_PC"},"LAHU03F04_PC AT%M452.0 :BOOL; (*空调机组03F04-程序控制*)","LAHU03F04_PC            AT%M452.0      :BOOL; (*空调机组03F04-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C103=\"REAL\",C103=\"DWORD\",C103=\"DINT\"),(IF(OR(C105=\"REAL\",C105=\"DWORD\",C105=\"DINT\"),A103+4+MOD(A103,4),A103+4)),(IF(OR(C105=\"REAL\",C105=\"DWORD\",C105=\"DINT\"),A103+4+MOD(A103,4),A103+2)))&\".0\"","v":"456.0"},{"$f":"IF((IF(OR(C105=\"INT\",C105=\"WORD\",C105=\"BOOL\"),MOD(A105,2),MOD(A105,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03F05","设定温度值",{"$f":"D105&F105&\"-\"&IF(E105=\"R\",\"新云平台\"&G105,G105)","v":"空调机组03F05-新云平台设定温度值"},{"$f":"E105&VLOOKUP(D105,list!$D$3:$F$501,2,FALSE)&F105&\"_\"&VLOOKUP(G105,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F05_TSET"},{"$f":"I105&\" \"&\"AT%M\"&A105&\" \"&\":\"&C105&\";\"&\" \"&\"(*\"&H105&\"*)\"","v":"RAHU03F05_TSET AT%M456.0 :REAL; (*空调机组03F05-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J105,SEARCH(\"AT%\",J105),,REPT(\" \",25-SEARCH(\"AT%\",J105))),SEARCH(\":\",REPLACE(J105,SEARCH(\"AT%\",J105),,REPT(\" \",25-SEARCH(\"AT%\",J105)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J105,SEARCH(\"AT%\",J105),,REPT(\" \",25-SEARCH(\"AT%\",J105))))))","v":"RAHU03F05_TSET          AT%M456.0      :REAL; (*空调机组03F05-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C105=\"REAL\",C105=\"DWORD\",C105=\"DINT\"),(IF(OR(C106=\"REAL\",C106=\"DWORD\",C106=\"DINT\"),A105+4+MOD(A105,4),A105+4)),(IF(OR(C106=\"REAL\",C106=\"DWORD\",C106=\"DINT\"),A105+4+MOD(A105,4),A105+2)))&\".0\"","v":"460.0"},"验证通过","INT","空调机组","R",{"$f":"F105","v":"03F05"},"季节模式","空调机组03F05-新云平台季节模式",{"$f":"E106&VLOOKUP(D106,list!$D$3:$F$501,2,FALSE)&F106&\"_\"&VLOOKUP(G106,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F05_SM"},"RAHU03F05_SM AT%M460.0 :INT; (*空调机组03F05-新云平台季节模式*)","RAHU03F05_SM            AT%M460.0      :INT; (*空调机组03F05-新云平台季节模式*)"]
[{"$f":"IF(OR(C106=\"REAL\",C106=\"DWORD\",C106=\"DINT\"),(IF(OR(C107=\"REAL\",C107=\"DWORD\",C107=\"DINT\"),A106+4+MOD(A106,4),A106+4)),(IF(OR(C107=\"REAL\",C107=\"DWORD\",C107=\"DINT\"),A106+4+MOD(A106,4),A106+2)))&\".0\"","v":"462.0"},"验证通过","BOOL","空调机组","R",{"$f":"F106","v":"03F05"},"程序控制","空调机组03F05-新云平台程序控制",{"$f":"E107&VLOOKUP(D107,list!$D$3:$F$501,2,FALSE)&F107&\"_\"&VLOOKUP(G107,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F05_PC"},"RAHU03F05_PC AT%M462.0 :BOOL; (*空调机组03F05-新云平台程序控制*)","RAHU03F05_PC            AT%M462.0      :BOOL; (*空调机组03F05-新云平台程序控制*)"]
["468.0","验证通过","REAL","空调机组","L","03F05","设定温度值","空调机组03F05-设定温度值",{"$f":"E108&VLOOKUP(D108,list!$D$3:$F$501,2,FALSE)&F108&\"_\"&VLOOKUP(G108,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_TSET"},"LAHU03F05_TSET AT%M468.0 :REAL; (*空调机组03F05-设定温度值*)","LAHU03F05_TSET          AT%M468.0      :REAL; (*空调机组03F05-设定温度值*)"]
["472.0","验证通过","INT","空调机组","L","03F05","季节模式","空调机组03F05-季节模式",{"$f":"E109&VLOOKUP(D109,list!$D$3:$F$501,2,FALSE)&F109&\"_\"&VLOOKUP(G109,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_SM"},"LAHU03F05_SM AT%M472.0 :INT; (*空调机组03F05-季节模式*)","LAHU03F05_SM            AT%M472.0      :INT; (*空调机组03F05-季节模式*)"]
["476.0","验证通过","REAL","空调机组","L","03F05","水阀反馈换算值","空调机组03F05-水阀反馈换算值",{"$f":"E110&VLOOKUP(D110,list!$D$3:$F$501,2,FALSE)&F110&\"_\"&VLOOKUP(G110,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_WVBS"},"LAHU03F05_WVBS AT%M476.0 :REAL; (*空调机组03F05-水阀反馈换算值*)","LAHU03F05_WVBS          AT%M476.0      :REAL; (*空调机组03F05-水阀反馈换算值*)"]
["480.0","验证通过","BOOL","空调机组","L","03F05","水阀手动控制","空调机组03F05-水阀手动控制",{"$f":"E111&VLOOKUP(D111,list!$D$3:$F$501,2,FALSE)&F111&\"_\"&VLOOKUP(G111,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_WVMC"},"LAHU03F05_WVMC AT%M480.0 :BOOL; (*空调机组03F05-水阀手动控制*)","LAHU03F05_WVMC          AT%M480.0      :BOOL; (*空调机组03F05-水阀手动控制*)"]
["484.0","验证通过","REAL","空调机组","L","03F05","水阀手动控制值","空调机组03F05-水阀手动控制值",{"$f":"E112&VLOOKUP(D112,list!$D$3:$F$501,2,FALSE)&F112&\"_\"&VLOOKUP(G112,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_WVMV"},"LAHU03F05_WVMV AT%M484.0 :REAL; (*空调机组03F05-水阀手动控制值*)","LAHU03F05_WVMV          AT%M484.0      :REAL; (*空调机组03F05-水阀手动控制值*)"]
["488.0","验证通过","REAL","空调机组","L","03F05","回风温度换算值","空调机组03F05-回风温度换算值",{"$f":"E113&VLOOKUP(D113,list!$D$3:$F$501,2,FALSE)&F113&\"_\"&VLOOKUP(G113,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_RTS"},"LAHU03F05_RTS AT%M488.0 :REAL; (*空调机组03F05-回风温度换算值*)","LAHU03F05_RTS           AT%M488.0      :REAL; (*空调机组03F05-回风温度换算值*)"]
["492.0","验证通过","BOOL","空调机组","L","03F05","运行时间累积重置","空调机组03F05-运行时间累积重置",{"$f":"E114&VLOOKUP(D114,list!$D$3:$F$501,2,FALSE)&F114&\"_\"&VLOOKUP(G114,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_RST"},"LAHU03F05_RST AT%M492.0 :BOOL; (*空调机组03F05-运行时间累积重置*)","LAHU03F05_RST           AT%M492.0      :BOOL; (*空调机组03F05-运行时间累积重置*)"]
["496.0","验证通过","REAL","空调机组","L","03F05","运行时间累积重置值","空调机组03F05-运行时间累积重置值",{"$f":"E115&VLOOKUP(D115,list!$D$3:$F$501,2,FALSE)&F115&\"_\"&VLOOKUP(G115,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_RSTV"},"LAHU03F05_RSTV AT%M496.0 :REAL; (*空调机组03F05-运行时间累积重置值*)","LAHU03F05_RSTV          AT%M496.0      :REAL; (*空调机组03F05-运行时间累积重置值*)"]
["500.0","验证通过","BOOL","空调机组","L","03F05","隔离开关1","空调机组03F05-隔离开关1",{"$f":"E116&VLOOKUP(D116,list!$D$3:$F$501,2,FALSE)&F116&\"_\"&VLOOKUP(G116,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_ISO1"},"LAHU03F05_ISO1 AT%M500.0 :BOOL; (*空调机组03F05-隔离开关1*)","LAHU03F05_ISO1          AT%M500.0      :BOOL; (*空调机组03F05-隔离开关1*)"]
["502.0","验证通过","BOOL","空调机组","L","03F05","隔离开关2","空调机组03F05-隔离开关2",{"$f":"E117&VLOOKUP(D117,list!$D$3:$F$501,2,FALSE)&F117&\"_\"&VLOOKUP(G117,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_ISO2"},"LAHU03F05_ISO2 AT%M502.0 :BOOL; (*空调机组03F05-隔离开关2*)","LAHU03F05_ISO2          AT%M502.0      :BOOL; (*空调机组03F05-隔离开关2*)"]
["508.0","验证通过","REAL","空调机组","L","03F05","P调节参数","空调机组03F05-P调节参数",{"$f":"E118&VLOOKUP(D118,list!$D$3:$F$501,2,FALSE)&F118&\"_\"&VLOOKUP(G118,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_VP"},"LAHU03F05_VP AT%M508.0 :REAL; (*空调机组03F05-P调节参数*)","LAHU03F05_VP            AT%M508.0      :REAL; (*空调机组03F05-P调节参数*)"]
["512.0","验证通过","REAL","空调机组","L","03F05","I调节参数","空调机组03F05-I调节参数",{"$f":"E119&VLOOKUP(D119,list!$D$3:$F$501,2,FALSE)&F119&\"_\"&VLOOKUP(G119,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_VI"},"LAHU03F05_VI AT%M512.0 :REAL; (*空调机组03F05-I调节参数*)","LAHU03F05_VI            AT%M512.0      :REAL; (*空调机组03F05-I调节参数*)"]
["516.0","验证通过","REAL","空调机组","L","03F05","运行时间累积值","空调机组03F05-运行时间累积值",{"$f":"E120&VLOOKUP(D120,list!$D$3:$F$501,2,FALSE)&F120&\"_\"&VLOOKUP(G120,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_RH"},"LAHU03F05_RH AT%M516.0 :REAL; (*空调机组03F05-运行时间累积值*)","LAHU03F05_RH            AT%M516.0      :REAL; (*空调机组03F05-运行时间累积值*)"]
["520.0","验证通过","INT","空调机组","L","03F05","设备状态代码","空调机组03F05-设备状态代码",{"$f":"E121&VLOOKUP(D121,list!$D$3:$F$501,2,FALSE)&F121&\"_\"&VLOOKUP(G121,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_SN"},"LAHU03F05_SN AT%M520.0 :INT; (*空调机组03F05-设备状态代码*)","LAHU03F05_SN            AT%M520.0      :INT; (*空调机组03F05-设备状态代码*)"]
["522.0","验证通过","INT","空调机组","L","03F05","水阀控制转换值","空调机组03F05-水阀控制转换值",{"$f":"E122&VLOOKUP(D122,list!$D$3:$F$501,2,FALSE)&F122&\"_\"&VLOOKUP(G122,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_WVCS"},"LAHU03F05_WVCS AT%M522.0 :INT; (*空调机组03F05-水阀控制转换值*)","LAHU03F05_WVCS          AT%M522.0      :INT; (*空调机组03F05-水阀控制转换值*)"]
["524.0","验证通过","BOOL","空调机组","L","03F05","程序控制","空调机组03F05-程序控制",{"$f":"E123&VLOOKUP(D123,list!$D$3:$F$501,2,FALSE)&F123&\"_\"&VLOOKUP(G123,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F05_PC"},"LAHU03F05_PC AT%M524.0 :BOOL; (*空调机组03F05-程序控制*)","LAHU03F05_PC            AT%M524.0      :BOOL; (*空调机组03F05-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C123=\"REAL\",C123=\"DWORD\",C123=\"DINT\"),(IF(OR(C125=\"REAL\",C125=\"DWORD\",C125=\"DINT\"),A123+4+MOD(A123,4),A123+4)),(IF(OR(C125=\"REAL\",C125=\"DWORD\",C125=\"DINT\"),A123+4+MOD(A123,4),A123+2)))&\".0\"","v":"528.0"},{"$f":"IF((IF(OR(C125=\"INT\",C125=\"WORD\",C125=\"BOOL\"),MOD(A125,2),MOD(A125,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03F06","设定温度值",{"$f":"D125&F125&\"-\"&IF(E125=\"R\",\"新云平台\"&G125,G125)","v":"空调机组03F06-新云平台设定温度值"},{"$f":"E125&VLOOKUP(D125,list!$D$3:$F$501,2,FALSE)&F125&\"_\"&VLOOKUP(G125,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F06_TSET"},{"$f":"I125&\" \"&\"AT%M\"&A125&\" \"&\":\"&C125&\";\"&\" \"&\"(*\"&H125&\"*)\"","v":"RAHU03F06_TSET AT%M528.0 :REAL; (*空调机组03F06-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J125,SEARCH(\"AT%\",J125),,REPT(\" \",25-SEARCH(\"AT%\",J125))),SEARCH(\":\",REPLACE(J125,SEARCH(\"AT%\",J125),,REPT(\" \",25-SEARCH(\"AT%\",J125)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J125,SEARCH(\"AT%\",J125),,REPT(\" \",25-SEARCH(\"AT%\",J125))))))","v":"RAHU03F06_TSET          AT%M528.0      :REAL; (*空调机组03F06-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C125=\"REAL\",C125=\"DWORD\",C125=\"DINT\"),(IF(OR(C126=\"REAL\",C126=\"DWORD\",C126=\"DINT\"),A125+4+MOD(A125,4),A125+4)),(IF(OR(C126=\"REAL\",C126=\"DWORD\",C126=\"DINT\"),A125+4+MOD(A125,4),A125+2)))&\".0\"","v":"532.0"},"验证通过","INT","空调机组","R",{"$f":"F125","v":"03F06"},"季节模式","空调机组03F06-新云平台季节模式",{"$f":"E126&VLOOKUP(D126,list!$D$3:$F$501,2,FALSE)&F126&\"_\"&VLOOKUP(G126,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F06_SM"},"RAHU03F06_SM AT%M532.0 :INT; (*空调机组03F06-新云平台季节模式*)","RAHU03F06_SM            AT%M532.0      :INT; (*空调机组03F06-新云平台季节模式*)"]
["534.0","验证通过","BOOL","空调机组","R","03F06","程序控制","空调机组03F06-新云平台程序控制",{"$f":"E127&VLOOKUP(D127,list!$D$3:$F$501,2,FALSE)&F127&\"_\"&VLOOKUP(G127,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F06_PC"},"RAHU03F06_PC AT%M534.0 :BOOL; (*空调机组03F06-新云平台程序控制*)","RAHU03F06_PC            AT%M534.0      :BOOL; (*空调机组03F06-新云平台程序控制*)"]
["540.0","验证通过","REAL","空调机组","L","03F06","设定温度值","空调机组03F06-设定温度值",{"$f":"E128&VLOOKUP(D128,list!$D$3:$F$501,2,FALSE)&F128&\"_\"&VLOOKUP(G128,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_TSET"},"LAHU03F06_TSET AT%M540.0 :REAL; (*空调机组03F06-设定温度值*)","LAHU03F06_TSET          AT%M540.0      :REAL; (*空调机组03F06-设定温度值*)"]
["544.0","验证通过","INT","空调机组","L","03F06","季节模式","空调机组03F06-季节模式",{"$f":"E129&VLOOKUP(D129,list!$D$3:$F$501,2,FALSE)&F129&\"_\"&VLOOKUP(G129,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_SM"},"LAHU03F06_SM AT%M544.0 :INT; (*空调机组03F06-季节模式*)","LAHU03F06_SM            AT%M544.0      :INT; (*空调机组03F06-季节模式*)"]
["548.0","验证通过","REAL","空调机组","L","03F06","水阀反馈换算值","空调机组03F06-水阀反馈换算值",{"$f":"E130&VLOOKUP(D130,list!$D$3:$F$501,2,FALSE)&F130&\"_\"&VLOOKUP(G130,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_WVBS"},"LAHU03F06_WVBS AT%M548.0 :REAL; (*空调机组03F06-水阀反馈换算值*)","LAHU03F06_WVBS          AT%M548.0      :REAL; (*空调机组03F06-水阀反馈换算值*)"]
["552.0","验证通过","BOOL","空调机组","L","03F06","水阀手动控制","空调机组03F06-水阀手动控制",{"$f":"E131&VLOOKUP(D131,list!$D$3:$F$501,2,FALSE)&F131&\"_\"&VLOOKUP(G131,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_WVMC"},"LAHU03F06_WVMC AT%M552.0 :BOOL; (*空调机组03F06-水阀手动控制*)","LAHU03F06_WVMC          AT%M552.0      :BOOL; (*空调机组03F06-水阀手动控制*)"]
["556.0","验证通过","REAL","空调机组","L","03F06","水阀手动控制值","空调机组03F06-水阀手动控制值",{"$f":"E132&VLOOKUP(D132,list!$D$3:$F$501,2,FALSE)&F132&\"_\"&VLOOKUP(G132,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_WVMV"},"LAHU03F06_WVMV AT%M556.0 :REAL; (*空调机组03F06-水阀手动控制值*)","LAHU03F06_WVMV          AT%M556.0      :REAL; (*空调机组03F06-水阀手动控制值*)"]
["560.0","验证通过","REAL","空调机组","L","03F06","回风温度换算值","空调机组03F06-回风温度换算值",{"$f":"E133&VLOOKUP(D133,list!$D$3:$F$501,2,FALSE)&F133&\"_\"&VLOOKUP(G133,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_RTS"},"LAHU03F06_RTS AT%M560.0 :REAL; (*空调机组03F06-回风温度换算值*)","LAHU03F06_RTS           AT%M560.0      :REAL; (*空调机组03F06-回风温度换算值*)"]
["564.0","验证通过","BOOL","空调机组","L","03F06","运行时间累积重置","空调机组03F06-运行时间累积重置",{"$f":"E134&VLOOKUP(D134,list!$D$3:$F$501,2,FALSE)&F134&\"_\"&VLOOKUP(G134,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_RST"},"LAHU03F06_RST AT%M564.0 :BOOL; (*空调机组03F06-运行时间累积重置*)","LAHU03F06_RST           AT%M564.0      :BOOL; (*空调机组03F06-运行时间累积重置*)"]
["568.0","验证通过","REAL","空调机组","L","03F06","运行时间累积重置值","空调机组03F06-运行时间累积重置值",{"$f":"E135&VLOOKUP(D135,list!$D$3:$F$501,2,FALSE)&F135&\"_\"&VLOOKUP(G135,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_RSTV"},"LAHU03F06_RSTV AT%M568.0 :REAL; (*空调机组03F06-运行时间累积重置值*)","LAHU03F06_RSTV          AT%M568.0      :REAL; (*空调机组03F06-运行时间累积重置值*)"]
["572.0","验证通过","BOOL","空调机组","L","03F06","隔离开关1","空调机组03F06-隔离开关1",{"$f":"E136&VLOOKUP(D136,list!$D$3:$F$501,2,FALSE)&F136&\"_\"&VLOOKUP(G136,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_ISO1"},"LAHU03F06_ISO1 AT%M572.0 :BOOL; (*空调机组03F06-隔离开关1*)","LAHU03F06_ISO1          AT%M572.0      :BOOL; (*空调机组03F06-隔离开关1*)"]
["574.0","验证通过","BOOL","空调机组","L","03F06","隔离开关2","空调机组03F06-隔离开关2",{"$f":"E137&VLOOKUP(D137,list!$D$3:$F$501,2,FALSE)&F137&\"_\"&VLOOKUP(G137,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_ISO2"},"LAHU03F06_ISO2 AT%M574.0 :BOOL; (*空调机组03F06-隔离开关2*)","LAHU03F06_ISO2          AT%M574.0      :BOOL; (*空调机组03F06-隔离开关2*)"]
["580.0","验证通过","REAL","空调机组","L","03F06","P调节参数","空调机组03F06-P调节参数",{"$f":"E138&VLOOKUP(D138,list!$D$3:$F$501,2,FALSE)&F138&\"_\"&VLOOKUP(G138,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_VP"},"LAHU03F06_VP AT%M580.0 :REAL; (*空调机组03F06-P调节参数*)","LAHU03F06_VP            AT%M580.0      :REAL; (*空调机组03F06-P调节参数*)"]
["584.0","验证通过","REAL","空调机组","L","03F06","I调节参数","空调机组03F06-I调节参数",{"$f":"E139&VLOOKUP(D139,list!$D$3:$F$501,2,FALSE)&F139&\"_\"&VLOOKUP(G139,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_VI"},"LAHU03F06_VI AT%M584.0 :REAL; (*空调机组03F06-I调节参数*)","LAHU03F06_VI            AT%M584.0      :REAL; (*空调机组03F06-I调节参数*)"]
["588.0","验证通过","REAL","空调机组","L","03F06","运行时间累积值","空调机组03F06-运行时间累积值",{"$f":"E140&VLOOKUP(D140,list!$D$3:$F$501,2,FALSE)&F140&\"_\"&VLOOKUP(G140,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_RH"},"LAHU03F06_RH AT%M588.0 :REAL; (*空调机组03F06-运行时间累积值*)","LAHU03F06_RH            AT%M588.0      :REAL; (*空调机组03F06-运行时间累积值*)"]
["592.0","验证通过","INT","空调机组","L","03F06","设备状态代码","空调机组03F06-设备状态代码",{"$f":"E141&VLOOKUP(D141,list!$D$3:$F$501,2,FALSE)&F141&\"_\"&VLOOKUP(G141,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_SN"},"LAHU03F06_SN AT%M592.0 :INT; (*空调机组03F06-设备状态代码*)","LAHU03F06_SN            AT%M592.0      :INT; (*空调机组03F06-设备状态代码*)"]
["594.0","验证通过","INT","空调机组","L","03F06","水阀控制转换值","空调机组03F06-水阀控制转换值",{"$f":"E142&VLOOKUP(D142,list!$D$3:$F$501,2,FALSE)&F142&\"_\"&VLOOKUP(G142,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_WVCS"},"LAHU03F06_WVCS AT%M594.0 :INT; (*空调机组03F06-水阀控制转换值*)","LAHU03F06_WVCS          AT%M594.0      :INT; (*空调机组03F06-水阀控制转换值*)"]
["596.0","验证通过","BOOL","空调机组","L","03F06","程序控制","空调机组03F06-程序控制",{"$f":"E143&VLOOKUP(D143,list!$D$3:$F$501,2,FALSE)&F143&\"_\"&VLOOKUP(G143,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F06_PC"},"LAHU03F06_PC AT%M596.0 :BOOL; (*空调机组03F06-程序控制*)","LAHU03F06_PC            AT%M596.0      :BOOL; (*空调机组03F06-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C143=\"REAL\",C143=\"DWORD\",C143=\"DINT\"),(IF(OR(C145=\"REAL\",C145=\"DWORD\",C145=\"DINT\"),A143+4+MOD(A143,4),A143+4)),(IF(OR(C145=\"REAL\",C145=\"DWORD\",C145=\"DINT\"),A143+4+MOD(A143,4),A143+2)))&\".0\"","v":"600.0"},{"$f":"IF((IF(OR(C145=\"INT\",C145=\"WORD\",C145=\"BOOL\"),MOD(A145,2),MOD(A145,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03F07","设定温度值",{"$f":"D145&F145&\"-\"&IF(E145=\"R\",\"新云平台\"&G145,G145)","v":"空调机组03F07-新云平台设定温度值"},{"$f":"E145&VLOOKUP(D145,list!$D$3:$F$501,2,FALSE)&F145&\"_\"&VLOOKUP(G145,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F07_TSET"},{"$f":"I145&\" \"&\"AT%M\"&A145&\" \"&\":\"&C145&\";\"&\" \"&\"(*\"&H145&\"*)\"","v":"RAHU03F07_TSET AT%M600.0 :REAL; (*空调机组03F07-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J145,SEARCH(\"AT%\",J145),,REPT(\" \",25-SEARCH(\"AT%\",J145))),SEARCH(\":\",REPLACE(J145,SEARCH(\"AT%\",J145),,REPT(\" \",25-SEARCH(\"AT%\",J145)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J145,SEARCH(\"AT%\",J145),,REPT(\" \",25-SEARCH(\"AT%\",J145))))))","v":"RAHU03F07_TSET          AT%M600.0      :REAL; (*空调机组03F07-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C145=\"REAL\",C145=\"DWORD\",C145=\"DINT\"),(IF(OR(C146=\"REAL\",C146=\"DWORD\",C146=\"DINT\"),A145+4+MOD(A145,4),A145+4)),(IF(OR(C146=\"REAL\",C146=\"DWORD\",C146=\"DINT\"),A145+4+MOD(A145,4),A145+2)))&\".0\"","v":"604.0"},"验证通过","INT","空调机组","R",{"$f":"F145","v":"03F07"},"季节模式","空调机组03F07-新云平台季节模式",{"$f":"E146&VLOOKUP(D146,list!$D$3:$F$501,2,FALSE)&F146&\"_\"&VLOOKUP(G146,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F07_SM"},"RAHU03F07_SM AT%M604.0 :INT; (*空调机组03F07-新云平台季节模式*)","RAHU03F07_SM            AT%M604.0      :INT; (*空调机组03F07-新云平台季节模式*)"]
["606.0","验证通过","BOOL","空调机组","R","03F07","程序控制","空调机组03F07-新云平台程序控制",{"$f":"E147&VLOOKUP(D147,list!$D$3:$F$501,2,FALSE)&F147&\"_\"&VLOOKUP(G147,list!$I$2:$K$502,2,FALSE)","v":"RAHU03F07_PC"},"RAHU03F07_PC AT%M606.0 :BOOL; (*空调机组03F07-新云平台程序控制*)","RAHU03F07_PC            AT%M606.0      :BOOL; (*空调机组03F07-新云平台程序控制*)"]
["612.0","验证通过","REAL","空调机组","L","03F07","设定温度值","空调机组03F07-设定温度值",{"$f":"E148&VLOOKUP(D148,list!$D$3:$F$501,2,FALSE)&F148&\"_\"&VLOOKUP(G148,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_TSET"},"LAHU03F07_TSET AT%M612.0 :REAL; (*空调机组03F07-设定温度值*)","LAHU03F07_TSET          AT%M612.0      :REAL; (*空调机组03F07-设定温度值*)"]
["616.0","验证通过","INT","空调机组","L","03F07","季节模式","空调机组03F07-季节模式",{"$f":"E149&VLOOKUP(D149,list!$D$3:$F$501,2,FALSE)&F149&\"_\"&VLOOKUP(G149,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_SM"},"LAHU03F07_SM AT%M616.0 :INT; (*空调机组03F07-季节模式*)","LAHU03F07_SM            AT%M616.0      :INT; (*空调机组03F07-季节模式*)"]
["620.0","验证通过","REAL","空调机组","L","03F07","水阀反馈换算值","空调机组03F07-水阀反馈换算值",{"$f":"E150&VLOOKUP(D150,list!$D$3:$F$501,2,FALSE)&F150&\"_\"&VLOOKUP(G150,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_WVBS"},"LAHU03F07_WVBS AT%M620.0 :REAL; (*空调机组03F07-水阀反馈换算值*)","LAHU03F07_WVBS          AT%M620.0      :REAL; (*空调机组03F07-水阀反馈换算值*)"]
["624.0","验证通过","BOOL","空调机组","L","03F07","水阀手动控制","空调机组03F07-水阀手动控制",{"$f":"E151&VLOOKUP(D151,list!$D$3:$F$501,2,FALSE)&F151&\"_\"&VLOOKUP(G151,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_WVMC"},"LAHU03F07_WVMC AT%M624.0 :BOOL; (*空调机组03F07-水阀手动控制*)","LAHU03F07_WVMC          AT%M624.0      :BOOL; (*空调机组03F07-水阀手动控制*)"]
["628.0","验证通过","REAL","空调机组","L","03F07","水阀手动控制值","空调机组03F07-水阀手动控制值",{"$f":"E152&VLOOKUP(D152,list!$D$3:$F$501,2,FALSE)&F152&\"_\"&VLOOKUP(G152,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_WVMV"},"LAHU03F07_WVMV AT%M628.0 :REAL; (*空调机组03F07-水阀手动控制值*)","LAHU03F07_WVMV          AT%M628.0      :REAL; (*空调机组03F07-水阀手动控制值*)"]
["632.0","验证通过","REAL","空调机组","L","03F07","回风温度换算值","空调机组03F07-回风温度换算值",{"$f":"E153&VLOOKUP(D153,list!$D$3:$F$501,2,FALSE)&F153&\"_\"&VLOOKUP(G153,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_RTS"},"LAHU03F07_RTS AT%M632.0 :REAL; (*空调机组03F07-回风温度换算值*)","LAHU03F07_RTS           AT%M632.0      :REAL; (*空调机组03F07-回风温度换算值*)"]
["636.0","验证通过","BOOL","空调机组","L","03F07","运行时间累积重置","空调机组03F07-运行时间累积重置",{"$f":"E154&VLOOKUP(D154,list!$D$3:$F$501,2,FALSE)&F154&\"_\"&VLOOKUP(G154,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_RST"},"LAHU03F07_RST AT%M636.0 :BOOL; (*空调机组03F07-运行时间累积重置*)","LAHU03F07_RST           AT%M636.0      :BOOL; (*空调机组03F07-运行时间累积重置*)"]
["640.0","验证通过","REAL","空调机组","L","03F07","运行时间累积重置值","空调机组03F07-运行时间累积重置值",{"$f":"E155&VLOOKUP(D155,list!$D$3:$F$501,2,FALSE)&F155&\"_\"&VLOOKUP(G155,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_RSTV"},"LAHU03F07_RSTV AT%M640.0 :REAL; (*空调机组03F07-运行时间累积重置值*)","LAHU03F07_RSTV          AT%M640.0      :REAL; (*空调机组03F07-运行时间累积重置值*)"]
["644.0","验证通过","BOOL","空调机组","L","03F07","隔离开关1","空调机组03F07-隔离开关1",{"$f":"E156&VLOOKUP(D156,list!$D$3:$F$501,2,FALSE)&F156&\"_\"&VLOOKUP(G156,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_ISO1"},"LAHU03F07_ISO1 AT%M644.0 :BOOL; (*空调机组03F07-隔离开关1*)","LAHU03F07_ISO1          AT%M644.0      :BOOL; (*空调机组03F07-隔离开关1*)"]
["646.0","验证通过","BOOL","空调机组","L","03F07","隔离开关2","空调机组03F07-隔离开关2",{"$f":"E157&VLOOKUP(D157,list!$D$3:$F$501,2,FALSE)&F157&\"_\"&VLOOKUP(G157,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_ISO2"},"LAHU03F07_ISO2 AT%M646.0 :BOOL; (*空调机组03F07-隔离开关2*)","LAHU03F07_ISO2          AT%M646.0      :BOOL; (*空调机组03F07-隔离开关2*)"]
["652.0","验证通过","REAL","空调机组","L","03F07","P调节参数","空调机组03F07-P调节参数",{"$f":"E158&VLOOKUP(D158,list!$D$3:$F$501,2,FALSE)&F158&\"_\"&VLOOKUP(G158,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_VP"},"LAHU03F07_VP AT%M652.0 :REAL; (*空调机组03F07-P调节参数*)","LAHU03F07_VP            AT%M652.0      :REAL; (*空调机组03F07-P调节参数*)"]
["656.0","验证通过","REAL","空调机组","L","03F07","I调节参数","空调机组03F07-I调节参数",{"$f":"E159&VLOOKUP(D159,list!$D$3:$F$501,2,FALSE)&F159&\"_\"&VLOOKUP(G159,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_VI"},"LAHU03F07_VI AT%M656.0 :REAL; (*空调机组03F07-I调节参数*)","LAHU03F07_VI            AT%M656.0      :REAL; (*空调机组03F07-I调节参数*)"]
["660.0","验证通过","REAL","空调机组","L","03F07","运行时间累积值","空调机组03F07-运行时间累积值",{"$f":"E160&VLOOKUP(D160,list!$D$3:$F$501,2,FALSE)&F160&\"_\"&VLOOKUP(G160,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_RH"},"LAHU03F07_RH AT%M660.0 :REAL; (*空调机组03F07-运行时间累积值*)","LAHU03F07_RH            AT%M660.0      :REAL; (*空调机组03F07-运行时间累积值*)"]
["664.0","验证通过","INT","空调机组","L","03F07","设备状态代码","空调机组03F07-设备状态代码",{"$f":"E161&VLOOKUP(D161,list!$D$3:$F$501,2,FALSE)&F161&\"_\"&VLOOKUP(G161,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_SN"},"LAHU03F07_SN AT%M664.0 :INT; (*空调机组03F07-设备状态代码*)","LAHU03F07_SN            AT%M664.0      :INT; (*空调机组03F07-设备状态代码*)"]
["666.0","验证通过","INT","空调机组","L","03F07","水阀控制转换值","空调机组03F07-水阀控制转换值",{"$f":"E162&VLOOKUP(D162,list!$D$3:$F$501,2,FALSE)&F162&\"_\"&VLOOKUP(G162,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_WVCS"},"LAHU03F07_WVCS AT%M666.0 :INT; (*空调机组03F07-水阀控制转换值*)","LAHU03F07_WVCS          AT%M666.0      :INT; (*空调机组03F07-水阀控制转换值*)"]
["668.0","验证通过","BOOL","空调机组","L","03F07","程序控制","空调机组03F07-程序控制",{"$f":"E163&VLOOKUP(D163,list!$D$3:$F$501,2,FALSE)&F163&\"_\"&VLOOKUP(G163,list!$I$2:$K$502,2,FALSE)","v":"LAHU03F07_PC"},"LAHU03F07_PC AT%M668.0 :BOOL; (*空调机组03F07-程序控制*)","LAHU03F07_PC            AT%M668.0      :BOOL; (*空调机组03F07-程序控制*)"]
["FCU"]
[{"$f":"IF(OR(C163=\"REAL\",C163=\"DWORD\",C163=\"DINT\"),(IF(OR(C165=\"REAL\",C165=\"DWORD\",C165=\"DINT\"),A163+4+MOD(A163,4),A163+4)),(IF(OR(C165=\"REAL\",C165=\"DWORD\",C165=\"DINT\"),A163+4+MOD(A163,4),A163+2)))&\".0\"","v":"672.0"},{"$f":"IF((IF(OR(C165=\"INT\",C165=\"WORD\",C165=\"BOOL\"),MOD(A165,2),MOD(A165,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","03F01","设定温度值",{"$f":"D165&F165&\"-\"&IF(E165=\"R\",\"新云平台\"&G165,G165)","v":"风机盘管03F01-新云平台设定温度值"},{"$f":"E165&VLOOKUP(D165,list!$D$3:$F$501,2,FALSE)&F165&\"_\"&VLOOKUP(G165,list!$I$2:$K$502,2,FALSE)","v":"RFCU03F01_TSET"},{"$f":"I165&\" \"&\"AT%M\"&A165&\" \"&\":\"&C165&\";\"&\" \"&\"(*\"&H165&\"*)\"","v":"RFCU03F01_TSET AT%M672.0 :REAL; (*风机盘管03F01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J165,SEARCH(\"AT%\",J165),,REPT(\" \",25-SEARCH(\"AT%\",J165))),SEARCH(\":\",REPLACE(J165,SEARCH(\"AT%\",J165),,REPT(\" \",25-SEARCH(\"AT%\",J165)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J165,SEARCH(\"AT%\",J165),,REPT(\" \",25-SEARCH(\"AT%\",J165))))))","v":"RFCU03F01_TSET          AT%M672.0      :REAL; (*风机盘管03F01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C165=\"REAL\",C165=\"DWORD\",C165=\"DINT\"),(IF(OR(C166=\"REAL\",C166=\"DWORD\",C166=\"DINT\"),A165+4+MOD(A165,4),A165+4)),(IF(OR(C166=\"REAL\",C166=\"DWORD\",C166=\"DINT\"),A165+4+MOD(A165,4),A165+2)))&\".0\"","v":"676.0"},"验证通过","INT","风机盘管","R",{"$f":"F165","v":"03F01"},"季节模式","风机盘管03F01-新云平台季节模式",{"$f":"E166&VLOOKUP(D166,list!$D$3:$F$501,2,FALSE)&F166&\"_\"&VLOOKUP(G166,list!$I$2:$K$502,2,FALSE)","v":"RFCU03F01_SM"},"RFCU03F01_SM AT%M676.0 :INT; (*风机盘管03F01-新云平台季节模式*)","RFCU03F01_SM            AT%M676.0      :INT; (*风机盘管03F01-新云平台季节模式*)"]
["678.0","验证通过","BOOL","风机盘管","R","03F01","程序控制","风机盘管03F01-新云平台程序控制",{"$f":"E167&VLOOKUP(D167,list!$D$3:$F$501,2,FALSE)&F167&\"_\"&VLOOKUP(G167,list!$I$2:$K$502,2,FALSE)","v":"RFCU03F01_PC"},"RFCU03F01_PC AT%M678.0 :BOOL; (*风机盘管03F01-新云平台程序控制*)","RFCU03F01_PC            AT%M678.0      :BOOL; (*风机盘管03F01-新云平台程序控制*)"]
["684.0","验证通过","REAL","风机盘管","L","03F01","设定温度值","风机盘管03F01-设定温度值",{"$f":"E168&VLOOKUP(D168,list!$D$3:$F$501,2,FALSE)&F168&\"_\"&VLOOKUP(G168,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_TSET"},"LFCU03F01_TSET AT%M684.0 :REAL; (*风机盘管03F01-设定温度值*)","LFCU03F01_TSET          AT%M684.0      :REAL; (*风机盘管03F01-设定温度值*)"]
["688.0","验证通过","INT","风机盘管","L","03F01","季节模式","风机盘管03F01-季节模式",{"$f":"E169&VLOOKUP(D169,list!$D$3:$F$501,2,FALSE)&F169&\"_\"&VLOOKUP(G169,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_SM"},"LFCU03F01_SM AT%M688.0 :INT; (*风机盘管03F01-季节模式*)","LFCU03F01_SM            AT%M688.0      :INT; (*风机盘管03F01-季节模式*)"]
["692.0","验证通过","REAL","风机盘管","L","03F01","温度换算值","风机盘管03F01-温度换算值",{"$f":"E170&VLOOKUP(D170,list!$D$3:$F$501,2,FALSE)&F170&\"_\"&VLOOKUP(G170,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_TS"},"LFCU03F01_TS AT%M692.0 :REAL; (*风机盘管03F01-温度换算值*)","LFCU03F01_TS            AT%M692.0      :REAL; (*风机盘管03F01-温度换算值*)"]
["696.0","验证通过","BOOL","风机盘管","L","03F01","电磁阀手动控制","风机盘管03F01-电磁阀手动控制",{"$f":"E171&VLOOKUP(D171,list!$D$3:$F$501,2,FALSE)&F171&\"_\"&VLOOKUP(G171,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_EVMC"},"LFCU03F01_EVMC AT%M696.0 :BOOL; (*风机盘管03F01-电磁阀手动控制*)","LFCU03F01_EVMC          AT%M696.0      :BOOL; (*风机盘管03F01-电磁阀手动控制*)"]
["698.0","验证通过","BOOL","风机盘管","L","03F01","电磁阀手动控制值","风机盘管03F01-电磁阀手动控制值",{"$f":"E172&VLOOKUP(D172,list!$D$3:$F$501,2,FALSE)&F172&\"_\"&VLOOKUP(G172,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_EVMV"},"LFCU03F01_EVMV AT%M698.0 :BOOL; (*风机盘管03F01-电磁阀手动控制值*)","LFCU03F01_EVMV          AT%M698.0      :BOOL; (*风机盘管03F01-电磁阀手动控制值*)"]
["704.0","验证通过","REAL","风机盘管","L","03F01","回风温度换算值","风机盘管03F01-回风温度换算值",{"$f":"E173&VLOOKUP(D173,list!$D$3:$F$501,2,FALSE)&F173&\"_\"&VLOOKUP(G173,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_RTS"},"LFCU03F01_RTS AT%M704.0 :REAL; (*风机盘管03F01-回风温度换算值*)","LFCU03F01_RTS           AT%M704.0      :REAL; (*风机盘管03F01-回风温度换算值*)"]
["708.0","验证通过","BOOL","风机盘管","L","03F01","运行时间累积重置","风机盘管03F01-运行时间累积重置",{"$f":"E174&VLOOKUP(D174,list!$D$3:$F$501,2,FALSE)&F174&\"_\"&VLOOKUP(G174,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_RST"},"LFCU03F01_RST AT%M708.0 :BOOL; (*风机盘管03F01-运行时间累积重置*)","LFCU03F01_RST           AT%M708.0      :BOOL; (*风机盘管03F01-运行时间累积重置*)"]
["712.0","验证通过","REAL","风机盘管","L","03F01","运行时间累积重置值","风机盘管03F01-运行时间累积重置值",{"$f":"E175&VLOOKUP(D175,list!$D$3:$F$501,2,FALSE)&F175&\"_\"&VLOOKUP(G175,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_RSTV"},"LFCU03F01_RSTV AT%M712.0 :REAL; (*风机盘管03F01-运行时间累积重置值*)","LFCU03F01_RSTV          AT%M712.0      :REAL; (*风机盘管03F01-运行时间累积重置值*)"]
["716.0","验证通过","BOOL","风机盘管","L","03F01","隔离开关1","风机盘管03F01-隔离开关1",{"$f":"E176&VLOOKUP(D176,list!$D$3:$F$501,2,FALSE)&F176&\"_\"&VLOOKUP(G176,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_ISO1"},"LFCU03F01_ISO1 AT%M716.0 :BOOL; (*风机盘管03F01-隔离开关1*)","LFCU03F01_ISO1          AT%M716.0      :BOOL; (*风机盘管03F01-隔离开关1*)"]
["720.0","验证通过","REAL","风机盘管","L","03F01","运行时间累积值","风机盘管03F01-运行时间累积值",{"$f":"E177&VLOOKUP(D177,list!$D$3:$F$501,2,FALSE)&F177&\"_\"&VLOOKUP(G177,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_RH"},"LFCU03F01_RH AT%M720.0 :REAL; (*风机盘管03F01-运行时间累积值*)","LFCU03F01_RH            AT%M720.0      :REAL; (*风机盘管03F01-运行时间累积值*)"]
["724.0","验证通过","INT","风机盘管","L","03F01","设备状态代码","风机盘管03F01-设备状态代码",{"$f":"E178&VLOOKUP(D178,list!$D$3:$F$501,2,FALSE)&F178&\"_\"&VLOOKUP(G178,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_SN"},"LFCU03F01_SN AT%M724.0 :INT; (*风机盘管03F01-设备状态代码*)","LFCU03F01_SN            AT%M724.0      :INT; (*风机盘管03F01-设备状态代码*)"]
["726.0","验证通过","INT","风机盘管","L","03F01","水阀控制转换值","风机盘管03F01-水阀控制转换值",{"$f":"E179&VLOOKUP(D179,list!$D$3:$F$501,2,FALSE)&F179&\"_\"&VLOOKUP(G179,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_WVCS"},"LFCU03F01_WVCS AT%M726.0 :INT; (*风机盘管03F01-水阀控制转换值*)","LFCU03F01_WVCS          AT%M726.0      :INT; (*风机盘管03F01-水阀控制转换值*)"]
["728.0","验证通过","BOOL","风机盘管","L","03F01","程序控制","风机盘管03F01-程序控制",{"$f":"E180&VLOOKUP(D180,list!$D$3:$F$501,2,FALSE)&F180&\"_\"&VLOOKUP(G180,list!$I$2:$K$502,2,FALSE)","v":"LFCU03F01_PC"},"LFCU03F01_PC AT%M728.0 :BOOL; (*风机盘管03F01-程序控制*)","LFCU03F01_PC            AT%M728.0      :BOOL; (*风机盘管03F01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C163=\"REAL\",C163=\"DWORD\",C163=\"DINT\"),(IF(OR(C182=\"REAL\",C182=\"DWORD\",C182=\"DINT\"),A163+4+MOD(A163,4),A163+4)),(IF(OR(C182=\"REAL\",C182=\"DWORD\",C182=\"DINT\"),A163+4+MOD(A163,4),A163+2)))&\".0\"","v":"672.0"},{"$f":"IF((IF(OR(C182=\"INT\",C182=\"WORD\",C182=\"BOOL\"),MOD(A182,2),MOD(A182,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F01","设定温度值",{"$f":"D182&F182&\"-\"&IF(E182=\"R\",\"新云平台\"&G182,G182)","v":"空调机组04F01-新云平台设定温度值"},{"$f":"E182&VLOOKUP(D182,list!$D$3:$F$501,2,FALSE)&F182&\"_\"&VLOOKUP(G182,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F01_TSET"},{"$f":"I182&\" \"&\"AT%M\"&A182&\" \"&\":\"&C182&\";\"&\" \"&\"(*\"&H182&\"*)\"","v":"RAHU04F01_TSET AT%M672.0 :REAL; (*空调机组04F01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J182,SEARCH(\"AT%\",J182),,REPT(\" \",25-SEARCH(\"AT%\",J182))),SEARCH(\":\",REPLACE(J182,SEARCH(\"AT%\",J182),,REPT(\" \",25-SEARCH(\"AT%\",J182)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J182,SEARCH(\"AT%\",J182),,REPT(\" \",25-SEARCH(\"AT%\",J182))))))","v":"RAHU04F01_TSET          AT%M672.0      :REAL; (*空调机组04F01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C182=\"REAL\",C182=\"DWORD\",C182=\"DINT\"),(IF(OR(C183=\"REAL\",C183=\"DWORD\",C183=\"DINT\"),A182+4+MOD(A182,4),A182+4)),(IF(OR(C183=\"REAL\",C183=\"DWORD\",C183=\"DINT\"),A182+4+MOD(A182,4),A182+2)))&\".0\"","v":"676.0"},"验证通过","INT","空调机组","R",{"$f":"F182","v":"04F01"},"季节模式","空调机组04F01-新云平台季节模式",{"$f":"E183&VLOOKUP(D183,list!$D$3:$F$501,2,FALSE)&F183&\"_\"&VLOOKUP(G183,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F01_SM"},"RAHU04F01_SM AT%M676.0 :INT; (*空调机组04F01-新云平台季节模式*)","RAHU04F01_SM            AT%M676.0      :INT; (*空调机组04F01-新云平台季节模式*)"]
["678.0","验证通过","BOOL","空调机组","R","04F01","程序控制","空调机组04F01-新云平台程序控制",{"$f":"E184&VLOOKUP(D184,list!$D$3:$F$501,2,FALSE)&F184&\"_\"&VLOOKUP(G184,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F01_PC"},"RAHU04F01_PC AT%M678.0 :BOOL; (*空调机组04F01-新云平台程序控制*)","RAHU04F01_PC            AT%M678.0      :BOOL; (*空调机组04F01-新云平台程序控制*)"]
["684.0","验证通过","REAL","空调机组","L","04F01","设定温度值","空调机组04F01-设定温度值",{"$f":"E185&VLOOKUP(D185,list!$D$3:$F$501,2,FALSE)&F185&\"_\"&VLOOKUP(G185,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_TSET"},"LAHU04F01_TSET AT%M684.0 :REAL; (*空调机组04F01-设定温度值*)","LAHU04F01_TSET          AT%M684.0      :REAL; (*空调机组04F01-设定温度值*)"]
["688.0","验证通过","INT","空调机组","L","04F01","季节模式","空调机组04F01-季节模式",{"$f":"E186&VLOOKUP(D186,list!$D$3:$F$501,2,FALSE)&F186&\"_\"&VLOOKUP(G186,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_SM"},"LAHU04F01_SM AT%M688.0 :INT; (*空调机组04F01-季节模式*)","LAHU04F01_SM            AT%M688.0      :INT; (*空调机组04F01-季节模式*)"]
["692.0","验证通过","REAL","空调机组","L","04F01","水阀反馈换算值","空调机组04F01-水阀反馈换算值",{"$f":"E187&VLOOKUP(D187,list!$D$3:$F$501,2,FALSE)&F187&\"_\"&VLOOKUP(G187,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_WVBS"},"LAHU04F01_WVBS AT%M692.0 :REAL; (*空调机组04F01-水阀反馈换算值*)","LAHU04F01_WVBS          AT%M692.0      :REAL; (*空调机组04F01-水阀反馈换算值*)"]
["696.0","验证通过","BOOL","空调机组","L","04F01","水阀手动控制","空调机组04F01-水阀手动控制",{"$f":"E188&VLOOKUP(D188,list!$D$3:$F$501,2,FALSE)&F188&\"_\"&VLOOKUP(G188,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_WVMC"},"LAHU04F01_WVMC AT%M696.0 :BOOL; (*空调机组04F01-水阀手动控制*)","LAHU04F01_WVMC          AT%M696.0      :BOOL; (*空调机组04F01-水阀手动控制*)"]
["700.0","验证通过","REAL","空调机组","L","04F01","水阀手动控制值","空调机组04F01-水阀手动控制值",{"$f":"E189&VLOOKUP(D189,list!$D$3:$F$501,2,FALSE)&F189&\"_\"&VLOOKUP(G189,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_WVMV"},"LAHU04F01_WVMV AT%M700.0 :REAL; (*空调机组04F01-水阀手动控制值*)","LAHU04F01_WVMV          AT%M700.0      :REAL; (*空调机组04F01-水阀手动控制值*)"]
["704.0","验证通过","REAL","空调机组","L","04F01","回风温度换算值","空调机组04F01-回风温度换算值",{"$f":"E190&VLOOKUP(D190,list!$D$3:$F$501,2,FALSE)&F190&\"_\"&VLOOKUP(G190,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_RTS"},"LAHU04F01_RTS AT%M704.0 :REAL; (*空调机组04F01-回风温度换算值*)","LAHU04F01_RTS           AT%M704.0      :REAL; (*空调机组04F01-回风温度换算值*)"]
["708.0","验证通过","BOOL","空调机组","L","04F01","运行时间累积重置","空调机组04F01-运行时间累积重置",{"$f":"E191&VLOOKUP(D191,list!$D$3:$F$501,2,FALSE)&F191&\"_\"&VLOOKUP(G191,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_RST"},"LAHU04F01_RST AT%M708.0 :BOOL; (*空调机组04F01-运行时间累积重置*)","LAHU04F01_RST           AT%M708.0      :BOOL; (*空调机组04F01-运行时间累积重置*)"]
["712.0","验证通过","REAL","空调机组","L","04F01","运行时间累积重置值","空调机组04F01-运行时间累积重置值",{"$f":"E192&VLOOKUP(D192,list!$D$3:$F$501,2,FALSE)&F192&\"_\"&VLOOKUP(G192,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_RSTV"},"LAHU04F01_RSTV AT%M712.0 :REAL; (*空调机组04F01-运行时间累积重置值*)","LAHU04F01_RSTV          AT%M712.0      :REAL; (*空调机组04F01-运行时间累积重置值*)"]
["716.0","验证通过","BOOL","空调机组","L","04F01","隔离开关1","空调机组04F01-隔离开关1",{"$f":"E193&VLOOKUP(D193,list!$D$3:$F$501,2,FALSE)&F193&\"_\"&VLOOKUP(G193,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_ISO1"},"LAHU04F01_ISO1 AT%M716.0 :BOOL; (*空调机组04F01-隔离开关1*)","LAHU04F01_ISO1          AT%M716.0      :BOOL; (*空调机组04F01-隔离开关1*)"]
["718.0","验证通过","BOOL","空调机组","L","04F01","隔离开关2","空调机组04F01-隔离开关2",{"$f":"E194&VLOOKUP(D194,list!$D$3:$F$501,2,FALSE)&F194&\"_\"&VLOOKUP(G194,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_ISO2"},"LAHU04F01_ISO2 AT%M718.0 :BOOL; (*空调机组04F01-隔离开关2*)","LAHU04F01_ISO2          AT%M718.0      :BOOL; (*空调机组04F01-隔离开关2*)"]
["724.0","验证通过","REAL","空调机组","L","04F01","P调节参数","空调机组04F01-P调节参数",{"$f":"E195&VLOOKUP(D195,list!$D$3:$F$501,2,FALSE)&F195&\"_\"&VLOOKUP(G195,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_VP"},"LAHU04F01_VP AT%M724.0 :REAL; (*空调机组04F01-P调节参数*)","LAHU04F01_VP            AT%M724.0      :REAL; (*空调机组04F01-P调节参数*)"]
["728.0","验证通过","REAL","空调机组","L","04F01","I调节参数","空调机组04F01-I调节参数",{"$f":"E196&VLOOKUP(D196,list!$D$3:$F$501,2,FALSE)&F196&\"_\"&VLOOKUP(G196,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_VI"},"LAHU04F01_VI AT%M728.0 :REAL; (*空调机组04F01-I调节参数*)","LAHU04F01_VI            AT%M728.0      :REAL; (*空调机组04F01-I调节参数*)"]
["732.0","验证通过","REAL","空调机组","L","04F01","运行时间累积值","空调机组04F01-运行时间累积值",{"$f":"E197&VLOOKUP(D197,list!$D$3:$F$501,2,FALSE)&F197&\"_\"&VLOOKUP(G197,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_RH"},"LAHU04F01_RH AT%M732.0 :REAL; (*空调机组04F01-运行时间累积值*)","LAHU04F01_RH            AT%M732.0      :REAL; (*空调机组04F01-运行时间累积值*)"]
["736.0","验证通过","INT","空调机组","L","04F01","设备状态代码","空调机组04F01-设备状态代码",{"$f":"E198&VLOOKUP(D198,list!$D$3:$F$501,2,FALSE)&F198&\"_\"&VLOOKUP(G198,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_SN"},"LAHU04F01_SN AT%M736.0 :INT; (*空调机组04F01-设备状态代码*)","LAHU04F01_SN            AT%M736.0      :INT; (*空调机组04F01-设备状态代码*)"]
["738.0","验证通过","INT","空调机组","L","04F01","水阀控制转换值","空调机组04F01-水阀控制转换值",{"$f":"E199&VLOOKUP(D199,list!$D$3:$F$501,2,FALSE)&F199&\"_\"&VLOOKUP(G199,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_WVCS"},"LAHU04F01_WVCS AT%M738.0 :INT; (*空调机组04F01-水阀控制转换值*)","LAHU04F01_WVCS          AT%M738.0      :INT; (*空调机组04F01-水阀控制转换值*)"]
["740.0","验证通过","BOOL","空调机组","L","04F01","程序控制","空调机组04F01-程序控制",{"$f":"E200&VLOOKUP(D200,list!$D$3:$F$501,2,FALSE)&F200&\"_\"&VLOOKUP(G200,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F01_PC"},"LAHU04F01_PC AT%M740.0 :BOOL; (*空调机组04F01-程序控制*)","LAHU04F01_PC            AT%M740.0      :BOOL; (*空调机组04F01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C200=\"REAL\",C200=\"DWORD\",C200=\"DINT\"),(IF(OR(C202=\"REAL\",C202=\"DWORD\",C202=\"DINT\"),A200+4+MOD(A200,4),A200+4)),(IF(OR(C202=\"REAL\",C202=\"DWORD\",C202=\"DINT\"),A200+4+MOD(A200,4),A200+2)))&\".0\"","v":"744.0"},{"$f":"IF((IF(OR(C202=\"INT\",C202=\"WORD\",C202=\"BOOL\"),MOD(A202,2),MOD(A202,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F02","设定温度值",{"$f":"D202&F202&\"-\"&IF(E202=\"R\",\"新云平台\"&G202,G202)","v":"空调机组04F02-新云平台设定温度值"},{"$f":"E202&VLOOKUP(D202,list!$D$3:$F$501,2,FALSE)&F202&\"_\"&VLOOKUP(G202,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F02_TSET"},{"$f":"I202&\" \"&\"AT%M\"&A202&\" \"&\":\"&C202&\";\"&\" \"&\"(*\"&H202&\"*)\"","v":"RAHU04F02_TSET AT%M744.0 :REAL; (*空调机组04F02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J202,SEARCH(\"AT%\",J202),,REPT(\" \",25-SEARCH(\"AT%\",J202))),SEARCH(\":\",REPLACE(J202,SEARCH(\"AT%\",J202),,REPT(\" \",25-SEARCH(\"AT%\",J202)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J202,SEARCH(\"AT%\",J202),,REPT(\" \",25-SEARCH(\"AT%\",J202))))))","v":"RAHU04F02_TSET          AT%M744.0      :REAL; (*空调机组04F02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C202=\"REAL\",C202=\"DWORD\",C202=\"DINT\"),(IF(OR(C203=\"REAL\",C203=\"DWORD\",C203=\"DINT\"),A202+4+MOD(A202,4),A202+4)),(IF(OR(C203=\"REAL\",C203=\"DWORD\",C203=\"DINT\"),A202+4+MOD(A202,4),A202+2)))&\".0\"","v":"748.0"},"验证通过","INT","空调机组","R",{"$f":"F202","v":"04F02"},"季节模式","空调机组04F02-新云平台季节模式",{"$f":"E203&VLOOKUP(D203,list!$D$3:$F$501,2,FALSE)&F203&\"_\"&VLOOKUP(G203,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F02_SM"},"RAHU04F02_SM AT%M748.0 :INT; (*空调机组04F02-新云平台季节模式*)","RAHU04F02_SM            AT%M748.0      :INT; (*空调机组04F02-新云平台季节模式*)"]
["750.0","验证通过","BOOL","空调机组","R","04F02","程序控制","空调机组04F02-新云平台程序控制",{"$f":"E204&VLOOKUP(D204,list!$D$3:$F$501,2,FALSE)&F204&\"_\"&VLOOKUP(G204,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F02_PC"},"RAHU04F02_PC AT%M750.0 :BOOL; (*空调机组04F02-新云平台程序控制*)","RAHU04F02_PC            AT%M750.0      :BOOL; (*空调机组04F02-新云平台程序控制*)"]
["756.0","验证通过","REAL","空调机组","L","04F02","设定温度值","空调机组04F02-设定温度值",{"$f":"E205&VLOOKUP(D205,list!$D$3:$F$501,2,FALSE)&F205&\"_\"&VLOOKUP(G205,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_TSET"},"LAHU04F02_TSET AT%M756.0 :REAL; (*空调机组04F02-设定温度值*)","LAHU04F02_TSET          AT%M756.0      :REAL; (*空调机组04F02-设定温度值*)"]
["760.0","验证通过","INT","空调机组","L","04F02","季节模式","空调机组04F02-季节模式",{"$f":"E206&VLOOKUP(D206,list!$D$3:$F$501,2,FALSE)&F206&\"_\"&VLOOKUP(G206,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_SM"},"LAHU04F02_SM AT%M760.0 :INT; (*空调机组04F02-季节模式*)","LAHU04F02_SM            AT%M760.0      :INT; (*空调机组04F02-季节模式*)"]
["764.0","验证通过","REAL","空调机组","L","04F02","水阀反馈换算值","空调机组04F02-水阀反馈换算值",{"$f":"E207&VLOOKUP(D207,list!$D$3:$F$501,2,FALSE)&F207&\"_\"&VLOOKUP(G207,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_WVBS"},"LAHU04F02_WVBS AT%M764.0 :REAL; (*空调机组04F02-水阀反馈换算值*)","LAHU04F02_WVBS          AT%M764.0      :REAL; (*空调机组04F02-水阀反馈换算值*)"]
["768.0","验证通过","BOOL","空调机组","L","04F02","水阀手动控制","空调机组04F02-水阀手动控制",{"$f":"E208&VLOOKUP(D208,list!$D$3:$F$501,2,FALSE)&F208&\"_\"&VLOOKUP(G208,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_WVMC"},"LAHU04F02_WVMC AT%M768.0 :BOOL; (*空调机组04F02-水阀手动控制*)","LAHU04F02_WVMC          AT%M768.0      :BOOL; (*空调机组04F02-水阀手动控制*)"]
["772.0","验证通过","REAL","空调机组","L","04F02","水阀手动控制值","空调机组04F02-水阀手动控制值",{"$f":"E209&VLOOKUP(D209,list!$D$3:$F$501,2,FALSE)&F209&\"_\"&VLOOKUP(G209,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_WVMV"},"LAHU04F02_WVMV AT%M772.0 :REAL; (*空调机组04F02-水阀手动控制值*)","LAHU04F02_WVMV          AT%M772.0      :REAL; (*空调机组04F02-水阀手动控制值*)"]
["776.0","验证通过","REAL","空调机组","L","04F02","回风温度换算值","空调机组04F02-回风温度换算值",{"$f":"E210&VLOOKUP(D210,list!$D$3:$F$501,2,FALSE)&F210&\"_\"&VLOOKUP(G210,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_RTS"},"LAHU04F02_RTS AT%M776.0 :REAL; (*空调机组04F02-回风温度换算值*)","LAHU04F02_RTS           AT%M776.0      :REAL; (*空调机组04F02-回风温度换算值*)"]
["780.0","验证通过","BOOL","空调机组","L","04F02","运行时间累积重置","空调机组04F02-运行时间累积重置",{"$f":"E211&VLOOKUP(D211,list!$D$3:$F$501,2,FALSE)&F211&\"_\"&VLOOKUP(G211,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_RST"},"LAHU04F02_RST AT%M780.0 :BOOL; (*空调机组04F02-运行时间累积重置*)","LAHU04F02_RST           AT%M780.0      :BOOL; (*空调机组04F02-运行时间累积重置*)"]
["784.0","验证通过","REAL","空调机组","L","04F02","运行时间累积重置值","空调机组04F02-运行时间累积重置值",{"$f":"E212&VLOOKUP(D212,list!$D$3:$F$501,2,FALSE)&F212&\"_\"&VLOOKUP(G212,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_RSTV"},"LAHU04F02_RSTV AT%M784.0 :REAL; (*空调机组04F02-运行时间累积重置值*)","LAHU04F02_RSTV          AT%M784.0      :REAL; (*空调机组04F02-运行时间累积重置值*)"]
["788.0","验证通过","BOOL","空调机组","L","04F02","隔离开关1","空调机组04F02-隔离开关1",{"$f":"E213&VLOOKUP(D213,list!$D$3:$F$501,2,FALSE)&F213&\"_\"&VLOOKUP(G213,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_ISO1"},"LAHU04F02_ISO1 AT%M788.0 :BOOL; (*空调机组04F02-隔离开关1*)","LAHU04F02_ISO1          AT%M788.0      :BOOL; (*空调机组04F02-隔离开关1*)"]
["790.0","验证通过","BOOL","空调机组","L","04F02","隔离开关2","空调机组04F02-隔离开关2",{"$f":"E214&VLOOKUP(D214,list!$D$3:$F$501,2,FALSE)&F214&\"_\"&VLOOKUP(G214,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_ISO2"},"LAHU04F02_ISO2 AT%M790.0 :BOOL; (*空调机组04F02-隔离开关2*)","LAHU04F02_ISO2          AT%M790.0      :BOOL; (*空调机组04F02-隔离开关2*)"]
["796.0","验证通过","REAL","空调机组","L","04F02","P调节参数","空调机组04F02-P调节参数",{"$f":"E215&VLOOKUP(D215,list!$D$3:$F$501,2,FALSE)&F215&\"_\"&VLOOKUP(G215,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_VP"},"LAHU04F02_VP AT%M796.0 :REAL; (*空调机组04F02-P调节参数*)","LAHU04F02_VP            AT%M796.0      :REAL; (*空调机组04F02-P调节参数*)"]
["800.0","验证通过","REAL","空调机组","L","04F02","I调节参数","空调机组04F02-I调节参数",{"$f":"E216&VLOOKUP(D216,list!$D$3:$F$501,2,FALSE)&F216&\"_\"&VLOOKUP(G216,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_VI"},"LAHU04F02_VI AT%M800.0 :REAL; (*空调机组04F02-I调节参数*)","LAHU04F02_VI            AT%M800.0      :REAL; (*空调机组04F02-I调节参数*)"]
["804.0","验证通过","REAL","空调机组","L","04F02","运行时间累积值","空调机组04F02-运行时间累积值",{"$f":"E217&VLOOKUP(D217,list!$D$3:$F$501,2,FALSE)&F217&\"_\"&VLOOKUP(G217,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_RH"},"LAHU04F02_RH AT%M804.0 :REAL; (*空调机组04F02-运行时间累积值*)","LAHU04F02_RH            AT%M804.0      :REAL; (*空调机组04F02-运行时间累积值*)"]
["808.0","验证通过","INT","空调机组","L","04F02","设备状态代码","空调机组04F02-设备状态代码",{"$f":"E218&VLOOKUP(D218,list!$D$3:$F$501,2,FALSE)&F218&\"_\"&VLOOKUP(G218,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_SN"},"LAHU04F02_SN AT%M808.0 :INT; (*空调机组04F02-设备状态代码*)","LAHU04F02_SN            AT%M808.0      :INT; (*空调机组04F02-设备状态代码*)"]
["810.0","验证通过","INT","空调机组","L","04F02","水阀控制转换值","空调机组04F02-水阀控制转换值",{"$f":"E219&VLOOKUP(D219,list!$D$3:$F$501,2,FALSE)&F219&\"_\"&VLOOKUP(G219,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_WVCS"},"LAHU04F02_WVCS AT%M810.0 :INT; (*空调机组04F02-水阀控制转换值*)","LAHU04F02_WVCS          AT%M810.0      :INT; (*空调机组04F02-水阀控制转换值*)"]
["812.0","验证通过","BOOL","空调机组","L","04F02","程序控制","空调机组04F02-程序控制",{"$f":"E220&VLOOKUP(D220,list!$D$3:$F$501,2,FALSE)&F220&\"_\"&VLOOKUP(G220,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F02_PC"},"LAHU04F02_PC AT%M812.0 :BOOL; (*空调机组04F02-程序控制*)","LAHU04F02_PC            AT%M812.0      :BOOL; (*空调机组04F02-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C220=\"REAL\",C220=\"DWORD\",C220=\"DINT\"),(IF(OR(C222=\"REAL\",C222=\"DWORD\",C222=\"DINT\"),A220+4+MOD(A220,4),A220+4)),(IF(OR(C222=\"REAL\",C222=\"DWORD\",C222=\"DINT\"),A220+4+MOD(A220,4),A220+2)))&\".0\"","v":"816.0"},{"$f":"IF((IF(OR(C222=\"INT\",C222=\"WORD\",C222=\"BOOL\"),MOD(A222,2),MOD(A222,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F03","设定温度值",{"$f":"D222&F222&\"-\"&IF(E222=\"R\",\"新云平台\"&G222,G222)","v":"空调机组04F03-新云平台设定温度值"},{"$f":"E222&VLOOKUP(D222,list!$D$3:$F$501,2,FALSE)&F222&\"_\"&VLOOKUP(G222,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F03_TSET"},{"$f":"I222&\" \"&\"AT%M\"&A222&\" \"&\":\"&C222&\";\"&\" \"&\"(*\"&H222&\"*)\"","v":"RAHU04F03_TSET AT%M816.0 :REAL; (*空调机组04F03-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J222,SEARCH(\"AT%\",J222),,REPT(\" \",25-SEARCH(\"AT%\",J222))),SEARCH(\":\",REPLACE(J222,SEARCH(\"AT%\",J222),,REPT(\" \",25-SEARCH(\"AT%\",J222)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J222,SEARCH(\"AT%\",J222),,REPT(\" \",25-SEARCH(\"AT%\",J222))))))","v":"RAHU04F03_TSET          AT%M816.0      :REAL; (*空调机组04F03-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C222=\"REAL\",C222=\"DWORD\",C222=\"DINT\"),(IF(OR(C223=\"REAL\",C223=\"DWORD\",C223=\"DINT\"),A222+4+MOD(A222,4),A222+4)),(IF(OR(C223=\"REAL\",C223=\"DWORD\",C223=\"DINT\"),A222+4+MOD(A222,4),A222+2)))&\".0\"","v":"820.0"},"验证通过","INT","空调机组","R",{"$f":"F222","v":"04F03"},"季节模式","空调机组04F03-新云平台季节模式",{"$f":"E223&VLOOKUP(D223,list!$D$3:$F$501,2,FALSE)&F223&\"_\"&VLOOKUP(G223,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F03_SM"},"RAHU04F03_SM AT%M820.0 :INT; (*空调机组04F03-新云平台季节模式*)","RAHU04F03_SM            AT%M820.0      :INT; (*空调机组04F03-新云平台季节模式*)"]
["822.0","验证通过","BOOL","空调机组","R","04F03","程序控制","空调机组04F03-新云平台程序控制",{"$f":"E224&VLOOKUP(D224,list!$D$3:$F$501,2,FALSE)&F224&\"_\"&VLOOKUP(G224,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F03_PC"},"RAHU04F03_PC AT%M822.0 :BOOL; (*空调机组04F03-新云平台程序控制*)","RAHU04F03_PC            AT%M822.0      :BOOL; (*空调机组04F03-新云平台程序控制*)"]
["828.0","验证通过","REAL","空调机组","L","04F03","设定温度值","空调机组04F03-设定温度值",{"$f":"E225&VLOOKUP(D225,list!$D$3:$F$501,2,FALSE)&F225&\"_\"&VLOOKUP(G225,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_TSET"},"LAHU04F03_TSET AT%M828.0 :REAL; (*空调机组04F03-设定温度值*)","LAHU04F03_TSET          AT%M828.0      :REAL; (*空调机组04F03-设定温度值*)"]
["832.0","验证通过","INT","空调机组","L","04F03","季节模式","空调机组04F03-季节模式",{"$f":"E226&VLOOKUP(D226,list!$D$3:$F$501,2,FALSE)&F226&\"_\"&VLOOKUP(G226,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_SM"},"LAHU04F03_SM AT%M832.0 :INT; (*空调机组04F03-季节模式*)","LAHU04F03_SM            AT%M832.0      :INT; (*空调机组04F03-季节模式*)"]
["836.0","验证通过","REAL","空调机组","L","04F03","水阀反馈换算值","空调机组04F03-水阀反馈换算值",{"$f":"E227&VLOOKUP(D227,list!$D$3:$F$501,2,FALSE)&F227&\"_\"&VLOOKUP(G227,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_WVBS"},"LAHU04F03_WVBS AT%M836.0 :REAL; (*空调机组04F03-水阀反馈换算值*)","LAHU04F03_WVBS          AT%M836.0      :REAL; (*空调机组04F03-水阀反馈换算值*)"]
["840.0","验证通过","BOOL","空调机组","L","04F03","水阀手动控制","空调机组04F03-水阀手动控制",{"$f":"E228&VLOOKUP(D228,list!$D$3:$F$501,2,FALSE)&F228&\"_\"&VLOOKUP(G228,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_WVMC"},"LAHU04F03_WVMC AT%M840.0 :BOOL; (*空调机组04F03-水阀手动控制*)","LAHU04F03_WVMC          AT%M840.0      :BOOL; (*空调机组04F03-水阀手动控制*)"]
["844.0","验证通过","REAL","空调机组","L","04F03","水阀手动控制值","空调机组04F03-水阀手动控制值",{"$f":"E229&VLOOKUP(D229,list!$D$3:$F$501,2,FALSE)&F229&\"_\"&VLOOKUP(G229,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_WVMV"},"LAHU04F03_WVMV AT%M844.0 :REAL; (*空调机组04F03-水阀手动控制值*)","LAHU04F03_WVMV          AT%M844.0      :REAL; (*空调机组04F03-水阀手动控制值*)"]
["848.0","验证通过","REAL","空调机组","L","04F03","回风温度换算值","空调机组04F03-回风温度换算值",{"$f":"E230&VLOOKUP(D230,list!$D$3:$F$501,2,FALSE)&F230&\"_\"&VLOOKUP(G230,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_RTS"},"LAHU04F03_RTS AT%M848.0 :REAL; (*空调机组04F03-回风温度换算值*)","LAHU04F03_RTS           AT%M848.0      :REAL; (*空调机组04F03-回风温度换算值*)"]
["852.0","验证通过","BOOL","空调机组","L","04F03","运行时间累积重置","空调机组04F03-运行时间累积重置",{"$f":"E231&VLOOKUP(D231,list!$D$3:$F$501,2,FALSE)&F231&\"_\"&VLOOKUP(G231,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_RST"},"LAHU04F03_RST AT%M852.0 :BOOL; (*空调机组04F03-运行时间累积重置*)","LAHU04F03_RST           AT%M852.0      :BOOL; (*空调机组04F03-运行时间累积重置*)"]
["856.0","验证通过","REAL","空调机组","L","04F03","运行时间累积重置值","空调机组04F03-运行时间累积重置值",{"$f":"E232&VLOOKUP(D232,list!$D$3:$F$501,2,FALSE)&F232&\"_\"&VLOOKUP(G232,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_RSTV"},"LAHU04F03_RSTV AT%M856.0 :REAL; (*空调机组04F03-运行时间累积重置值*)","LAHU04F03_RSTV          AT%M856.0      :REAL; (*空调机组04F03-运行时间累积重置值*)"]
["860.0","验证通过","BOOL","空调机组","L","04F03","隔离开关1","空调机组04F03-隔离开关1",{"$f":"E233&VLOOKUP(D233,list!$D$3:$F$501,2,FALSE)&F233&\"_\"&VLOOKUP(G233,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_ISO1"},"LAHU04F03_ISO1 AT%M860.0 :BOOL; (*空调机组04F03-隔离开关1*)","LAHU04F03_ISO1          AT%M860.0      :BOOL; (*空调机组04F03-隔离开关1*)"]
["862.0","验证通过","BOOL","空调机组","L","04F03","隔离开关2","空调机组04F03-隔离开关2",{"$f":"E234&VLOOKUP(D234,list!$D$3:$F$501,2,FALSE)&F234&\"_\"&VLOOKUP(G234,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_ISO2"},"LAHU04F03_ISO2 AT%M862.0 :BOOL; (*空调机组04F03-隔离开关2*)","LAHU04F03_ISO2          AT%M862.0      :BOOL; (*空调机组04F03-隔离开关2*)"]
["868.0","验证通过","REAL","空调机组","L","04F03","P调节参数","空调机组04F03-P调节参数",{"$f":"E235&VLOOKUP(D235,list!$D$3:$F$501,2,FALSE)&F235&\"_\"&VLOOKUP(G235,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_VP"},"LAHU04F03_VP AT%M868.0 :REAL; (*空调机组04F03-P调节参数*)","LAHU04F03_VP            AT%M868.0      :REAL; (*空调机组04F03-P调节参数*)"]
["872.0","验证通过","REAL","空调机组","L","04F03","I调节参数","空调机组04F03-I调节参数",{"$f":"E236&VLOOKUP(D236,list!$D$3:$F$501,2,FALSE)&F236&\"_\"&VLOOKUP(G236,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_VI"},"LAHU04F03_VI AT%M872.0 :REAL; (*空调机组04F03-I调节参数*)","LAHU04F03_VI            AT%M872.0      :REAL; (*空调机组04F03-I调节参数*)"]
["876.0","验证通过","REAL","空调机组","L","04F03","运行时间累积值","空调机组04F03-运行时间累积值",{"$f":"E237&VLOOKUP(D237,list!$D$3:$F$501,2,FALSE)&F237&\"_\"&VLOOKUP(G237,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_RH"},"LAHU04F03_RH AT%M876.0 :REAL; (*空调机组04F03-运行时间累积值*)","LAHU04F03_RH            AT%M876.0      :REAL; (*空调机组04F03-运行时间累积值*)"]
["880.0","验证通过","INT","空调机组","L","04F03","设备状态代码","空调机组04F03-设备状态代码",{"$f":"E238&VLOOKUP(D238,list!$D$3:$F$501,2,FALSE)&F238&\"_\"&VLOOKUP(G238,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_SN"},"LAHU04F03_SN AT%M880.0 :INT; (*空调机组04F03-设备状态代码*)","LAHU04F03_SN            AT%M880.0      :INT; (*空调机组04F03-设备状态代码*)"]
["882.0","验证通过","INT","空调机组","L","04F03","水阀控制转换值","空调机组04F03-水阀控制转换值",{"$f":"E239&VLOOKUP(D239,list!$D$3:$F$501,2,FALSE)&F239&\"_\"&VLOOKUP(G239,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_WVCS"},"LAHU04F03_WVCS AT%M882.0 :INT; (*空调机组04F03-水阀控制转换值*)","LAHU04F03_WVCS          AT%M882.0      :INT; (*空调机组04F03-水阀控制转换值*)"]
["884.0","验证通过","BOOL","空调机组","L","04F03","程序控制","空调机组04F03-程序控制",{"$f":"E240&VLOOKUP(D240,list!$D$3:$F$501,2,FALSE)&F240&\"_\"&VLOOKUP(G240,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F03_PC"},"LAHU04F03_PC AT%M884.0 :BOOL; (*空调机组04F03-程序控制*)","LAHU04F03_PC            AT%M884.0      :BOOL; (*空调机组04F03-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C240=\"REAL\",C240=\"DWORD\",C240=\"DINT\"),(IF(OR(C242=\"REAL\",C242=\"DWORD\",C242=\"DINT\"),A240+4+MOD(A240,4),A240+4)),(IF(OR(C242=\"REAL\",C242=\"DWORD\",C242=\"DINT\"),A240+4+MOD(A240,4),A240+2)))&\".0\"","v":"888.0"},{"$f":"IF((IF(OR(C242=\"INT\",C242=\"WORD\",C242=\"BOOL\"),MOD(A242,2),MOD(A242,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F04","设定温度值",{"$f":"D242&F242&\"-\"&IF(E242=\"R\",\"新云平台\"&G242,G242)","v":"空调机组04F04-新云平台设定温度值"},{"$f":"E242&VLOOKUP(D242,list!$D$3:$F$501,2,FALSE)&F242&\"_\"&VLOOKUP(G242,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F04_TSET"},{"$f":"I242&\" \"&\"AT%M\"&A242&\" \"&\":\"&C242&\";\"&\" \"&\"(*\"&H242&\"*)\"","v":"RAHU04F04_TSET AT%M888.0 :REAL; (*空调机组04F04-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J242,SEARCH(\"AT%\",J242),,REPT(\" \",25-SEARCH(\"AT%\",J242))),SEARCH(\":\",REPLACE(J242,SEARCH(\"AT%\",J242),,REPT(\" \",25-SEARCH(\"AT%\",J242)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J242,SEARCH(\"AT%\",J242),,REPT(\" \",25-SEARCH(\"AT%\",J242))))))","v":"RAHU04F04_TSET          AT%M888.0      :REAL; (*空调机组04F04-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C242=\"REAL\",C242=\"DWORD\",C242=\"DINT\"),(IF(OR(C243=\"REAL\",C243=\"DWORD\",C243=\"DINT\"),A242+4+MOD(A242,4),A242+4)),(IF(OR(C243=\"REAL\",C243=\"DWORD\",C243=\"DINT\"),A242+4+MOD(A242,4),A242+2)))&\".0\"","v":"892.0"},"验证通过","INT","空调机组","R",{"$f":"F242","v":"04F04"},"季节模式","空调机组04F04-新云平台季节模式",{"$f":"E243&VLOOKUP(D243,list!$D$3:$F$501,2,FALSE)&F243&\"_\"&VLOOKUP(G243,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F04_SM"},"RAHU04F04_SM AT%M892.0 :INT; (*空调机组04F04-新云平台季节模式*)","RAHU04F04_SM            AT%M892.0      :INT; (*空调机组04F04-新云平台季节模式*)"]
["894.0","验证通过","BOOL","空调机组","R","04F04","程序控制","空调机组04F04-新云平台程序控制",{"$f":"E244&VLOOKUP(D244,list!$D$3:$F$501,2,FALSE)&F244&\"_\"&VLOOKUP(G244,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F04_PC"},"RAHU04F04_PC AT%M894.0 :BOOL; (*空调机组04F04-新云平台程序控制*)","RAHU04F04_PC            AT%M894.0      :BOOL; (*空调机组04F04-新云平台程序控制*)"]
["900.0","验证通过","REAL","空调机组","L","04F04","设定温度值","空调机组04F04-设定温度值",{"$f":"E245&VLOOKUP(D245,list!$D$3:$F$501,2,FALSE)&F245&\"_\"&VLOOKUP(G245,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_TSET"},"LAHU04F04_TSET AT%M900.0 :REAL; (*空调机组04F04-设定温度值*)","LAHU04F04_TSET          AT%M900.0      :REAL; (*空调机组04F04-设定温度值*)"]
["904.0","验证通过","INT","空调机组","L","04F04","季节模式","空调机组04F04-季节模式",{"$f":"E246&VLOOKUP(D246,list!$D$3:$F$501,2,FALSE)&F246&\"_\"&VLOOKUP(G246,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_SM"},"LAHU04F04_SM AT%M904.0 :INT; (*空调机组04F04-季节模式*)","LAHU04F04_SM            AT%M904.0      :INT; (*空调机组04F04-季节模式*)"]
["908.0","验证通过","REAL","空调机组","L","04F04","水阀反馈换算值","空调机组04F04-水阀反馈换算值",{"$f":"E247&VLOOKUP(D247,list!$D$3:$F$501,2,FALSE)&F247&\"_\"&VLOOKUP(G247,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_WVBS"},"LAHU04F04_WVBS AT%M908.0 :REAL; (*空调机组04F04-水阀反馈换算值*)","LAHU04F04_WVBS          AT%M908.0      :REAL; (*空调机组04F04-水阀反馈换算值*)"]
["912.0","验证通过","BOOL","空调机组","L","04F04","水阀手动控制","空调机组04F04-水阀手动控制",{"$f":"E248&VLOOKUP(D248,list!$D$3:$F$501,2,FALSE)&F248&\"_\"&VLOOKUP(G248,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_WVMC"},"LAHU04F04_WVMC AT%M912.0 :BOOL; (*空调机组04F04-水阀手动控制*)","LAHU04F04_WVMC          AT%M912.0      :BOOL; (*空调机组04F04-水阀手动控制*)"]
["916.0","验证通过","REAL","空调机组","L","04F04","水阀手动控制值","空调机组04F04-水阀手动控制值",{"$f":"E249&VLOOKUP(D249,list!$D$3:$F$501,2,FALSE)&F249&\"_\"&VLOOKUP(G249,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_WVMV"},"LAHU04F04_WVMV AT%M916.0 :REAL; (*空调机组04F04-水阀手动控制值*)","LAHU04F04_WVMV          AT%M916.0      :REAL; (*空调机组04F04-水阀手动控制值*)"]
["920.0","验证通过","REAL","空调机组","L","04F04","回风温度换算值","空调机组04F04-回风温度换算值",{"$f":"E250&VLOOKUP(D250,list!$D$3:$F$501,2,FALSE)&F250&\"_\"&VLOOKUP(G250,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_RTS"},"LAHU04F04_RTS AT%M920.0 :REAL; (*空调机组04F04-回风温度换算值*)","LAHU04F04_RTS           AT%M920.0      :REAL; (*空调机组04F04-回风温度换算值*)"]
["924.0","验证通过","BOOL","空调机组","L","04F04","运行时间累积重置","空调机组04F04-运行时间累积重置",{"$f":"E251&VLOOKUP(D251,list!$D$3:$F$501,2,FALSE)&F251&\"_\"&VLOOKUP(G251,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_RST"},"LAHU04F04_RST AT%M924.0 :BOOL; (*空调机组04F04-运行时间累积重置*)","LAHU04F04_RST           AT%M924.0      :BOOL; (*空调机组04F04-运行时间累积重置*)"]
["928.0","验证通过","REAL","空调机组","L","04F04","运行时间累积重置值","空调机组04F04-运行时间累积重置值",{"$f":"E252&VLOOKUP(D252,list!$D$3:$F$501,2,FALSE)&F252&\"_\"&VLOOKUP(G252,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_RSTV"},"LAHU04F04_RSTV AT%M928.0 :REAL; (*空调机组04F04-运行时间累积重置值*)","LAHU04F04_RSTV          AT%M928.0      :REAL; (*空调机组04F04-运行时间累积重置值*)"]
["932.0","验证通过","BOOL","空调机组","L","04F04","隔离开关1","空调机组04F04-隔离开关1",{"$f":"E253&VLOOKUP(D253,list!$D$3:$F$501,2,FALSE)&F253&\"_\"&VLOOKUP(G253,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_ISO1"},"LAHU04F04_ISO1 AT%M932.0 :BOOL; (*空调机组04F04-隔离开关1*)","LAHU04F04_ISO1          AT%M932.0      :BOOL; (*空调机组04F04-隔离开关1*)"]
["934.0","验证通过","BOOL","空调机组","L","04F04","隔离开关2","空调机组04F04-隔离开关2",{"$f":"E254&VLOOKUP(D254,list!$D$3:$F$501,2,FALSE)&F254&\"_\"&VLOOKUP(G254,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_ISO2"},"LAHU04F04_ISO2 AT%M934.0 :BOOL; (*空调机组04F04-隔离开关2*)","LAHU04F04_ISO2          AT%M934.0      :BOOL; (*空调机组04F04-隔离开关2*)"]
["940.0","验证通过","REAL","空调机组","L","04F04","P调节参数","空调机组04F04-P调节参数",{"$f":"E255&VLOOKUP(D255,list!$D$3:$F$501,2,FALSE)&F255&\"_\"&VLOOKUP(G255,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_VP"},"LAHU04F04_VP AT%M940.0 :REAL; (*空调机组04F04-P调节参数*)","LAHU04F04_VP            AT%M940.0      :REAL; (*空调机组04F04-P调节参数*)"]
["944.0","验证通过","REAL","空调机组","L","04F04","I调节参数","空调机组04F04-I调节参数",{"$f":"E256&VLOOKUP(D256,list!$D$3:$F$501,2,FALSE)&F256&\"_\"&VLOOKUP(G256,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_VI"},"LAHU04F04_VI AT%M944.0 :REAL; (*空调机组04F04-I调节参数*)","LAHU04F04_VI            AT%M944.0      :REAL; (*空调机组04F04-I调节参数*)"]
["948.0","验证通过","REAL","空调机组","L","04F04","运行时间累积值","空调机组04F04-运行时间累积值",{"$f":"E257&VLOOKUP(D257,list!$D$3:$F$501,2,FALSE)&F257&\"_\"&VLOOKUP(G257,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_RH"},"LAHU04F04_RH AT%M948.0 :REAL; (*空调机组04F04-运行时间累积值*)","LAHU04F04_RH            AT%M948.0      :REAL; (*空调机组04F04-运行时间累积值*)"]
["952.0","验证通过","INT","空调机组","L","04F04","设备状态代码","空调机组04F04-设备状态代码",{"$f":"E258&VLOOKUP(D258,list!$D$3:$F$501,2,FALSE)&F258&\"_\"&VLOOKUP(G258,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_SN"},"LAHU04F04_SN AT%M952.0 :INT; (*空调机组04F04-设备状态代码*)","LAHU04F04_SN            AT%M952.0      :INT; (*空调机组04F04-设备状态代码*)"]
["954.0","验证通过","INT","空调机组","L","04F04","水阀控制转换值","空调机组04F04-水阀控制转换值",{"$f":"E259&VLOOKUP(D259,list!$D$3:$F$501,2,FALSE)&F259&\"_\"&VLOOKUP(G259,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_WVCS"},"LAHU04F04_WVCS AT%M954.0 :INT; (*空调机组04F04-水阀控制转换值*)","LAHU04F04_WVCS          AT%M954.0      :INT; (*空调机组04F04-水阀控制转换值*)"]
["956.0","验证通过","BOOL","空调机组","L","04F04","程序控制","空调机组04F04-程序控制",{"$f":"E260&VLOOKUP(D260,list!$D$3:$F$501,2,FALSE)&F260&\"_\"&VLOOKUP(G260,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F04_PC"},"LAHU04F04_PC AT%M956.0 :BOOL; (*空调机组04F04-程序控制*)","LAHU04F04_PC            AT%M956.0      :BOOL; (*空调机组04F04-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C260=\"REAL\",C260=\"DWORD\",C260=\"DINT\"),(IF(OR(C262=\"REAL\",C262=\"DWORD\",C262=\"DINT\"),A260+4+MOD(A260,4),A260+4)),(IF(OR(C262=\"REAL\",C262=\"DWORD\",C262=\"DINT\"),A260+4+MOD(A260,4),A260+2)))&\".0\"","v":"960.0"},{"$f":"IF((IF(OR(C262=\"INT\",C262=\"WORD\",C262=\"BOOL\"),MOD(A262,2),MOD(A262,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F05","设定温度值",{"$f":"D262&F262&\"-\"&IF(E262=\"R\",\"新云平台\"&G262,G262)","v":"空调机组04F05-新云平台设定温度值"},{"$f":"E262&VLOOKUP(D262,list!$D$3:$F$501,2,FALSE)&F262&\"_\"&VLOOKUP(G262,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F05_TSET"},{"$f":"I262&\" \"&\"AT%M\"&A262&\" \"&\":\"&C262&\";\"&\" \"&\"(*\"&H262&\"*)\"","v":"RAHU04F05_TSET AT%M960.0 :REAL; (*空调机组04F05-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J262,SEARCH(\"AT%\",J262),,REPT(\" \",25-SEARCH(\"AT%\",J262))),SEARCH(\":\",REPLACE(J262,SEARCH(\"AT%\",J262),,REPT(\" \",25-SEARCH(\"AT%\",J262)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J262,SEARCH(\"AT%\",J262),,REPT(\" \",25-SEARCH(\"AT%\",J262))))))","v":"RAHU04F05_TSET          AT%M960.0      :REAL; (*空调机组04F05-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C262=\"REAL\",C262=\"DWORD\",C262=\"DINT\"),(IF(OR(C263=\"REAL\",C263=\"DWORD\",C263=\"DINT\"),A262+4+MOD(A262,4),A262+4)),(IF(OR(C263=\"REAL\",C263=\"DWORD\",C263=\"DINT\"),A262+4+MOD(A262,4),A262+2)))&\".0\"","v":"964.0"},"验证通过","INT","空调机组","R",{"$f":"F262","v":"04F05"},"季节模式","空调机组04F05-新云平台季节模式",{"$f":"E263&VLOOKUP(D263,list!$D$3:$F$501,2,FALSE)&F263&\"_\"&VLOOKUP(G263,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F05_SM"},"RAHU04F05_SM AT%M964.0 :INT; (*空调机组04F05-新云平台季节模式*)","RAHU04F05_SM            AT%M964.0      :INT; (*空调机组04F05-新云平台季节模式*)"]
["966.0","验证通过","BOOL","空调机组","R","04F05","程序控制","空调机组04F05-新云平台程序控制",{"$f":"E264&VLOOKUP(D264,list!$D$3:$F$501,2,FALSE)&F264&\"_\"&VLOOKUP(G264,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F05_PC"},"RAHU04F05_PC AT%M966.0 :BOOL; (*空调机组04F05-新云平台程序控制*)","RAHU04F05_PC            AT%M966.0      :BOOL; (*空调机组04F05-新云平台程序控制*)"]
["972.0","验证通过","REAL","空调机组","L","04F05","设定温度值","空调机组04F05-设定温度值",{"$f":"E265&VLOOKUP(D265,list!$D$3:$F$501,2,FALSE)&F265&\"_\"&VLOOKUP(G265,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_TSET"},"LAHU04F05_TSET AT%M972.0 :REAL; (*空调机组04F05-设定温度值*)","LAHU04F05_TSET          AT%M972.0      :REAL; (*空调机组04F05-设定温度值*)"]
["976.0","验证通过","INT","空调机组","L","04F05","季节模式","空调机组04F05-季节模式",{"$f":"E266&VLOOKUP(D266,list!$D$3:$F$501,2,FALSE)&F266&\"_\"&VLOOKUP(G266,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_SM"},"LAHU04F05_SM AT%M976.0 :INT; (*空调机组04F05-季节模式*)","LAHU04F05_SM            AT%M976.0      :INT; (*空调机组04F05-季节模式*)"]
["980.0","验证通过","REAL","空调机组","L","04F05","水阀反馈换算值","空调机组04F05-水阀反馈换算值",{"$f":"E267&VLOOKUP(D267,list!$D$3:$F$501,2,FALSE)&F267&\"_\"&VLOOKUP(G267,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_WVBS"},"LAHU04F05_WVBS AT%M980.0 :REAL; (*空调机组04F05-水阀反馈换算值*)","LAHU04F05_WVBS          AT%M980.0      :REAL; (*空调机组04F05-水阀反馈换算值*)"]
["984.0","验证通过","BOOL","空调机组","L","04F05","水阀手动控制","空调机组04F05-水阀手动控制",{"$f":"E268&VLOOKUP(D268,list!$D$3:$F$501,2,FALSE)&F268&\"_\"&VLOOKUP(G268,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_WVMC"},"LAHU04F05_WVMC AT%M984.0 :BOOL; (*空调机组04F05-水阀手动控制*)","LAHU04F05_WVMC          AT%M984.0      :BOOL; (*空调机组04F05-水阀手动控制*)"]
["988.0","验证通过","REAL","空调机组","L","04F05","水阀手动控制值","空调机组04F05-水阀手动控制值",{"$f":"E269&VLOOKUP(D269,list!$D$3:$F$501,2,FALSE)&F269&\"_\"&VLOOKUP(G269,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_WVMV"},"LAHU04F05_WVMV AT%M988.0 :REAL; (*空调机组04F05-水阀手动控制值*)","LAHU04F05_WVMV          AT%M988.0      :REAL; (*空调机组04F05-水阀手动控制值*)"]
["992.0","验证通过","REAL","空调机组","L","04F05","回风温度换算值","空调机组04F05-回风温度换算值",{"$f":"E270&VLOOKUP(D270,list!$D$3:$F$501,2,FALSE)&F270&\"_\"&VLOOKUP(G270,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_RTS"},"LAHU04F05_RTS AT%M992.0 :REAL; (*空调机组04F05-回风温度换算值*)","LAHU04F05_RTS           AT%M992.0      :REAL; (*空调机组04F05-回风温度换算值*)"]
["996.0","验证通过","BOOL","空调机组","L","04F05","运行时间累积重置","空调机组04F05-运行时间累积重置",{"$f":"E271&VLOOKUP(D271,list!$D$3:$F$501,2,FALSE)&F271&\"_\"&VLOOKUP(G271,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_RST"},"LAHU04F05_RST AT%M996.0 :BOOL; (*空调机组04F05-运行时间累积重置*)","LAHU04F05_RST           AT%M996.0      :BOOL; (*空调机组04F05-运行时间累积重置*)"]
["1000.0","验证通过","REAL","空调机组","L","04F05","运行时间累积重置值","空调机组04F05-运行时间累积重置值",{"$f":"E272&VLOOKUP(D272,list!$D$3:$F$501,2,FALSE)&F272&\"_\"&VLOOKUP(G272,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_RSTV"},"LAHU04F05_RSTV AT%M1000.0 :REAL; (*空调机组04F05-运行时间累积重置值*)","LAHU04F05_RSTV          AT%M1000.0     :REAL; (*空调机组04F05-运行时间累积重置值*)"]
["1004.0","验证通过","BOOL","空调机组","L","04F05","隔离开关1","空调机组04F05-隔离开关1",{"$f":"E273&VLOOKUP(D273,list!$D$3:$F$501,2,FALSE)&F273&\"_\"&VLOOKUP(G273,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_ISO1"},"LAHU04F05_ISO1 AT%M1004.0 :BOOL; (*空调机组04F05-隔离开关1*)","LAHU04F05_ISO1          AT%M1004.0     :BOOL; (*空调机组04F05-隔离开关1*)"]
["1006.0","验证通过","BOOL","空调机组","L","04F05","隔离开关2","空调机组04F05-隔离开关2",{"$f":"E274&VLOOKUP(D274,list!$D$3:$F$501,2,FALSE)&F274&\"_\"&VLOOKUP(G274,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_ISO2"},"LAHU04F05_ISO2 AT%M1006.0 :BOOL; (*空调机组04F05-隔离开关2*)","LAHU04F05_ISO2          AT%M1006.0     :BOOL; (*空调机组04F05-隔离开关2*)"]
["1012.0","验证通过","REAL","空调机组","L","04F05","P调节参数","空调机组04F05-P调节参数",{"$f":"E275&VLOOKUP(D275,list!$D$3:$F$501,2,FALSE)&F275&\"_\"&VLOOKUP(G275,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_VP"},"LAHU04F05_VP AT%M1012.0 :REAL; (*空调机组04F05-P调节参数*)","LAHU04F05_VP            AT%M1012.0     :REAL; (*空调机组04F05-P调节参数*)"]
["1016.0","验证通过","REAL","空调机组","L","04F05","I调节参数","空调机组04F05-I调节参数",{"$f":"E276&VLOOKUP(D276,list!$D$3:$F$501,2,FALSE)&F276&\"_\"&VLOOKUP(G276,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_VI"},"LAHU04F05_VI AT%M1016.0 :REAL; (*空调机组04F05-I调节参数*)","LAHU04F05_VI            AT%M1016.0     :REAL; (*空调机组04F05-I调节参数*)"]
["1020.0","验证通过","REAL","空调机组","L","04F05","运行时间累积值","空调机组04F05-运行时间累积值",{"$f":"E277&VLOOKUP(D277,list!$D$3:$F$501,2,FALSE)&F277&\"_\"&VLOOKUP(G277,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_RH"},"LAHU04F05_RH AT%M1020.0 :REAL; (*空调机组04F05-运行时间累积值*)","LAHU04F05_RH            AT%M1020.0     :REAL; (*空调机组04F05-运行时间累积值*)"]
["1024.0","验证通过","INT","空调机组","L","04F05","设备状态代码","空调机组04F05-设备状态代码",{"$f":"E278&VLOOKUP(D278,list!$D$3:$F$501,2,FALSE)&F278&\"_\"&VLOOKUP(G278,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_SN"},"LAHU04F05_SN AT%M1024.0 :INT; (*空调机组04F05-设备状态代码*)","LAHU04F05_SN            AT%M1024.0     :INT; (*空调机组04F05-设备状态代码*)"]
["1026.0","验证通过","INT","空调机组","L","04F05","水阀控制转换值","空调机组04F05-水阀控制转换值",{"$f":"E279&VLOOKUP(D279,list!$D$3:$F$501,2,FALSE)&F279&\"_\"&VLOOKUP(G279,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_WVCS"},"LAHU04F05_WVCS AT%M1026.0 :INT; (*空调机组04F05-水阀控制转换值*)","LAHU04F05_WVCS          AT%M1026.0     :INT; (*空调机组04F05-水阀控制转换值*)"]
["1028.0","验证通过","BOOL","空调机组","L","04F05","程序控制","空调机组04F05-程序控制",{"$f":"E280&VLOOKUP(D280,list!$D$3:$F$501,2,FALSE)&F280&\"_\"&VLOOKUP(G280,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F05_PC"},"LAHU04F05_PC AT%M1028.0 :BOOL; (*空调机组04F05-程序控制*)","LAHU04F05_PC            AT%M1028.0     :BOOL; (*空调机组04F05-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C280=\"REAL\",C280=\"DWORD\",C280=\"DINT\"),(IF(OR(C282=\"REAL\",C282=\"DWORD\",C282=\"DINT\"),A280+4+MOD(A280,4),A280+4)),(IF(OR(C282=\"REAL\",C282=\"DWORD\",C282=\"DINT\"),A280+4+MOD(A280,4),A280+2)))&\".0\"","v":"1032.0"},{"$f":"IF((IF(OR(C282=\"INT\",C282=\"WORD\",C282=\"BOOL\"),MOD(A282,2),MOD(A282,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F06","设定温度值",{"$f":"D282&F282&\"-\"&IF(E282=\"R\",\"新云平台\"&G282,G282)","v":"空调机组04F06-新云平台设定温度值"},{"$f":"E282&VLOOKUP(D282,list!$D$3:$F$501,2,FALSE)&F282&\"_\"&VLOOKUP(G282,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F06_TSET"},{"$f":"I282&\" \"&\"AT%M\"&A282&\" \"&\":\"&C282&\";\"&\" \"&\"(*\"&H282&\"*)\"","v":"RAHU04F06_TSET AT%M1032.0 :REAL; (*空调机组04F06-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J282,SEARCH(\"AT%\",J282),,REPT(\" \",25-SEARCH(\"AT%\",J282))),SEARCH(\":\",REPLACE(J282,SEARCH(\"AT%\",J282),,REPT(\" \",25-SEARCH(\"AT%\",J282)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J282,SEARCH(\"AT%\",J282),,REPT(\" \",25-SEARCH(\"AT%\",J282))))))","v":"RAHU04F06_TSET          AT%M1032.0     :REAL; (*空调机组04F06-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C282=\"REAL\",C282=\"DWORD\",C282=\"DINT\"),(IF(OR(C283=\"REAL\",C283=\"DWORD\",C283=\"DINT\"),A282+4+MOD(A282,4),A282+4)),(IF(OR(C283=\"REAL\",C283=\"DWORD\",C283=\"DINT\"),A282+4+MOD(A282,4),A282+2)))&\".0\"","v":"1036.0"},"验证通过","INT","空调机组","R",{"$f":"F282","v":"04F06"},"季节模式","空调机组04F06-新云平台季节模式",{"$f":"E283&VLOOKUP(D283,list!$D$3:$F$501,2,FALSE)&F283&\"_\"&VLOOKUP(G283,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F06_SM"},"RAHU04F06_SM AT%M1036.0 :INT; (*空调机组04F06-新云平台季节模式*)","RAHU04F06_SM            AT%M1036.0     :INT; (*空调机组04F06-新云平台季节模式*)"]
["1038.0","验证通过","BOOL","空调机组","R","04F06","程序控制","空调机组04F06-新云平台程序控制",{"$f":"E284&VLOOKUP(D284,list!$D$3:$F$501,2,FALSE)&F284&\"_\"&VLOOKUP(G284,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F06_PC"},"RAHU04F06_PC AT%M1038.0 :BOOL; (*空调机组04F06-新云平台程序控制*)","RAHU04F06_PC            AT%M1038.0     :BOOL; (*空调机组04F06-新云平台程序控制*)"]
["1044.0","验证通过","REAL","空调机组","L","04F06","设定温度值","空调机组04F06-设定温度值",{"$f":"E285&VLOOKUP(D285,list!$D$3:$F$501,2,FALSE)&F285&\"_\"&VLOOKUP(G285,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_TSET"},"LAHU04F06_TSET AT%M1044.0 :REAL; (*空调机组04F06-设定温度值*)","LAHU04F06_TSET          AT%M1044.0     :REAL; (*空调机组04F06-设定温度值*)"]
["1048.0","验证通过","INT","空调机组","L","04F06","季节模式","空调机组04F06-季节模式",{"$f":"E286&VLOOKUP(D286,list!$D$3:$F$501,2,FALSE)&F286&\"_\"&VLOOKUP(G286,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_SM"},"LAHU04F06_SM AT%M1048.0 :INT; (*空调机组04F06-季节模式*)","LAHU04F06_SM            AT%M1048.0     :INT; (*空调机组04F06-季节模式*)"]
["1052.0","验证通过","REAL","空调机组","L","04F06","水阀反馈换算值","空调机组04F06-水阀反馈换算值",{"$f":"E287&VLOOKUP(D287,list!$D$3:$F$501,2,FALSE)&F287&\"_\"&VLOOKUP(G287,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_WVBS"},"LAHU04F06_WVBS AT%M1052.0 :REAL; (*空调机组04F06-水阀反馈换算值*)","LAHU04F06_WVBS          AT%M1052.0     :REAL; (*空调机组04F06-水阀反馈换算值*)"]
["1056.0","验证通过","BOOL","空调机组","L","04F06","水阀手动控制","空调机组04F06-水阀手动控制",{"$f":"E288&VLOOKUP(D288,list!$D$3:$F$501,2,FALSE)&F288&\"_\"&VLOOKUP(G288,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_WVMC"},"LAHU04F06_WVMC AT%M1056.0 :BOOL; (*空调机组04F06-水阀手动控制*)","LAHU04F06_WVMC          AT%M1056.0     :BOOL; (*空调机组04F06-水阀手动控制*)"]
["1060.0","验证通过","REAL","空调机组","L","04F06","水阀手动控制值","空调机组04F06-水阀手动控制值",{"$f":"E289&VLOOKUP(D289,list!$D$3:$F$501,2,FALSE)&F289&\"_\"&VLOOKUP(G289,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_WVMV"},"LAHU04F06_WVMV AT%M1060.0 :REAL; (*空调机组04F06-水阀手动控制值*)","LAHU04F06_WVMV          AT%M1060.0     :REAL; (*空调机组04F06-水阀手动控制值*)"]
["1064.0","验证通过","REAL","空调机组","L","04F06","回风温度换算值","空调机组04F06-回风温度换算值",{"$f":"E290&VLOOKUP(D290,list!$D$3:$F$501,2,FALSE)&F290&\"_\"&VLOOKUP(G290,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_RTS"},"LAHU04F06_RTS AT%M1064.0 :REAL; (*空调机组04F06-回风温度换算值*)","LAHU04F06_RTS           AT%M1064.0     :REAL; (*空调机组04F06-回风温度换算值*)"]
["1068.0","验证通过","BOOL","空调机组","L","04F06","运行时间累积重置","空调机组04F06-运行时间累积重置",{"$f":"E291&VLOOKUP(D291,list!$D$3:$F$501,2,FALSE)&F291&\"_\"&VLOOKUP(G291,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_RST"},"LAHU04F06_RST AT%M1068.0 :BOOL; (*空调机组04F06-运行时间累积重置*)","LAHU04F06_RST           AT%M1068.0     :BOOL; (*空调机组04F06-运行时间累积重置*)"]
["1072.0","验证通过","REAL","空调机组","L","04F06","运行时间累积重置值","空调机组04F06-运行时间累积重置值",{"$f":"E292&VLOOKUP(D292,list!$D$3:$F$501,2,FALSE)&F292&\"_\"&VLOOKUP(G292,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_RSTV"},"LAHU04F06_RSTV AT%M1072.0 :REAL; (*空调机组04F06-运行时间累积重置值*)","LAHU04F06_RSTV          AT%M1072.0     :REAL; (*空调机组04F06-运行时间累积重置值*)"]
["1076.0","验证通过","BOOL","空调机组","L","04F06","隔离开关1","空调机组04F06-隔离开关1",{"$f":"E293&VLOOKUP(D293,list!$D$3:$F$501,2,FALSE)&F293&\"_\"&VLOOKUP(G293,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_ISO1"},"LAHU04F06_ISO1 AT%M1076.0 :BOOL; (*空调机组04F06-隔离开关1*)","LAHU04F06_ISO1          AT%M1076.0     :BOOL; (*空调机组04F06-隔离开关1*)"]
["1078.0","验证通过","BOOL","空调机组","L","04F06","隔离开关2","空调机组04F06-隔离开关2",{"$f":"E294&VLOOKUP(D294,list!$D$3:$F$501,2,FALSE)&F294&\"_\"&VLOOKUP(G294,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_ISO2"},"LAHU04F06_ISO2 AT%M1078.0 :BOOL; (*空调机组04F06-隔离开关2*)","LAHU04F06_ISO2          AT%M1078.0     :BOOL; (*空调机组04F06-隔离开关2*)"]
["1084.0","验证通过","REAL","空调机组","L","04F06","P调节参数","空调机组04F06-P调节参数",{"$f":"E295&VLOOKUP(D295,list!$D$3:$F$501,2,FALSE)&F295&\"_\"&VLOOKUP(G295,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_VP"},"LAHU04F06_VP AT%M1084.0 :REAL; (*空调机组04F06-P调节参数*)","LAHU04F06_VP            AT%M1084.0     :REAL; (*空调机组04F06-P调节参数*)"]
["1088.0","验证通过","REAL","空调机组","L","04F06","I调节参数","空调机组04F06-I调节参数",{"$f":"E296&VLOOKUP(D296,list!$D$3:$F$501,2,FALSE)&F296&\"_\"&VLOOKUP(G296,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_VI"},"LAHU04F06_VI AT%M1088.0 :REAL; (*空调机组04F06-I调节参数*)","LAHU04F06_VI            AT%M1088.0     :REAL; (*空调机组04F06-I调节参数*)"]
["1092.0","验证通过","REAL","空调机组","L","04F06","运行时间累积值","空调机组04F06-运行时间累积值",{"$f":"E297&VLOOKUP(D297,list!$D$3:$F$501,2,FALSE)&F297&\"_\"&VLOOKUP(G297,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_RH"},"LAHU04F06_RH AT%M1092.0 :REAL; (*空调机组04F06-运行时间累积值*)","LAHU04F06_RH            AT%M1092.0     :REAL; (*空调机组04F06-运行时间累积值*)"]
["1096.0","验证通过","INT","空调机组","L","04F06","设备状态代码","空调机组04F06-设备状态代码",{"$f":"E298&VLOOKUP(D298,list!$D$3:$F$501,2,FALSE)&F298&\"_\"&VLOOKUP(G298,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_SN"},"LAHU04F06_SN AT%M1096.0 :INT; (*空调机组04F06-设备状态代码*)","LAHU04F06_SN            AT%M1096.0     :INT; (*空调机组04F06-设备状态代码*)"]
["1098.0","验证通过","INT","空调机组","L","04F06","水阀控制转换值","空调机组04F06-水阀控制转换值",{"$f":"E299&VLOOKUP(D299,list!$D$3:$F$501,2,FALSE)&F299&\"_\"&VLOOKUP(G299,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_WVCS"},"LAHU04F06_WVCS AT%M1098.0 :INT; (*空调机组04F06-水阀控制转换值*)","LAHU04F06_WVCS          AT%M1098.0     :INT; (*空调机组04F06-水阀控制转换值*)"]
["1100.0","验证通过","BOOL","空调机组","L","04F06","程序控制","空调机组04F06-程序控制",{"$f":"E300&VLOOKUP(D300,list!$D$3:$F$501,2,FALSE)&F300&\"_\"&VLOOKUP(G300,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F06_PC"},"LAHU04F06_PC AT%M1100.0 :BOOL; (*空调机组04F06-程序控制*)","LAHU04F06_PC            AT%M1100.0     :BOOL; (*空调机组04F06-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C300=\"REAL\",C300=\"DWORD\",C300=\"DINT\"),(IF(OR(C302=\"REAL\",C302=\"DWORD\",C302=\"DINT\"),A300+4+MOD(A300,4),A300+4)),(IF(OR(C302=\"REAL\",C302=\"DWORD\",C302=\"DINT\"),A300+4+MOD(A300,4),A300+2)))&\".0\"","v":"1104.0"},{"$f":"IF((IF(OR(C302=\"INT\",C302=\"WORD\",C302=\"BOOL\"),MOD(A302,2),MOD(A302,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F07","设定温度值",{"$f":"D302&F302&\"-\"&IF(E302=\"R\",\"新云平台\"&G302,G302)","v":"空调机组04F07-新云平台设定温度值"},{"$f":"E302&VLOOKUP(D302,list!$D$3:$F$501,2,FALSE)&F302&\"_\"&VLOOKUP(G302,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F07_TSET"},{"$f":"I302&\" \"&\"AT%M\"&A302&\" \"&\":\"&C302&\";\"&\" \"&\"(*\"&H302&\"*)\"","v":"RAHU04F07_TSET AT%M1104.0 :REAL; (*空调机组04F07-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J302,SEARCH(\"AT%\",J302),,REPT(\" \",25-SEARCH(\"AT%\",J302))),SEARCH(\":\",REPLACE(J302,SEARCH(\"AT%\",J302),,REPT(\" \",25-SEARCH(\"AT%\",J302)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J302,SEARCH(\"AT%\",J302),,REPT(\" \",25-SEARCH(\"AT%\",J302))))))","v":"RAHU04F07_TSET          AT%M1104.0     :REAL; (*空调机组04F07-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C302=\"REAL\",C302=\"DWORD\",C302=\"DINT\"),(IF(OR(C303=\"REAL\",C303=\"DWORD\",C303=\"DINT\"),A302+4+MOD(A302,4),A302+4)),(IF(OR(C303=\"REAL\",C303=\"DWORD\",C303=\"DINT\"),A302+4+MOD(A302,4),A302+2)))&\".0\"","v":"1108.0"},"验证通过","INT","空调机组","R",{"$f":"F302","v":"04F07"},"季节模式","空调机组04F07-新云平台季节模式",{"$f":"E303&VLOOKUP(D303,list!$D$3:$F$501,2,FALSE)&F303&\"_\"&VLOOKUP(G303,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F07_SM"},"RAHU04F07_SM AT%M1108.0 :INT; (*空调机组04F07-新云平台季节模式*)","RAHU04F07_SM            AT%M1108.0     :INT; (*空调机组04F07-新云平台季节模式*)"]
["1110.0","验证通过","BOOL","空调机组","R","04F07","程序控制","空调机组04F07-新云平台程序控制",{"$f":"E304&VLOOKUP(D304,list!$D$3:$F$501,2,FALSE)&F304&\"_\"&VLOOKUP(G304,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F07_PC"},"RAHU04F07_PC AT%M1110.0 :BOOL; (*空调机组04F07-新云平台程序控制*)","RAHU04F07_PC            AT%M1110.0     :BOOL; (*空调机组04F07-新云平台程序控制*)"]
["1116.0","验证通过","REAL","空调机组","L","04F07","设定温度值","空调机组04F07-设定温度值",{"$f":"E305&VLOOKUP(D305,list!$D$3:$F$501,2,FALSE)&F305&\"_\"&VLOOKUP(G305,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_TSET"},"LAHU04F07_TSET AT%M1116.0 :REAL; (*空调机组04F07-设定温度值*)","LAHU04F07_TSET          AT%M1116.0     :REAL; (*空调机组04F07-设定温度值*)"]
["1120.0","验证通过","INT","空调机组","L","04F07","季节模式","空调机组04F07-季节模式",{"$f":"E306&VLOOKUP(D306,list!$D$3:$F$501,2,FALSE)&F306&\"_\"&VLOOKUP(G306,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_SM"},"LAHU04F07_SM AT%M1120.0 :INT; (*空调机组04F07-季节模式*)","LAHU04F07_SM            AT%M1120.0     :INT; (*空调机组04F07-季节模式*)"]
["1124.0","验证通过","REAL","空调机组","L","04F07","水阀反馈换算值","空调机组04F07-水阀反馈换算值",{"$f":"E307&VLOOKUP(D307,list!$D$3:$F$501,2,FALSE)&F307&\"_\"&VLOOKUP(G307,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_WVBS"},"LAHU04F07_WVBS AT%M1124.0 :REAL; (*空调机组04F07-水阀反馈换算值*)","LAHU04F07_WVBS          AT%M1124.0     :REAL; (*空调机组04F07-水阀反馈换算值*)"]
["1128.0","验证通过","BOOL","空调机组","L","04F07","水阀手动控制","空调机组04F07-水阀手动控制",{"$f":"E308&VLOOKUP(D308,list!$D$3:$F$501,2,FALSE)&F308&\"_\"&VLOOKUP(G308,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_WVMC"},"LAHU04F07_WVMC AT%M1128.0 :BOOL; (*空调机组04F07-水阀手动控制*)","LAHU04F07_WVMC          AT%M1128.0     :BOOL; (*空调机组04F07-水阀手动控制*)"]
["1132.0","验证通过","REAL","空调机组","L","04F07","水阀手动控制值","空调机组04F07-水阀手动控制值",{"$f":"E309&VLOOKUP(D309,list!$D$3:$F$501,2,FALSE)&F309&\"_\"&VLOOKUP(G309,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_WVMV"},"LAHU04F07_WVMV AT%M1132.0 :REAL; (*空调机组04F07-水阀手动控制值*)","LAHU04F07_WVMV          AT%M1132.0     :REAL; (*空调机组04F07-水阀手动控制值*)"]
["1136.0","验证通过","REAL","空调机组","L","04F07","回风温度换算值","空调机组04F07-回风温度换算值",{"$f":"E310&VLOOKUP(D310,list!$D$3:$F$501,2,FALSE)&F310&\"_\"&VLOOKUP(G310,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_RTS"},"LAHU04F07_RTS AT%M1136.0 :REAL; (*空调机组04F07-回风温度换算值*)","LAHU04F07_RTS           AT%M1136.0     :REAL; (*空调机组04F07-回风温度换算值*)"]
["1140.0","验证通过","BOOL","空调机组","L","04F07","运行时间累积重置","空调机组04F07-运行时间累积重置",{"$f":"E311&VLOOKUP(D311,list!$D$3:$F$501,2,FALSE)&F311&\"_\"&VLOOKUP(G311,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_RST"},"LAHU04F07_RST AT%M1140.0 :BOOL; (*空调机组04F07-运行时间累积重置*)","LAHU04F07_RST           AT%M1140.0     :BOOL; (*空调机组04F07-运行时间累积重置*)"]
["1144.0","验证通过","REAL","空调机组","L","04F07","运行时间累积重置值","空调机组04F07-运行时间累积重置值",{"$f":"E312&VLOOKUP(D312,list!$D$3:$F$501,2,FALSE)&F312&\"_\"&VLOOKUP(G312,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_RSTV"},"LAHU04F07_RSTV AT%M1144.0 :REAL; (*空调机组04F07-运行时间累积重置值*)","LAHU04F07_RSTV          AT%M1144.0     :REAL; (*空调机组04F07-运行时间累积重置值*)"]
["1148.0","验证通过","BOOL","空调机组","L","04F07","隔离开关1","空调机组04F07-隔离开关1",{"$f":"E313&VLOOKUP(D313,list!$D$3:$F$501,2,FALSE)&F313&\"_\"&VLOOKUP(G313,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_ISO1"},"LAHU04F07_ISO1 AT%M1148.0 :BOOL; (*空调机组04F07-隔离开关1*)","LAHU04F07_ISO1          AT%M1148.0     :BOOL; (*空调机组04F07-隔离开关1*)"]
["1150.0","验证通过","BOOL","空调机组","L","04F07","隔离开关2","空调机组04F07-隔离开关2",{"$f":"E314&VLOOKUP(D314,list!$D$3:$F$501,2,FALSE)&F314&\"_\"&VLOOKUP(G314,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_ISO2"},"LAHU04F07_ISO2 AT%M1150.0 :BOOL; (*空调机组04F07-隔离开关2*)","LAHU04F07_ISO2          AT%M1150.0     :BOOL; (*空调机组04F07-隔离开关2*)"]
["1156.0","验证通过","REAL","空调机组","L","04F07","P调节参数","空调机组04F07-P调节参数",{"$f":"E315&VLOOKUP(D315,list!$D$3:$F$501,2,FALSE)&F315&\"_\"&VLOOKUP(G315,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_VP"},"LAHU04F07_VP AT%M1156.0 :REAL; (*空调机组04F07-P调节参数*)","LAHU04F07_VP            AT%M1156.0     :REAL; (*空调机组04F07-P调节参数*)"]
["1160.0","验证通过","REAL","空调机组","L","04F07","I调节参数","空调机组04F07-I调节参数",{"$f":"E316&VLOOKUP(D316,list!$D$3:$F$501,2,FALSE)&F316&\"_\"&VLOOKUP(G316,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_VI"},"LAHU04F07_VI AT%M1160.0 :REAL; (*空调机组04F07-I调节参数*)","LAHU04F07_VI            AT%M1160.0     :REAL; (*空调机组04F07-I调节参数*)"]
["1164.0","验证通过","REAL","空调机组","L","04F07","运行时间累积值","空调机组04F07-运行时间累积值",{"$f":"E317&VLOOKUP(D317,list!$D$3:$F$501,2,FALSE)&F317&\"_\"&VLOOKUP(G317,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_RH"},"LAHU04F07_RH AT%M1164.0 :REAL; (*空调机组04F07-运行时间累积值*)","LAHU04F07_RH            AT%M1164.0     :REAL; (*空调机组04F07-运行时间累积值*)"]
["1168.0","验证通过","INT","空调机组","L","04F07","设备状态代码","空调机组04F07-设备状态代码",{"$f":"E318&VLOOKUP(D318,list!$D$3:$F$501,2,FALSE)&F318&\"_\"&VLOOKUP(G318,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_SN"},"LAHU04F07_SN AT%M1168.0 :INT; (*空调机组04F07-设备状态代码*)","LAHU04F07_SN            AT%M1168.0     :INT; (*空调机组04F07-设备状态代码*)"]
["1170.0","验证通过","INT","空调机组","L","04F07","水阀控制转换值","空调机组04F07-水阀控制转换值",{"$f":"E319&VLOOKUP(D319,list!$D$3:$F$501,2,FALSE)&F319&\"_\"&VLOOKUP(G319,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_WVCS"},"LAHU04F07_WVCS AT%M1170.0 :INT; (*空调机组04F07-水阀控制转换值*)","LAHU04F07_WVCS          AT%M1170.0     :INT; (*空调机组04F07-水阀控制转换值*)"]
["1172.0","验证通过","BOOL","空调机组","L","04F07","程序控制","空调机组04F07-程序控制",{"$f":"E320&VLOOKUP(D320,list!$D$3:$F$501,2,FALSE)&F320&\"_\"&VLOOKUP(G320,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F07_PC"},"LAHU04F07_PC AT%M1172.0 :BOOL; (*空调机组04F07-程序控制*)","LAHU04F07_PC            AT%M1172.0     :BOOL; (*空调机组04F07-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C320=\"REAL\",C320=\"DWORD\",C320=\"DINT\"),(IF(OR(C322=\"REAL\",C322=\"DWORD\",C322=\"DINT\"),A320+4+MOD(A320,4),A320+4)),(IF(OR(C322=\"REAL\",C322=\"DWORD\",C322=\"DINT\"),A320+4+MOD(A320,4),A320+2)))&\".0\"","v":"1176.0"},{"$f":"IF((IF(OR(C322=\"INT\",C322=\"WORD\",C322=\"BOOL\"),MOD(A322,2),MOD(A322,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F08","设定温度值",{"$f":"D322&F322&\"-\"&IF(E322=\"R\",\"新云平台\"&G322,G322)","v":"空调机组04F08-新云平台设定温度值"},{"$f":"E322&VLOOKUP(D322,list!$D$3:$F$501,2,FALSE)&F322&\"_\"&VLOOKUP(G322,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F08_TSET"},{"$f":"I322&\" \"&\"AT%M\"&A322&\" \"&\":\"&C322&\";\"&\" \"&\"(*\"&H322&\"*)\"","v":"RAHU04F08_TSET AT%M1176.0 :REAL; (*空调机组04F08-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J322,SEARCH(\"AT%\",J322),,REPT(\" \",25-SEARCH(\"AT%\",J322))),SEARCH(\":\",REPLACE(J322,SEARCH(\"AT%\",J322),,REPT(\" \",25-SEARCH(\"AT%\",J322)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J322,SEARCH(\"AT%\",J322),,REPT(\" \",25-SEARCH(\"AT%\",J322))))))","v":"RAHU04F08_TSET          AT%M1176.0     :REAL; (*空调机组04F08-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C322=\"REAL\",C322=\"DWORD\",C322=\"DINT\"),(IF(OR(C323=\"REAL\",C323=\"DWORD\",C323=\"DINT\"),A322+4+MOD(A322,4),A322+4)),(IF(OR(C323=\"REAL\",C323=\"DWORD\",C323=\"DINT\"),A322+4+MOD(A322,4),A322+2)))&\".0\"","v":"1180.0"},"验证通过","INT","空调机组","R",{"$f":"F322","v":"04F08"},"季节模式","空调机组04F08-新云平台季节模式",{"$f":"E323&VLOOKUP(D323,list!$D$3:$F$501,2,FALSE)&F323&\"_\"&VLOOKUP(G323,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F08_SM"},"RAHU04F08_SM AT%M1180.0 :INT; (*空调机组04F08-新云平台季节模式*)","RAHU04F08_SM            AT%M1180.0     :INT; (*空调机组04F08-新云平台季节模式*)"]
["1182.0","验证通过","BOOL","空调机组","R","04F08","程序控制","空调机组04F08-新云平台程序控制",{"$f":"E324&VLOOKUP(D324,list!$D$3:$F$501,2,FALSE)&F324&\"_\"&VLOOKUP(G324,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F08_PC"},"RAHU04F08_PC AT%M1182.0 :BOOL; (*空调机组04F08-新云平台程序控制*)","RAHU04F08_PC            AT%M1182.0     :BOOL; (*空调机组04F08-新云平台程序控制*)"]
["1188.0","验证通过","REAL","空调机组","L","04F08","设定温度值","空调机组04F08-设定温度值",{"$f":"E325&VLOOKUP(D325,list!$D$3:$F$501,2,FALSE)&F325&\"_\"&VLOOKUP(G325,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_TSET"},"LAHU04F08_TSET AT%M1188.0 :REAL; (*空调机组04F08-设定温度值*)","LAHU04F08_TSET          AT%M1188.0     :REAL; (*空调机组04F08-设定温度值*)"]
["1192.0","验证通过","INT","空调机组","L","04F08","季节模式","空调机组04F08-季节模式",{"$f":"E326&VLOOKUP(D326,list!$D$3:$F$501,2,FALSE)&F326&\"_\"&VLOOKUP(G326,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_SM"},"LAHU04F08_SM AT%M1192.0 :INT; (*空调机组04F08-季节模式*)","LAHU04F08_SM            AT%M1192.0     :INT; (*空调机组04F08-季节模式*)"]
["1196.0","验证通过","REAL","空调机组","L","04F08","水阀反馈换算值","空调机组04F08-水阀反馈换算值",{"$f":"E327&VLOOKUP(D327,list!$D$3:$F$501,2,FALSE)&F327&\"_\"&VLOOKUP(G327,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_WVBS"},"LAHU04F08_WVBS AT%M1196.0 :REAL; (*空调机组04F08-水阀反馈换算值*)","LAHU04F08_WVBS          AT%M1196.0     :REAL; (*空调机组04F08-水阀反馈换算值*)"]
["1200.0","验证通过","BOOL","空调机组","L","04F08","水阀手动控制","空调机组04F08-水阀手动控制",{"$f":"E328&VLOOKUP(D328,list!$D$3:$F$501,2,FALSE)&F328&\"_\"&VLOOKUP(G328,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_WVMC"},"LAHU04F08_WVMC AT%M1200.0 :BOOL; (*空调机组04F08-水阀手动控制*)","LAHU04F08_WVMC          AT%M1200.0     :BOOL; (*空调机组04F08-水阀手动控制*)"]
["1204.0","验证通过","REAL","空调机组","L","04F08","水阀手动控制值","空调机组04F08-水阀手动控制值",{"$f":"E329&VLOOKUP(D329,list!$D$3:$F$501,2,FALSE)&F329&\"_\"&VLOOKUP(G329,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_WVMV"},"LAHU04F08_WVMV AT%M1204.0 :REAL; (*空调机组04F08-水阀手动控制值*)","LAHU04F08_WVMV          AT%M1204.0     :REAL; (*空调机组04F08-水阀手动控制值*)"]
["1208.0","验证通过","REAL","空调机组","L","04F08","回风温度换算值","空调机组04F08-回风温度换算值",{"$f":"E330&VLOOKUP(D330,list!$D$3:$F$501,2,FALSE)&F330&\"_\"&VLOOKUP(G330,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_RTS"},"LAHU04F08_RTS AT%M1208.0 :REAL; (*空调机组04F08-回风温度换算值*)","LAHU04F08_RTS           AT%M1208.0     :REAL; (*空调机组04F08-回风温度换算值*)"]
["1212.0","验证通过","BOOL","空调机组","L","04F08","运行时间累积重置","空调机组04F08-运行时间累积重置",{"$f":"E331&VLOOKUP(D331,list!$D$3:$F$501,2,FALSE)&F331&\"_\"&VLOOKUP(G331,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_RST"},"LAHU04F08_RST AT%M1212.0 :BOOL; (*空调机组04F08-运行时间累积重置*)","LAHU04F08_RST           AT%M1212.0     :BOOL; (*空调机组04F08-运行时间累积重置*)"]
["1216.0","验证通过","REAL","空调机组","L","04F08","运行时间累积重置值","空调机组04F08-运行时间累积重置值",{"$f":"E332&VLOOKUP(D332,list!$D$3:$F$501,2,FALSE)&F332&\"_\"&VLOOKUP(G332,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_RSTV"},"LAHU04F08_RSTV AT%M1216.0 :REAL; (*空调机组04F08-运行时间累积重置值*)","LAHU04F08_RSTV          AT%M1216.0     :REAL; (*空调机组04F08-运行时间累积重置值*)"]
["1220.0","验证通过","BOOL","空调机组","L","04F08","隔离开关1","空调机组04F08-隔离开关1",{"$f":"E333&VLOOKUP(D333,list!$D$3:$F$501,2,FALSE)&F333&\"_\"&VLOOKUP(G333,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_ISO1"},"LAHU04F08_ISO1 AT%M1220.0 :BOOL; (*空调机组04F08-隔离开关1*)","LAHU04F08_ISO1          AT%M1220.0     :BOOL; (*空调机组04F08-隔离开关1*)"]
["1222.0","验证通过","BOOL","空调机组","L","04F08","隔离开关2","空调机组04F08-隔离开关2",{"$f":"E334&VLOOKUP(D334,list!$D$3:$F$501,2,FALSE)&F334&\"_\"&VLOOKUP(G334,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_ISO2"},"LAHU04F08_ISO2 AT%M1222.0 :BOOL; (*空调机组04F08-隔离开关2*)","LAHU04F08_ISO2          AT%M1222.0     :BOOL; (*空调机组04F08-隔离开关2*)"]
["1228.0","验证通过","REAL","空调机组","L","04F08","P调节参数","空调机组04F08-P调节参数",{"$f":"E335&VLOOKUP(D335,list!$D$3:$F$501,2,FALSE)&F335&\"_\"&VLOOKUP(G335,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_VP"},"LAHU04F08_VP AT%M1228.0 :REAL; (*空调机组04F08-P调节参数*)","LAHU04F08_VP            AT%M1228.0     :REAL; (*空调机组04F08-P调节参数*)"]
["1232.0","验证通过","REAL","空调机组","L","04F08","I调节参数","空调机组04F08-I调节参数",{"$f":"E336&VLOOKUP(D336,list!$D$3:$F$501,2,FALSE)&F336&\"_\"&VLOOKUP(G336,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_VI"},"LAHU04F08_VI AT%M1232.0 :REAL; (*空调机组04F08-I调节参数*)","LAHU04F08_VI            AT%M1232.0     :REAL; (*空调机组04F08-I调节参数*)"]
["1236.0","验证通过","REAL","空调机组","L","04F08","运行时间累积值","空调机组04F08-运行时间累积值",{"$f":"E337&VLOOKUP(D337,list!$D$3:$F$501,2,FALSE)&F337&\"_\"&VLOOKUP(G337,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_RH"},"LAHU04F08_RH AT%M1236.0 :REAL; (*空调机组04F08-运行时间累积值*)","LAHU04F08_RH            AT%M1236.0     :REAL; (*空调机组04F08-运行时间累积值*)"]
["1240.0","验证通过","INT","空调机组","L","04F08","设备状态代码","空调机组04F08-设备状态代码",{"$f":"E338&VLOOKUP(D338,list!$D$3:$F$501,2,FALSE)&F338&\"_\"&VLOOKUP(G338,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_SN"},"LAHU04F08_SN AT%M1240.0 :INT; (*空调机组04F08-设备状态代码*)","LAHU04F08_SN            AT%M1240.0     :INT; (*空调机组04F08-设备状态代码*)"]
["1242.0","验证通过","INT","空调机组","L","04F08","水阀控制转换值","空调机组04F08-水阀控制转换值",{"$f":"E339&VLOOKUP(D339,list!$D$3:$F$501,2,FALSE)&F339&\"_\"&VLOOKUP(G339,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_WVCS"},"LAHU04F08_WVCS AT%M1242.0 :INT; (*空调机组04F08-水阀控制转换值*)","LAHU04F08_WVCS          AT%M1242.0     :INT; (*空调机组04F08-水阀控制转换值*)"]
["1244.0","验证通过","BOOL","空调机组","L","04F08","程序控制","空调机组04F08-程序控制",{"$f":"E340&VLOOKUP(D340,list!$D$3:$F$501,2,FALSE)&F340&\"_\"&VLOOKUP(G340,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F08_PC"},"LAHU04F08_PC AT%M1244.0 :BOOL; (*空调机组04F08-程序控制*)","LAHU04F08_PC            AT%M1244.0     :BOOL; (*空调机组04F08-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C340=\"REAL\",C340=\"DWORD\",C340=\"DINT\"),(IF(OR(C342=\"REAL\",C342=\"DWORD\",C342=\"DINT\"),A340+4+MOD(A340,4),A340+4)),(IF(OR(C342=\"REAL\",C342=\"DWORD\",C342=\"DINT\"),A340+4+MOD(A340,4),A340+2)))&\".0\"","v":"1248.0"},{"$f":"IF((IF(OR(C342=\"INT\",C342=\"WORD\",C342=\"BOOL\"),MOD(A342,2),MOD(A342,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04F09","设定温度值",{"$f":"D342&F342&\"-\"&IF(E342=\"R\",\"新云平台\"&G342,G342)","v":"空调机组04F09-新云平台设定温度值"},{"$f":"E342&VLOOKUP(D342,list!$D$3:$F$501,2,FALSE)&F342&\"_\"&VLOOKUP(G342,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F09_TSET"},{"$f":"I342&\" \"&\"AT%M\"&A342&\" \"&\":\"&C342&\";\"&\" \"&\"(*\"&H342&\"*)\"","v":"RAHU04F09_TSET AT%M1248.0 :REAL; (*空调机组04F09-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J342,SEARCH(\"AT%\",J342),,REPT(\" \",25-SEARCH(\"AT%\",J342))),SEARCH(\":\",REPLACE(J342,SEARCH(\"AT%\",J342),,REPT(\" \",25-SEARCH(\"AT%\",J342)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J342,SEARCH(\"AT%\",J342),,REPT(\" \",25-SEARCH(\"AT%\",J342))))))","v":"RAHU04F09_TSET          AT%M1248.0     :REAL; (*空调机组04F09-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C342=\"REAL\",C342=\"DWORD\",C342=\"DINT\"),(IF(OR(C343=\"REAL\",C343=\"DWORD\",C343=\"DINT\"),A342+4+MOD(A342,4),A342+4)),(IF(OR(C343=\"REAL\",C343=\"DWORD\",C343=\"DINT\"),A342+4+MOD(A342,4),A342+2)))&\".0\"","v":"1252.0"},"验证通过","INT","空调机组","R",{"$f":"F342","v":"04F09"},"季节模式","空调机组04F09-新云平台季节模式",{"$f":"E343&VLOOKUP(D343,list!$D$3:$F$501,2,FALSE)&F343&\"_\"&VLOOKUP(G343,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F09_SM"},"RAHU04F09_SM AT%M1252.0 :INT; (*空调机组04F09-新云平台季节模式*)","RAHU04F09_SM            AT%M1252.0     :INT; (*空调机组04F09-新云平台季节模式*)"]
["1254.0","验证通过","BOOL","空调机组","R","04F09","程序控制","空调机组04F09-新云平台程序控制",{"$f":"E344&VLOOKUP(D344,list!$D$3:$F$501,2,FALSE)&F344&\"_\"&VLOOKUP(G344,list!$I$2:$K$502,2,FALSE)","v":"RAHU04F09_PC"},"RAHU04F09_PC AT%M1254.0 :BOOL; (*空调机组04F09-新云平台程序控制*)","RAHU04F09_PC            AT%M1254.0     :BOOL; (*空调机组04F09-新云平台程序控制*)"]
["1260.0","验证通过","REAL","空调机组","L","04F09","设定温度值","空调机组04F09-设定温度值",{"$f":"E345&VLOOKUP(D345,list!$D$3:$F$501,2,FALSE)&F345&\"_\"&VLOOKUP(G345,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_TSET"},"LAHU04F09_TSET AT%M1260.0 :REAL; (*空调机组04F09-设定温度值*)","LAHU04F09_TSET          AT%M1260.0     :REAL; (*空调机组04F09-设定温度值*)"]
["1264.0","验证通过","INT","空调机组","L","04F09","季节模式","空调机组04F09-季节模式",{"$f":"E346&VLOOKUP(D346,list!$D$3:$F$501,2,FALSE)&F346&\"_\"&VLOOKUP(G346,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_SM"},"LAHU04F09_SM AT%M1264.0 :INT; (*空调机组04F09-季节模式*)","LAHU04F09_SM            AT%M1264.0     :INT; (*空调机组04F09-季节模式*)"]
["1268.0","验证通过","REAL","空调机组","L","04F09","水阀反馈换算值","空调机组04F09-水阀反馈换算值",{"$f":"E347&VLOOKUP(D347,list!$D$3:$F$501,2,FALSE)&F347&\"_\"&VLOOKUP(G347,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_WVBS"},"LAHU04F09_WVBS AT%M1268.0 :REAL; (*空调机组04F09-水阀反馈换算值*)","LAHU04F09_WVBS          AT%M1268.0     :REAL; (*空调机组04F09-水阀反馈换算值*)"]
["1272.0","验证通过","BOOL","空调机组","L","04F09","水阀手动控制","空调机组04F09-水阀手动控制",{"$f":"E348&VLOOKUP(D348,list!$D$3:$F$501,2,FALSE)&F348&\"_\"&VLOOKUP(G348,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_WVMC"},"LAHU04F09_WVMC AT%M1272.0 :BOOL; (*空调机组04F09-水阀手动控制*)","LAHU04F09_WVMC          AT%M1272.0     :BOOL; (*空调机组04F09-水阀手动控制*)"]
["1276.0","验证通过","REAL","空调机组","L","04F09","水阀手动控制值","空调机组04F09-水阀手动控制值",{"$f":"E349&VLOOKUP(D349,list!$D$3:$F$501,2,FALSE)&F349&\"_\"&VLOOKUP(G349,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_WVMV"},"LAHU04F09_WVMV AT%M1276.0 :REAL; (*空调机组04F09-水阀手动控制值*)","LAHU04F09_WVMV          AT%M1276.0     :REAL; (*空调机组04F09-水阀手动控制值*)"]
["1280.0","验证通过","REAL","空调机组","L","04F09","回风温度换算值","空调机组04F09-回风温度换算值",{"$f":"E350&VLOOKUP(D350,list!$D$3:$F$501,2,FALSE)&F350&\"_\"&VLOOKUP(G350,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_RTS"},"LAHU04F09_RTS AT%M1280.0 :REAL; (*空调机组04F09-回风温度换算值*)","LAHU04F09_RTS           AT%M1280.0     :REAL; (*空调机组04F09-回风温度换算值*)"]
["1284.0","验证通过","BOOL","空调机组","L","04F09","运行时间累积重置","空调机组04F09-运行时间累积重置",{"$f":"E351&VLOOKUP(D351,list!$D$3:$F$501,2,FALSE)&F351&\"_\"&VLOOKUP(G351,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_RST"},"LAHU04F09_RST AT%M1284.0 :BOOL; (*空调机组04F09-运行时间累积重置*)","LAHU04F09_RST           AT%M1284.0     :BOOL; (*空调机组04F09-运行时间累积重置*)"]
["1288.0","验证通过","REAL","空调机组","L","04F09","运行时间累积重置值","空调机组04F09-运行时间累积重置值",{"$f":"E352&VLOOKUP(D352,list!$D$3:$F$501,2,FALSE)&F352&\"_\"&VLOOKUP(G352,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_RSTV"},"LAHU04F09_RSTV AT%M1288.0 :REAL; (*空调机组04F09-运行时间累积重置值*)","LAHU04F09_RSTV          AT%M1288.0     :REAL; (*空调机组04F09-运行时间累积重置值*)"]
["1292.0","验证通过","BOOL","空调机组","L","04F09","隔离开关1","空调机组04F09-隔离开关1",{"$f":"E353&VLOOKUP(D353,list!$D$3:$F$501,2,FALSE)&F353&\"_\"&VLOOKUP(G353,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_ISO1"},"LAHU04F09_ISO1 AT%M1292.0 :BOOL; (*空调机组04F09-隔离开关1*)","LAHU04F09_ISO1          AT%M1292.0     :BOOL; (*空调机组04F09-隔离开关1*)"]
["1294.0","验证通过","BOOL","空调机组","L","04F09","隔离开关2","空调机组04F09-隔离开关2",{"$f":"E354&VLOOKUP(D354,list!$D$3:$F$501,2,FALSE)&F354&\"_\"&VLOOKUP(G354,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_ISO2"},"LAHU04F09_ISO2 AT%M1294.0 :BOOL; (*空调机组04F09-隔离开关2*)","LAHU04F09_ISO2          AT%M1294.0     :BOOL; (*空调机组04F09-隔离开关2*)"]
["1300.0","验证通过","REAL","空调机组","L","04F09","P调节参数","空调机组04F09-P调节参数",{"$f":"E355&VLOOKUP(D355,list!$D$3:$F$501,2,FALSE)&F355&\"_\"&VLOOKUP(G355,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_VP"},"LAHU04F09_VP AT%M1300.0 :REAL; (*空调机组04F09-P调节参数*)","LAHU04F09_VP            AT%M1300.0     :REAL; (*空调机组04F09-P调节参数*)"]
["1304.0","验证通过","REAL","空调机组","L","04F09","I调节参数","空调机组04F09-I调节参数",{"$f":"E356&VLOOKUP(D356,list!$D$3:$F$501,2,FALSE)&F356&\"_\"&VLOOKUP(G356,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_VI"},"LAHU04F09_VI AT%M1304.0 :REAL; (*空调机组04F09-I调节参数*)","LAHU04F09_VI            AT%M1304.0     :REAL; (*空调机组04F09-I调节参数*)"]
["1308.0","验证通过","REAL","空调机组","L","04F09","运行时间累积值","空调机组04F09-运行时间累积值",{"$f":"E357&VLOOKUP(D357,list!$D$3:$F$501,2,FALSE)&F357&\"_\"&VLOOKUP(G357,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_RH"},"LAHU04F09_RH AT%M1308.0 :REAL; (*空调机组04F09-运行时间累积值*)","LAHU04F09_RH            AT%M1308.0     :REAL; (*空调机组04F09-运行时间累积值*)"]
["1312.0","验证通过","INT","空调机组","L","04F09","设备状态代码","空调机组04F09-设备状态代码",{"$f":"E358&VLOOKUP(D358,list!$D$3:$F$501,2,FALSE)&F358&\"_\"&VLOOKUP(G358,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_SN"},"LAHU04F09_SN AT%M1312.0 :INT; (*空调机组04F09-设备状态代码*)","LAHU04F09_SN            AT%M1312.0     :INT; (*空调机组04F09-设备状态代码*)"]
["1314.0","验证通过","INT","空调机组","L","04F09","水阀控制转换值","空调机组04F09-水阀控制转换值",{"$f":"E359&VLOOKUP(D359,list!$D$3:$F$501,2,FALSE)&F359&\"_\"&VLOOKUP(G359,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_WVCS"},"LAHU04F09_WVCS AT%M1314.0 :INT; (*空调机组04F09-水阀控制转换值*)","LAHU04F09_WVCS          AT%M1314.0     :INT; (*空调机组04F09-水阀控制转换值*)"]
["1316.0","验证通过","BOOL","空调机组","L","04F09","程序控制","空调机组04F09-程序控制",{"$f":"E360&VLOOKUP(D360,list!$D$3:$F$501,2,FALSE)&F360&\"_\"&VLOOKUP(G360,list!$I$2:$K$502,2,FALSE)","v":"LAHU04F09_PC"},"LAHU04F09_PC AT%M1316.0 :BOOL; (*空调机组04F09-程序控制*)","LAHU04F09_PC            AT%M1316.0     :BOOL; (*空调机组04F09-程序控制*)"]
["EAF"]
[1750,{"$f":"IF((IF(OR(C362=\"INT\",C362=\"WORD\",C362=\"BOOL\"),MOD(A362,2),MOD(A362,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","05E01","启停控制",{"$f":"D362&F362&\"-\"&IF(E362=\"R\",\"新云平台\"&G362,G362)","v":"排风机05E01-新云平台启停控制"},{"$f":"E362&VLOOKUP(D362,[1]list!$D$3:$F$501,2,FALSE)&F362&\"_\"&VLOOKUP(G362,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF05E01_C"},{"$f":"I362&\" \"&\"AT%M\"&A362&\" \"&\":\"&C362&\";\"&\" \"&\"(*\"&H362&\"*)\"","v":"REAF05E01_C AT%M1750 :BOOL; (*排风机05E01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J362,SEARCH(\"AT%\",J362),,REPT(\" \",25-SEARCH(\"AT%\",J362))),SEARCH(\":\",REPLACE(J362,SEARCH(\"AT%\",J362),,REPT(\" \",25-SEARCH(\"AT%\",J362)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J362,SEARCH(\"AT%\",J362),,REPT(\" \",25-SEARCH(\"AT%\",J362))))))","v":"REAF05E01_C             AT%M1750       :BOOL; (*排风机05E01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C362=\"REAL\",C362=\"DWORD\",C362=\"DINT\"),(IF(OR(C363=\"REAL\",C363=\"DWORD\",C363=\"DINT\"),A362+4+MOD(A362,4),A362+4)),(IF(OR(C363=\"REAL\",C363=\"DWORD\",C363=\"DINT\"),A362+4+MOD(A362,4),A362+2)))&\".0\"","v":"1752.0"},"验证通过","BOOL","排风机","L","05E01","运行时间累积重置","排风机05E01-运行时间累积重置",{"$f":"E363&VLOOKUP(D363,[1]list!$D$3:$F$501,2,FALSE)&F363&\"_\"&VLOOKUP(G363,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_RST"},"LEAF05E01_RST AT%M1752.0 :BOOL; (*排风机05E01-运行时间累积重置*)","LEAF05E01_RST           AT%M1752.0     :BOOL; (*排风机05E01-运行时间累积重置*)"]
["1756.0","验证通过","REAL","排风机","L","05E01","运行时间累积重置值","排风机05E01-运行时间累积重置值",{"$f":"E364&VLOOKUP(D364,[1]list!$D$3:$F$501,2,FALSE)&F364&\"_\"&VLOOKUP(G364,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_RSTV"},"LEAF05E01_RSTV AT%M1756.0 :REAL; (*排风机05E01-运行时间累积重置值*)","LEAF05E01_RSTV          AT%M1756.0     :REAL; (*排风机05E01-运行时间累积重置值*)"]
["1760.0","验证通过","REAL","排风机","L","05E01","运行时间累积值","排风机05E01-运行时间累积值",{"$f":"E365&VLOOKUP(D365,[1]list!$D$3:$F$501,2,FALSE)&F365&\"_\"&VLOOKUP(G365,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_RH"},"LEAF05E01_RH AT%M1760.0 :REAL; (*排风机05E01-运行时间累积值*)","LEAF05E01_RH            AT%M1760.0     :REAL; (*排风机05E01-运行时间累积值*)"]
["1764.0","验证通过","BOOL","排风机","L","05E01","定时模式","排风机05E01-定时模式",{"$f":"E366&VLOOKUP(D366,[1]list!$D$3:$F$501,2,FALSE)&F366&\"_\"&VLOOKUP(G366,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_TM"},"LEAF05E01_TM AT%M1764.0 :BOOL; (*排风机05E01-定时模式*)","LEAF05E01_TM            AT%M1764.0     :BOOL; (*排风机05E01-定时模式*)"]
["1766.0","验证通过","BOOL","排风机","L","05E01","定时控制","排风机05E01-定时控制",{"$f":"E367&VLOOKUP(D367,[1]list!$D$3:$F$501,2,FALSE)&F367&\"_\"&VLOOKUP(G367,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_TC"},"LEAF05E01_TC AT%M1766.0 :BOOL; (*排风机05E01-定时控制*)","LEAF05E01_TC            AT%M1766.0     :BOOL; (*排风机05E01-定时控制*)"]
["1768.0","验证通过","BOOL","排风机","L","05E01","全天候模式","排风机05E01-全天候模式",{"$f":"E368&VLOOKUP(D368,[1]list!$D$3:$F$501,2,FALSE)&F368&\"_\"&VLOOKUP(G368,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_DM"},"LEAF05E01_DM AT%M1768.0 :BOOL; (*排风机05E01-全天候模式*)","LEAF05E01_DM            AT%M1768.0     :BOOL; (*排风机05E01-全天候模式*)"]
["1772.0","验证通过","REAL","排风机","L","05E01","CO设定值","排风机05E01-CO设定值",{"$f":"E369&VLOOKUP(D369,[1]list!$D$3:$F$501,2,FALSE)&F369&\"_\"&VLOOKUP(G369,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_COSET"},"LEAF05E01_COSET AT%M1772.0 :REAL; (*排风机05E01-CO设定值*)","LEAF05E01_COSET         AT%M1772.0     :REAL; (*排风机05E01-CO设定值*)"]
["1776.0","验证通过","REAL","排风机","L","05E01","设定温度值","排风机05E01-设定温度值",{"$f":"E370&VLOOKUP(D370,[1]list!$D$3:$F$501,2,FALSE)&F370&\"_\"&VLOOKUP(G370,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF05E01_TSET"},"LEAF05E01_TSET AT%M1776.0 :REAL; (*排风机05E01-设定温度值*)","LEAF05E01_TSET          AT%M1776.0     :REAL; (*排风机05E01-设定温度值*)"]
["FCU"]
[{"$f":"IF(OR(C370=\"REAL\",C370=\"DWORD\",C370=\"DINT\"),(IF(OR(C372=\"REAL\",C372=\"DWORD\",C372=\"DINT\"),A370+4+MOD(A370,4),A370+4)),(IF(OR(C372=\"REAL\",C372=\"DWORD\",C372=\"DINT\"),A370+4+MOD(A370,4),A370+2)))&\".0\"","v":"1780.0"},{"$f":"IF((IF(OR(C372=\"INT\",C372=\"WORD\",C372=\"BOOL\"),MOD(A372,2),MOD(A372,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","04F01","设定温度值",{"$f":"D372&F372&\"-\"&IF(E372=\"R\",\"新云平台\"&G372,G372)","v":"风机盘管04F01-新云平台设定温度值"},{"$f":"E372&VLOOKUP(D372,list!$D$3:$F$501,2,FALSE)&F372&\"_\"&VLOOKUP(G372,list!$I$2:$K$502,2,FALSE)","v":"RFCU04F01_TSET"},{"$f":"I372&\" \"&\"AT%M\"&A372&\" \"&\":\"&C372&\";\"&\" \"&\"(*\"&H372&\"*)\"","v":"RFCU04F01_TSET AT%M1780.0 :REAL; (*风机盘管04F01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J372,SEARCH(\"AT%\",J372),,REPT(\" \",25-SEARCH(\"AT%\",J372))),SEARCH(\":\",REPLACE(J372,SEARCH(\"AT%\",J372),,REPT(\" \",25-SEARCH(\"AT%\",J372)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J372,SEARCH(\"AT%\",J372),,REPT(\" \",25-SEARCH(\"AT%\",J372))))))","v":"RFCU04F01_TSET          AT%M1780.0     :REAL; (*风机盘管04F01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C372=\"REAL\",C372=\"DWORD\",C372=\"DINT\"),(IF(OR(C373=\"REAL\",C373=\"DWORD\",C373=\"DINT\"),A372+4+MOD(A372,4),A372+4)),(IF(OR(C373=\"REAL\",C373=\"DWORD\",C373=\"DINT\"),A372+4+MOD(A372,4),A372+2)))&\".0\"","v":"1784.0"},"验证通过","INT","风机盘管","R",{"$f":"F372","v":"04F01"},"季节模式","风机盘管04F01-新云平台季节模式",{"$f":"E373&VLOOKUP(D373,list!$D$3:$F$501,2,FALSE)&F373&\"_\"&VLOOKUP(G373,list!$I$2:$K$502,2,FALSE)","v":"RFCU04F01_SM"},"RFCU04F01_SM AT%M1784.0 :INT; (*风机盘管04F01-新云平台季节模式*)","RFCU04F01_SM            AT%M1784.0     :INT; (*风机盘管04F01-新云平台季节模式*)"]
["1786.0","验证通过","BOOL","风机盘管","R","04F01","程序控制","风机盘管04F01-新云平台程序控制",{"$f":"E374&VLOOKUP(D374,list!$D$3:$F$501,2,FALSE)&F374&\"_\"&VLOOKUP(G374,list!$I$2:$K$502,2,FALSE)","v":"RFCU04F01_PC"},"RFCU04F01_PC AT%M1786.0 :BOOL; (*风机盘管04F01-新云平台程序控制*)","RFCU04F01_PC            AT%M1786.0     :BOOL; (*风机盘管04F01-新云平台程序控制*)"]
["1792.0","验证通过","REAL","风机盘管","L","04F01","设定温度值","风机盘管04F01-设定温度值",{"$f":"E375&VLOOKUP(D375,list!$D$3:$F$501,2,FALSE)&F375&\"_\"&VLOOKUP(G375,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_TSET"},"LFCU04F01_TSET AT%M1792.0 :REAL; (*风机盘管04F01-设定温度值*)","LFCU04F01_TSET          AT%M1792.0     :REAL; (*风机盘管04F01-设定温度值*)"]
["1796.0","验证通过","INT","风机盘管","L","04F01","季节模式","风机盘管04F01-季节模式",{"$f":"E376&VLOOKUP(D376,list!$D$3:$F$501,2,FALSE)&F376&\"_\"&VLOOKUP(G376,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_SM"},"LFCU04F01_SM AT%M1796.0 :INT; (*风机盘管04F01-季节模式*)","LFCU04F01_SM            AT%M1796.0     :INT; (*风机盘管04F01-季节模式*)"]
["1800.0","验证通过","REAL","风机盘管","L","04F01","温度换算值","风机盘管04F01-温度换算值",{"$f":"E377&VLOOKUP(D377,list!$D$3:$F$501,2,FALSE)&F377&\"_\"&VLOOKUP(G377,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_TS"},"LFCU04F01_TS AT%M1800.0 :REAL; (*风机盘管04F01-温度换算值*)","LFCU04F01_TS            AT%M1800.0     :REAL; (*风机盘管04F01-温度换算值*)"]
["1804.0","验证通过","BOOL","风机盘管","L","04F01","电磁阀手动控制","风机盘管04F01-电磁阀手动控制",{"$f":"E378&VLOOKUP(D378,list!$D$3:$F$501,2,FALSE)&F378&\"_\"&VLOOKUP(G378,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_EVMC"},"LFCU04F01_EVMC AT%M1804.0 :BOOL; (*风机盘管04F01-电磁阀手动控制*)","LFCU04F01_EVMC          AT%M1804.0     :BOOL; (*风机盘管04F01-电磁阀手动控制*)"]
["1806.0","验证通过","BOOL","风机盘管","L","04F01","电磁阀手动控制值","风机盘管04F01-电磁阀手动控制值",{"$f":"E379&VLOOKUP(D379,list!$D$3:$F$501,2,FALSE)&F379&\"_\"&VLOOKUP(G379,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_EVMV"},"LFCU04F01_EVMV AT%M1806.0 :BOOL; (*风机盘管04F01-电磁阀手动控制值*)","LFCU04F01_EVMV          AT%M1806.0     :BOOL; (*风机盘管04F01-电磁阀手动控制值*)"]
["1812.0","验证通过","REAL","风机盘管","L","04F01","回风温度换算值","风机盘管04F01-回风温度换算值",{"$f":"E380&VLOOKUP(D380,list!$D$3:$F$501,2,FALSE)&F380&\"_\"&VLOOKUP(G380,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RTS"},"LFCU04F01_RTS AT%M1812.0 :REAL; (*风机盘管04F01-回风温度换算值*)","LFCU04F01_RTS           AT%M1812.0     :REAL; (*风机盘管04F01-回风温度换算值*)"]
["1816.0","验证通过","BOOL","风机盘管","L","04F01","运行时间累积重置","风机盘管04F01-运行时间累积重置",{"$f":"E381&VLOOKUP(D381,list!$D$3:$F$501,2,FALSE)&F381&\"_\"&VLOOKUP(G381,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RST"},"LFCU04F01_RST AT%M1816.0 :BOOL; (*风机盘管04F01-运行时间累积重置*)","LFCU04F01_RST           AT%M1816.0     :BOOL; (*风机盘管04F01-运行时间累积重置*)"]
["1820.0","验证通过","REAL","风机盘管","L","04F01","运行时间累积重置值","风机盘管04F01-运行时间累积重置值",{"$f":"E382&VLOOKUP(D382,list!$D$3:$F$501,2,FALSE)&F382&\"_\"&VLOOKUP(G382,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RSTV"},"LFCU04F01_RSTV AT%M1820.0 :REAL; (*风机盘管04F01-运行时间累积重置值*)","LFCU04F01_RSTV          AT%M1820.0     :REAL; (*风机盘管04F01-运行时间累积重置值*)"]
["1824.0","验证通过","BOOL","风机盘管","L","04F01","隔离开关1","风机盘管04F01-隔离开关1",{"$f":"E383&VLOOKUP(D383,list!$D$3:$F$501,2,FALSE)&F383&\"_\"&VLOOKUP(G383,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_ISO1"},"LFCU04F01_ISO1 AT%M1824.0 :BOOL; (*风机盘管04F01-隔离开关1*)","LFCU04F01_ISO1          AT%M1824.0     :BOOL; (*风机盘管04F01-隔离开关1*)"]
["1828.0","验证通过","REAL","风机盘管","L","04F01","运行时间累积值","风机盘管04F01-运行时间累积值",{"$f":"E384&VLOOKUP(D384,list!$D$3:$F$501,2,FALSE)&F384&\"_\"&VLOOKUP(G384,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RH"},"LFCU04F01_RH AT%M1828.0 :REAL; (*风机盘管04F01-运行时间累积值*)","LFCU04F01_RH            AT%M1828.0     :REAL; (*风机盘管04F01-运行时间累积值*)"]
["1832.0","验证通过","INT","风机盘管","L","04F01","设备状态代码","风机盘管04F01-设备状态代码",{"$f":"E385&VLOOKUP(D385,list!$D$3:$F$501,2,FALSE)&F385&\"_\"&VLOOKUP(G385,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_SN"},"LFCU04F01_SN AT%M1832.0 :INT; (*风机盘管04F01-设备状态代码*)","LFCU04F01_SN            AT%M1832.0     :INT; (*风机盘管04F01-设备状态代码*)"]
["1834.0","验证通过","INT","风机盘管","L","04F01","水阀控制转换值","风机盘管04F01-水阀控制转换值",{"$f":"E386&VLOOKUP(D386,list!$D$3:$F$501,2,FALSE)&F386&\"_\"&VLOOKUP(G386,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_WVCS"},"LFCU04F01_WVCS AT%M1834.0 :INT; (*风机盘管04F01-水阀控制转换值*)","LFCU04F01_WVCS          AT%M1834.0     :INT; (*风机盘管04F01-水阀控制转换值*)"]
["1836.0","验证通过","BOOL","风机盘管","L","04F01","程序控制","风机盘管04F01-程序控制",{"$f":"E387&VLOOKUP(D387,list!$D$3:$F$501,2,FALSE)&F387&\"_\"&VLOOKUP(G387,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_PC"},"LFCU04F01_PC AT%M1836.0 :BOOL; (*风机盘管04F01-程序控制*)","LFCU04F01_PC            AT%M1836.0     :BOOL; (*风机盘管04F01-程序控制*)"]
["PAU"]
[{"$f":"IF(OR(C387=\"REAL\",C387=\"DWORD\",C387=\"DINT\"),(IF(OR(C389=\"REAL\",C389=\"DWORD\",C389=\"DINT\"),A387+4+MOD(A387,4),A387+4)),(IF(OR(C389=\"REAL\",C389=\"DWORD\",C389=\"DINT\"),A387+4+MOD(A387,4),A387+2)))&\".0\"","v":"1840.0"},{"$f":"IF((IF(OR(C389=\"INT\",C389=\"WORD\",C389=\"BOOL\"),MOD(A389,2),MOD(A389,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05A01","设定温度值",{"$f":"D389&F389&\"-\"&IF(E389=\"R\",\"新云平台\"&G389,G389)","v":"P新风机组05A01-新云平台设定温度值"},{"$f":"E389&VLOOKUP(D389,list!$D$3:$F$501,2,FALSE)&F389&\"_\"&VLOOKUP(G389,list!$I$2:$K$502,2,FALSE)","v":"RPAU05A01_TSET"},{"$f":"I389&\" \"&\"AT%M\"&A389&\" \"&\":\"&C389&\";\"&\" \"&\"(*\"&H389&\"*)\"","v":"RPAU05A01_TSET AT%M1840.0 :REAL; (*P新风机组05A01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J389,SEARCH(\"AT%\",J389),,REPT(\" \",25-SEARCH(\"AT%\",J389))),SEARCH(\":\",REPLACE(J389,SEARCH(\"AT%\",J389),,REPT(\" \",25-SEARCH(\"AT%\",J389)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J389,SEARCH(\"AT%\",J389),,REPT(\" \",25-SEARCH(\"AT%\",J389))))))","v":"RPAU05A01_TSET          AT%M1840.0     :REAL; (*P新风机组05A01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C389=\"REAL\",C389=\"DWORD\",C389=\"DINT\"),(IF(OR(C390=\"REAL\",C390=\"DWORD\",C390=\"DINT\"),A389+4+MOD(A389,4),A389+4)),(IF(OR(C390=\"REAL\",C390=\"DWORD\",C390=\"DINT\"),A389+4+MOD(A389,4),A389+2)))&\".0\"","v":"1844.0"},"验证通过","INT","P新风机组","R",{"$f":"F389","v":"05A01"},"季节模式","P新风机组05A01-新云平台季节模式",{"$f":"E390&VLOOKUP(D390,list!$D$3:$F$501,2,FALSE)&F390&\"_\"&VLOOKUP(G390,list!$I$2:$K$502,2,FALSE)","v":"RPAU05A01_SM"},"RPAU05A01_SM AT%M1844.0 :INT; (*P新风机组05A01-新云平台季节模式*)","RPAU05A01_SM            AT%M1844.0     :INT; (*P新风机组05A01-新云平台季节模式*)"]
["1846.0","验证通过","BOOL","P新风机组","R","05A01","程序控制","P新风机组05A01-新云平台程序控制",{"$f":"E391&VLOOKUP(D391,list!$D$3:$F$501,2,FALSE)&F391&\"_\"&VLOOKUP(G391,list!$I$2:$K$502,2,FALSE)","v":"RPAU05A01_PC"},"RPAU05A01_PC AT%M1846.0 :BOOL; (*P新风机组05A01-新云平台程序控制*)","RPAU05A01_PC            AT%M1846.0     :BOOL; (*P新风机组05A01-新云平台程序控制*)"]
["1852.0","验证通过","REAL","P新风机组","L","05A01","设定温度值","P新风机组05A01-设定温度值",{"$f":"E392&VLOOKUP(D392,list!$D$3:$F$501,2,FALSE)&F392&\"_\"&VLOOKUP(G392,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_TSET"},"LPAU05A01_TSET AT%M1852.0 :REAL; (*P新风机组05A01-设定温度值*)","LPAU05A01_TSET          AT%M1852.0     :REAL; (*P新风机组05A01-设定温度值*)"]
["1856.0","验证通过","INT","P新风机组","L","05A01","季节模式","P新风机组05A01-季节模式",{"$f":"E393&VLOOKUP(D393,list!$D$3:$F$501,2,FALSE)&F393&\"_\"&VLOOKUP(G393,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_SM"},"LPAU05A01_SM AT%M1856.0 :INT; (*P新风机组05A01-季节模式*)","LPAU05A01_SM            AT%M1856.0     :INT; (*P新风机组05A01-季节模式*)"]
["1860.0","验证通过","REAL","P新风机组","L","05A01","水阀反馈换算值","P新风机组05A01-水阀反馈换算值",{"$f":"E394&VLOOKUP(D394,list!$D$3:$F$501,2,FALSE)&F394&\"_\"&VLOOKUP(G394,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVBS"},"LPAU05A01_WVBS AT%M1860.0 :REAL; (*P新风机组05A01-水阀反馈换算值*)","LPAU05A01_WVBS          AT%M1860.0     :REAL; (*P新风机组05A01-水阀反馈换算值*)"]
["1864.0","验证通过","BOOL","P新风机组","L","05A01","水阀手动控制","P新风机组05A01-水阀手动控制",{"$f":"E395&VLOOKUP(D395,list!$D$3:$F$501,2,FALSE)&F395&\"_\"&VLOOKUP(G395,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVMC"},"LPAU05A01_WVMC AT%M1864.0 :BOOL; (*P新风机组05A01-水阀手动控制*)","LPAU05A01_WVMC          AT%M1864.0     :BOOL; (*P新风机组05A01-水阀手动控制*)"]
["1868.0","验证通过","REAL","P新风机组","L","05A01","水阀手动控制值","P新风机组05A01-水阀手动控制值",{"$f":"E396&VLOOKUP(D396,list!$D$3:$F$501,2,FALSE)&F396&\"_\"&VLOOKUP(G396,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVMV"},"LPAU05A01_WVMV AT%M1868.0 :REAL; (*P新风机组05A01-水阀手动控制值*)","LPAU05A01_WVMV          AT%M1868.0     :REAL; (*P新风机组05A01-水阀手动控制值*)"]
["1872.0","验证通过","REAL","P新风机组","L","05A01","送风温度换算值","P新风机组05A01-送风温度换算值",{"$f":"E397&VLOOKUP(D397,list!$D$3:$F$501,2,FALSE)&F397&\"_\"&VLOOKUP(G397,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_STS"},"LPAU05A01_STS AT%M1872.0 :REAL; (*P新风机组05A01-送风温度换算值*)","LPAU05A01_STS           AT%M1872.0     :REAL; (*P新风机组05A01-送风温度换算值*)"]
["1876.0","验证通过","BOOL","P新风机组","L","05A01","运行时间累积重置","P新风机组05A01-运行时间累积重置",{"$f":"E398&VLOOKUP(D398,list!$D$3:$F$501,2,FALSE)&F398&\"_\"&VLOOKUP(G398,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_RST"},"LPAU05A01_RST AT%M1876.0 :BOOL; (*P新风机组05A01-运行时间累积重置*)","LPAU05A01_RST           AT%M1876.0     :BOOL; (*P新风机组05A01-运行时间累积重置*)"]
["1880.0","验证通过","REAL","P新风机组","L","05A01","运行时间累积重置值","P新风机组05A01-运行时间累积重置值",{"$f":"E399&VLOOKUP(D399,list!$D$3:$F$501,2,FALSE)&F399&\"_\"&VLOOKUP(G399,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_RSTV"},"LPAU05A01_RSTV AT%M1880.0 :REAL; (*P新风机组05A01-运行时间累积重置值*)","LPAU05A01_RSTV          AT%M1880.0     :REAL; (*P新风机组05A01-运行时间累积重置值*)"]
["1884.0","验证通过","BOOL","P新风机组","L","05A01","隔离开关1","P新风机组05A01-隔离开关1",{"$f":"E400&VLOOKUP(D400,list!$D$3:$F$501,2,FALSE)&F400&\"_\"&VLOOKUP(G400,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_ISO1"},"LPAU05A01_ISO1 AT%M1884.0 :BOOL; (*P新风机组05A01-隔离开关1*)","LPAU05A01_ISO1          AT%M1884.0     :BOOL; (*P新风机组05A01-隔离开关1*)"]
["1886.0","验证通过","BOOL","P新风机组","L","05A01","隔离开关2","P新风机组05A01-隔离开关2",{"$f":"E401&VLOOKUP(D401,list!$D$3:$F$501,2,FALSE)&F401&\"_\"&VLOOKUP(G401,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_ISO2"},"LPAU05A01_ISO2 AT%M1886.0 :BOOL; (*P新风机组05A01-隔离开关2*)","LPAU05A01_ISO2          AT%M1886.0     :BOOL; (*P新风机组05A01-隔离开关2*)"]
["1892.0","验证通过","REAL","P新风机组","L","05A01","P调节参数","P新风机组05A01-P调节参数",{"$f":"E402&VLOOKUP(D402,list!$D$3:$F$501,2,FALSE)&F402&\"_\"&VLOOKUP(G402,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VP"},"LPAU05A01_VP AT%M1892.0 :REAL; (*P新风机组05A01-P调节参数*)","LPAU05A01_VP            AT%M1892.0     :REAL; (*P新风机组05A01-P调节参数*)"]
["1896.0","验证通过","REAL","P新风机组","L","05A01","I调节参数","P新风机组05A01-I调节参数",{"$f":"E403&VLOOKUP(D403,list!$D$3:$F$501,2,FALSE)&F403&\"_\"&VLOOKUP(G403,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VI"},"LPAU05A01_VI AT%M1896.0 :REAL; (*P新风机组05A01-I调节参数*)","LPAU05A01_VI            AT%M1896.0     :REAL; (*P新风机组05A01-I调节参数*)"]
["1900.0","验证通过","REAL","P新风机组","L","05A01","运行时间累积值","P新风机组05A01-运行时间累积值",{"$f":"E404&VLOOKUP(D404,list!$D$3:$F$501,2,FALSE)&F404&\"_\"&VLOOKUP(G404,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_RH"},"LPAU05A01_RH AT%M1900.0 :REAL; (*P新风机组05A01-运行时间累积值*)","LPAU05A01_RH            AT%M1900.0     :REAL; (*P新风机组05A01-运行时间累积值*)"]
["1904.0","验证通过","INT","P新风机组","L","05A01","设备状态代码","P新风机组05A01-设备状态代码",{"$f":"E405&VLOOKUP(D405,list!$D$3:$F$501,2,FALSE)&F405&\"_\"&VLOOKUP(G405,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_SN"},"LPAU05A01_SN AT%M1904.0 :INT; (*P新风机组05A01-设备状态代码*)","LPAU05A01_SN            AT%M1904.0     :INT; (*P新风机组05A01-设备状态代码*)"]
["1906.0","验证通过","INT","P新风机组","L","05A01","水阀控制转换值","P新风机组05A01-水阀控制转换值",{"$f":"E406&VLOOKUP(D406,list!$D$3:$F$501,2,FALSE)&F406&\"_\"&VLOOKUP(G406,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVCS"},"LPAU05A01_WVCS AT%M1906.0 :INT; (*P新风机组05A01-水阀控制转换值*)","LPAU05A01_WVCS          AT%M1906.0     :INT; (*P新风机组05A01-水阀控制转换值*)"]
["1908.0","验证通过","BOOL","P新风机组","L","05A01","程序控制","P新风机组05A01-程序控制",{"$f":"E407&VLOOKUP(D407,list!$D$3:$F$501,2,FALSE)&F407&\"_\"&VLOOKUP(G407,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_PC"},"LPAU05A01_PC AT%M1908.0 :BOOL; (*P新风机组05A01-程序控制*)","LPAU05A01_PC            AT%M1908.0     :BOOL; (*P新风机组05A01-程序控制*)"]
["1910.0","验证通过","INT","P新风机组","L","05A01","变频手动控制值","P新风机组05A01-变频手动控制值",{"$f":"E408&VLOOKUP(D408,list!$D$3:$F$501,2,FALSE)&F408&\"_\"&VLOOKUP(G408,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VFMV"},"LPAU05A01_VFMV AT%M1910.0 :INT; (*P新风机组05A01-变频手动控制值*)","LPAU05A01_VFMV          AT%M1910.0     :INT; (*P新风机组05A01-变频手动控制值*)"]
["1912.0","验证通过","BOOL","P新风机组","L","05A01","低温断路报警隔离","P新风机组05A01-低温断路报警隔离",{"$f":"E409&VLOOKUP(D409,list!$D$3:$F$501,2,FALSE)&F409&\"_\"&VLOOKUP(G409,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_ISO3"},"LPAU05A01_ISO3 AT%M1912.0 :BOOL; (*P新风机组05A01-低温断路报警隔离*)","LPAU05A01_ISO3          AT%M1912.0     :BOOL; (*P新风机组05A01-低温断路报警隔离*)"]
["1914.0","验证通过","INT","P新风机组","L","05A01","变频器频率控制值","P新风机组05A01-变频器频率控制值",{"$f":"E410&VLOOKUP(D410,list!$D$3:$F$501,2,FALSE)&F410&\"_\"&VLOOKUP(G410,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VFCS"},"LPAU05A01_VFCS AT%M1914.0 :INT; (*P新风机组05A01-变频器频率控制值*)","LPAU05A01_VFCS          AT%M1914.0     :INT; (*P新风机组05A01-变频器频率控制值*)"]
["1916.0","验证通过","INT","P新风机组","L","05A01","变频器频率反馈值","P新风机组05A01-变频器频率反馈值",{"$f":"E411&VLOOKUP(D411,list!$D$3:$F$501,2,FALSE)&F411&\"_\"&VLOOKUP(G411,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VFBS"},"LPAU05A01_VFBS AT%M1916.0 :INT; (*P新风机组05A01-变频器频率反馈值*)","LPAU05A01_VFBS          AT%M1916.0     :INT; (*P新风机组05A01-变频器频率反馈值*)"]
["1918.0","验证通过","BOOL","P新风机组","L","05A01","联动模式","P新风机组05A01-联动模式",{"$f":"E412&VLOOKUP(D412,list!$D$3:$F$501,2,FALSE)&F412&\"_\"&VLOOKUP(G412,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_LM"},"LPAU05A01_LM AT%M1918.0 :BOOL; (*P新风机组05A01-联动模式*)","LPAU05A01_LM            AT%M1918.0     :BOOL; (*P新风机组05A01-联动模式*)"]
["1920.0","验证通过","BOOL","P新风机组","L","05A01","全天候模式","P新风机组05A01-全天候模式",{"$f":"E413&VLOOKUP(D413,list!$D$3:$F$501,2,FALSE)&F413&\"_\"&VLOOKUP(G413,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_DM"},"LPAU05A01_DM AT%M1920.0 :BOOL; (*P新风机组05A01-全天候模式*)","LPAU05A01_DM            AT%M1920.0     :BOOL; (*P新风机组05A01-全天候模式*)"]
["1924.0","验证通过","REAL","P新风机组","L","05A01","CO2设定值","P新风机组05A01-CO2设定值",{"$f":"E414&VLOOKUP(D414,list!$D$3:$F$501,2,FALSE)&F414&\"_\"&VLOOKUP(G414,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_CO2SET"},"LPAU05A01_CO2SET AT%M1924.0 :REAL; (*P新风机组05A01-CO2设定值*)","LPAU05A01_CO2SET        AT%M1924.0     :REAL; (*P新风机组05A01-CO2设定值*)"]
["1928.0","验证通过","BOOL","P新风机组","L","05A01","定时控制","P新风机组05A01-定时控制",{"$f":"E415&VLOOKUP(D415,list!$D$3:$F$501,2,FALSE)&F415&\"_\"&VLOOKUP(G415,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_TC"},"LPAU05A01_TC AT%M1928.0 :BOOL; (*P新风机组05A01-定时控制*)","LPAU05A01_TC            AT%M1928.0     :BOOL; (*P新风机组05A01-定时控制*)"]
["1930.0","验证通过","BOOL","P新风机组","L","05A01","定时模式","P新风机组05A01-定时模式",{"$f":"E416&VLOOKUP(D416,list!$D$3:$F$501,2,FALSE)&F416&\"_\"&VLOOKUP(G416,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_TM"},"LPAU05A01_TM AT%M1930.0 :BOOL; (*P新风机组05A01-定时模式*)","LPAU05A01_TM            AT%M1930.0     :BOOL; (*P新风机组05A01-定时模式*)"]
["PAU"]
[{"$f":"IF(OR(C416=\"REAL\",C416=\"DWORD\",C416=\"DINT\"),(IF(OR(C418=\"REAL\",C418=\"DWORD\",C418=\"DINT\"),A416+4+MOD(A416,4),A416+4)),(IF(OR(C418=\"REAL\",C418=\"DWORD\",C418=\"DINT\"),A416+4+MOD(A416,4),A416+2)))&\".0\"","v":"1936.0"},{"$f":"IF((IF(OR(C418=\"INT\",C418=\"WORD\",C418=\"BOOL\"),MOD(A418,2),MOD(A418,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","06A01","设定温度值",{"$f":"D418&F418&\"-\"&IF(E418=\"R\",\"新云平台\"&G418,G418)","v":"P新风机组06A01-新云平台设定温度值"},{"$f":"E418&VLOOKUP(D418,list!$D$3:$F$501,2,FALSE)&F418&\"_\"&VLOOKUP(G418,list!$I$2:$K$502,2,FALSE)","v":"RPAU06A01_TSET"},{"$f":"I418&\" \"&\"AT%M\"&A418&\" \"&\":\"&C418&\";\"&\" \"&\"(*\"&H418&\"*)\"","v":"RPAU06A01_TSET AT%M1936.0 :REAL; (*P新风机组06A01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J418,SEARCH(\"AT%\",J418),,REPT(\" \",25-SEARCH(\"AT%\",J418))),SEARCH(\":\",REPLACE(J418,SEARCH(\"AT%\",J418),,REPT(\" \",25-SEARCH(\"AT%\",J418)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J418,SEARCH(\"AT%\",J418),,REPT(\" \",25-SEARCH(\"AT%\",J418))))))","v":"RPAU06A01_TSET          AT%M1936.0     :REAL; (*P新风机组06A01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C418=\"REAL\",C418=\"DWORD\",C418=\"DINT\"),(IF(OR(C419=\"REAL\",C419=\"DWORD\",C419=\"DINT\"),A418+4+MOD(A418,4),A418+4)),(IF(OR(C419=\"REAL\",C419=\"DWORD\",C419=\"DINT\"),A418+4+MOD(A418,4),A418+2)))&\".0\"","v":"1940.0"},"验证通过","INT","P新风机组","R",{"$f":"F418","v":"06A01"},"季节模式","P新风机组06A01-新云平台季节模式",{"$f":"E419&VLOOKUP(D419,list!$D$3:$F$501,2,FALSE)&F419&\"_\"&VLOOKUP(G419,list!$I$2:$K$502,2,FALSE)","v":"RPAU06A01_SM"},"RPAU06A01_SM AT%M1940.0 :INT; (*P新风机组06A01-新云平台季节模式*)","RPAU06A01_SM            AT%M1940.0     :INT; (*P新风机组06A01-新云平台季节模式*)"]
["1942.0","验证通过","BOOL","P新风机组","R","06A01","程序控制","P新风机组06A01-新云平台程序控制",{"$f":"E420&VLOOKUP(D420,list!$D$3:$F$501,2,FALSE)&F420&\"_\"&VLOOKUP(G420,list!$I$2:$K$502,2,FALSE)","v":"RPAU06A01_PC"},"RPAU06A01_PC AT%M1942.0 :BOOL; (*P新风机组06A01-新云平台程序控制*)","RPAU06A01_PC            AT%M1942.0     :BOOL; (*P新风机组06A01-新云平台程序控制*)"]
["1948.0","验证通过","REAL","P新风机组","L","06A01","设定温度值","P新风机组06A01-设定温度值",{"$f":"E421&VLOOKUP(D421,list!$D$3:$F$501,2,FALSE)&F421&\"_\"&VLOOKUP(G421,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_TSET"},"LPAU06A01_TSET AT%M1948.0 :REAL; (*P新风机组06A01-设定温度值*)","LPAU06A01_TSET          AT%M1948.0     :REAL; (*P新风机组06A01-设定温度值*)"]
["1952.0","验证通过","INT","P新风机组","L","06A01","季节模式","P新风机组06A01-季节模式",{"$f":"E422&VLOOKUP(D422,list!$D$3:$F$501,2,FALSE)&F422&\"_\"&VLOOKUP(G422,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_SM"},"LPAU06A01_SM AT%M1952.0 :INT; (*P新风机组06A01-季节模式*)","LPAU06A01_SM            AT%M1952.0     :INT; (*P新风机组06A01-季节模式*)"]
["1956.0","验证通过","REAL","P新风机组","L","06A01","水阀反馈换算值","P新风机组06A01-水阀反馈换算值",{"$f":"E423&VLOOKUP(D423,list!$D$3:$F$501,2,FALSE)&F423&\"_\"&VLOOKUP(G423,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVBS"},"LPAU06A01_WVBS AT%M1956.0 :REAL; (*P新风机组06A01-水阀反馈换算值*)","LPAU06A01_WVBS          AT%M1956.0     :REAL; (*P新风机组06A01-水阀反馈换算值*)"]
["1960.0","验证通过","BOOL","P新风机组","L","06A01","水阀手动控制","P新风机组06A01-水阀手动控制",{"$f":"E424&VLOOKUP(D424,list!$D$3:$F$501,2,FALSE)&F424&\"_\"&VLOOKUP(G424,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVMC"},"LPAU06A01_WVMC AT%M1960.0 :BOOL; (*P新风机组06A01-水阀手动控制*)","LPAU06A01_WVMC          AT%M1960.0     :BOOL; (*P新风机组06A01-水阀手动控制*)"]
["1964.0","验证通过","REAL","P新风机组","L","06A01","水阀手动控制值","P新风机组06A01-水阀手动控制值",{"$f":"E425&VLOOKUP(D425,list!$D$3:$F$501,2,FALSE)&F425&\"_\"&VLOOKUP(G425,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVMV"},"LPAU06A01_WVMV AT%M1964.0 :REAL; (*P新风机组06A01-水阀手动控制值*)","LPAU06A01_WVMV          AT%M1964.0     :REAL; (*P新风机组06A01-水阀手动控制值*)"]
["1968.0","验证通过","REAL","P新风机组","L","06A01","送风温度换算值","P新风机组06A01-送风温度换算值",{"$f":"E426&VLOOKUP(D426,list!$D$3:$F$501,2,FALSE)&F426&\"_\"&VLOOKUP(G426,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_STS"},"LPAU06A01_STS AT%M1968.0 :REAL; (*P新风机组06A01-送风温度换算值*)","LPAU06A01_STS           AT%M1968.0     :REAL; (*P新风机组06A01-送风温度换算值*)"]
["1972.0","验证通过","BOOL","P新风机组","L","06A01","运行时间累积重置","P新风机组06A01-运行时间累积重置",{"$f":"E427&VLOOKUP(D427,list!$D$3:$F$501,2,FALSE)&F427&\"_\"&VLOOKUP(G427,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_RST"},"LPAU06A01_RST AT%M1972.0 :BOOL; (*P新风机组06A01-运行时间累积重置*)","LPAU06A01_RST           AT%M1972.0     :BOOL; (*P新风机组06A01-运行时间累积重置*)"]
["1976.0","验证通过","REAL","P新风机组","L","06A01","运行时间累积重置值","P新风机组06A01-运行时间累积重置值",{"$f":"E428&VLOOKUP(D428,list!$D$3:$F$501,2,FALSE)&F428&\"_\"&VLOOKUP(G428,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_RSTV"},"LPAU06A01_RSTV AT%M1976.0 :REAL; (*P新风机组06A01-运行时间累积重置值*)","LPAU06A01_RSTV          AT%M1976.0     :REAL; (*P新风机组06A01-运行时间累积重置值*)"]
["1980.0","验证通过","BOOL","P新风机组","L","06A01","隔离开关1","P新风机组06A01-隔离开关1",{"$f":"E429&VLOOKUP(D429,list!$D$3:$F$501,2,FALSE)&F429&\"_\"&VLOOKUP(G429,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_ISO1"},"LPAU06A01_ISO1 AT%M1980.0 :BOOL; (*P新风机组06A01-隔离开关1*)","LPAU06A01_ISO1          AT%M1980.0     :BOOL; (*P新风机组06A01-隔离开关1*)"]
["1982.0","验证通过","BOOL","P新风机组","L","06A01","隔离开关2","P新风机组06A01-隔离开关2",{"$f":"E430&VLOOKUP(D430,list!$D$3:$F$501,2,FALSE)&F430&\"_\"&VLOOKUP(G430,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_ISO2"},"LPAU06A01_ISO2 AT%M1982.0 :BOOL; (*P新风机组06A01-隔离开关2*)","LPAU06A01_ISO2          AT%M1982.0     :BOOL; (*P新风机组06A01-隔离开关2*)"]
["1988.0","验证通过","REAL","P新风机组","L","06A01","P调节参数","P新风机组06A01-P调节参数",{"$f":"E431&VLOOKUP(D431,list!$D$3:$F$501,2,FALSE)&F431&\"_\"&VLOOKUP(G431,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VP"},"LPAU06A01_VP AT%M1988.0 :REAL; (*P新风机组06A01-P调节参数*)","LPAU06A01_VP            AT%M1988.0     :REAL; (*P新风机组06A01-P调节参数*)"]
["1992.0","验证通过","REAL","P新风机组","L","06A01","I调节参数","P新风机组06A01-I调节参数",{"$f":"E432&VLOOKUP(D432,list!$D$3:$F$501,2,FALSE)&F432&\"_\"&VLOOKUP(G432,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VI"},"LPAU06A01_VI AT%M1992.0 :REAL; (*P新风机组06A01-I调节参数*)","LPAU06A01_VI            AT%M1992.0     :REAL; (*P新风机组06A01-I调节参数*)"]
["1996.0","验证通过","REAL","P新风机组","L","06A01","运行时间累积值","P新风机组06A01-运行时间累积值",{"$f":"E433&VLOOKUP(D433,list!$D$3:$F$501,2,FALSE)&F433&\"_\"&VLOOKUP(G433,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_RH"},"LPAU06A01_RH AT%M1996.0 :REAL; (*P新风机组06A01-运行时间累积值*)","LPAU06A01_RH            AT%M1996.0     :REAL; (*P新风机组06A01-运行时间累积值*)"]
["2000.0","验证通过","INT","P新风机组","L","06A01","设备状态代码","P新风机组06A01-设备状态代码",{"$f":"E434&VLOOKUP(D434,list!$D$3:$F$501,2,FALSE)&F434&\"_\"&VLOOKUP(G434,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_SN"},"LPAU06A01_SN AT%M2000.0 :INT; (*P新风机组06A01-设备状态代码*)","LPAU06A01_SN            AT%M2000.0     :INT; (*P新风机组06A01-设备状态代码*)"]
["2002.0","验证通过","INT","P新风机组","L","06A01","水阀控制转换值","P新风机组06A01-水阀控制转换值",{"$f":"E435&VLOOKUP(D435,list!$D$3:$F$501,2,FALSE)&F435&\"_\"&VLOOKUP(G435,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVCS"},"LPAU06A01_WVCS AT%M2002.0 :INT; (*P新风机组06A01-水阀控制转换值*)","LPAU06A01_WVCS          AT%M2002.0     :INT; (*P新风机组06A01-水阀控制转换值*)"]
["2004.0","验证通过","BOOL","P新风机组","L","06A01","程序控制","P新风机组06A01-程序控制",{"$f":"E436&VLOOKUP(D436,list!$D$3:$F$501,2,FALSE)&F436&\"_\"&VLOOKUP(G436,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_PC"},"LPAU06A01_PC AT%M2004.0 :BOOL; (*P新风机组06A01-程序控制*)","LPAU06A01_PC            AT%M2004.0     :BOOL; (*P新风机组06A01-程序控制*)"]
["2006.0","验证通过","INT","P新风机组","L","06A01","变频手动控制值","P新风机组06A01-变频手动控制值",{"$f":"E437&VLOOKUP(D437,list!$D$3:$F$501,2,FALSE)&F437&\"_\"&VLOOKUP(G437,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VFMV"},"LPAU06A01_VFMV AT%M2006.0 :INT; (*P新风机组06A01-变频手动控制值*)","LPAU06A01_VFMV          AT%M2006.0     :INT; (*P新风机组06A01-变频手动控制值*)"]
["2008.0","验证通过","BOOL","P新风机组","L","06A01","低温断路报警隔离","P新风机组06A01-低温断路报警隔离",{"$f":"E438&VLOOKUP(D438,list!$D$3:$F$501,2,FALSE)&F438&\"_\"&VLOOKUP(G438,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_ISO3"},"LPAU06A01_ISO3 AT%M2008.0 :BOOL; (*P新风机组06A01-低温断路报警隔离*)","LPAU06A01_ISO3          AT%M2008.0     :BOOL; (*P新风机组06A01-低温断路报警隔离*)"]
["2010.0","验证通过","INT","P新风机组","L","06A01","变频器频率控制值","P新风机组06A01-变频器频率控制值",{"$f":"E439&VLOOKUP(D439,list!$D$3:$F$501,2,FALSE)&F439&\"_\"&VLOOKUP(G439,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VFCS"},"LPAU06A01_VFCS AT%M2010.0 :INT; (*P新风机组06A01-变频器频率控制值*)","LPAU06A01_VFCS          AT%M2010.0     :INT; (*P新风机组06A01-变频器频率控制值*)"]
["2012.0","验证通过","INT","P新风机组","L","06A01","变频器频率反馈值","P新风机组06A01-变频器频率反馈值",{"$f":"E440&VLOOKUP(D440,list!$D$3:$F$501,2,FALSE)&F440&\"_\"&VLOOKUP(G440,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VFBS"},"LPAU06A01_VFBS AT%M2012.0 :INT; (*P新风机组06A01-变频器频率反馈值*)","LPAU06A01_VFBS          AT%M2012.0     :INT; (*P新风机组06A01-变频器频率反馈值*)"]
["2014.0","验证通过","BOOL","P新风机组","L","06A01","联动模式","P新风机组06A01-联动模式",{"$f":"E441&VLOOKUP(D441,list!$D$3:$F$501,2,FALSE)&F441&\"_\"&VLOOKUP(G441,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_LM"},"LPAU06A01_LM AT%M2014.0 :BOOL; (*P新风机组06A01-联动模式*)","LPAU06A01_LM            AT%M2014.0     :BOOL; (*P新风机组06A01-联动模式*)"]
["2016.0","验证通过","BOOL","P新风机组","L","06A01","全天候模式","P新风机组06A01-全天候模式",{"$f":"E442&VLOOKUP(D442,list!$D$3:$F$501,2,FALSE)&F442&\"_\"&VLOOKUP(G442,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_DM"},"LPAU06A01_DM AT%M2016.0 :BOOL; (*P新风机组06A01-全天候模式*)","LPAU06A01_DM            AT%M2016.0     :BOOL; (*P新风机组06A01-全天候模式*)"]
["2020.0","验证通过","REAL","P新风机组","L","06A01","CO2设定值","P新风机组06A01-CO2设定值",{"$f":"E443&VLOOKUP(D443,list!$D$3:$F$501,2,FALSE)&F443&\"_\"&VLOOKUP(G443,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_CO2SET"},"LPAU06A01_CO2SET AT%M2020.0 :REAL; (*P新风机组06A01-CO2设定值*)","LPAU06A01_CO2SET        AT%M2020.0     :REAL; (*P新风机组06A01-CO2设定值*)"]
["2024.0","验证通过","BOOL","P新风机组","L","06A01","定时控制","P新风机组06A01-定时控制",{"$f":"E444&VLOOKUP(D444,list!$D$3:$F$501,2,FALSE)&F444&\"_\"&VLOOKUP(G444,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_TC"},"LPAU06A01_TC AT%M2024.0 :BOOL; (*P新风机组06A01-定时控制*)","LPAU06A01_TC            AT%M2024.0     :BOOL; (*P新风机组06A01-定时控制*)"]
["2026.0","验证通过","BOOL","P新风机组","L","06A01","定时模式","P新风机组06A01-定时模式",{"$f":"E445&VLOOKUP(D445,list!$D$3:$F$501,2,FALSE)&F445&\"_\"&VLOOKUP(G445,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_TM"},"LPAU06A01_TM AT%M2026.0 :BOOL; (*P新风机组06A01-定时模式*)","LPAU06A01_TM            AT%M2026.0     :BOOL; (*P新风机组06A01-定时模式*)"]
["AHU"]
[{"$f":"IF(OR(C360=\"REAL\",C360=\"DWORD\",C360=\"DINT\"),(IF(OR(C447=\"REAL\",C447=\"DWORD\",C447=\"DINT\"),A360+4+MOD(A360,4),A360+4)),(IF(OR(C447=\"REAL\",C447=\"DWORD\",C447=\"DINT\"),A360+4+MOD(A360,4),A360+2)))&\".0\"","v":"1320.0"},{"$f":"IF((IF(OR(C447=\"INT\",C447=\"WORD\",C447=\"BOOL\"),MOD(A447,2),MOD(A447,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04H07","设定温度值",{"$f":"D447&F447&\"-\"&IF(E447=\"R\",\"新云平台\"&G447,G447)","v":"空调机组04H07-新云平台设定温度值"},{"$f":"E447&VLOOKUP(D447,list!$D$3:$F$501,2,FALSE)&F447&\"_\"&VLOOKUP(G447,list!$I$2:$K$502,2,FALSE)","v":"RAHU04H07_TSET"},{"$f":"I447&\" \"&\"AT%M\"&A447&\" \"&\":\"&C447&\";\"&\" \"&\"(*\"&H447&\"*)\"","v":"RAHU04H07_TSET AT%M1320.0 :REAL; (*空调机组04H07-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J447,SEARCH(\"AT%\",J447),,REPT(\" \",25-SEARCH(\"AT%\",J447))),SEARCH(\":\",REPLACE(J447,SEARCH(\"AT%\",J447),,REPT(\" \",25-SEARCH(\"AT%\",J447)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J447,SEARCH(\"AT%\",J447),,REPT(\" \",25-SEARCH(\"AT%\",J447))))))","v":"RAHU04H07_TSET          AT%M1320.0     :REAL; (*空调机组04H07-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C447=\"REAL\",C447=\"DWORD\",C447=\"DINT\"),(IF(OR(C448=\"REAL\",C448=\"DWORD\",C448=\"DINT\"),A447+4+MOD(A447,4),A447+4)),(IF(OR(C448=\"REAL\",C448=\"DWORD\",C448=\"DINT\"),A447+4+MOD(A447,4),A447+2)))&\".0\"","v":"1324.0"},"验证通过","INT","空调机组","R",{"$f":"F447","v":"04H07"},"季节模式","空调机组04H07-新云平台季节模式",{"$f":"E448&VLOOKUP(D448,list!$D$3:$F$501,2,FALSE)&F448&\"_\"&VLOOKUP(G448,list!$I$2:$K$502,2,FALSE)","v":"RAHU04H07_SM"},"RAHU04H07_SM AT%M1324.0 :INT; (*空调机组04H07-新云平台季节模式*)","RAHU04H07_SM            AT%M1324.0     :INT; (*空调机组04H07-新云平台季节模式*)"]
["1326.0","验证通过","BOOL","空调机组","R","04H07","程序控制","空调机组04H07-新云平台程序控制",{"$f":"E449&VLOOKUP(D449,list!$D$3:$F$501,2,FALSE)&F449&\"_\"&VLOOKUP(G449,list!$I$2:$K$502,2,FALSE)","v":"RAHU04H07_PC"},"RAHU04H07_PC AT%M1326.0 :BOOL; (*空调机组04H07-新云平台程序控制*)","RAHU04H07_PC            AT%M1326.0     :BOOL; (*空调机组04H07-新云平台程序控制*)"]
["1332.0","验证通过","REAL","空调机组","L","04H07","设定温度值","空调机组04H07-设定温度值",{"$f":"E450&VLOOKUP(D450,list!$D$3:$F$501,2,FALSE)&F450&\"_\"&VLOOKUP(G450,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_TSET"},"LAHU04H07_TSET AT%M1332.0 :REAL; (*空调机组04H07-设定温度值*)","LAHU04H07_TSET          AT%M1332.0     :REAL; (*空调机组04H07-设定温度值*)"]
["1336.0","验证通过","INT","空调机组","L","04H07","季节模式","空调机组04H07-季节模式",{"$f":"E451&VLOOKUP(D451,list!$D$3:$F$501,2,FALSE)&F451&\"_\"&VLOOKUP(G451,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_SM"},"LAHU04H07_SM AT%M1336.0 :INT; (*空调机组04H07-季节模式*)","LAHU04H07_SM            AT%M1336.0     :INT; (*空调机组04H07-季节模式*)"]
["1340.0","验证通过","REAL","空调机组","L","04H07","水阀反馈换算值","空调机组04H07-水阀反馈换算值",{"$f":"E452&VLOOKUP(D452,list!$D$3:$F$501,2,FALSE)&F452&\"_\"&VLOOKUP(G452,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_WVBS"},"LAHU04H07_WVBS AT%M1340.0 :REAL; (*空调机组04H07-水阀反馈换算值*)","LAHU04H07_WVBS          AT%M1340.0     :REAL; (*空调机组04H07-水阀反馈换算值*)"]
["1344.0","验证通过","BOOL","空调机组","L","04H07","水阀手动控制","空调机组04H07-水阀手动控制",{"$f":"E453&VLOOKUP(D453,list!$D$3:$F$501,2,FALSE)&F453&\"_\"&VLOOKUP(G453,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_WVMC"},"LAHU04H07_WVMC AT%M1344.0 :BOOL; (*空调机组04H07-水阀手动控制*)","LAHU04H07_WVMC          AT%M1344.0     :BOOL; (*空调机组04H07-水阀手动控制*)"]
["1348.0","验证通过","REAL","空调机组","L","04H07","水阀手动控制值","空调机组04H07-水阀手动控制值",{"$f":"E454&VLOOKUP(D454,list!$D$3:$F$501,2,FALSE)&F454&\"_\"&VLOOKUP(G454,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_WVMV"},"LAHU04H07_WVMV AT%M1348.0 :REAL; (*空调机组04H07-水阀手动控制值*)","LAHU04H07_WVMV          AT%M1348.0     :REAL; (*空调机组04H07-水阀手动控制值*)"]
["1352.0","验证通过","REAL","空调机组","L","04H07","回风温度换算值","空调机组04H07-回风温度换算值",{"$f":"E455&VLOOKUP(D455,list!$D$3:$F$501,2,FALSE)&F455&\"_\"&VLOOKUP(G455,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_RTS"},"LAHU04H07_RTS AT%M1352.0 :REAL; (*空调机组04H07-回风温度换算值*)","LAHU04H07_RTS           AT%M1352.0     :REAL; (*空调机组04H07-回风温度换算值*)"]
["1356.0","验证通过","BOOL","空调机组","L","04H07","运行时间累积重置","空调机组04H07-运行时间累积重置",{"$f":"E456&VLOOKUP(D456,list!$D$3:$F$501,2,FALSE)&F456&\"_\"&VLOOKUP(G456,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_RST"},"LAHU04H07_RST AT%M1356.0 :BOOL; (*空调机组04H07-运行时间累积重置*)","LAHU04H07_RST           AT%M1356.0     :BOOL; (*空调机组04H07-运行时间累积重置*)"]
["1360.0","验证通过","REAL","空调机组","L","04H07","运行时间累积重置值","空调机组04H07-运行时间累积重置值",{"$f":"E457&VLOOKUP(D457,list!$D$3:$F$501,2,FALSE)&F457&\"_\"&VLOOKUP(G457,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_RSTV"},"LAHU04H07_RSTV AT%M1360.0 :REAL; (*空调机组04H07-运行时间累积重置值*)","LAHU04H07_RSTV          AT%M1360.0     :REAL; (*空调机组04H07-运行时间累积重置值*)"]
["1364.0","验证通过","BOOL","空调机组","L","04H07","隔离开关1","空调机组04H07-隔离开关1",{"$f":"E458&VLOOKUP(D458,list!$D$3:$F$501,2,FALSE)&F458&\"_\"&VLOOKUP(G458,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_ISO1"},"LAHU04H07_ISO1 AT%M1364.0 :BOOL; (*空调机组04H07-隔离开关1*)","LAHU04H07_ISO1          AT%M1364.0     :BOOL; (*空调机组04H07-隔离开关1*)"]
["1366.0","验证通过","BOOL","空调机组","L","04H07","隔离开关2","空调机组04H07-隔离开关2",{"$f":"E459&VLOOKUP(D459,list!$D$3:$F$501,2,FALSE)&F459&\"_\"&VLOOKUP(G459,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_ISO2"},"LAHU04H07_ISO2 AT%M1366.0 :BOOL; (*空调机组04H07-隔离开关2*)","LAHU04H07_ISO2          AT%M1366.0     :BOOL; (*空调机组04H07-隔离开关2*)"]
["1372.0","验证通过","REAL","空调机组","L","04H07","P调节参数","空调机组04H07-P调节参数",{"$f":"E460&VLOOKUP(D460,list!$D$3:$F$501,2,FALSE)&F460&\"_\"&VLOOKUP(G460,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_VP"},"LAHU04H07_VP AT%M1372.0 :REAL; (*空调机组04H07-P调节参数*)","LAHU04H07_VP            AT%M1372.0     :REAL; (*空调机组04H07-P调节参数*)"]
["1376.0","验证通过","REAL","空调机组","L","04H07","I调节参数","空调机组04H07-I调节参数",{"$f":"E461&VLOOKUP(D461,list!$D$3:$F$501,2,FALSE)&F461&\"_\"&VLOOKUP(G461,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_VI"},"LAHU04H07_VI AT%M1376.0 :REAL; (*空调机组04H07-I调节参数*)","LAHU04H07_VI            AT%M1376.0     :REAL; (*空调机组04H07-I调节参数*)"]
["1380.0","验证通过","REAL","空调机组","L","04H07","运行时间累积值","空调机组04H07-运行时间累积值",{"$f":"E462&VLOOKUP(D462,list!$D$3:$F$501,2,FALSE)&F462&\"_\"&VLOOKUP(G462,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_RH"},"LAHU04H07_RH AT%M1380.0 :REAL; (*空调机组04H07-运行时间累积值*)","LAHU04H07_RH            AT%M1380.0     :REAL; (*空调机组04H07-运行时间累积值*)"]
["1384.0","验证通过","INT","空调机组","L","04H07","设备状态代码","空调机组04H07-设备状态代码",{"$f":"E463&VLOOKUP(D463,list!$D$3:$F$501,2,FALSE)&F463&\"_\"&VLOOKUP(G463,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_SN"},"LAHU04H07_SN AT%M1384.0 :INT; (*空调机组04H07-设备状态代码*)","LAHU04H07_SN            AT%M1384.0     :INT; (*空调机组04H07-设备状态代码*)"]
["1386.0","验证通过","INT","空调机组","L","04H07","水阀控制转换值","空调机组04H07-水阀控制转换值",{"$f":"E464&VLOOKUP(D464,list!$D$3:$F$501,2,FALSE)&F464&\"_\"&VLOOKUP(G464,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_WVCS"},"LAHU04H07_WVCS AT%M1386.0 :INT; (*空调机组04H07-水阀控制转换值*)","LAHU04H07_WVCS          AT%M1386.0     :INT; (*空调机组04H07-水阀控制转换值*)"]
["1388.0","验证通过","BOOL","空调机组","L","04H07","程序控制","空调机组04H07-程序控制",{"$f":"E465&VLOOKUP(D465,list!$D$3:$F$501,2,FALSE)&F465&\"_\"&VLOOKUP(G465,list!$I$2:$K$502,2,FALSE)","v":"LAHU04H07_PC"},"LAHU04H07_PC AT%M1388.0 :BOOL; (*空调机组04H07-程序控制*)","LAHU04H07_PC            AT%M1388.0     :BOOL; (*空调机组04H07-程序控制*)"]
["EAF"]
[{"$f":"IF(OR(C465=\"REAL\",C465=\"DWORD\",C465=\"DINT\"),(IF(OR(C467=\"REAL\",C467=\"DWORD\",C467=\"DINT\"),A465+4+MOD(A465,4),A465+4)),(IF(OR(C467=\"REAL\",C467=\"DWORD\",C467=\"DINT\"),A465+4+MOD(A465,4),A465+2)))&\".0\"","v":"1390.0"},{"$f":"IF((IF(OR(C467=\"INT\",C467=\"WORD\",C467=\"BOOL\"),MOD(A467,2),MOD(A467,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","04H01","启停控制",{"$f":"D467&F467&\"-\"&IF(E467=\"R\",\"新云平台\"&G467,G467)","v":"排风机04H01-新云平台启停控制"},{"$f":"E467&VLOOKUP(D467,[1]list!$D$3:$F$501,2,FALSE)&F467&\"_\"&VLOOKUP(G467,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04H01_C"},{"$f":"I467&\" \"&\"AT%M\"&A467&\" \"&\":\"&C467&\";\"&\" \"&\"(*\"&H467&\"*)\"","v":"REAF04H01_C AT%M1390.0 :BOOL; (*排风机04H01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J467,SEARCH(\"AT%\",J467),,REPT(\" \",25-SEARCH(\"AT%\",J467))),SEARCH(\":\",REPLACE(J467,SEARCH(\"AT%\",J467),,REPT(\" \",25-SEARCH(\"AT%\",J467)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J467,SEARCH(\"AT%\",J467),,REPT(\" \",25-SEARCH(\"AT%\",J467))))))","v":"REAF04H01_C             AT%M1390.0     :BOOL; (*排风机04H01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C467=\"REAL\",C467=\"DWORD\",C467=\"DINT\"),(IF(OR(C468=\"REAL\",C468=\"DWORD\",C468=\"DINT\"),A467+4+MOD(A467,4),A467+4)),(IF(OR(C468=\"REAL\",C468=\"DWORD\",C468=\"DINT\"),A467+4+MOD(A467,4),A467+2)))&\".0\"","v":"1392.0"},"验证通过","BOOL","排风机","L","04H01","运行时间累积重置","排风机04H01-运行时间累积重置",{"$f":"E468&VLOOKUP(D468,[1]list!$D$3:$F$501,2,FALSE)&F468&\"_\"&VLOOKUP(G468,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_RST"},"LEAF04H01_RST AT%M1392.0 :BOOL; (*排风机04H01-运行时间累积重置*)","LEAF04H01_RST           AT%M1392.0     :BOOL; (*排风机04H01-运行时间累积重置*)"]
["1396.0","验证通过","REAL","排风机","L","04H01","运行时间累积重置值","排风机04H01-运行时间累积重置值",{"$f":"E469&VLOOKUP(D469,[1]list!$D$3:$F$501,2,FALSE)&F469&\"_\"&VLOOKUP(G469,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_RSTV"},"LEAF04H01_RSTV AT%M1396.0 :REAL; (*排风机04H01-运行时间累积重置值*)","LEAF04H01_RSTV          AT%M1396.0     :REAL; (*排风机04H01-运行时间累积重置值*)"]
["1400.0","验证通过","REAL","排风机","L","04H01","运行时间累积值","排风机04H01-运行时间累积值",{"$f":"E470&VLOOKUP(D470,[1]list!$D$3:$F$501,2,FALSE)&F470&\"_\"&VLOOKUP(G470,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_RH"},"LEAF04H01_RH AT%M1400.0 :REAL; (*排风机04H01-运行时间累积值*)","LEAF04H01_RH            AT%M1400.0     :REAL; (*排风机04H01-运行时间累积值*)"]
["1404.0","验证通过","BOOL","排风机","L","04H01","定时模式","排风机04H01-定时模式",{"$f":"E471&VLOOKUP(D471,[1]list!$D$3:$F$501,2,FALSE)&F471&\"_\"&VLOOKUP(G471,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_TM"},"LEAF04H01_TM AT%M1404.0 :BOOL; (*排风机04H01-定时模式*)","LEAF04H01_TM            AT%M1404.0     :BOOL; (*排风机04H01-定时模式*)"]
["1406.0","验证通过","BOOL","排风机","L","04H01","定时控制","排风机04H01-定时控制",{"$f":"E472&VLOOKUP(D472,[1]list!$D$3:$F$501,2,FALSE)&F472&\"_\"&VLOOKUP(G472,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_TC"},"LEAF04H01_TC AT%M1406.0 :BOOL; (*排风机04H01-定时控制*)","LEAF04H01_TC            AT%M1406.0     :BOOL; (*排风机04H01-定时控制*)"]
["1408.0","验证通过","BOOL","排风机","L","04H01","全天候模式","排风机04H01-全天候模式",{"$f":"E473&VLOOKUP(D473,[1]list!$D$3:$F$501,2,FALSE)&F473&\"_\"&VLOOKUP(G473,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_DM"},"LEAF04H01_DM AT%M1408.0 :BOOL; (*排风机04H01-全天候模式*)","LEAF04H01_DM            AT%M1408.0     :BOOL; (*排风机04H01-全天候模式*)"]
["1412.0","验证通过","REAL","排风机","L","04H01","CO设定值","排风机04H01-CO设定值",{"$f":"E474&VLOOKUP(D474,[1]list!$D$3:$F$501,2,FALSE)&F474&\"_\"&VLOOKUP(G474,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_COSET"},"LEAF04H01_COSET AT%M1412.0 :REAL; (*排风机04H01-CO设定值*)","LEAF04H01_COSET         AT%M1412.0     :REAL; (*排风机04H01-CO设定值*)"]
["1416.0","验证通过","REAL","排风机","L","04H01","设定温度值","排风机04H01-设定温度值",{"$f":"E475&VLOOKUP(D475,[1]list!$D$3:$F$501,2,FALSE)&F475&\"_\"&VLOOKUP(G475,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H01_TSET"},"LEAF04H01_TSET AT%M1416.0 :REAL; (*排风机04H01-设定温度值*)","LEAF04H01_TSET          AT%M1416.0     :REAL; (*排风机04H01-设定温度值*)"]
["EAF"]
[{"$f":"IF(OR(C475=\"REAL\",C475=\"DWORD\",C475=\"DINT\"),(IF(OR(C477=\"REAL\",C477=\"DWORD\",C477=\"DINT\"),A475+4+MOD(A475,4),A475+4)),(IF(OR(C477=\"REAL\",C477=\"DWORD\",C477=\"DINT\"),A475+4+MOD(A475,4),A475+2)))&\".0\"","v":"1420.0"},{"$f":"IF((IF(OR(C477=\"INT\",C477=\"WORD\",C477=\"BOOL\"),MOD(A477,2),MOD(A477,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","04H02","启停控制",{"$f":"D477&F477&\"-\"&IF(E477=\"R\",\"新云平台\"&G477,G477)","v":"排风机04H02-新云平台启停控制"},{"$f":"E477&VLOOKUP(D477,[1]list!$D$3:$F$501,2,FALSE)&F477&\"_\"&VLOOKUP(G477,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04H02_C"},{"$f":"I477&\" \"&\"AT%M\"&A477&\" \"&\":\"&C477&\";\"&\" \"&\"(*\"&H477&\"*)\"","v":"REAF04H02_C AT%M1420.0 :BOOL; (*排风机04H02-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J477,SEARCH(\"AT%\",J477),,REPT(\" \",25-SEARCH(\"AT%\",J477))),SEARCH(\":\",REPLACE(J477,SEARCH(\"AT%\",J477),,REPT(\" \",25-SEARCH(\"AT%\",J477)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J477,SEARCH(\"AT%\",J477),,REPT(\" \",25-SEARCH(\"AT%\",J477))))))","v":"REAF04H02_C             AT%M1420.0     :BOOL; (*排风机04H02-新云平台启停控制*)"}]
[{"$f":"IF(OR(C477=\"REAL\",C477=\"DWORD\",C477=\"DINT\"),(IF(OR(C478=\"REAL\",C478=\"DWORD\",C478=\"DINT\"),A477+4+MOD(A477,4),A477+4)),(IF(OR(C478=\"REAL\",C478=\"DWORD\",C478=\"DINT\"),A477+4+MOD(A477,4),A477+2)))&\".0\"","v":"1422.0"},"验证通过","BOOL","排风机","L","04H02","运行时间累积重置","排风机04H02-运行时间累积重置",{"$f":"E478&VLOOKUP(D478,[1]list!$D$3:$F$501,2,FALSE)&F478&\"_\"&VLOOKUP(G478,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_RST"},"LEAF04H02_RST AT%M1422.0 :BOOL; (*排风机04H02-运行时间累积重置*)","LEAF04H02_RST           AT%M1422.0     :BOOL; (*排风机04H02-运行时间累积重置*)"]
["1428.0","验证通过","REAL","排风机","L","04H02","运行时间累积重置值","排风机04H02-运行时间累积重置值",{"$f":"E479&VLOOKUP(D479,[1]list!$D$3:$F$501,2,FALSE)&F479&\"_\"&VLOOKUP(G479,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_RSTV"},"LEAF04H02_RSTV AT%M1428.0 :REAL; (*排风机04H02-运行时间累积重置值*)","LEAF04H02_RSTV          AT%M1428.0     :REAL; (*排风机04H02-运行时间累积重置值*)"]
["1432.0","验证通过","REAL","排风机","L","04H02","运行时间累积值","排风机04H02-运行时间累积值",{"$f":"E480&VLOOKUP(D480,[1]list!$D$3:$F$501,2,FALSE)&F480&\"_\"&VLOOKUP(G480,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_RH"},"LEAF04H02_RH AT%M1432.0 :REAL; (*排风机04H02-运行时间累积值*)","LEAF04H02_RH            AT%M1432.0     :REAL; (*排风机04H02-运行时间累积值*)"]
["1436.0","验证通过","BOOL","排风机","L","04H02","定时模式","排风机04H02-定时模式",{"$f":"E481&VLOOKUP(D481,[1]list!$D$3:$F$501,2,FALSE)&F481&\"_\"&VLOOKUP(G481,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_TM"},"LEAF04H02_TM AT%M1436.0 :BOOL; (*排风机04H02-定时模式*)","LEAF04H02_TM            AT%M1436.0     :BOOL; (*排风机04H02-定时模式*)"]
["1438.0","验证通过","BOOL","排风机","L","04H02","定时控制","排风机04H02-定时控制",{"$f":"E482&VLOOKUP(D482,[1]list!$D$3:$F$501,2,FALSE)&F482&\"_\"&VLOOKUP(G482,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_TC"},"LEAF04H02_TC AT%M1438.0 :BOOL; (*排风机04H02-定时控制*)","LEAF04H02_TC            AT%M1438.0     :BOOL; (*排风机04H02-定时控制*)"]
["1440.0","验证通过","BOOL","排风机","L","04H02","全天候模式","排风机04H02-全天候模式",{"$f":"E483&VLOOKUP(D483,[1]list!$D$3:$F$501,2,FALSE)&F483&\"_\"&VLOOKUP(G483,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_DM"},"LEAF04H02_DM AT%M1440.0 :BOOL; (*排风机04H02-全天候模式*)","LEAF04H02_DM            AT%M1440.0     :BOOL; (*排风机04H02-全天候模式*)"]
["1444.0","验证通过","REAL","排风机","L","04H02","CO设定值","排风机04H02-CO设定值",{"$f":"E484&VLOOKUP(D484,[1]list!$D$3:$F$501,2,FALSE)&F484&\"_\"&VLOOKUP(G484,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_COSET"},"LEAF04H02_COSET AT%M1444.0 :REAL; (*排风机04H02-CO设定值*)","LEAF04H02_COSET         AT%M1444.0     :REAL; (*排风机04H02-CO设定值*)"]
["1448.0","验证通过","REAL","排风机","L","04H02","设定温度值","排风机04H02-设定温度值",{"$f":"E485&VLOOKUP(D485,[1]list!$D$3:$F$501,2,FALSE)&F485&\"_\"&VLOOKUP(G485,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H02_TSET"},"LEAF04H02_TSET AT%M1448.0 :REAL; (*排风机04H02-设定温度值*)","LEAF04H02_TSET          AT%M1448.0     :REAL; (*排风机04H02-设定温度值*)"]
["EAF"]
[{"$f":"IF(OR(C465=\"REAL\",C465=\"DWORD\",C465=\"DINT\"),(IF(OR(C487=\"REAL\",C487=\"DWORD\",C487=\"DINT\"),A465+4+MOD(A465,4),A465+4)),(IF(OR(C487=\"REAL\",C487=\"DWORD\",C487=\"DINT\"),A465+4+MOD(A465,4),A465+2)))&\".0\"","v":"1390.0"},{"$f":"IF((IF(OR(C487=\"INT\",C487=\"WORD\",C487=\"BOOL\"),MOD(A487,2),MOD(A487,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","04H03","启停控制",{"$f":"D487&F487&\"-\"&IF(E487=\"R\",\"新云平台\"&G487,G487)","v":"排风机04H03-新云平台启停控制"},{"$f":"E487&VLOOKUP(D487,[1]list!$D$3:$F$501,2,FALSE)&F487&\"_\"&VLOOKUP(G487,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04H03_C"},{"$f":"I487&\" \"&\"AT%M\"&A487&\" \"&\":\"&C487&\";\"&\" \"&\"(*\"&H487&\"*)\"","v":"REAF04H03_C AT%M1390.0 :BOOL; (*排风机04H03-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J487,SEARCH(\"AT%\",J487),,REPT(\" \",25-SEARCH(\"AT%\",J487))),SEARCH(\":\",REPLACE(J487,SEARCH(\"AT%\",J487),,REPT(\" \",25-SEARCH(\"AT%\",J487)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J487,SEARCH(\"AT%\",J487),,REPT(\" \",25-SEARCH(\"AT%\",J487))))))","v":"REAF04H03_C             AT%M1390.0     :BOOL; (*排风机04H03-新云平台启停控制*)"}]
[{"$f":"IF(OR(C487=\"REAL\",C487=\"DWORD\",C487=\"DINT\"),(IF(OR(C488=\"REAL\",C488=\"DWORD\",C488=\"DINT\"),A487+4+MOD(A487,4),A487+4)),(IF(OR(C488=\"REAL\",C488=\"DWORD\",C488=\"DINT\"),A487+4+MOD(A487,4),A487+2)))&\".0\"","v":"1392.0"},"验证通过","BOOL","排风机","L","04H03","运行时间累积重置","排风机04H03-运行时间累积重置",{"$f":"E488&VLOOKUP(D488,[1]list!$D$3:$F$501,2,FALSE)&F488&\"_\"&VLOOKUP(G488,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_RST"},"LEAF04H03_RST AT%M1392.0 :BOOL; (*排风机04H03-运行时间累积重置*)","LEAF04H03_RST           AT%M1392.0     :BOOL; (*排风机04H03-运行时间累积重置*)"]
["1396.0","验证通过","REAL","排风机","L","04H03","运行时间累积重置值","排风机04H03-运行时间累积重置值",{"$f":"E489&VLOOKUP(D489,[1]list!$D$3:$F$501,2,FALSE)&F489&\"_\"&VLOOKUP(G489,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_RSTV"},"LEAF04H03_RSTV AT%M1396.0 :REAL; (*排风机04H03-运行时间累积重置值*)","LEAF04H03_RSTV          AT%M1396.0     :REAL; (*排风机04H03-运行时间累积重置值*)"]
["1400.0","验证通过","REAL","排风机","L","04H03","运行时间累积值","排风机04H03-运行时间累积值",{"$f":"E490&VLOOKUP(D490,[1]list!$D$3:$F$501,2,FALSE)&F490&\"_\"&VLOOKUP(G490,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_RH"},"LEAF04H03_RH AT%M1400.0 :REAL; (*排风机04H03-运行时间累积值*)","LEAF04H03_RH            AT%M1400.0     :REAL; (*排风机04H03-运行时间累积值*)"]
["1404.0","验证通过","BOOL","排风机","L","04H03","定时模式","排风机04H03-定时模式",{"$f":"E491&VLOOKUP(D491,[1]list!$D$3:$F$501,2,FALSE)&F491&\"_\"&VLOOKUP(G491,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_TM"},"LEAF04H03_TM AT%M1404.0 :BOOL; (*排风机04H03-定时模式*)","LEAF04H03_TM            AT%M1404.0     :BOOL; (*排风机04H03-定时模式*)"]
["1406.0","验证通过","BOOL","排风机","L","04H03","定时控制","排风机04H03-定时控制",{"$f":"E492&VLOOKUP(D492,[1]list!$D$3:$F$501,2,FALSE)&F492&\"_\"&VLOOKUP(G492,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_TC"},"LEAF04H03_TC AT%M1406.0 :BOOL; (*排风机04H03-定时控制*)","LEAF04H03_TC            AT%M1406.0     :BOOL; (*排风机04H03-定时控制*)"]
["1408.0","验证通过","BOOL","排风机","L","04H03","全天候模式","排风机04H03-全天候模式",{"$f":"E493&VLOOKUP(D493,[1]list!$D$3:$F$501,2,FALSE)&F493&\"_\"&VLOOKUP(G493,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_DM"},"LEAF04H03_DM AT%M1408.0 :BOOL; (*排风机04H03-全天候模式*)","LEAF04H03_DM            AT%M1408.0     :BOOL; (*排风机04H03-全天候模式*)"]
["1412.0","验证通过","REAL","排风机","L","04H03","CO设定值","排风机04H03-CO设定值",{"$f":"E494&VLOOKUP(D494,[1]list!$D$3:$F$501,2,FALSE)&F494&\"_\"&VLOOKUP(G494,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_COSET"},"LEAF04H03_COSET AT%M1412.0 :REAL; (*排风机04H03-CO设定值*)","LEAF04H03_COSET         AT%M1412.0     :REAL; (*排风机04H03-CO设定值*)"]
["1416.0","验证通过","REAL","排风机","L","04H03","设定温度值","排风机04H03-设定温度值",{"$f":"E495&VLOOKUP(D495,[1]list!$D$3:$F$501,2,FALSE)&F495&\"_\"&VLOOKUP(G495,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H03_TSET"},"LEAF04H03_TSET AT%M1416.0 :REAL; (*排风机04H03-设定温度值*)","LEAF04H03_TSET          AT%M1416.0     :REAL; (*排风机04H03-设定温度值*)"]
["EAF"]
[{"$f":"IF(OR(C495=\"REAL\",C495=\"DWORD\",C495=\"DINT\"),(IF(OR(C497=\"REAL\",C497=\"DWORD\",C497=\"DINT\"),A495+4+MOD(A495,4),A495+4)),(IF(OR(C497=\"REAL\",C497=\"DWORD\",C497=\"DINT\"),A495+4+MOD(A495,4),A495+2)))&\".0\"","v":"1420.0"},{"$f":"IF((IF(OR(C497=\"INT\",C497=\"WORD\",C497=\"BOOL\"),MOD(A497,2),MOD(A497,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","04H04","启停控制",{"$f":"D497&F497&\"-\"&IF(E497=\"R\",\"新云平台\"&G497,G497)","v":"排风机04H04-新云平台启停控制"},{"$f":"E497&VLOOKUP(D497,[1]list!$D$3:$F$501,2,FALSE)&F497&\"_\"&VLOOKUP(G497,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04H04_C"},{"$f":"I497&\" \"&\"AT%M\"&A497&\" \"&\":\"&C497&\";\"&\" \"&\"(*\"&H497&\"*)\"","v":"REAF04H04_C AT%M1420.0 :BOOL; (*排风机04H04-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J497,SEARCH(\"AT%\",J497),,REPT(\" \",25-SEARCH(\"AT%\",J497))),SEARCH(\":\",REPLACE(J497,SEARCH(\"AT%\",J497),,REPT(\" \",25-SEARCH(\"AT%\",J497)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J497,SEARCH(\"AT%\",J497),,REPT(\" \",25-SEARCH(\"AT%\",J497))))))","v":"REAF04H04_C             AT%M1420.0     :BOOL; (*排风机04H04-新云平台启停控制*)"}]
[{"$f":"IF(OR(C497=\"REAL\",C497=\"DWORD\",C497=\"DINT\"),(IF(OR(C498=\"REAL\",C498=\"DWORD\",C498=\"DINT\"),A497+4+MOD(A497,4),A497+4)),(IF(OR(C498=\"REAL\",C498=\"DWORD\",C498=\"DINT\"),A497+4+MOD(A497,4),A497+2)))&\".0\"","v":"1422.0"},"验证通过","BOOL","排风机","L","04H04","运行时间累积重置","排风机04H04-运行时间累积重置",{"$f":"E498&VLOOKUP(D498,[1]list!$D$3:$F$501,2,FALSE)&F498&\"_\"&VLOOKUP(G498,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_RST"},"LEAF04H04_RST AT%M1422.0 :BOOL; (*排风机04H04-运行时间累积重置*)","LEAF04H04_RST           AT%M1422.0     :BOOL; (*排风机04H04-运行时间累积重置*)"]
["1428.0","验证通过","REAL","排风机","L","04H04","运行时间累积重置值","排风机04H04-运行时间累积重置值",{"$f":"E499&VLOOKUP(D499,[1]list!$D$3:$F$501,2,FALSE)&F499&\"_\"&VLOOKUP(G499,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_RSTV"},"LEAF04H04_RSTV AT%M1428.0 :REAL; (*排风机04H04-运行时间累积重置值*)","LEAF04H04_RSTV          AT%M1428.0     :REAL; (*排风机04H04-运行时间累积重置值*)"]
["1432.0","验证通过","REAL","排风机","L","04H04","运行时间累积值","排风机04H04-运行时间累积值",{"$f":"E500&VLOOKUP(D500,[1]list!$D$3:$F$501,2,FALSE)&F500&\"_\"&VLOOKUP(G500,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_RH"},"LEAF04H04_RH AT%M1432.0 :REAL; (*排风机04H04-运行时间累积值*)","LEAF04H04_RH            AT%M1432.0     :REAL; (*排风机04H04-运行时间累积值*)"]
["1436.0","验证通过","BOOL","排风机","L","04H04","定时模式","排风机04H04-定时模式",{"$f":"E501&VLOOKUP(D501,[1]list!$D$3:$F$501,2,FALSE)&F501&\"_\"&VLOOKUP(G501,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_TM"},"LEAF04H04_TM AT%M1436.0 :BOOL; (*排风机04H04-定时模式*)","LEAF04H04_TM            AT%M1436.0     :BOOL; (*排风机04H04-定时模式*)"]
["1438.0","验证通过","BOOL","排风机","L","04H04","定时控制","排风机04H04-定时控制",{"$f":"E502&VLOOKUP(D502,[1]list!$D$3:$F$501,2,FALSE)&F502&\"_\"&VLOOKUP(G502,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_TC"},"LEAF04H04_TC AT%M1438.0 :BOOL; (*排风机04H04-定时控制*)","LEAF04H04_TC            AT%M1438.0     :BOOL; (*排风机04H04-定时控制*)"]
["1440.0","验证通过","BOOL","排风机","L","04H04","全天候模式","排风机04H04-全天候模式",{"$f":"E503&VLOOKUP(D503,[1]list!$D$3:$F$501,2,FALSE)&F503&\"_\"&VLOOKUP(G503,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_DM"},"LEAF04H04_DM AT%M1440.0 :BOOL; (*排风机04H04-全天候模式*)","LEAF04H04_DM            AT%M1440.0     :BOOL; (*排风机04H04-全天候模式*)"]
["1444.0","验证通过","REAL","排风机","L","04H04","CO设定值","排风机04H04-CO设定值",{"$f":"E504&VLOOKUP(D504,[1]list!$D$3:$F$501,2,FALSE)&F504&\"_\"&VLOOKUP(G504,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_COSET"},"LEAF04H04_COSET AT%M1444.0 :REAL; (*排风机04H04-CO设定值*)","LEAF04H04_COSET         AT%M1444.0     :REAL; (*排风机04H04-CO设定值*)"]
["1448.0","验证通过","REAL","排风机","L","04H04","设定温度值","排风机04H04-设定温度值",{"$f":"E505&VLOOKUP(D505,[1]list!$D$3:$F$501,2,FALSE)&F505&\"_\"&VLOOKUP(G505,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H04_TSET"},"LEAF04H04_TSET AT%M1448.0 :REAL; (*排风机04H04-设定温度值*)","LEAF04H04_TSET          AT%M1448.0     :REAL; (*排风机04H04-设定温度值*)"]
["EAF"]
[{"$f":"IF(OR(C505=\"REAL\",C505=\"DWORD\",C505=\"DINT\"),(IF(OR(C507=\"REAL\",C507=\"DWORD\",C507=\"DINT\"),A505+4+MOD(A505,4),A505+4)),(IF(OR(C507=\"REAL\",C507=\"DWORD\",C507=\"DINT\"),A505+4+MOD(A505,4),A505+2)))&\".0\"","v":"1452.0"},{"$f":"IF((IF(OR(C507=\"INT\",C507=\"WORD\",C507=\"BOOL\"),MOD(A507,2),MOD(A507,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","04H05","启停控制",{"$f":"D507&F507&\"-\"&IF(E507=\"R\",\"新云平台\"&G507,G507)","v":"排风机04H05-新云平台启停控制"},{"$f":"E507&VLOOKUP(D507,[1]list!$D$3:$F$501,2,FALSE)&F507&\"_\"&VLOOKUP(G507,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04H05_C"},{"$f":"I507&\" \"&\"AT%M\"&A507&\" \"&\":\"&C507&\";\"&\" \"&\"(*\"&H507&\"*)\"","v":"REAF04H05_C AT%M1452.0 :BOOL; (*排风机04H05-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J507,SEARCH(\"AT%\",J507),,REPT(\" \",25-SEARCH(\"AT%\",J507))),SEARCH(\":\",REPLACE(J507,SEARCH(\"AT%\",J507),,REPT(\" \",25-SEARCH(\"AT%\",J507)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J507,SEARCH(\"AT%\",J507),,REPT(\" \",25-SEARCH(\"AT%\",J507))))))","v":"REAF04H05_C             AT%M1452.0     :BOOL; (*排风机04H05-新云平台启停控制*)"}]
[{"$f":"IF(OR(C507=\"REAL\",C507=\"DWORD\",C507=\"DINT\"),(IF(OR(C508=\"REAL\",C508=\"DWORD\",C508=\"DINT\"),A507+4+MOD(A507,4),A507+4)),(IF(OR(C508=\"REAL\",C508=\"DWORD\",C508=\"DINT\"),A507+4+MOD(A507,4),A507+2)))&\".0\"","v":"1454.0"},"验证通过","BOOL","排风机","L","04H05","运行时间累积重置","排风机04H05-运行时间累积重置",{"$f":"E508&VLOOKUP(D508,[1]list!$D$3:$F$501,2,FALSE)&F508&\"_\"&VLOOKUP(G508,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_RST"},"LEAF04H05_RST AT%M1454.0 :BOOL; (*排风机04H05-运行时间累积重置*)","LEAF04H05_RST           AT%M1454.0     :BOOL; (*排风机04H05-运行时间累积重置*)"]
["1460.0","验证通过","REAL","排风机","L","04H05","运行时间累积重置值","排风机04H05-运行时间累积重置值",{"$f":"E509&VLOOKUP(D509,[1]list!$D$3:$F$501,2,FALSE)&F509&\"_\"&VLOOKUP(G509,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_RSTV"},"LEAF04H05_RSTV AT%M1460.0 :REAL; (*排风机04H05-运行时间累积重置值*)","LEAF04H05_RSTV          AT%M1460.0     :REAL; (*排风机04H05-运行时间累积重置值*)"]
["1464.0","验证通过","REAL","排风机","L","04H05","运行时间累积值","排风机04H05-运行时间累积值",{"$f":"E510&VLOOKUP(D510,[1]list!$D$3:$F$501,2,FALSE)&F510&\"_\"&VLOOKUP(G510,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_RH"},"LEAF04H05_RH AT%M1464.0 :REAL; (*排风机04H05-运行时间累积值*)","LEAF04H05_RH            AT%M1464.0     :REAL; (*排风机04H05-运行时间累积值*)"]
["1468.0","验证通过","BOOL","排风机","L","04H05","定时模式","排风机04H05-定时模式",{"$f":"E511&VLOOKUP(D511,[1]list!$D$3:$F$501,2,FALSE)&F511&\"_\"&VLOOKUP(G511,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_TM"},"LEAF04H05_TM AT%M1468.0 :BOOL; (*排风机04H05-定时模式*)","LEAF04H05_TM            AT%M1468.0     :BOOL; (*排风机04H05-定时模式*)"]
["1470.0","验证通过","BOOL","排风机","L","04H05","定时控制","排风机04H05-定时控制",{"$f":"E512&VLOOKUP(D512,[1]list!$D$3:$F$501,2,FALSE)&F512&\"_\"&VLOOKUP(G512,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_TC"},"LEAF04H05_TC AT%M1470.0 :BOOL; (*排风机04H05-定时控制*)","LEAF04H05_TC            AT%M1470.0     :BOOL; (*排风机04H05-定时控制*)"]
["1472.0","验证通过","BOOL","排风机","L","04H05","全天候模式","排风机04H05-全天候模式",{"$f":"E513&VLOOKUP(D513,[1]list!$D$3:$F$501,2,FALSE)&F513&\"_\"&VLOOKUP(G513,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_DM"},"LEAF04H05_DM AT%M1472.0 :BOOL; (*排风机04H05-全天候模式*)","LEAF04H05_DM            AT%M1472.0     :BOOL; (*排风机04H05-全天候模式*)"]
["1476.0","验证通过","REAL","排风机","L","04H05","CO设定值","排风机04H05-CO设定值",{"$f":"E514&VLOOKUP(D514,[1]list!$D$3:$F$501,2,FALSE)&F514&\"_\"&VLOOKUP(G514,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_COSET"},"LEAF04H05_COSET AT%M1476.0 :REAL; (*排风机04H05-CO设定值*)","LEAF04H05_COSET         AT%M1476.0     :REAL; (*排风机04H05-CO设定值*)"]
["1480.0","验证通过","REAL","排风机","L","04H05","设定温度值","排风机04H05-设定温度值",{"$f":"E515&VLOOKUP(D515,[1]list!$D$3:$F$501,2,FALSE)&F515&\"_\"&VLOOKUP(G515,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04H05_TSET"},"LEAF04H05_TSET AT%M1480.0 :REAL; (*排风机04H05-设定温度值*)","LEAF04H05_TSET          AT%M1480.0     :REAL; (*排风机04H05-设定温度值*)"]
["FCU"]
[{"$f":"IF(OR(C515=\"REAL\",C515=\"DWORD\",C515=\"DINT\"),(IF(OR(C517=\"REAL\",C517=\"DWORD\",C517=\"DINT\"),A515+4+MOD(A515,4),A515+4)),(IF(OR(C517=\"REAL\",C517=\"DWORD\",C517=\"DINT\"),A515+4+MOD(A515,4),A515+2)))&\".0\"","v":"1484.0"},{"$f":"IF((IF(OR(C517=\"INT\",C517=\"WORD\",C517=\"BOOL\"),MOD(A517,2),MOD(A517,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","04H01","设定温度值",{"$f":"D517&F517&\"-\"&IF(E517=\"R\",\"新云平台\"&G517,G517)","v":"风机盘管04H01-新云平台设定温度值"},{"$f":"E517&VLOOKUP(D517,list!$D$3:$F$501,2,FALSE)&F517&\"_\"&VLOOKUP(G517,list!$I$2:$K$502,2,FALSE)","v":"RFCU04H01_TSET"},{"$f":"I517&\" \"&\"AT%M\"&A517&\" \"&\":\"&C517&\";\"&\" \"&\"(*\"&H517&\"*)\"","v":"RFCU04H01_TSET AT%M1484.0 :REAL; (*风机盘管04H01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J517,SEARCH(\"AT%\",J517),,REPT(\" \",25-SEARCH(\"AT%\",J517))),SEARCH(\":\",REPLACE(J517,SEARCH(\"AT%\",J517),,REPT(\" \",25-SEARCH(\"AT%\",J517)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J517,SEARCH(\"AT%\",J517),,REPT(\" \",25-SEARCH(\"AT%\",J517))))))","v":"RFCU04H01_TSET          AT%M1484.0     :REAL; (*风机盘管04H01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C517=\"REAL\",C517=\"DWORD\",C517=\"DINT\"),(IF(OR(C518=\"REAL\",C518=\"DWORD\",C518=\"DINT\"),A517+4+MOD(A517,4),A517+4)),(IF(OR(C518=\"REAL\",C518=\"DWORD\",C518=\"DINT\"),A517+4+MOD(A517,4),A517+2)))&\".0\"","v":"1488.0"},"验证通过","INT","风机盘管","R",{"$f":"F517","v":"04H01"},"季节模式","风机盘管04H01-新云平台季节模式",{"$f":"E518&VLOOKUP(D518,list!$D$3:$F$501,2,FALSE)&F518&\"_\"&VLOOKUP(G518,list!$I$2:$K$502,2,FALSE)","v":"RFCU04H01_SM"},"RFCU04H01_SM AT%M1488.0 :INT; (*风机盘管04H01-新云平台季节模式*)","RFCU04H01_SM            AT%M1488.0     :INT; (*风机盘管04H01-新云平台季节模式*)"]
["1490.0","验证通过","BOOL","风机盘管","R","04H01","程序控制","风机盘管04H01-新云平台程序控制",{"$f":"E519&VLOOKUP(D519,list!$D$3:$F$501,2,FALSE)&F519&\"_\"&VLOOKUP(G519,list!$I$2:$K$502,2,FALSE)","v":"RFCU04H01_PC"},"RFCU04H01_PC AT%M1490.0 :BOOL; (*风机盘管04H01-新云平台程序控制*)","RFCU04H01_PC            AT%M1490.0     :BOOL; (*风机盘管04H01-新云平台程序控制*)"]
["1496.0","验证通过","REAL","风机盘管","L","04H01","设定温度值","风机盘管04H01-设定温度值",{"$f":"E520&VLOOKUP(D520,list!$D$3:$F$501,2,FALSE)&F520&\"_\"&VLOOKUP(G520,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_TSET"},"LFCU04H01_TSET AT%M1496.0 :REAL; (*风机盘管04H01-设定温度值*)","LFCU04H01_TSET          AT%M1496.0     :REAL; (*风机盘管04H01-设定温度值*)"]
["1500.0","验证通过","INT","风机盘管","L","04H01","季节模式","风机盘管04H01-季节模式",{"$f":"E521&VLOOKUP(D521,list!$D$3:$F$501,2,FALSE)&F521&\"_\"&VLOOKUP(G521,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_SM"},"LFCU04H01_SM AT%M1500.0 :INT; (*风机盘管04H01-季节模式*)","LFCU04H01_SM            AT%M1500.0     :INT; (*风机盘管04H01-季节模式*)"]
["1504.0","验证通过","REAL","风机盘管","L","04H01","温度换算值","风机盘管04H01-温度换算值",{"$f":"E522&VLOOKUP(D522,list!$D$3:$F$501,2,FALSE)&F522&\"_\"&VLOOKUP(G522,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_TS"},"LFCU04H01_TS AT%M1504.0 :REAL; (*风机盘管04H01-温度换算值*)","LFCU04H01_TS            AT%M1504.0     :REAL; (*风机盘管04H01-温度换算值*)"]
["1508.0","验证通过","BOOL","风机盘管","L","04H01","电磁阀手动控制","风机盘管04H01-电磁阀手动控制",{"$f":"E523&VLOOKUP(D523,list!$D$3:$F$501,2,FALSE)&F523&\"_\"&VLOOKUP(G523,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_EVMC"},"LFCU04H01_EVMC AT%M1508.0 :BOOL; (*风机盘管04H01-电磁阀手动控制*)","LFCU04H01_EVMC          AT%M1508.0     :BOOL; (*风机盘管04H01-电磁阀手动控制*)"]
["1510.0","验证通过","BOOL","风机盘管","L","04H01","电磁阀手动控制值","风机盘管04H01-电磁阀手动控制值",{"$f":"E524&VLOOKUP(D524,list!$D$3:$F$501,2,FALSE)&F524&\"_\"&VLOOKUP(G524,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_EVMV"},"LFCU04H01_EVMV AT%M1510.0 :BOOL; (*风机盘管04H01-电磁阀手动控制值*)","LFCU04H01_EVMV          AT%M1510.0     :BOOL; (*风机盘管04H01-电磁阀手动控制值*)"]
["1516.0","验证通过","REAL","风机盘管","L","04H01","回风温度换算值","风机盘管04H01-回风温度换算值",{"$f":"E525&VLOOKUP(D525,list!$D$3:$F$501,2,FALSE)&F525&\"_\"&VLOOKUP(G525,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_RTS"},"LFCU04H01_RTS AT%M1516.0 :REAL; (*风机盘管04H01-回风温度换算值*)","LFCU04H01_RTS           AT%M1516.0     :REAL; (*风机盘管04H01-回风温度换算值*)"]
["1520.0","验证通过","BOOL","风机盘管","L","04H01","运行时间累积重置","风机盘管04H01-运行时间累积重置",{"$f":"E526&VLOOKUP(D526,list!$D$3:$F$501,2,FALSE)&F526&\"_\"&VLOOKUP(G526,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_RST"},"LFCU04H01_RST AT%M1520.0 :BOOL; (*风机盘管04H01-运行时间累积重置*)","LFCU04H01_RST           AT%M1520.0     :BOOL; (*风机盘管04H01-运行时间累积重置*)"]
["1524.0","验证通过","REAL","风机盘管","L","04H01","运行时间累积重置值","风机盘管04H01-运行时间累积重置值",{"$f":"E527&VLOOKUP(D527,list!$D$3:$F$501,2,FALSE)&F527&\"_\"&VLOOKUP(G527,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_RSTV"},"LFCU04H01_RSTV AT%M1524.0 :REAL; (*风机盘管04H01-运行时间累积重置值*)","LFCU04H01_RSTV          AT%M1524.0     :REAL; (*风机盘管04H01-运行时间累积重置值*)"]
["1528.0","验证通过","BOOL","风机盘管","L","04H01","隔离开关1","风机盘管04H01-隔离开关1",{"$f":"E528&VLOOKUP(D528,list!$D$3:$F$501,2,FALSE)&F528&\"_\"&VLOOKUP(G528,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_ISO1"},"LFCU04H01_ISO1 AT%M1528.0 :BOOL; (*风机盘管04H01-隔离开关1*)","LFCU04H01_ISO1          AT%M1528.0     :BOOL; (*风机盘管04H01-隔离开关1*)"]
["1532.0","验证通过","REAL","风机盘管","L","04H01","运行时间累积值","风机盘管04H01-运行时间累积值",{"$f":"E529&VLOOKUP(D529,list!$D$3:$F$501,2,FALSE)&F529&\"_\"&VLOOKUP(G529,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_RH"},"LFCU04H01_RH AT%M1532.0 :REAL; (*风机盘管04H01-运行时间累积值*)","LFCU04H01_RH            AT%M1532.0     :REAL; (*风机盘管04H01-运行时间累积值*)"]
["1536.0","验证通过","INT","风机盘管","L","04H01","设备状态代码","风机盘管04H01-设备状态代码",{"$f":"E530&VLOOKUP(D530,list!$D$3:$F$501,2,FALSE)&F530&\"_\"&VLOOKUP(G530,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_SN"},"LFCU04H01_SN AT%M1536.0 :INT; (*风机盘管04H01-设备状态代码*)","LFCU04H01_SN            AT%M1536.0     :INT; (*风机盘管04H01-设备状态代码*)"]
["1538.0","验证通过","INT","风机盘管","L","04H01","水阀控制转换值","风机盘管04H01-水阀控制转换值",{"$f":"E531&VLOOKUP(D531,list!$D$3:$F$501,2,FALSE)&F531&\"_\"&VLOOKUP(G531,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_WVCS"},"LFCU04H01_WVCS AT%M1538.0 :INT; (*风机盘管04H01-水阀控制转换值*)","LFCU04H01_WVCS          AT%M1538.0     :INT; (*风机盘管04H01-水阀控制转换值*)"]
["1540.0","验证通过","BOOL","风机盘管","L","04H01","程序控制","风机盘管04H01-程序控制",{"$f":"E532&VLOOKUP(D532,list!$D$3:$F$501,2,FALSE)&F532&\"_\"&VLOOKUP(G532,list!$I$2:$K$502,2,FALSE)","v":"LFCU04H01_PC"},"LFCU04H01_PC AT%M1540.0 :BOOL; (*风机盘管04H01-程序控制*)","LFCU04H01_PC            AT%M1540.0     :BOOL; (*风机盘管04H01-程序控制*)"]
["PAU"]
[{"$f":"IF(OR(C532=\"REAL\",C532=\"DWORD\",C532=\"DINT\"),(IF(OR(C534=\"REAL\",C534=\"DWORD\",C534=\"DINT\"),A532+4+MOD(A532,4),A532+4)),(IF(OR(C534=\"REAL\",C534=\"DWORD\",C534=\"DINT\"),A532+4+MOD(A532,4),A532+2)))&\".0\"","v":"1544.0"},{"$f":"IF((IF(OR(C534=\"INT\",C534=\"WORD\",C534=\"BOOL\"),MOD(A534,2),MOD(A534,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05E01","设定温度值",{"$f":"D534&F534&\"-\"&IF(E534=\"R\",\"新云平台\"&G534,G534)","v":"P新风机组05E01-新云平台设定温度值"},{"$f":"E534&VLOOKUP(D534,list!$D$3:$F$501,2,FALSE)&F534&\"_\"&VLOOKUP(G534,list!$I$2:$K$502,2,FALSE)","v":"RPAU05E01_TSET"},{"$f":"I534&\" \"&\"AT%M\"&A534&\" \"&\":\"&C534&\";\"&\" \"&\"(*\"&H534&\"*)\"","v":"RPAU05E01_TSET AT%M1544.0 :REAL; (*P新风机组05E01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J534,SEARCH(\"AT%\",J534),,REPT(\" \",25-SEARCH(\"AT%\",J534))),SEARCH(\":\",REPLACE(J534,SEARCH(\"AT%\",J534),,REPT(\" \",25-SEARCH(\"AT%\",J534)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J534,SEARCH(\"AT%\",J534),,REPT(\" \",25-SEARCH(\"AT%\",J534))))))","v":"RPAU05E01_TSET          AT%M1544.0     :REAL; (*P新风机组05E01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C534=\"REAL\",C534=\"DWORD\",C534=\"DINT\"),(IF(OR(C535=\"REAL\",C535=\"DWORD\",C535=\"DINT\"),A534+4+MOD(A534,4),A534+4)),(IF(OR(C535=\"REAL\",C535=\"DWORD\",C535=\"DINT\"),A534+4+MOD(A534,4),A534+2)))&\".0\"","v":"1548.0"},"验证通过","INT","P新风机组","R",{"$f":"F534","v":"05E01"},"季节模式","P新风机组05E01-新云平台季节模式",{"$f":"E535&VLOOKUP(D535,list!$D$3:$F$501,2,FALSE)&F535&\"_\"&VLOOKUP(G535,list!$I$2:$K$502,2,FALSE)","v":"RPAU05E01_SM"},"RPAU05E01_SM AT%M1548.0 :INT; (*P新风机组05E01-新云平台季节模式*)","RPAU05E01_SM            AT%M1548.0     :INT; (*P新风机组05E01-新云平台季节模式*)"]
["1550.0","验证通过","BOOL","P新风机组","R","05E01","程序控制","P新风机组05E01-新云平台程序控制",{"$f":"E536&VLOOKUP(D536,list!$D$3:$F$501,2,FALSE)&F536&\"_\"&VLOOKUP(G536,list!$I$2:$K$502,2,FALSE)","v":"RPAU05E01_PC"},"RPAU05E01_PC AT%M1550.0 :BOOL; (*P新风机组05E01-新云平台程序控制*)","RPAU05E01_PC            AT%M1550.0     :BOOL; (*P新风机组05E01-新云平台程序控制*)"]
["1556.0","验证通过","REAL","P新风机组","L","05E01","设定温度值","P新风机组05E01-设定温度值",{"$f":"E537&VLOOKUP(D537,list!$D$3:$F$501,2,FALSE)&F537&\"_\"&VLOOKUP(G537,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_TSET"},"LPAU05E01_TSET AT%M1556.0 :REAL; (*P新风机组05E01-设定温度值*)","LPAU05E01_TSET          AT%M1556.0     :REAL; (*P新风机组05E01-设定温度值*)"]
["1560.0","验证通过","INT","P新风机组","L","05E01","季节模式","P新风机组05E01-季节模式",{"$f":"E538&VLOOKUP(D538,list!$D$3:$F$501,2,FALSE)&F538&\"_\"&VLOOKUP(G538,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_SM"},"LPAU05E01_SM AT%M1560.0 :INT; (*P新风机组05E01-季节模式*)","LPAU05E01_SM            AT%M1560.0     :INT; (*P新风机组05E01-季节模式*)"]
["1564.0","验证通过","REAL","P新风机组","L","05E01","水阀反馈换算值","P新风机组05E01-水阀反馈换算值",{"$f":"E539&VLOOKUP(D539,list!$D$3:$F$501,2,FALSE)&F539&\"_\"&VLOOKUP(G539,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_WVBS"},"LPAU05E01_WVBS AT%M1564.0 :REAL; (*P新风机组05E01-水阀反馈换算值*)","LPAU05E01_WVBS          AT%M1564.0     :REAL; (*P新风机组05E01-水阀反馈换算值*)"]
["1568.0","验证通过","BOOL","P新风机组","L","05E01","水阀手动控制","P新风机组05E01-水阀手动控制",{"$f":"E540&VLOOKUP(D540,list!$D$3:$F$501,2,FALSE)&F540&\"_\"&VLOOKUP(G540,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_WVMC"},"LPAU05E01_WVMC AT%M1568.0 :BOOL; (*P新风机组05E01-水阀手动控制*)","LPAU05E01_WVMC          AT%M1568.0     :BOOL; (*P新风机组05E01-水阀手动控制*)"]
["1572.0","验证通过","REAL","P新风机组","L","05E01","水阀手动控制值","P新风机组05E01-水阀手动控制值",{"$f":"E541&VLOOKUP(D541,list!$D$3:$F$501,2,FALSE)&F541&\"_\"&VLOOKUP(G541,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_WVMV"},"LPAU05E01_WVMV AT%M1572.0 :REAL; (*P新风机组05E01-水阀手动控制值*)","LPAU05E01_WVMV          AT%M1572.0     :REAL; (*P新风机组05E01-水阀手动控制值*)"]
["1576.0","验证通过","REAL","P新风机组","L","05E01","送风温度换算值","P新风机组05E01-送风温度换算值",{"$f":"E542&VLOOKUP(D542,list!$D$3:$F$501,2,FALSE)&F542&\"_\"&VLOOKUP(G542,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_STS"},"LPAU05E01_STS AT%M1576.0 :REAL; (*P新风机组05E01-送风温度换算值*)","LPAU05E01_STS           AT%M1576.0     :REAL; (*P新风机组05E01-送风温度换算值*)"]
["1580.0","验证通过","BOOL","P新风机组","L","05E01","运行时间累积重置","P新风机组05E01-运行时间累积重置",{"$f":"E543&VLOOKUP(D543,list!$D$3:$F$501,2,FALSE)&F543&\"_\"&VLOOKUP(G543,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_RST"},"LPAU05E01_RST AT%M1580.0 :BOOL; (*P新风机组05E01-运行时间累积重置*)","LPAU05E01_RST           AT%M1580.0     :BOOL; (*P新风机组05E01-运行时间累积重置*)"]
["1584.0","验证通过","REAL","P新风机组","L","05E01","运行时间累积重置值","P新风机组05E01-运行时间累积重置值",{"$f":"E544&VLOOKUP(D544,list!$D$3:$F$501,2,FALSE)&F544&\"_\"&VLOOKUP(G544,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_RSTV"},"LPAU05E01_RSTV AT%M1584.0 :REAL; (*P新风机组05E01-运行时间累积重置值*)","LPAU05E01_RSTV          AT%M1584.0     :REAL; (*P新风机组05E01-运行时间累积重置值*)"]
["1588.0","验证通过","BOOL","P新风机组","L","05E01","隔离开关1","P新风机组05E01-隔离开关1",{"$f":"E545&VLOOKUP(D545,list!$D$3:$F$501,2,FALSE)&F545&\"_\"&VLOOKUP(G545,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_ISO1"},"LPAU05E01_ISO1 AT%M1588.0 :BOOL; (*P新风机组05E01-隔离开关1*)","LPAU05E01_ISO1          AT%M1588.0     :BOOL; (*P新风机组05E01-隔离开关1*)"]
["1590.0","验证通过","BOOL","P新风机组","L","05E01","隔离开关2","P新风机组05E01-隔离开关2",{"$f":"E546&VLOOKUP(D546,list!$D$3:$F$501,2,FALSE)&F546&\"_\"&VLOOKUP(G546,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_ISO2"},"LPAU05E01_ISO2 AT%M1590.0 :BOOL; (*P新风机组05E01-隔离开关2*)","LPAU05E01_ISO2          AT%M1590.0     :BOOL; (*P新风机组05E01-隔离开关2*)"]
["1596.0","验证通过","REAL","P新风机组","L","05E01","P调节参数","P新风机组05E01-P调节参数",{"$f":"E547&VLOOKUP(D547,list!$D$3:$F$501,2,FALSE)&F547&\"_\"&VLOOKUP(G547,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_VP"},"LPAU05E01_VP AT%M1596.0 :REAL; (*P新风机组05E01-P调节参数*)","LPAU05E01_VP            AT%M1596.0     :REAL; (*P新风机组05E01-P调节参数*)"]
["1600.0","验证通过","REAL","P新风机组","L","05E01","I调节参数","P新风机组05E01-I调节参数",{"$f":"E548&VLOOKUP(D548,list!$D$3:$F$501,2,FALSE)&F548&\"_\"&VLOOKUP(G548,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_VI"},"LPAU05E01_VI AT%M1600.0 :REAL; (*P新风机组05E01-I调节参数*)","LPAU05E01_VI            AT%M1600.0     :REAL; (*P新风机组05E01-I调节参数*)"]
["1604.0","验证通过","REAL","P新风机组","L","05E01","运行时间累积值","P新风机组05E01-运行时间累积值",{"$f":"E549&VLOOKUP(D549,list!$D$3:$F$501,2,FALSE)&F549&\"_\"&VLOOKUP(G549,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_RH"},"LPAU05E01_RH AT%M1604.0 :REAL; (*P新风机组05E01-运行时间累积值*)","LPAU05E01_RH            AT%M1604.0     :REAL; (*P新风机组05E01-运行时间累积值*)"]
["1608.0","验证通过","INT","P新风机组","L","05E01","设备状态代码","P新风机组05E01-设备状态代码",{"$f":"E550&VLOOKUP(D550,list!$D$3:$F$501,2,FALSE)&F550&\"_\"&VLOOKUP(G550,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_SN"},"LPAU05E01_SN AT%M1608.0 :INT; (*P新风机组05E01-设备状态代码*)","LPAU05E01_SN            AT%M1608.0     :INT; (*P新风机组05E01-设备状态代码*)"]
["1610.0","验证通过","INT","P新风机组","L","05E01","水阀控制转换值","P新风机组05E01-水阀控制转换值",{"$f":"E551&VLOOKUP(D551,list!$D$3:$F$501,2,FALSE)&F551&\"_\"&VLOOKUP(G551,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_WVCS"},"LPAU05E01_WVCS AT%M1610.0 :INT; (*P新风机组05E01-水阀控制转换值*)","LPAU05E01_WVCS          AT%M1610.0     :INT; (*P新风机组05E01-水阀控制转换值*)"]
["1612.0","验证通过","BOOL","P新风机组","L","05E01","程序控制","P新风机组05E01-程序控制",{"$f":"E552&VLOOKUP(D552,list!$D$3:$F$501,2,FALSE)&F552&\"_\"&VLOOKUP(G552,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_PC"},"LPAU05E01_PC AT%M1612.0 :BOOL; (*P新风机组05E01-程序控制*)","LPAU05E01_PC            AT%M1612.0     :BOOL; (*P新风机组05E01-程序控制*)"]
["1614.0","验证通过","INT","P新风机组","L","05E01","变频手动控制值","P新风机组05E01-变频手动控制值",{"$f":"E553&VLOOKUP(D553,list!$D$3:$F$501,2,FALSE)&F553&\"_\"&VLOOKUP(G553,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_VFMV"},"LPAU05E01_VFMV AT%M1614.0 :INT; (*P新风机组05E01-变频手动控制值*)","LPAU05E01_VFMV          AT%M1614.0     :INT; (*P新风机组05E01-变频手动控制值*)"]
["1616.0","验证通过","BOOL","P新风机组","L","05E01","低温断路报警隔离","P新风机组05E01-低温断路报警隔离",{"$f":"E554&VLOOKUP(D554,list!$D$3:$F$501,2,FALSE)&F554&\"_\"&VLOOKUP(G554,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_ISO3"},"LPAU05E01_ISO3 AT%M1616.0 :BOOL; (*P新风机组05E01-低温断路报警隔离*)","LPAU05E01_ISO3          AT%M1616.0     :BOOL; (*P新风机组05E01-低温断路报警隔离*)"]
["1618.0","验证通过","INT","P新风机组","L","05E01","变频器频率控制值","P新风机组05E01-变频器频率控制值",{"$f":"E555&VLOOKUP(D555,list!$D$3:$F$501,2,FALSE)&F555&\"_\"&VLOOKUP(G555,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_VFCS"},"LPAU05E01_VFCS AT%M1618.0 :INT; (*P新风机组05E01-变频器频率控制值*)","LPAU05E01_VFCS          AT%M1618.0     :INT; (*P新风机组05E01-变频器频率控制值*)"]
["1620.0","验证通过","INT","P新风机组","L","05E01","变频器频率反馈值","P新风机组05E01-变频器频率反馈值",{"$f":"E556&VLOOKUP(D556,list!$D$3:$F$501,2,FALSE)&F556&\"_\"&VLOOKUP(G556,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_VFBS"},"LPAU05E01_VFBS AT%M1620.0 :INT; (*P新风机组05E01-变频器频率反馈值*)","LPAU05E01_VFBS          AT%M1620.0     :INT; (*P新风机组05E01-变频器频率反馈值*)"]
["1622.0","验证通过","BOOL","P新风机组","L","05E01","联动模式","P新风机组05E01-联动模式",{"$f":"E557&VLOOKUP(D557,list!$D$3:$F$501,2,FALSE)&F557&\"_\"&VLOOKUP(G557,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_LM"},"LPAU05E01_LM AT%M1622.0 :BOOL; (*P新风机组05E01-联动模式*)","LPAU05E01_LM            AT%M1622.0     :BOOL; (*P新风机组05E01-联动模式*)"]
["1624.0","验证通过","BOOL","P新风机组","L","05E01","全天候模式","P新风机组05E01-全天候模式",{"$f":"E558&VLOOKUP(D558,list!$D$3:$F$501,2,FALSE)&F558&\"_\"&VLOOKUP(G558,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_DM"},"LPAU05E01_DM AT%M1624.0 :BOOL; (*P新风机组05E01-全天候模式*)","LPAU05E01_DM            AT%M1624.0     :BOOL; (*P新风机组05E01-全天候模式*)"]
["1628.0","验证通过","REAL","P新风机组","L","05E01","CO2设定值","P新风机组05E01-CO2设定值",{"$f":"E559&VLOOKUP(D559,list!$D$3:$F$501,2,FALSE)&F559&\"_\"&VLOOKUP(G559,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_CO2SET"},"LPAU05E01_CO2SET AT%M1628.0 :REAL; (*P新风机组05E01-CO2设定值*)","LPAU05E01_CO2SET        AT%M1628.0     :REAL; (*P新风机组05E01-CO2设定值*)"]
["1632.0","验证通过","BOOL","P新风机组","L","05E01","定时控制","P新风机组05E01-定时控制",{"$f":"E560&VLOOKUP(D560,list!$D$3:$F$501,2,FALSE)&F560&\"_\"&VLOOKUP(G560,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_TC"},"LPAU05E01_TC AT%M1632.0 :BOOL; (*P新风机组05E01-定时控制*)","LPAU05E01_TC            AT%M1632.0     :BOOL; (*P新风机组05E01-定时控制*)"]
["1634.0","验证通过","BOOL","P新风机组","L","05E01","定时模式","P新风机组05E01-定时模式",{"$f":"E561&VLOOKUP(D561,list!$D$3:$F$501,2,FALSE)&F561&\"_\"&VLOOKUP(G561,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E01_TM"},"LPAU05E01_TM AT%M1634.0 :BOOL; (*P新风机组05E01-定时模式*)","LPAU05E01_TM            AT%M1634.0     :BOOL; (*P新风机组05E01-定时模式*)"]
["PAU"]
[{"$f":"IF(OR(C561=\"REAL\",C561=\"DWORD\",C561=\"DINT\"),(IF(OR(C563=\"REAL\",C563=\"DWORD\",C563=\"DINT\"),A561+4+MOD(A561,4),A561+4)),(IF(OR(C563=\"REAL\",C563=\"DWORD\",C563=\"DINT\"),A561+4+MOD(A561,4),A561+2)))&\".0\"","v":"1640.0"},{"$f":"IF((IF(OR(C563=\"INT\",C563=\"WORD\",C563=\"BOOL\"),MOD(A563,2),MOD(A563,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05E02","设定温度值",{"$f":"D563&F563&\"-\"&IF(E563=\"R\",\"新云平台\"&G563,G563)","v":"P新风机组05E02-新云平台设定温度值"},{"$f":"E563&VLOOKUP(D563,list!$D$3:$F$501,2,FALSE)&F563&\"_\"&VLOOKUP(G563,list!$I$2:$K$502,2,FALSE)","v":"RPAU05E02_TSET"},{"$f":"I563&\" \"&\"AT%M\"&A563&\" \"&\":\"&C563&\";\"&\" \"&\"(*\"&H563&\"*)\"","v":"RPAU05E02_TSET AT%M1640.0 :REAL; (*P新风机组05E02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J563,SEARCH(\"AT%\",J563),,REPT(\" \",25-SEARCH(\"AT%\",J563))),SEARCH(\":\",REPLACE(J563,SEARCH(\"AT%\",J563),,REPT(\" \",25-SEARCH(\"AT%\",J563)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J563,SEARCH(\"AT%\",J563),,REPT(\" \",25-SEARCH(\"AT%\",J563))))))","v":"RPAU05E02_TSET          AT%M1640.0     :REAL; (*P新风机组05E02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C563=\"REAL\",C563=\"DWORD\",C563=\"DINT\"),(IF(OR(C564=\"REAL\",C564=\"DWORD\",C564=\"DINT\"),A563+4+MOD(A563,4),A563+4)),(IF(OR(C564=\"REAL\",C564=\"DWORD\",C564=\"DINT\"),A563+4+MOD(A563,4),A563+2)))&\".0\"","v":"1644.0"},"验证通过","INT","P新风机组","R",{"$f":"F563","v":"05E02"},"季节模式","P新风机组05E02-新云平台季节模式",{"$f":"E564&VLOOKUP(D564,list!$D$3:$F$501,2,FALSE)&F564&\"_\"&VLOOKUP(G564,list!$I$2:$K$502,2,FALSE)","v":"RPAU05E02_SM"},"RPAU05E02_SM AT%M1644.0 :INT; (*P新风机组05E02-新云平台季节模式*)","RPAU05E02_SM            AT%M1644.0     :INT; (*P新风机组05E02-新云平台季节模式*)"]
["1646.0","验证通过","BOOL","P新风机组","R","05E02","程序控制","P新风机组05E02-新云平台程序控制",{"$f":"E565&VLOOKUP(D565,list!$D$3:$F$501,2,FALSE)&F565&\"_\"&VLOOKUP(G565,list!$I$2:$K$502,2,FALSE)","v":"RPAU05E02_PC"},"RPAU05E02_PC AT%M1646.0 :BOOL; (*P新风机组05E02-新云平台程序控制*)","RPAU05E02_PC            AT%M1646.0     :BOOL; (*P新风机组05E02-新云平台程序控制*)"]
["1652.0","验证通过","REAL","P新风机组","L","05E02","设定温度值","P新风机组05E02-设定温度值",{"$f":"E566&VLOOKUP(D566,list!$D$3:$F$501,2,FALSE)&F566&\"_\"&VLOOKUP(G566,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_TSET"},"LPAU05E02_TSET AT%M1652.0 :REAL; (*P新风机组05E02-设定温度值*)","LPAU05E02_TSET          AT%M1652.0     :REAL; (*P新风机组05E02-设定温度值*)"]
["1656.0","验证通过","INT","P新风机组","L","05E02","季节模式","P新风机组05E02-季节模式",{"$f":"E567&VLOOKUP(D567,list!$D$3:$F$501,2,FALSE)&F567&\"_\"&VLOOKUP(G567,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_SM"},"LPAU05E02_SM AT%M1656.0 :INT; (*P新风机组05E02-季节模式*)","LPAU05E02_SM            AT%M1656.0     :INT; (*P新风机组05E02-季节模式*)"]
["1660.0","验证通过","REAL","P新风机组","L","05E02","水阀反馈换算值","P新风机组05E02-水阀反馈换算值",{"$f":"E568&VLOOKUP(D568,list!$D$3:$F$501,2,FALSE)&F568&\"_\"&VLOOKUP(G568,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_WVBS"},"LPAU05E02_WVBS AT%M1660.0 :REAL; (*P新风机组05E02-水阀反馈换算值*)","LPAU05E02_WVBS          AT%M1660.0     :REAL; (*P新风机组05E02-水阀反馈换算值*)"]
["1664.0","验证通过","BOOL","P新风机组","L","05E02","水阀手动控制","P新风机组05E02-水阀手动控制",{"$f":"E569&VLOOKUP(D569,list!$D$3:$F$501,2,FALSE)&F569&\"_\"&VLOOKUP(G569,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_WVMC"},"LPAU05E02_WVMC AT%M1664.0 :BOOL; (*P新风机组05E02-水阀手动控制*)","LPAU05E02_WVMC          AT%M1664.0     :BOOL; (*P新风机组05E02-水阀手动控制*)"]
["1668.0","验证通过","REAL","P新风机组","L","05E02","水阀手动控制值","P新风机组05E02-水阀手动控制值",{"$f":"E570&VLOOKUP(D570,list!$D$3:$F$501,2,FALSE)&F570&\"_\"&VLOOKUP(G570,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_WVMV"},"LPAU05E02_WVMV AT%M1668.0 :REAL; (*P新风机组05E02-水阀手动控制值*)","LPAU05E02_WVMV          AT%M1668.0     :REAL; (*P新风机组05E02-水阀手动控制值*)"]
["1672.0","验证通过","REAL","P新风机组","L","05E02","送风温度换算值","P新风机组05E02-送风温度换算值",{"$f":"E571&VLOOKUP(D571,list!$D$3:$F$501,2,FALSE)&F571&\"_\"&VLOOKUP(G571,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_STS"},"LPAU05E02_STS AT%M1672.0 :REAL; (*P新风机组05E02-送风温度换算值*)","LPAU05E02_STS           AT%M1672.0     :REAL; (*P新风机组05E02-送风温度换算值*)"]
["1676.0","验证通过","BOOL","P新风机组","L","05E02","运行时间累积重置","P新风机组05E02-运行时间累积重置",{"$f":"E572&VLOOKUP(D572,list!$D$3:$F$501,2,FALSE)&F572&\"_\"&VLOOKUP(G572,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_RST"},"LPAU05E02_RST AT%M1676.0 :BOOL; (*P新风机组05E02-运行时间累积重置*)","LPAU05E02_RST           AT%M1676.0     :BOOL; (*P新风机组05E02-运行时间累积重置*)"]
["1680.0","验证通过","REAL","P新风机组","L","05E02","运行时间累积重置值","P新风机组05E02-运行时间累积重置值",{"$f":"E573&VLOOKUP(D573,list!$D$3:$F$501,2,FALSE)&F573&\"_\"&VLOOKUP(G573,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_RSTV"},"LPAU05E02_RSTV AT%M1680.0 :REAL; (*P新风机组05E02-运行时间累积重置值*)","LPAU05E02_RSTV          AT%M1680.0     :REAL; (*P新风机组05E02-运行时间累积重置值*)"]
["1684.0","验证通过","BOOL","P新风机组","L","05E02","隔离开关1","P新风机组05E02-隔离开关1",{"$f":"E574&VLOOKUP(D574,list!$D$3:$F$501,2,FALSE)&F574&\"_\"&VLOOKUP(G574,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_ISO1"},"LPAU05E02_ISO1 AT%M1684.0 :BOOL; (*P新风机组05E02-隔离开关1*)","LPAU05E02_ISO1          AT%M1684.0     :BOOL; (*P新风机组05E02-隔离开关1*)"]
["1686.0","验证通过","BOOL","P新风机组","L","05E02","隔离开关2","P新风机组05E02-隔离开关2",{"$f":"E575&VLOOKUP(D575,list!$D$3:$F$501,2,FALSE)&F575&\"_\"&VLOOKUP(G575,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_ISO2"},"LPAU05E02_ISO2 AT%M1686.0 :BOOL; (*P新风机组05E02-隔离开关2*)","LPAU05E02_ISO2          AT%M1686.0     :BOOL; (*P新风机组05E02-隔离开关2*)"]
["1692.0","验证通过","REAL","P新风机组","L","05E02","P调节参数","P新风机组05E02-P调节参数",{"$f":"E576&VLOOKUP(D576,list!$D$3:$F$501,2,FALSE)&F576&\"_\"&VLOOKUP(G576,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_VP"},"LPAU05E02_VP AT%M1692.0 :REAL; (*P新风机组05E02-P调节参数*)","LPAU05E02_VP            AT%M1692.0     :REAL; (*P新风机组05E02-P调节参数*)"]
["1696.0","验证通过","REAL","P新风机组","L","05E02","I调节参数","P新风机组05E02-I调节参数",{"$f":"E577&VLOOKUP(D577,list!$D$3:$F$501,2,FALSE)&F577&\"_\"&VLOOKUP(G577,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_VI"},"LPAU05E02_VI AT%M1696.0 :REAL; (*P新风机组05E02-I调节参数*)","LPAU05E02_VI            AT%M1696.0     :REAL; (*P新风机组05E02-I调节参数*)"]
["1700.0","验证通过","REAL","P新风机组","L","05E02","运行时间累积值","P新风机组05E02-运行时间累积值",{"$f":"E578&VLOOKUP(D578,list!$D$3:$F$501,2,FALSE)&F578&\"_\"&VLOOKUP(G578,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_RH"},"LPAU05E02_RH AT%M1700.0 :REAL; (*P新风机组05E02-运行时间累积值*)","LPAU05E02_RH            AT%M1700.0     :REAL; (*P新风机组05E02-运行时间累积值*)"]
["1704.0","验证通过","INT","P新风机组","L","05E02","设备状态代码","P新风机组05E02-设备状态代码",{"$f":"E579&VLOOKUP(D579,list!$D$3:$F$501,2,FALSE)&F579&\"_\"&VLOOKUP(G579,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_SN"},"LPAU05E02_SN AT%M1704.0 :INT; (*P新风机组05E02-设备状态代码*)","LPAU05E02_SN            AT%M1704.0     :INT; (*P新风机组05E02-设备状态代码*)"]
["1706.0","验证通过","INT","P新风机组","L","05E02","水阀控制转换值","P新风机组05E02-水阀控制转换值",{"$f":"E580&VLOOKUP(D580,list!$D$3:$F$501,2,FALSE)&F580&\"_\"&VLOOKUP(G580,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_WVCS"},"LPAU05E02_WVCS AT%M1706.0 :INT; (*P新风机组05E02-水阀控制转换值*)","LPAU05E02_WVCS          AT%M1706.0     :INT; (*P新风机组05E02-水阀控制转换值*)"]
["1708.0","验证通过","BOOL","P新风机组","L","05E02","程序控制","P新风机组05E02-程序控制",{"$f":"E581&VLOOKUP(D581,list!$D$3:$F$501,2,FALSE)&F581&\"_\"&VLOOKUP(G581,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_PC"},"LPAU05E02_PC AT%M1708.0 :BOOL; (*P新风机组05E02-程序控制*)","LPAU05E02_PC            AT%M1708.0     :BOOL; (*P新风机组05E02-程序控制*)"]
["1710.0","验证通过","INT","P新风机组","L","05E02","变频手动控制值","P新风机组05E02-变频手动控制值",{"$f":"E582&VLOOKUP(D582,list!$D$3:$F$501,2,FALSE)&F582&\"_\"&VLOOKUP(G582,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_VFMV"},"LPAU05E02_VFMV AT%M1710.0 :INT; (*P新风机组05E02-变频手动控制值*)","LPAU05E02_VFMV          AT%M1710.0     :INT; (*P新风机组05E02-变频手动控制值*)"]
["1712.0","验证通过","BOOL","P新风机组","L","05E02","低温断路报警隔离","P新风机组05E02-低温断路报警隔离",{"$f":"E583&VLOOKUP(D583,list!$D$3:$F$501,2,FALSE)&F583&\"_\"&VLOOKUP(G583,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_ISO3"},"LPAU05E02_ISO3 AT%M1712.0 :BOOL; (*P新风机组05E02-低温断路报警隔离*)","LPAU05E02_ISO3          AT%M1712.0     :BOOL; (*P新风机组05E02-低温断路报警隔离*)"]
["1714.0","验证通过","INT","P新风机组","L","05E02","变频器频率控制值","P新风机组05E02-变频器频率控制值",{"$f":"E584&VLOOKUP(D584,list!$D$3:$F$501,2,FALSE)&F584&\"_\"&VLOOKUP(G584,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_VFCS"},"LPAU05E02_VFCS AT%M1714.0 :INT; (*P新风机组05E02-变频器频率控制值*)","LPAU05E02_VFCS          AT%M1714.0     :INT; (*P新风机组05E02-变频器频率控制值*)"]
["1716.0","验证通过","INT","P新风机组","L","05E02","变频器频率反馈值","P新风机组05E02-变频器频率反馈值",{"$f":"E585&VLOOKUP(D585,list!$D$3:$F$501,2,FALSE)&F585&\"_\"&VLOOKUP(G585,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_VFBS"},"LPAU05E02_VFBS AT%M1716.0 :INT; (*P新风机组05E02-变频器频率反馈值*)","LPAU05E02_VFBS          AT%M1716.0     :INT; (*P新风机组05E02-变频器频率反馈值*)"]
["1718.0","验证通过","BOOL","P新风机组","L","05E02","联动模式","P新风机组05E02-联动模式",{"$f":"E586&VLOOKUP(D586,list!$D$3:$F$501,2,FALSE)&F586&\"_\"&VLOOKUP(G586,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_LM"},"LPAU05E02_LM AT%M1718.0 :BOOL; (*P新风机组05E02-联动模式*)","LPAU05E02_LM            AT%M1718.0     :BOOL; (*P新风机组05E02-联动模式*)"]
["1720.0","验证通过","BOOL","P新风机组","L","05E02","全天候模式","P新风机组05E02-全天候模式",{"$f":"E587&VLOOKUP(D587,list!$D$3:$F$501,2,FALSE)&F587&\"_\"&VLOOKUP(G587,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_DM"},"LPAU05E02_DM AT%M1720.0 :BOOL; (*P新风机组05E02-全天候模式*)","LPAU05E02_DM            AT%M1720.0     :BOOL; (*P新风机组05E02-全天候模式*)"]
["1724.0","验证通过","REAL","P新风机组","L","05E02","CO2设定值","P新风机组05E02-CO2设定值",{"$f":"E588&VLOOKUP(D588,list!$D$3:$F$501,2,FALSE)&F588&\"_\"&VLOOKUP(G588,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_CO2SET"},"LPAU05E02_CO2SET AT%M1724.0 :REAL; (*P新风机组05E02-CO2设定值*)","LPAU05E02_CO2SET        AT%M1724.0     :REAL; (*P新风机组05E02-CO2设定值*)"]
["1728.0","验证通过","BOOL","P新风机组","L","05E02","定时控制","P新风机组05E02-定时控制",{"$f":"E589&VLOOKUP(D589,list!$D$3:$F$501,2,FALSE)&F589&\"_\"&VLOOKUP(G589,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_TC"},"LPAU05E02_TC AT%M1728.0 :BOOL; (*P新风机组05E02-定时控制*)","LPAU05E02_TC            AT%M1728.0     :BOOL; (*P新风机组05E02-定时控制*)"]
["1730.0","验证通过","BOOL","P新风机组","L","05E02","定时模式","P新风机组05E02-定时模式",{"$f":"E590&VLOOKUP(D590,list!$D$3:$F$501,2,FALSE)&F590&\"_\"&VLOOKUP(G590,list!$I$2:$K$502,2,FALSE)","v":"LPAU05E02_TM"},"LPAU05E02_TM AT%M1730.0 :BOOL; (*P新风机组05E02-定时模式*)","LPAU05E02_TM            AT%M1730.0     :BOOL; (*P新风机组05E02-定时模式*)"]
["FCU"]
[{"$f":"IF(OR(C143=\"REAL\",C143=\"DWORD\",C143=\"DINT\"),(IF(OR(C592=\"REAL\",C592=\"DWORD\",C592=\"DINT\"),A143+4+MOD(A143,4),A143+4)),(IF(OR(C592=\"REAL\",C592=\"DWORD\",C592=\"DINT\"),A143+4+MOD(A143,4),A143+2)))&\".0\"","v":"600.0"},{"$f":"IF((IF(OR(C592=\"INT\",C592=\"WORD\",C592=\"BOOL\"),MOD(A592,2),MOD(A592,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","03G01","设定温度值",{"$f":"D592&F592&\"-\"&IF(E592=\"R\",\"新云平台\"&G592,G592)","v":"风机盘管03G01-新云平台设定温度值"},{"$f":"E592&VLOOKUP(D592,list!$D$3:$F$501,2,FALSE)&F592&\"_\"&VLOOKUP(G592,list!$I$2:$K$502,2,FALSE)","v":"RFCU03G01_TSET"},{"$f":"I592&\" \"&\"AT%M\"&A592&\" \"&\":\"&C592&\";\"&\" \"&\"(*\"&H592&\"*)\"","v":"RFCU03G01_TSET AT%M600.0 :REAL; (*风机盘管03G01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J592,SEARCH(\"AT%\",J592),,REPT(\" \",25-SEARCH(\"AT%\",J592))),SEARCH(\":\",REPLACE(J592,SEARCH(\"AT%\",J592),,REPT(\" \",25-SEARCH(\"AT%\",J592)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J592,SEARCH(\"AT%\",J592),,REPT(\" \",25-SEARCH(\"AT%\",J592))))))","v":"RFCU03G01_TSET          AT%M600.0      :REAL; (*风机盘管03G01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C592=\"REAL\",C592=\"DWORD\",C592=\"DINT\"),(IF(OR(C593=\"REAL\",C593=\"DWORD\",C593=\"DINT\"),A592+4+MOD(A592,4),A592+4)),(IF(OR(C593=\"REAL\",C593=\"DWORD\",C593=\"DINT\"),A592+4+MOD(A592,4),A592+2)))&\".0\"","v":"604.0"},"验证通过","INT","风机盘管","R",{"$f":"F592","v":"03G01"},"季节模式","风机盘管03G01-新云平台季节模式",{"$f":"E593&VLOOKUP(D593,list!$D$3:$F$501,2,FALSE)&F593&\"_\"&VLOOKUP(G593,list!$I$2:$K$502,2,FALSE)","v":"RFCU03G01_SM"},"RFCU03G01_SM AT%M604.0 :INT; (*风机盘管03G01-新云平台季节模式*)","RFCU03G01_SM            AT%M604.0      :INT; (*风机盘管03G01-新云平台季节模式*)"]
["606.0","验证通过","BOOL","风机盘管","R","03G01","程序控制","风机盘管03G01-新云平台程序控制",{"$f":"E594&VLOOKUP(D594,list!$D$3:$F$501,2,FALSE)&F594&\"_\"&VLOOKUP(G594,list!$I$2:$K$502,2,FALSE)","v":"RFCU03G01_PC"},"RFCU03G01_PC AT%M606.0 :BOOL; (*风机盘管03G01-新云平台程序控制*)","RFCU03G01_PC            AT%M606.0      :BOOL; (*风机盘管03G01-新云平台程序控制*)"]
["612.0","验证通过","REAL","风机盘管","L","03G01","设定温度值","风机盘管03G01-设定温度值",{"$f":"E595&VLOOKUP(D595,list!$D$3:$F$501,2,FALSE)&F595&\"_\"&VLOOKUP(G595,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_TSET"},"LFCU03G01_TSET AT%M612.0 :REAL; (*风机盘管03G01-设定温度值*)","LFCU03G01_TSET          AT%M612.0      :REAL; (*风机盘管03G01-设定温度值*)"]
["616.0","验证通过","INT","风机盘管","L","03G01","季节模式","风机盘管03G01-季节模式",{"$f":"E596&VLOOKUP(D596,list!$D$3:$F$501,2,FALSE)&F596&\"_\"&VLOOKUP(G596,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_SM"},"LFCU03G01_SM AT%M616.0 :INT; (*风机盘管03G01-季节模式*)","LFCU03G01_SM            AT%M616.0      :INT; (*风机盘管03G01-季节模式*)"]
["620.0","验证通过","REAL","风机盘管","L","03G01","温度换算值","风机盘管03G01-温度换算值",{"$f":"E597&VLOOKUP(D597,list!$D$3:$F$501,2,FALSE)&F597&\"_\"&VLOOKUP(G597,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_TS"},"LFCU03G01_TS AT%M620.0 :REAL; (*风机盘管03G01-温度换算值*)","LFCU03G01_TS            AT%M620.0      :REAL; (*风机盘管03G01-温度换算值*)"]
["624.0","验证通过","BOOL","风机盘管","L","03G01","电磁阀手动控制","风机盘管03G01-电磁阀手动控制",{"$f":"E598&VLOOKUP(D598,list!$D$3:$F$501,2,FALSE)&F598&\"_\"&VLOOKUP(G598,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_EVMC"},"LFCU03G01_EVMC AT%M624.0 :BOOL; (*风机盘管03G01-电磁阀手动控制*)","LFCU03G01_EVMC          AT%M624.0      :BOOL; (*风机盘管03G01-电磁阀手动控制*)"]
["626.0","验证通过","BOOL","风机盘管","L","03G01","电磁阀手动控制值","风机盘管03G01-电磁阀手动控制值",{"$f":"E599&VLOOKUP(D599,list!$D$3:$F$501,2,FALSE)&F599&\"_\"&VLOOKUP(G599,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_EVMV"},"LFCU03G01_EVMV AT%M626.0 :BOOL; (*风机盘管03G01-电磁阀手动控制值*)","LFCU03G01_EVMV          AT%M626.0      :BOOL; (*风机盘管03G01-电磁阀手动控制值*)"]
["632.0","验证通过","REAL","风机盘管","L","03G01","回风温度换算值","风机盘管03G01-回风温度换算值",{"$f":"E600&VLOOKUP(D600,list!$D$3:$F$501,2,FALSE)&F600&\"_\"&VLOOKUP(G600,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_RTS"},"LFCU03G01_RTS AT%M632.0 :REAL; (*风机盘管03G01-回风温度换算值*)","LFCU03G01_RTS           AT%M632.0      :REAL; (*风机盘管03G01-回风温度换算值*)"]
["636.0","验证通过","BOOL","风机盘管","L","03G01","运行时间累积重置","风机盘管03G01-运行时间累积重置",{"$f":"E601&VLOOKUP(D601,list!$D$3:$F$501,2,FALSE)&F601&\"_\"&VLOOKUP(G601,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_RST"},"LFCU03G01_RST AT%M636.0 :BOOL; (*风机盘管03G01-运行时间累积重置*)","LFCU03G01_RST           AT%M636.0      :BOOL; (*风机盘管03G01-运行时间累积重置*)"]
["640.0","验证通过","REAL","风机盘管","L","03G01","运行时间累积重置值","风机盘管03G01-运行时间累积重置值",{"$f":"E602&VLOOKUP(D602,list!$D$3:$F$501,2,FALSE)&F602&\"_\"&VLOOKUP(G602,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_RSTV"},"LFCU03G01_RSTV AT%M640.0 :REAL; (*风机盘管03G01-运行时间累积重置值*)","LFCU03G01_RSTV          AT%M640.0      :REAL; (*风机盘管03G01-运行时间累积重置值*)"]
["644.0","验证通过","BOOL","风机盘管","L","03G01","隔离开关1","风机盘管03G01-隔离开关1",{"$f":"E603&VLOOKUP(D603,list!$D$3:$F$501,2,FALSE)&F603&\"_\"&VLOOKUP(G603,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_ISO1"},"LFCU03G01_ISO1 AT%M644.0 :BOOL; (*风机盘管03G01-隔离开关1*)","LFCU03G01_ISO1          AT%M644.0      :BOOL; (*风机盘管03G01-隔离开关1*)"]
["648.0","验证通过","REAL","风机盘管","L","03G01","运行时间累积值","风机盘管03G01-运行时间累积值",{"$f":"E604&VLOOKUP(D604,list!$D$3:$F$501,2,FALSE)&F604&\"_\"&VLOOKUP(G604,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_RH"},"LFCU03G01_RH AT%M648.0 :REAL; (*风机盘管03G01-运行时间累积值*)","LFCU03G01_RH            AT%M648.0      :REAL; (*风机盘管03G01-运行时间累积值*)"]
["652.0","验证通过","INT","风机盘管","L","03G01","设备状态代码","风机盘管03G01-设备状态代码",{"$f":"E605&VLOOKUP(D605,list!$D$3:$F$501,2,FALSE)&F605&\"_\"&VLOOKUP(G605,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_SN"},"LFCU03G01_SN AT%M652.0 :INT; (*风机盘管03G01-设备状态代码*)","LFCU03G01_SN            AT%M652.0      :INT; (*风机盘管03G01-设备状态代码*)"]
["654.0","验证通过","INT","风机盘管","L","03G01","水阀控制转换值","风机盘管03G01-水阀控制转换值",{"$f":"E606&VLOOKUP(D606,list!$D$3:$F$501,2,FALSE)&F606&\"_\"&VLOOKUP(G606,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_WVCS"},"LFCU03G01_WVCS AT%M654.0 :INT; (*风机盘管03G01-水阀控制转换值*)","LFCU03G01_WVCS          AT%M654.0      :INT; (*风机盘管03G01-水阀控制转换值*)"]
["656.0","验证通过","BOOL","风机盘管","L","03G01","程序控制","风机盘管03G01-程序控制",{"$f":"E607&VLOOKUP(D607,list!$D$3:$F$501,2,FALSE)&F607&\"_\"&VLOOKUP(G607,list!$I$2:$K$502,2,FALSE)","v":"LFCU03G01_PC"},"LFCU03G01_PC AT%M656.0 :BOOL; (*风机盘管03G01-程序控制*)","LFCU03G01_PC            AT%M656.0      :BOOL; (*风机盘管03G01-程序控制*)"]
["PAU"]
[{"$f":"IF(OR(C607=\"REAL\",C607=\"DWORD\",C607=\"DINT\"),(IF(OR(C609=\"REAL\",C609=\"DWORD\",C609=\"DINT\"),A607+4+MOD(A607,4),A607+4)),(IF(OR(C609=\"REAL\",C609=\"DWORD\",C609=\"DINT\"),A607+4+MOD(A607,4),A607+2)))&\".0\"","v":"660.0"},{"$f":"IF((IF(OR(C609=\"INT\",C609=\"WORD\",C609=\"BOOL\"),MOD(A609,2),MOD(A609,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05B01","设定温度值",{"$f":"D609&F609&\"-\"&IF(E609=\"R\",\"新云平台\"&G609,G609)","v":"P新风机组05B01-新云平台设定温度值"},{"$f":"E609&VLOOKUP(D609,list!$D$3:$F$501,2,FALSE)&F609&\"_\"&VLOOKUP(G609,list!$I$2:$K$502,2,FALSE)","v":"RPAU05B01_TSET"},{"$f":"I609&\" \"&\"AT%M\"&A609&\" \"&\":\"&C609&\";\"&\" \"&\"(*\"&H609&\"*)\"","v":"RPAU05B01_TSET AT%M660.0 :REAL; (*P新风机组05B01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J609,SEARCH(\"AT%\",J609),,REPT(\" \",25-SEARCH(\"AT%\",J609))),SEARCH(\":\",REPLACE(J609,SEARCH(\"AT%\",J609),,REPT(\" \",25-SEARCH(\"AT%\",J609)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J609,SEARCH(\"AT%\",J609),,REPT(\" \",25-SEARCH(\"AT%\",J609))))))","v":"RPAU05B01_TSET          AT%M660.0      :REAL; (*P新风机组05B01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C609=\"REAL\",C609=\"DWORD\",C609=\"DINT\"),(IF(OR(C610=\"REAL\",C610=\"DWORD\",C610=\"DINT\"),A609+4+MOD(A609,4),A609+4)),(IF(OR(C610=\"REAL\",C610=\"DWORD\",C610=\"DINT\"),A609+4+MOD(A609,4),A609+2)))&\".0\"","v":"664.0"},"验证通过","INT","P新风机组","R",{"$f":"F609","v":"05B01"},"季节模式","P新风机组05B01-新云平台季节模式",{"$f":"E610&VLOOKUP(D610,list!$D$3:$F$501,2,FALSE)&F610&\"_\"&VLOOKUP(G610,list!$I$2:$K$502,2,FALSE)","v":"RPAU05B01_SM"},"RPAU05B01_SM AT%M664.0 :INT; (*P新风机组05B01-新云平台季节模式*)","RPAU05B01_SM            AT%M664.0      :INT; (*P新风机组05B01-新云平台季节模式*)"]
["666.0","验证通过","BOOL","P新风机组","R","05B01","程序控制","P新风机组05B01-新云平台程序控制",{"$f":"E611&VLOOKUP(D611,list!$D$3:$F$501,2,FALSE)&F611&\"_\"&VLOOKUP(G611,list!$I$2:$K$502,2,FALSE)","v":"RPAU05B01_PC"},"RPAU05B01_PC AT%M666.0 :BOOL; (*P新风机组05B01-新云平台程序控制*)","RPAU05B01_PC            AT%M666.0      :BOOL; (*P新风机组05B01-新云平台程序控制*)"]
["672.0","验证通过","REAL","P新风机组","L","05B01","设定温度值","P新风机组05B01-设定温度值",{"$f":"E612&VLOOKUP(D612,list!$D$3:$F$501,2,FALSE)&F612&\"_\"&VLOOKUP(G612,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_TSET"},"LPAU05B01_TSET AT%M672.0 :REAL; (*P新风机组05B01-设定温度值*)","LPAU05B01_TSET          AT%M672.0      :REAL; (*P新风机组05B01-设定温度值*)"]
["676.0","验证通过","INT","P新风机组","L","05B01","季节模式","P新风机组05B01-季节模式",{"$f":"E613&VLOOKUP(D613,list!$D$3:$F$501,2,FALSE)&F613&\"_\"&VLOOKUP(G613,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_SM"},"LPAU05B01_SM AT%M676.0 :INT; (*P新风机组05B01-季节模式*)","LPAU05B01_SM            AT%M676.0      :INT; (*P新风机组05B01-季节模式*)"]
["680.0","验证通过","REAL","P新风机组","L","05B01","水阀反馈换算值","P新风机组05B01-水阀反馈换算值",{"$f":"E614&VLOOKUP(D614,list!$D$3:$F$501,2,FALSE)&F614&\"_\"&VLOOKUP(G614,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_WVBS"},"LPAU05B01_WVBS AT%M680.0 :REAL; (*P新风机组05B01-水阀反馈换算值*)","LPAU05B01_WVBS          AT%M680.0      :REAL; (*P新风机组05B01-水阀反馈换算值*)"]
["684.0","验证通过","BOOL","P新风机组","L","05B01","水阀手动控制","P新风机组05B01-水阀手动控制",{"$f":"E615&VLOOKUP(D615,list!$D$3:$F$501,2,FALSE)&F615&\"_\"&VLOOKUP(G615,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_WVMC"},"LPAU05B01_WVMC AT%M684.0 :BOOL; (*P新风机组05B01-水阀手动控制*)","LPAU05B01_WVMC          AT%M684.0      :BOOL; (*P新风机组05B01-水阀手动控制*)"]
["688.0","验证通过","REAL","P新风机组","L","05B01","水阀手动控制值","P新风机组05B01-水阀手动控制值",{"$f":"E616&VLOOKUP(D616,list!$D$3:$F$501,2,FALSE)&F616&\"_\"&VLOOKUP(G616,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_WVMV"},"LPAU05B01_WVMV AT%M688.0 :REAL; (*P新风机组05B01-水阀手动控制值*)","LPAU05B01_WVMV          AT%M688.0      :REAL; (*P新风机组05B01-水阀手动控制值*)"]
["692.0","验证通过","REAL","P新风机组","L","05B01","送风温度换算值","P新风机组05B01-送风温度换算值",{"$f":"E617&VLOOKUP(D617,list!$D$3:$F$501,2,FALSE)&F617&\"_\"&VLOOKUP(G617,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_STS"},"LPAU05B01_STS AT%M692.0 :REAL; (*P新风机组05B01-送风温度换算值*)","LPAU05B01_STS           AT%M692.0      :REAL; (*P新风机组05B01-送风温度换算值*)"]
["696.0","验证通过","BOOL","P新风机组","L","05B01","运行时间累积重置","P新风机组05B01-运行时间累积重置",{"$f":"E618&VLOOKUP(D618,list!$D$3:$F$501,2,FALSE)&F618&\"_\"&VLOOKUP(G618,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_RST"},"LPAU05B01_RST AT%M696.0 :BOOL; (*P新风机组05B01-运行时间累积重置*)","LPAU05B01_RST           AT%M696.0      :BOOL; (*P新风机组05B01-运行时间累积重置*)"]
["700.0","验证通过","REAL","P新风机组","L","05B01","运行时间累积重置值","P新风机组05B01-运行时间累积重置值",{"$f":"E619&VLOOKUP(D619,list!$D$3:$F$501,2,FALSE)&F619&\"_\"&VLOOKUP(G619,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_RSTV"},"LPAU05B01_RSTV AT%M700.0 :REAL; (*P新风机组05B01-运行时间累积重置值*)","LPAU05B01_RSTV          AT%M700.0      :REAL; (*P新风机组05B01-运行时间累积重置值*)"]
["704.0","验证通过","BOOL","P新风机组","L","05B01","隔离开关1","P新风机组05B01-隔离开关1",{"$f":"E620&VLOOKUP(D620,list!$D$3:$F$501,2,FALSE)&F620&\"_\"&VLOOKUP(G620,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_ISO1"},"LPAU05B01_ISO1 AT%M704.0 :BOOL; (*P新风机组05B01-隔离开关1*)","LPAU05B01_ISO1          AT%M704.0      :BOOL; (*P新风机组05B01-隔离开关1*)"]
["706.0","验证通过","BOOL","P新风机组","L","05B01","隔离开关2","P新风机组05B01-隔离开关2",{"$f":"E621&VLOOKUP(D621,list!$D$3:$F$501,2,FALSE)&F621&\"_\"&VLOOKUP(G621,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_ISO2"},"LPAU05B01_ISO2 AT%M706.0 :BOOL; (*P新风机组05B01-隔离开关2*)","LPAU05B01_ISO2          AT%M706.0      :BOOL; (*P新风机组05B01-隔离开关2*)"]
["712.0","验证通过","REAL","P新风机组","L","05B01","P调节参数","P新风机组05B01-P调节参数",{"$f":"E622&VLOOKUP(D622,list!$D$3:$F$501,2,FALSE)&F622&\"_\"&VLOOKUP(G622,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_VP"},"LPAU05B01_VP AT%M712.0 :REAL; (*P新风机组05B01-P调节参数*)","LPAU05B01_VP            AT%M712.0      :REAL; (*P新风机组05B01-P调节参数*)"]
["716.0","验证通过","REAL","P新风机组","L","05B01","I调节参数","P新风机组05B01-I调节参数",{"$f":"E623&VLOOKUP(D623,list!$D$3:$F$501,2,FALSE)&F623&\"_\"&VLOOKUP(G623,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_VI"},"LPAU05B01_VI AT%M716.0 :REAL; (*P新风机组05B01-I调节参数*)","LPAU05B01_VI            AT%M716.0      :REAL; (*P新风机组05B01-I调节参数*)"]
["720.0","验证通过","REAL","P新风机组","L","05B01","运行时间累积值","P新风机组05B01-运行时间累积值",{"$f":"E624&VLOOKUP(D624,list!$D$3:$F$501,2,FALSE)&F624&\"_\"&VLOOKUP(G624,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_RH"},"LPAU05B01_RH AT%M720.0 :REAL; (*P新风机组05B01-运行时间累积值*)","LPAU05B01_RH            AT%M720.0      :REAL; (*P新风机组05B01-运行时间累积值*)"]
["724.0","验证通过","INT","P新风机组","L","05B01","设备状态代码","P新风机组05B01-设备状态代码",{"$f":"E625&VLOOKUP(D625,list!$D$3:$F$501,2,FALSE)&F625&\"_\"&VLOOKUP(G625,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_SN"},"LPAU05B01_SN AT%M724.0 :INT; (*P新风机组05B01-设备状态代码*)","LPAU05B01_SN            AT%M724.0      :INT; (*P新风机组05B01-设备状态代码*)"]
["726.0","验证通过","INT","P新风机组","L","05B01","水阀控制转换值","P新风机组05B01-水阀控制转换值",{"$f":"E626&VLOOKUP(D626,list!$D$3:$F$501,2,FALSE)&F626&\"_\"&VLOOKUP(G626,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_WVCS"},"LPAU05B01_WVCS AT%M726.0 :INT; (*P新风机组05B01-水阀控制转换值*)","LPAU05B01_WVCS          AT%M726.0      :INT; (*P新风机组05B01-水阀控制转换值*)"]
["728.0","验证通过","BOOL","P新风机组","L","05B01","程序控制","P新风机组05B01-程序控制",{"$f":"E627&VLOOKUP(D627,list!$D$3:$F$501,2,FALSE)&F627&\"_\"&VLOOKUP(G627,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_PC"},"LPAU05B01_PC AT%M728.0 :BOOL; (*P新风机组05B01-程序控制*)","LPAU05B01_PC            AT%M728.0      :BOOL; (*P新风机组05B01-程序控制*)"]
["730.0","验证通过","INT","P新风机组","L","05B01","变频手动控制值","P新风机组05B01-变频手动控制值",{"$f":"E628&VLOOKUP(D628,list!$D$3:$F$501,2,FALSE)&F628&\"_\"&VLOOKUP(G628,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_VFMV"},"LPAU05B01_VFMV AT%M730.0 :INT; (*P新风机组05B01-变频手动控制值*)","LPAU05B01_VFMV          AT%M730.0      :INT; (*P新风机组05B01-变频手动控制值*)"]
["732.0","验证通过","BOOL","P新风机组","L","05B01","低温断路报警隔离","P新风机组05B01-低温断路报警隔离",{"$f":"E629&VLOOKUP(D629,list!$D$3:$F$501,2,FALSE)&F629&\"_\"&VLOOKUP(G629,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_ISO3"},"LPAU05B01_ISO3 AT%M732.0 :BOOL; (*P新风机组05B01-低温断路报警隔离*)","LPAU05B01_ISO3          AT%M732.0      :BOOL; (*P新风机组05B01-低温断路报警隔离*)"]
["734.0","验证通过","INT","P新风机组","L","05B01","变频器频率控制值","P新风机组05B01-变频器频率控制值",{"$f":"E630&VLOOKUP(D630,list!$D$3:$F$501,2,FALSE)&F630&\"_\"&VLOOKUP(G630,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_VFCS"},"LPAU05B01_VFCS AT%M734.0 :INT; (*P新风机组05B01-变频器频率控制值*)","LPAU05B01_VFCS          AT%M734.0      :INT; (*P新风机组05B01-变频器频率控制值*)"]
["736.0","验证通过","INT","P新风机组","L","05B01","变频器频率反馈值","P新风机组05B01-变频器频率反馈值",{"$f":"E631&VLOOKUP(D631,list!$D$3:$F$501,2,FALSE)&F631&\"_\"&VLOOKUP(G631,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_VFBS"},"LPAU05B01_VFBS AT%M736.0 :INT; (*P新风机组05B01-变频器频率反馈值*)","LPAU05B01_VFBS          AT%M736.0      :INT; (*P新风机组05B01-变频器频率反馈值*)"]
["738.0","验证通过","BOOL","P新风机组","L","05B01","联动模式","P新风机组05B01-联动模式",{"$f":"E632&VLOOKUP(D632,list!$D$3:$F$501,2,FALSE)&F632&\"_\"&VLOOKUP(G632,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_LM"},"LPAU05B01_LM AT%M738.0 :BOOL; (*P新风机组05B01-联动模式*)","LPAU05B01_LM            AT%M738.0      :BOOL; (*P新风机组05B01-联动模式*)"]
["740.0","验证通过","BOOL","P新风机组","L","05B01","全天候模式","P新风机组05B01-全天候模式",{"$f":"E633&VLOOKUP(D633,list!$D$3:$F$501,2,FALSE)&F633&\"_\"&VLOOKUP(G633,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_DM"},"LPAU05B01_DM AT%M740.0 :BOOL; (*P新风机组05B01-全天候模式*)","LPAU05B01_DM            AT%M740.0      :BOOL; (*P新风机组05B01-全天候模式*)"]
["744.0","验证通过","REAL","P新风机组","L","05B01","CO2设定值","P新风机组05B01-CO2设定值",{"$f":"E634&VLOOKUP(D634,list!$D$3:$F$501,2,FALSE)&F634&\"_\"&VLOOKUP(G634,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_CO2SET"},"LPAU05B01_CO2SET AT%M744.0 :REAL; (*P新风机组05B01-CO2设定值*)","LPAU05B01_CO2SET        AT%M744.0      :REAL; (*P新风机组05B01-CO2设定值*)"]
["748.0","验证通过","BOOL","P新风机组","L","05B01","定时控制","P新风机组05B01-定时控制",{"$f":"E635&VLOOKUP(D635,list!$D$3:$F$501,2,FALSE)&F635&\"_\"&VLOOKUP(G635,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_TC"},"LPAU05B01_TC AT%M748.0 :BOOL; (*P新风机组05B01-定时控制*)","LPAU05B01_TC            AT%M748.0      :BOOL; (*P新风机组05B01-定时控制*)"]
["750.0","验证通过","BOOL","P新风机组","L","05B01","定时模式","P新风机组05B01-定时模式",{"$f":"E636&VLOOKUP(D636,list!$D$3:$F$501,2,FALSE)&F636&\"_\"&VLOOKUP(G636,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B01_TM"},"LPAU05B01_TM AT%M750.0 :BOOL; (*P新风机组05B01-定时模式*)","LPAU05B01_TM            AT%M750.0      :BOOL; (*P新风机组05B01-定时模式*)"]
["PAU"]
[{"$f":"IF(OR(C636=\"REAL\",C636=\"DWORD\",C636=\"DINT\"),(IF(OR(C638=\"REAL\",C638=\"DWORD\",C638=\"DINT\"),A636+4+MOD(A636,4),A636+4)),(IF(OR(C638=\"REAL\",C638=\"DWORD\",C638=\"DINT\"),A636+4+MOD(A636,4),A636+2)))&\".0\"","v":"756.0"},{"$f":"IF((IF(OR(C638=\"INT\",C638=\"WORD\",C638=\"BOOL\"),MOD(A638,2),MOD(A638,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05B02","设定温度值",{"$f":"D638&F638&\"-\"&IF(E638=\"R\",\"新云平台\"&G638,G638)","v":"P新风机组05B02-新云平台设定温度值"},{"$f":"E638&VLOOKUP(D638,list!$D$3:$F$501,2,FALSE)&F638&\"_\"&VLOOKUP(G638,list!$I$2:$K$502,2,FALSE)","v":"RPAU05B02_TSET"},{"$f":"I638&\" \"&\"AT%M\"&A638&\" \"&\":\"&C638&\";\"&\" \"&\"(*\"&H638&\"*)\"","v":"RPAU05B02_TSET AT%M756.0 :REAL; (*P新风机组05B02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J638,SEARCH(\"AT%\",J638),,REPT(\" \",25-SEARCH(\"AT%\",J638))),SEARCH(\":\",REPLACE(J638,SEARCH(\"AT%\",J638),,REPT(\" \",25-SEARCH(\"AT%\",J638)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J638,SEARCH(\"AT%\",J638),,REPT(\" \",25-SEARCH(\"AT%\",J638))))))","v":"RPAU05B02_TSET          AT%M756.0      :REAL; (*P新风机组05B02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C638=\"REAL\",C638=\"DWORD\",C638=\"DINT\"),(IF(OR(C639=\"REAL\",C639=\"DWORD\",C639=\"DINT\"),A638+4+MOD(A638,4),A638+4)),(IF(OR(C639=\"REAL\",C639=\"DWORD\",C639=\"DINT\"),A638+4+MOD(A638,4),A638+2)))&\".0\"","v":"760.0"},"验证通过","INT","P新风机组","R",{"$f":"F638","v":"05B02"},"季节模式","P新风机组05B02-新云平台季节模式",{"$f":"E639&VLOOKUP(D639,list!$D$3:$F$501,2,FALSE)&F639&\"_\"&VLOOKUP(G639,list!$I$2:$K$502,2,FALSE)","v":"RPAU05B02_SM"},"RPAU05B02_SM AT%M760.0 :INT; (*P新风机组05B02-新云平台季节模式*)","RPAU05B02_SM            AT%M760.0      :INT; (*P新风机组05B02-新云平台季节模式*)"]
["762.0","验证通过","BOOL","P新风机组","R","05B02","程序控制","P新风机组05B02-新云平台程序控制",{"$f":"E640&VLOOKUP(D640,list!$D$3:$F$501,2,FALSE)&F640&\"_\"&VLOOKUP(G640,list!$I$2:$K$502,2,FALSE)","v":"RPAU05B02_PC"},"RPAU05B02_PC AT%M762.0 :BOOL; (*P新风机组05B02-新云平台程序控制*)","RPAU05B02_PC            AT%M762.0      :BOOL; (*P新风机组05B02-新云平台程序控制*)"]
["768.0","验证通过","REAL","P新风机组","L","05B02","设定温度值","P新风机组05B02-设定温度值",{"$f":"E641&VLOOKUP(D641,list!$D$3:$F$501,2,FALSE)&F641&\"_\"&VLOOKUP(G641,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_TSET"},"LPAU05B02_TSET AT%M768.0 :REAL; (*P新风机组05B02-设定温度值*)","LPAU05B02_TSET          AT%M768.0      :REAL; (*P新风机组05B02-设定温度值*)"]
["772.0","验证通过","INT","P新风机组","L","05B02","季节模式","P新风机组05B02-季节模式",{"$f":"E642&VLOOKUP(D642,list!$D$3:$F$501,2,FALSE)&F642&\"_\"&VLOOKUP(G642,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_SM"},"LPAU05B02_SM AT%M772.0 :INT; (*P新风机组05B02-季节模式*)","LPAU05B02_SM            AT%M772.0      :INT; (*P新风机组05B02-季节模式*)"]
["776.0","验证通过","REAL","P新风机组","L","05B02","水阀反馈换算值","P新风机组05B02-水阀反馈换算值",{"$f":"E643&VLOOKUP(D643,list!$D$3:$F$501,2,FALSE)&F643&\"_\"&VLOOKUP(G643,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_WVBS"},"LPAU05B02_WVBS AT%M776.0 :REAL; (*P新风机组05B02-水阀反馈换算值*)","LPAU05B02_WVBS          AT%M776.0      :REAL; (*P新风机组05B02-水阀反馈换算值*)"]
["780.0","验证通过","BOOL","P新风机组","L","05B02","水阀手动控制","P新风机组05B02-水阀手动控制",{"$f":"E644&VLOOKUP(D644,list!$D$3:$F$501,2,FALSE)&F644&\"_\"&VLOOKUP(G644,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_WVMC"},"LPAU05B02_WVMC AT%M780.0 :BOOL; (*P新风机组05B02-水阀手动控制*)","LPAU05B02_WVMC          AT%M780.0      :BOOL; (*P新风机组05B02-水阀手动控制*)"]
["784.0","验证通过","REAL","P新风机组","L","05B02","水阀手动控制值","P新风机组05B02-水阀手动控制值",{"$f":"E645&VLOOKUP(D645,list!$D$3:$F$501,2,FALSE)&F645&\"_\"&VLOOKUP(G645,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_WVMV"},"LPAU05B02_WVMV AT%M784.0 :REAL; (*P新风机组05B02-水阀手动控制值*)","LPAU05B02_WVMV          AT%M784.0      :REAL; (*P新风机组05B02-水阀手动控制值*)"]
["788.0","验证通过","REAL","P新风机组","L","05B02","送风温度换算值","P新风机组05B02-送风温度换算值",{"$f":"E646&VLOOKUP(D646,list!$D$3:$F$501,2,FALSE)&F646&\"_\"&VLOOKUP(G646,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_STS"},"LPAU05B02_STS AT%M788.0 :REAL; (*P新风机组05B02-送风温度换算值*)","LPAU05B02_STS           AT%M788.0      :REAL; (*P新风机组05B02-送风温度换算值*)"]
["792.0","验证通过","BOOL","P新风机组","L","05B02","运行时间累积重置","P新风机组05B02-运行时间累积重置",{"$f":"E647&VLOOKUP(D647,list!$D$3:$F$501,2,FALSE)&F647&\"_\"&VLOOKUP(G647,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_RST"},"LPAU05B02_RST AT%M792.0 :BOOL; (*P新风机组05B02-运行时间累积重置*)","LPAU05B02_RST           AT%M792.0      :BOOL; (*P新风机组05B02-运行时间累积重置*)"]
["796.0","验证通过","REAL","P新风机组","L","05B02","运行时间累积重置值","P新风机组05B02-运行时间累积重置值",{"$f":"E648&VLOOKUP(D648,list!$D$3:$F$501,2,FALSE)&F648&\"_\"&VLOOKUP(G648,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_RSTV"},"LPAU05B02_RSTV AT%M796.0 :REAL; (*P新风机组05B02-运行时间累积重置值*)","LPAU05B02_RSTV          AT%M796.0      :REAL; (*P新风机组05B02-运行时间累积重置值*)"]
["800.0","验证通过","BOOL","P新风机组","L","05B02","隔离开关1","P新风机组05B02-隔离开关1",{"$f":"E649&VLOOKUP(D649,list!$D$3:$F$501,2,FALSE)&F649&\"_\"&VLOOKUP(G649,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_ISO1"},"LPAU05B02_ISO1 AT%M800.0 :BOOL; (*P新风机组05B02-隔离开关1*)","LPAU05B02_ISO1          AT%M800.0      :BOOL; (*P新风机组05B02-隔离开关1*)"]
["802.0","验证通过","BOOL","P新风机组","L","05B02","隔离开关2","P新风机组05B02-隔离开关2",{"$f":"E650&VLOOKUP(D650,list!$D$3:$F$501,2,FALSE)&F650&\"_\"&VLOOKUP(G650,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_ISO2"},"LPAU05B02_ISO2 AT%M802.0 :BOOL; (*P新风机组05B02-隔离开关2*)","LPAU05B02_ISO2          AT%M802.0      :BOOL; (*P新风机组05B02-隔离开关2*)"]
["808.0","验证通过","REAL","P新风机组","L","05B02","P调节参数","P新风机组05B02-P调节参数",{"$f":"E651&VLOOKUP(D651,list!$D$3:$F$501,2,FALSE)&F651&\"_\"&VLOOKUP(G651,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_VP"},"LPAU05B02_VP AT%M808.0 :REAL; (*P新风机组05B02-P调节参数*)","LPAU05B02_VP            AT%M808.0      :REAL; (*P新风机组05B02-P调节参数*)"]
["812.0","验证通过","REAL","P新风机组","L","05B02","I调节参数","P新风机组05B02-I调节参数",{"$f":"E652&VLOOKUP(D652,list!$D$3:$F$501,2,FALSE)&F652&\"_\"&VLOOKUP(G652,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_VI"},"LPAU05B02_VI AT%M812.0 :REAL; (*P新风机组05B02-I调节参数*)","LPAU05B02_VI            AT%M812.0      :REAL; (*P新风机组05B02-I调节参数*)"]
["816.0","验证通过","REAL","P新风机组","L","05B02","运行时间累积值","P新风机组05B02-运行时间累积值",{"$f":"E653&VLOOKUP(D653,list!$D$3:$F$501,2,FALSE)&F653&\"_\"&VLOOKUP(G653,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_RH"},"LPAU05B02_RH AT%M816.0 :REAL; (*P新风机组05B02-运行时间累积值*)","LPAU05B02_RH            AT%M816.0      :REAL; (*P新风机组05B02-运行时间累积值*)"]
["820.0","验证通过","INT","P新风机组","L","05B02","设备状态代码","P新风机组05B02-设备状态代码",{"$f":"E654&VLOOKUP(D654,list!$D$3:$F$501,2,FALSE)&F654&\"_\"&VLOOKUP(G654,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_SN"},"LPAU05B02_SN AT%M820.0 :INT; (*P新风机组05B02-设备状态代码*)","LPAU05B02_SN            AT%M820.0      :INT; (*P新风机组05B02-设备状态代码*)"]
["822.0","验证通过","INT","P新风机组","L","05B02","水阀控制转换值","P新风机组05B02-水阀控制转换值",{"$f":"E655&VLOOKUP(D655,list!$D$3:$F$501,2,FALSE)&F655&\"_\"&VLOOKUP(G655,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_WVCS"},"LPAU05B02_WVCS AT%M822.0 :INT; (*P新风机组05B02-水阀控制转换值*)","LPAU05B02_WVCS          AT%M822.0      :INT; (*P新风机组05B02-水阀控制转换值*)"]
["824.0","验证通过","BOOL","P新风机组","L","05B02","程序控制","P新风机组05B02-程序控制",{"$f":"E656&VLOOKUP(D656,list!$D$3:$F$501,2,FALSE)&F656&\"_\"&VLOOKUP(G656,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_PC"},"LPAU05B02_PC AT%M824.0 :BOOL; (*P新风机组05B02-程序控制*)","LPAU05B02_PC            AT%M824.0      :BOOL; (*P新风机组05B02-程序控制*)"]
["826.0","验证通过","INT","P新风机组","L","05B02","变频手动控制值","P新风机组05B02-变频手动控制值",{"$f":"E657&VLOOKUP(D657,list!$D$3:$F$501,2,FALSE)&F657&\"_\"&VLOOKUP(G657,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_VFMV"},"LPAU05B02_VFMV AT%M826.0 :INT; (*P新风机组05B02-变频手动控制值*)","LPAU05B02_VFMV          AT%M826.0      :INT; (*P新风机组05B02-变频手动控制值*)"]
["828.0","验证通过","BOOL","P新风机组","L","05B02","低温断路报警隔离","P新风机组05B02-低温断路报警隔离",{"$f":"E658&VLOOKUP(D658,list!$D$3:$F$501,2,FALSE)&F658&\"_\"&VLOOKUP(G658,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_ISO3"},"LPAU05B02_ISO3 AT%M828.0 :BOOL; (*P新风机组05B02-低温断路报警隔离*)","LPAU05B02_ISO3          AT%M828.0      :BOOL; (*P新风机组05B02-低温断路报警隔离*)"]
["830.0","验证通过","INT","P新风机组","L","05B02","变频器频率控制值","P新风机组05B02-变频器频率控制值",{"$f":"E659&VLOOKUP(D659,list!$D$3:$F$501,2,FALSE)&F659&\"_\"&VLOOKUP(G659,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_VFCS"},"LPAU05B02_VFCS AT%M830.0 :INT; (*P新风机组05B02-变频器频率控制值*)","LPAU05B02_VFCS          AT%M830.0      :INT; (*P新风机组05B02-变频器频率控制值*)"]
["832.0","验证通过","INT","P新风机组","L","05B02","变频器频率反馈值","P新风机组05B02-变频器频率反馈值",{"$f":"E660&VLOOKUP(D660,list!$D$3:$F$501,2,FALSE)&F660&\"_\"&VLOOKUP(G660,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_VFBS"},"LPAU05B02_VFBS AT%M832.0 :INT; (*P新风机组05B02-变频器频率反馈值*)","LPAU05B02_VFBS          AT%M832.0      :INT; (*P新风机组05B02-变频器频率反馈值*)"]
["834.0","验证通过","BOOL","P新风机组","L","05B02","联动模式","P新风机组05B02-联动模式",{"$f":"E661&VLOOKUP(D661,list!$D$3:$F$501,2,FALSE)&F661&\"_\"&VLOOKUP(G661,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_LM"},"LPAU05B02_LM AT%M834.0 :BOOL; (*P新风机组05B02-联动模式*)","LPAU05B02_LM            AT%M834.0      :BOOL; (*P新风机组05B02-联动模式*)"]
["836.0","验证通过","BOOL","P新风机组","L","05B02","全天候模式","P新风机组05B02-全天候模式",{"$f":"E662&VLOOKUP(D662,list!$D$3:$F$501,2,FALSE)&F662&\"_\"&VLOOKUP(G662,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_DM"},"LPAU05B02_DM AT%M836.0 :BOOL; (*P新风机组05B02-全天候模式*)","LPAU05B02_DM            AT%M836.0      :BOOL; (*P新风机组05B02-全天候模式*)"]
["840.0","验证通过","REAL","P新风机组","L","05B02","CO2设定值","P新风机组05B02-CO2设定值",{"$f":"E663&VLOOKUP(D663,list!$D$3:$F$501,2,FALSE)&F663&\"_\"&VLOOKUP(G663,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_CO2SET"},"LPAU05B02_CO2SET AT%M840.0 :REAL; (*P新风机组05B02-CO2设定值*)","LPAU05B02_CO2SET        AT%M840.0      :REAL; (*P新风机组05B02-CO2设定值*)"]
["844.0","验证通过","BOOL","P新风机组","L","05B02","定时控制","P新风机组05B02-定时控制",{"$f":"E664&VLOOKUP(D664,list!$D$3:$F$501,2,FALSE)&F664&\"_\"&VLOOKUP(G664,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_TC"},"LPAU05B02_TC AT%M844.0 :BOOL; (*P新风机组05B02-定时控制*)","LPAU05B02_TC            AT%M844.0      :BOOL; (*P新风机组05B02-定时控制*)"]
["846.0","验证通过","BOOL","P新风机组","L","05B02","定时模式","P新风机组05B02-定时模式",{"$f":"E665&VLOOKUP(D665,list!$D$3:$F$501,2,FALSE)&F665&\"_\"&VLOOKUP(G665,list!$I$2:$K$502,2,FALSE)","v":"LPAU05B02_TM"},"LPAU05B02_TM AT%M846.0 :BOOL; (*P新风机组05B02-定时模式*)","LPAU05B02_TM            AT%M846.0      :BOOL; (*P新风机组05B02-定时模式*)"]
["EAF"]
[{"$f":"IF(OR(#REF!=\"REAL\",#REF!=\"DWORD\",#REF!=\"DINT\"),(IF(OR(C667=\"REAL\",C667=\"DWORD\",C667=\"DINT\"),#REF!+4+MOD(#REF!,4),#REF!+4)),(IF(OR(C667=\"REAL\",C667=\"DWORD\",C667=\"DINT\"),#REF!+4+MOD(#REF!,4),#REF!+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C667=\"INT\",C667=\"WORD\",C667=\"BOOL\"),MOD(A667,2),MOD(A667,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"BOOL","排风机","R","04F01","启停控制",{"$f":"D667&F667&\"-\"&IF(E667=\"R\",\"新云平台\"&G667,G667)","v":"排风机04F01-新云平台启停控制"},{"$f":"E667&VLOOKUP(D667,[1]list!$D$3:$F$501,2,FALSE)&F667&\"_\"&VLOOKUP(G667,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04F01_C"},{"$f":"I667&\" \"&\"AT%M\"&A667&\" \"&\":\"&C667&\";\"&\" \"&\"(*\"&H667&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J667,SEARCH(\"AT%\",J667),,REPT(\" \",25-SEARCH(\"AT%\",J667))),SEARCH(\":\",REPLACE(J667,SEARCH(\"AT%\",J667),,REPT(\" \",25-SEARCH(\"AT%\",J667)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J667,SEARCH(\"AT%\",J667),,REPT(\" \",25-SEARCH(\"AT%\",J667))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C667=\"REAL\",C667=\"DWORD\",C667=\"DINT\"),(IF(OR(C668=\"REAL\",C668=\"DWORD\",C668=\"DINT\"),A667+4+MOD(A667,4),A667+4)),(IF(OR(C668=\"REAL\",C668=\"DWORD\",C668=\"DINT\"),A667+4+MOD(A667,4),A667+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"BOOL","排风机","L","04F01","运行时间累积重置","排风机04F01-运行时间累积重置",{"$f":"E668&VLOOKUP(D668,[1]list!$D$3:$F$501,2,FALSE)&F668&\"_\"&VLOOKUP(G668,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04F01_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","排风机","L","04F01","运行时间累积重置值","排风机04F01-运行时间累积重置值",{"$f":"E669&VLOOKUP(D669,[1]list!$D$3:$F$501,2,FALSE)&F669&\"_\"&VLOOKUP(G669,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04F01_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","排风机","L","04F01","运行时间累积值","排风机04F01-运行时间累积值",{"$f":"E670&VLOOKUP(D670,[1]list!$D$3:$F$501,2,FALSE)&F670&\"_\"&VLOOKUP(G670,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04F01_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","排风机","L","04F01","定时模式","排风机04F01-定时模式",{"$f":"E671&VLOOKUP(D671,[1]list!$D$3:$F$501,2,FALSE)&F671&\"_\"&VLOOKUP(G671,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04F01_TM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","排风机","L","04F01","定时控制","排风机04F01-定时控制",{"$f":"E672&VLOOKUP(D672,[1]list!$D$3:$F$501,2,FALSE)&F672&\"_\"&VLOOKUP(G672,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04F01_TC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","排风机","L","04F01","全天候模式","排风机04F01-全天候模式",{"$f":"E673&VLOOKUP(D673,[1]list!$D$3:$F$501,2,FALSE)&F673&\"_\"&VLOOKUP(G673,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04F01_DM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","排风机","L","04F01","CO设定值","排风机04F01-CO设定值",{"$f":"E674&VLOOKUP(D674,[1]list!$D$3:$F$501,2,FALSE)&F674&\"_\"&VLOOKUP(G674,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04F01_COSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","排烟机","L","04F01","设定温度值","排烟机04F01-设定温度值",{"$f":"E675&VLOOKUP(D675,[1]list!$D$3:$F$501,2,FALSE)&F675&\"_\"&VLOOKUP(G675,[1]list!$I$2:$K$502,2,FALSE)","v":"LESF04F01_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
["FCU"]
[{"$f":"IF(OR(C675=\"REAL\",C675=\"DWORD\",C675=\"DINT\"),(IF(OR(C677=\"REAL\",C677=\"DWORD\",C677=\"DINT\"),A675+4+MOD(A675,4),A675+4)),(IF(OR(C677=\"REAL\",C677=\"DWORD\",C677=\"DINT\"),A675+4+MOD(A675,4),A675+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C677=\"INT\",C677=\"WORD\",C677=\"BOOL\"),MOD(A677,2),MOD(A677,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","风机盘管","R","04F01","设定温度值",{"$f":"D677&F677&\"-\"&IF(E677=\"R\",\"新云平台\"&G677,G677)","v":"风机盘管04F01-新云平台设定温度值"},{"$f":"E677&VLOOKUP(D677,list!$D$3:$F$501,2,FALSE)&F677&\"_\"&VLOOKUP(G677,list!$I$2:$K$502,2,FALSE)","v":"RFCU04F01_TSET"},{"$f":"I677&\" \"&\"AT%M\"&A677&\" \"&\":\"&C677&\";\"&\" \"&\"(*\"&H677&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J677,SEARCH(\"AT%\",J677),,REPT(\" \",25-SEARCH(\"AT%\",J677))),SEARCH(\":\",REPLACE(J677,SEARCH(\"AT%\",J677),,REPT(\" \",25-SEARCH(\"AT%\",J677)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J677,SEARCH(\"AT%\",J677),,REPT(\" \",25-SEARCH(\"AT%\",J677))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C677=\"REAL\",C677=\"DWORD\",C677=\"DINT\"),(IF(OR(C678=\"REAL\",C678=\"DWORD\",C678=\"DINT\"),A677+4+MOD(A677,4),A677+4)),(IF(OR(C678=\"REAL\",C678=\"DWORD\",C678=\"DINT\"),A677+4+MOD(A677,4),A677+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","风机盘管","R",{"$f":"F677","v":"04F01"},"季节模式","风机盘管04F01-新云平台季节模式",{"$f":"E678&VLOOKUP(D678,list!$D$3:$F$501,2,FALSE)&F678&\"_\"&VLOOKUP(G678,list!$I$2:$K$502,2,FALSE)","v":"RFCU04F01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","R","04F01","程序控制","风机盘管04F01-新云平台程序控制",{"$f":"E679&VLOOKUP(D679,list!$D$3:$F$501,2,FALSE)&F679&\"_\"&VLOOKUP(G679,list!$I$2:$K$502,2,FALSE)","v":"RFCU04F01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","04F01","设定温度值","风机盘管04F01-设定温度值",{"$f":"E680&VLOOKUP(D680,list!$D$3:$F$501,2,FALSE)&F680&\"_\"&VLOOKUP(G680,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","04F01","季节模式","风机盘管04F01-季节模式",{"$f":"E681&VLOOKUP(D681,list!$D$3:$F$501,2,FALSE)&F681&\"_\"&VLOOKUP(G681,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","04F01","温度换算值","风机盘管04F01-温度换算值",{"$f":"E682&VLOOKUP(D682,list!$D$3:$F$501,2,FALSE)&F682&\"_\"&VLOOKUP(G682,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_TS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","04F01","电磁阀手动控制","风机盘管04F01-电磁阀手动控制",{"$f":"E683&VLOOKUP(D683,list!$D$3:$F$501,2,FALSE)&F683&\"_\"&VLOOKUP(G683,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_EVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","04F01","电磁阀手动控制值","风机盘管04F01-电磁阀手动控制值",{"$f":"E684&VLOOKUP(D684,list!$D$3:$F$501,2,FALSE)&F684&\"_\"&VLOOKUP(G684,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_EVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","04F01","回风温度换算值","风机盘管04F01-回风温度换算值",{"$f":"E685&VLOOKUP(D685,list!$D$3:$F$501,2,FALSE)&F685&\"_\"&VLOOKUP(G685,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RTS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","04F01","运行时间累积重置","风机盘管04F01-运行时间累积重置",{"$f":"E686&VLOOKUP(D686,list!$D$3:$F$501,2,FALSE)&F686&\"_\"&VLOOKUP(G686,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","04F01","运行时间累积重置值","风机盘管04F01-运行时间累积重置值",{"$f":"E687&VLOOKUP(D687,list!$D$3:$F$501,2,FALSE)&F687&\"_\"&VLOOKUP(G687,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","04F01","隔离开关1","风机盘管04F01-隔离开关1",{"$f":"E688&VLOOKUP(D688,list!$D$3:$F$501,2,FALSE)&F688&\"_\"&VLOOKUP(G688,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","04F01","运行时间累积值","风机盘管04F01-运行时间累积值",{"$f":"E689&VLOOKUP(D689,list!$D$3:$F$501,2,FALSE)&F689&\"_\"&VLOOKUP(G689,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","04F01","设备状态代码","风机盘管04F01-设备状态代码",{"$f":"E690&VLOOKUP(D690,list!$D$3:$F$501,2,FALSE)&F690&\"_\"&VLOOKUP(G690,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","04F01","水阀控制转换值","风机盘管04F01-水阀控制转换值",{"$f":"E691&VLOOKUP(D691,list!$D$3:$F$501,2,FALSE)&F691&\"_\"&VLOOKUP(G691,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","04F01","程序控制","风机盘管04F01-程序控制",{"$f":"E692&VLOOKUP(D692,list!$D$3:$F$501,2,FALSE)&F692&\"_\"&VLOOKUP(G692,list!$I$2:$K$502,2,FALSE)","v":"LFCU04F01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
["PAU"]
[{"$f":"IF(OR(C692=\"REAL\",C692=\"DWORD\",C692=\"DINT\"),(IF(OR(C694=\"REAL\",C694=\"DWORD\",C694=\"DINT\"),A692+4+MOD(A692,4),A692+4)),(IF(OR(C694=\"REAL\",C694=\"DWORD\",C694=\"DINT\"),A692+4+MOD(A692,4),A692+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C694=\"INT\",C694=\"WORD\",C694=\"BOOL\"),MOD(A694,2),MOD(A694,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","P新风机组","R","05A01","设定温度值",{"$f":"D694&F694&\"-\"&IF(E694=\"R\",\"新云平台\"&G694,G694)","v":"P新风机组05A01-新云平台设定温度值"},{"$f":"E694&VLOOKUP(D694,list!$D$3:$F$501,2,FALSE)&F694&\"_\"&VLOOKUP(G694,list!$I$2:$K$502,2,FALSE)","v":"RPAU05A01_TSET"},{"$f":"I694&\" \"&\"AT%M\"&A694&\" \"&\":\"&C694&\";\"&\" \"&\"(*\"&H694&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J694,SEARCH(\"AT%\",J694),,REPT(\" \",25-SEARCH(\"AT%\",J694))),SEARCH(\":\",REPLACE(J694,SEARCH(\"AT%\",J694),,REPT(\" \",25-SEARCH(\"AT%\",J694)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J694,SEARCH(\"AT%\",J694),,REPT(\" \",25-SEARCH(\"AT%\",J694))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C694=\"REAL\",C694=\"DWORD\",C694=\"DINT\"),(IF(OR(C695=\"REAL\",C695=\"DWORD\",C695=\"DINT\"),A694+4+MOD(A694,4),A694+4)),(IF(OR(C695=\"REAL\",C695=\"DWORD\",C695=\"DINT\"),A694+4+MOD(A694,4),A694+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","P新风机组","R",{"$f":"F694","v":"05A01"},"季节模式","P新风机组05A01-新云平台季节模式",{"$f":"E695&VLOOKUP(D695,list!$D$3:$F$501,2,FALSE)&F695&\"_\"&VLOOKUP(G695,list!$I$2:$K$502,2,FALSE)","v":"RPAU05A01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","R","05A01","程序控制","P新风机组05A01-新云平台程序控制",{"$f":"E696&VLOOKUP(D696,list!$D$3:$F$501,2,FALSE)&F696&\"_\"&VLOOKUP(G696,list!$I$2:$K$502,2,FALSE)","v":"RPAU05A01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","设定温度值","P新风机组05A01-设定温度值",{"$f":"E697&VLOOKUP(D697,list!$D$3:$F$501,2,FALSE)&F697&\"_\"&VLOOKUP(G697,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","05A01","季节模式","P新风机组05A01-季节模式",{"$f":"E698&VLOOKUP(D698,list!$D$3:$F$501,2,FALSE)&F698&\"_\"&VLOOKUP(G698,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","水阀反馈换算值","P新风机组05A01-水阀反馈换算值",{"$f":"E699&VLOOKUP(D699,list!$D$3:$F$501,2,FALSE)&F699&\"_\"&VLOOKUP(G699,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","水阀手动控制","P新风机组05A01-水阀手动控制",{"$f":"E700&VLOOKUP(D700,list!$D$3:$F$501,2,FALSE)&F700&\"_\"&VLOOKUP(G700,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","水阀手动控制值","P新风机组05A01-水阀手动控制值",{"$f":"E701&VLOOKUP(D701,list!$D$3:$F$501,2,FALSE)&F701&\"_\"&VLOOKUP(G701,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","送风温度换算值","P新风机组05A01-送风温度换算值",{"$f":"E702&VLOOKUP(D702,list!$D$3:$F$501,2,FALSE)&F702&\"_\"&VLOOKUP(G702,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_STS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","运行时间累积重置","P新风机组05A01-运行时间累积重置",{"$f":"E703&VLOOKUP(D703,list!$D$3:$F$501,2,FALSE)&F703&\"_\"&VLOOKUP(G703,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","运行时间累积重置值","P新风机组05A01-运行时间累积重置值",{"$f":"E704&VLOOKUP(D704,list!$D$3:$F$501,2,FALSE)&F704&\"_\"&VLOOKUP(G704,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","隔离开关1","P新风机组05A01-隔离开关1",{"$f":"E705&VLOOKUP(D705,list!$D$3:$F$501,2,FALSE)&F705&\"_\"&VLOOKUP(G705,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","隔离开关2","P新风机组05A01-隔离开关2",{"$f":"E706&VLOOKUP(D706,list!$D$3:$F$501,2,FALSE)&F706&\"_\"&VLOOKUP(G706,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_ISO2"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","P调节参数","P新风机组05A01-P调节参数",{"$f":"E707&VLOOKUP(D707,list!$D$3:$F$501,2,FALSE)&F707&\"_\"&VLOOKUP(G707,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VP"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","I调节参数","P新风机组05A01-I调节参数",{"$f":"E708&VLOOKUP(D708,list!$D$3:$F$501,2,FALSE)&F708&\"_\"&VLOOKUP(G708,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VI"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","运行时间累积值","P新风机组05A01-运行时间累积值",{"$f":"E709&VLOOKUP(D709,list!$D$3:$F$501,2,FALSE)&F709&\"_\"&VLOOKUP(G709,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","05A01","设备状态代码","P新风机组05A01-设备状态代码",{"$f":"E710&VLOOKUP(D710,list!$D$3:$F$501,2,FALSE)&F710&\"_\"&VLOOKUP(G710,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","05A01","水阀控制转换值","P新风机组05A01-水阀控制转换值",{"$f":"E711&VLOOKUP(D711,list!$D$3:$F$501,2,FALSE)&F711&\"_\"&VLOOKUP(G711,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","程序控制","P新风机组05A01-程序控制",{"$f":"E712&VLOOKUP(D712,list!$D$3:$F$501,2,FALSE)&F712&\"_\"&VLOOKUP(G712,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","05A01","变频手动控制值","P新风机组05A01-变频手动控制值",{"$f":"E713&VLOOKUP(D713,list!$D$3:$F$501,2,FALSE)&F713&\"_\"&VLOOKUP(G713,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VFMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","低温断路报警隔离","P新风机组05A01-低温断路报警隔离",{"$f":"E714&VLOOKUP(D714,list!$D$3:$F$501,2,FALSE)&F714&\"_\"&VLOOKUP(G714,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_ISO3"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","05A01","变频器频率控制值","P新风机组05A01-变频器频率控制值",{"$f":"E715&VLOOKUP(D715,list!$D$3:$F$501,2,FALSE)&F715&\"_\"&VLOOKUP(G715,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VFCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","05A01","变频器频率反馈值","P新风机组05A01-变频器频率反馈值",{"$f":"E716&VLOOKUP(D716,list!$D$3:$F$501,2,FALSE)&F716&\"_\"&VLOOKUP(G716,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_VFBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","联动模式","P新风机组05A01-联动模式",{"$f":"E717&VLOOKUP(D717,list!$D$3:$F$501,2,FALSE)&F717&\"_\"&VLOOKUP(G717,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_LM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","全天候模式","P新风机组05A01-全天候模式",{"$f":"E718&VLOOKUP(D718,list!$D$3:$F$501,2,FALSE)&F718&\"_\"&VLOOKUP(G718,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_DM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","05A01","CO2设定值","P新风机组05A01-CO2设定值",{"$f":"E719&VLOOKUP(D719,list!$D$3:$F$501,2,FALSE)&F719&\"_\"&VLOOKUP(G719,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_CO2SET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","定时控制","P新风机组05A01-定时控制",{"$f":"E720&VLOOKUP(D720,list!$D$3:$F$501,2,FALSE)&F720&\"_\"&VLOOKUP(G720,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_TC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","05A01","定时模式","P新风机组05A01-定时模式",{"$f":"E721&VLOOKUP(D721,list!$D$3:$F$501,2,FALSE)&F721&\"_\"&VLOOKUP(G721,list!$I$2:$K$502,2,FALSE)","v":"LPAU05A01_TM"},{"$error":"#REF!"},{"$error":"#REF!"}]
["PAU"]
[{"$f":"IF(OR(C721=\"REAL\",C721=\"DWORD\",C721=\"DINT\"),(IF(OR(C723=\"REAL\",C723=\"DWORD\",C723=\"DINT\"),A721+4+MOD(A721,4),A721+4)),(IF(OR(C723=\"REAL\",C723=\"DWORD\",C723=\"DINT\"),A721+4+MOD(A721,4),A721+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C723=\"INT\",C723=\"WORD\",C723=\"BOOL\"),MOD(A723,2),MOD(A723,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","P新风机组","R","06A01","设定温度值",{"$f":"D723&F723&\"-\"&IF(E723=\"R\",\"新云平台\"&G723,G723)","v":"P新风机组06A01-新云平台设定温度值"},{"$f":"E723&VLOOKUP(D723,list!$D$3:$F$501,2,FALSE)&F723&\"_\"&VLOOKUP(G723,list!$I$2:$K$502,2,FALSE)","v":"RPAU06A01_TSET"},{"$f":"I723&\" \"&\"AT%M\"&A723&\" \"&\":\"&C723&\";\"&\" \"&\"(*\"&H723&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J723,SEARCH(\"AT%\",J723),,REPT(\" \",25-SEARCH(\"AT%\",J723))),SEARCH(\":\",REPLACE(J723,SEARCH(\"AT%\",J723),,REPT(\" \",25-SEARCH(\"AT%\",J723)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J723,SEARCH(\"AT%\",J723),,REPT(\" \",25-SEARCH(\"AT%\",J723))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C723=\"REAL\",C723=\"DWORD\",C723=\"DINT\"),(IF(OR(C724=\"REAL\",C724=\"DWORD\",C724=\"DINT\"),A723+4+MOD(A723,4),A723+4)),(IF(OR(C724=\"REAL\",C724=\"DWORD\",C724=\"DINT\"),A723+4+MOD(A723,4),A723+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","P新风机组","R",{"$f":"F723","v":"06A01"},"季节模式","P新风机组06A01-新云平台季节模式",{"$f":"E724&VLOOKUP(D724,list!$D$3:$F$501,2,FALSE)&F724&\"_\"&VLOOKUP(G724,list!$I$2:$K$502,2,FALSE)","v":"RPAU06A01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","R","06A01","程序控制","P新风机组06A01-新云平台程序控制",{"$f":"E725&VLOOKUP(D725,list!$D$3:$F$501,2,FALSE)&F725&\"_\"&VLOOKUP(G725,list!$I$2:$K$502,2,FALSE)","v":"RPAU06A01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","设定温度值","P新风机组06A01-设定温度值",{"$f":"E726&VLOOKUP(D726,list!$D$3:$F$501,2,FALSE)&F726&\"_\"&VLOOKUP(G726,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","06A01","季节模式","P新风机组06A01-季节模式",{"$f":"E727&VLOOKUP(D727,list!$D$3:$F$501,2,FALSE)&F727&\"_\"&VLOOKUP(G727,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","水阀反馈换算值","P新风机组06A01-水阀反馈换算值",{"$f":"E728&VLOOKUP(D728,list!$D$3:$F$501,2,FALSE)&F728&\"_\"&VLOOKUP(G728,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","水阀手动控制","P新风机组06A01-水阀手动控制",{"$f":"E729&VLOOKUP(D729,list!$D$3:$F$501,2,FALSE)&F729&\"_\"&VLOOKUP(G729,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","水阀手动控制值","P新风机组06A01-水阀手动控制值",{"$f":"E730&VLOOKUP(D730,list!$D$3:$F$501,2,FALSE)&F730&\"_\"&VLOOKUP(G730,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","送风温度换算值","P新风机组06A01-送风温度换算值",{"$f":"E731&VLOOKUP(D731,list!$D$3:$F$501,2,FALSE)&F731&\"_\"&VLOOKUP(G731,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_STS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","运行时间累积重置","P新风机组06A01-运行时间累积重置",{"$f":"E732&VLOOKUP(D732,list!$D$3:$F$501,2,FALSE)&F732&\"_\"&VLOOKUP(G732,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","运行时间累积重置值","P新风机组06A01-运行时间累积重置值",{"$f":"E733&VLOOKUP(D733,list!$D$3:$F$501,2,FALSE)&F733&\"_\"&VLOOKUP(G733,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","隔离开关1","P新风机组06A01-隔离开关1",{"$f":"E734&VLOOKUP(D734,list!$D$3:$F$501,2,FALSE)&F734&\"_\"&VLOOKUP(G734,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","隔离开关2","P新风机组06A01-隔离开关2",{"$f":"E735&VLOOKUP(D735,list!$D$3:$F$501,2,FALSE)&F735&\"_\"&VLOOKUP(G735,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_ISO2"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","P调节参数","P新风机组06A01-P调节参数",{"$f":"E736&VLOOKUP(D736,list!$D$3:$F$501,2,FALSE)&F736&\"_\"&VLOOKUP(G736,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VP"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","I调节参数","P新风机组06A01-I调节参数",{"$f":"E737&VLOOKUP(D737,list!$D$3:$F$501,2,FALSE)&F737&\"_\"&VLOOKUP(G737,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VI"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","运行时间累积值","P新风机组06A01-运行时间累积值",{"$f":"E738&VLOOKUP(D738,list!$D$3:$F$501,2,FALSE)&F738&\"_\"&VLOOKUP(G738,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","06A01","设备状态代码","P新风机组06A01-设备状态代码",{"$f":"E739&VLOOKUP(D739,list!$D$3:$F$501,2,FALSE)&F739&\"_\"&VLOOKUP(G739,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","06A01","水阀控制转换值","P新风机组06A01-水阀控制转换值",{"$f":"E740&VLOOKUP(D740,list!$D$3:$F$501,2,FALSE)&F740&\"_\"&VLOOKUP(G740,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","程序控制","P新风机组06A01-程序控制",{"$f":"E741&VLOOKUP(D741,list!$D$3:$F$501,2,FALSE)&F741&\"_\"&VLOOKUP(G741,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","06A01","变频手动控制值","P新风机组06A01-变频手动控制值",{"$f":"E742&VLOOKUP(D742,list!$D$3:$F$501,2,FALSE)&F742&\"_\"&VLOOKUP(G742,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VFMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","低温断路报警隔离","P新风机组06A01-低温断路报警隔离",{"$f":"E743&VLOOKUP(D743,list!$D$3:$F$501,2,FALSE)&F743&\"_\"&VLOOKUP(G743,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_ISO3"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","06A01","变频器频率控制值","P新风机组06A01-变频器频率控制值",{"$f":"E744&VLOOKUP(D744,list!$D$3:$F$501,2,FALSE)&F744&\"_\"&VLOOKUP(G744,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VFCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","P新风机组","L","06A01","变频器频率反馈值","P新风机组06A01-变频器频率反馈值",{"$f":"E745&VLOOKUP(D745,list!$D$3:$F$501,2,FALSE)&F745&\"_\"&VLOOKUP(G745,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_VFBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","联动模式","P新风机组06A01-联动模式",{"$f":"E746&VLOOKUP(D746,list!$D$3:$F$501,2,FALSE)&F746&\"_\"&VLOOKUP(G746,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_LM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","全天候模式","P新风机组06A01-全天候模式",{"$f":"E747&VLOOKUP(D747,list!$D$3:$F$501,2,FALSE)&F747&\"_\"&VLOOKUP(G747,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_DM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","P新风机组","L","06A01","CO2设定值","P新风机组06A01-CO2设定值",{"$f":"E748&VLOOKUP(D748,list!$D$3:$F$501,2,FALSE)&F748&\"_\"&VLOOKUP(G748,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_CO2SET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","定时控制","P新风机组06A01-定时控制",{"$f":"E749&VLOOKUP(D749,list!$D$3:$F$501,2,FALSE)&F749&\"_\"&VLOOKUP(G749,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_TC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","P新风机组","L","06A01","定时模式","P新风机组06A01-定时模式",{"$f":"E750&VLOOKUP(D750,list!$D$3:$F$501,2,FALSE)&F750&\"_\"&VLOOKUP(G750,list!$I$2:$K$502,2,FALSE)","v":"LPAU06A01_TM"},{"$error":"#REF!"},{"$error":"#REF!"}]
["FCU"]
[1104,{"$f":"IF((IF(OR(C752=\"INT\",C752=\"WORD\",C752=\"BOOL\"),MOD(A752,2),MOD(A752,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","04B01","设定温度值",{"$f":"D752&F752&\"-\"&IF(E752=\"R\",\"新云平台\"&G752,G752)","v":"风机盘管04B01-新云平台设定温度值"},{"$f":"E752&VLOOKUP(D752,list!$D$3:$F$501,2,FALSE)&F752&\"_\"&VLOOKUP(G752,list!$I$2:$K$502,2,FALSE)","v":"RFCU04B01_TSET"},{"$f":"I752&\" \"&\"AT%M\"&A752&\" \"&\":\"&C752&\";\"&\" \"&\"(*\"&H752&\"*)\"","v":"RFCU04B01_TSET AT%M1104 :REAL; (*风机盘管04B01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J752,SEARCH(\"AT%\",J752),,REPT(\" \",25-SEARCH(\"AT%\",J752))),SEARCH(\":\",REPLACE(J752,SEARCH(\"AT%\",J752),,REPT(\" \",25-SEARCH(\"AT%\",J752)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J752,SEARCH(\"AT%\",J752),,REPT(\" \",25-SEARCH(\"AT%\",J752))))))","v":"RFCU04B01_TSET          AT%M1104       :REAL; (*风机盘管04B01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C752=\"REAL\",C752=\"DWORD\",C752=\"DINT\"),(IF(OR(C753=\"REAL\",C753=\"DWORD\",C753=\"DINT\"),A752+4+MOD(A752,4),A752+4)),(IF(OR(C753=\"REAL\",C753=\"DWORD\",C753=\"DINT\"),A752+4+MOD(A752,4),A752+2)))&\".0\"","v":"1108.0"},"验证通过","INT","风机盘管","R",{"$f":"F752","v":"04B01"},"季节模式","风机盘管04B01-新云平台季节模式",{"$f":"E753&VLOOKUP(D753,list!$D$3:$F$501,2,FALSE)&F753&\"_\"&VLOOKUP(G753,list!$I$2:$K$502,2,FALSE)","v":"RFCU04B01_SM"},"RFCU04B01_SM AT%M1108.0 :INT; (*风机盘管04B01-新云平台季节模式*)","RFCU04B01_SM            AT%M1108.0     :INT; (*风机盘管04B01-新云平台季节模式*)"]
["1110.0","验证通过","BOOL","风机盘管","R","04B01","程序控制","风机盘管04B01-新云平台程序控制",{"$f":"E754&VLOOKUP(D754,list!$D$3:$F$501,2,FALSE)&F754&\"_\"&VLOOKUP(G754,list!$I$2:$K$502,2,FALSE)","v":"RFCU04B01_PC"},"RFCU04B01_PC AT%M1110.0 :BOOL; (*风机盘管04B01-新云平台程序控制*)","RFCU04B01_PC            AT%M1110.0     :BOOL; (*风机盘管04B01-新云平台程序控制*)"]
["1116.0","验证通过","REAL","风机盘管","L","04B01","设定温度值","风机盘管04B01-设定温度值",{"$f":"E755&VLOOKUP(D755,list!$D$3:$F$501,2,FALSE)&F755&\"_\"&VLOOKUP(G755,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_TSET"},"LFCU04B01_TSET AT%M1116.0 :REAL; (*风机盘管04B01-设定温度值*)","LFCU04B01_TSET          AT%M1116.0     :REAL; (*风机盘管04B01-设定温度值*)"]
["1120.0","验证通过","INT","风机盘管","L","04B01","季节模式","风机盘管04B01-季节模式",{"$f":"E756&VLOOKUP(D756,list!$D$3:$F$501,2,FALSE)&F756&\"_\"&VLOOKUP(G756,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_SM"},"LFCU04B01_SM AT%M1120.0 :INT; (*风机盘管04B01-季节模式*)","LFCU04B01_SM            AT%M1120.0     :INT; (*风机盘管04B01-季节模式*)"]
["1124.0","验证通过","REAL","风机盘管","L","04B01","温度换算值","风机盘管04B01-温度换算值",{"$f":"E757&VLOOKUP(D757,list!$D$3:$F$501,2,FALSE)&F757&\"_\"&VLOOKUP(G757,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_TS"},"LFCU04B01_TS AT%M1124.0 :REAL; (*风机盘管04B01-温度换算值*)","LFCU04B01_TS            AT%M1124.0     :REAL; (*风机盘管04B01-温度换算值*)"]
["1128.0","验证通过","BOOL","风机盘管","L","04B01","电磁阀手动控制","风机盘管04B01-电磁阀手动控制",{"$f":"E758&VLOOKUP(D758,list!$D$3:$F$501,2,FALSE)&F758&\"_\"&VLOOKUP(G758,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_EVMC"},"LFCU04B01_EVMC AT%M1128.0 :BOOL; (*风机盘管04B01-电磁阀手动控制*)","LFCU04B01_EVMC          AT%M1128.0     :BOOL; (*风机盘管04B01-电磁阀手动控制*)"]
["1130.0","验证通过","BOOL","风机盘管","L","04B01","电磁阀手动控制值","风机盘管04B01-电磁阀手动控制值",{"$f":"E759&VLOOKUP(D759,list!$D$3:$F$501,2,FALSE)&F759&\"_\"&VLOOKUP(G759,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_EVMV"},"LFCU04B01_EVMV AT%M1130.0 :BOOL; (*风机盘管04B01-电磁阀手动控制值*)","LFCU04B01_EVMV          AT%M1130.0     :BOOL; (*风机盘管04B01-电磁阀手动控制值*)"]
["1136.0","验证通过","REAL","风机盘管","L","04B01","回风温度换算值","风机盘管04B01-回风温度换算值",{"$f":"E760&VLOOKUP(D760,list!$D$3:$F$501,2,FALSE)&F760&\"_\"&VLOOKUP(G760,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_RTS"},"LFCU04B01_RTS AT%M1136.0 :REAL; (*风机盘管04B01-回风温度换算值*)","LFCU04B01_RTS           AT%M1136.0     :REAL; (*风机盘管04B01-回风温度换算值*)"]
["1140.0","验证通过","BOOL","风机盘管","L","04B01","运行时间累积重置","风机盘管04B01-运行时间累积重置",{"$f":"E761&VLOOKUP(D761,list!$D$3:$F$501,2,FALSE)&F761&\"_\"&VLOOKUP(G761,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_RST"},"LFCU04B01_RST AT%M1140.0 :BOOL; (*风机盘管04B01-运行时间累积重置*)","LFCU04B01_RST           AT%M1140.0     :BOOL; (*风机盘管04B01-运行时间累积重置*)"]
["1144.0","验证通过","REAL","风机盘管","L","04B01","运行时间累积重置值","风机盘管04B01-运行时间累积重置值",{"$f":"E762&VLOOKUP(D762,list!$D$3:$F$501,2,FALSE)&F762&\"_\"&VLOOKUP(G762,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_RSTV"},"LFCU04B01_RSTV AT%M1144.0 :REAL; (*风机盘管04B01-运行时间累积重置值*)","LFCU04B01_RSTV          AT%M1144.0     :REAL; (*风机盘管04B01-运行时间累积重置值*)"]
["1148.0","验证通过","BOOL","风机盘管","L","04B01","隔离开关1","风机盘管04B01-隔离开关1",{"$f":"E763&VLOOKUP(D763,list!$D$3:$F$501,2,FALSE)&F763&\"_\"&VLOOKUP(G763,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_ISO1"},"LFCU04B01_ISO1 AT%M1148.0 :BOOL; (*风机盘管04B01-隔离开关1*)","LFCU04B01_ISO1          AT%M1148.0     :BOOL; (*风机盘管04B01-隔离开关1*)"]
["1152.0","验证通过","REAL","风机盘管","L","04B01","运行时间累积值","风机盘管04B01-运行时间累积值",{"$f":"E764&VLOOKUP(D764,list!$D$3:$F$501,2,FALSE)&F764&\"_\"&VLOOKUP(G764,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_RH"},"LFCU04B01_RH AT%M1152.0 :REAL; (*风机盘管04B01-运行时间累积值*)","LFCU04B01_RH            AT%M1152.0     :REAL; (*风机盘管04B01-运行时间累积值*)"]
["1156.0","验证通过","INT","风机盘管","L","04B01","设备状态代码","风机盘管04B01-设备状态代码",{"$f":"E765&VLOOKUP(D765,list!$D$3:$F$501,2,FALSE)&F765&\"_\"&VLOOKUP(G765,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_SN"},"LFCU04B01_SN AT%M1156.0 :INT; (*风机盘管04B01-设备状态代码*)","LFCU04B01_SN            AT%M1156.0     :INT; (*风机盘管04B01-设备状态代码*)"]
["1158.0","验证通过","INT","风机盘管","L","04B01","水阀控制转换值","风机盘管04B01-水阀控制转换值",{"$f":"E766&VLOOKUP(D766,list!$D$3:$F$501,2,FALSE)&F766&\"_\"&VLOOKUP(G766,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_WVCS"},"LFCU04B01_WVCS AT%M1158.0 :INT; (*风机盘管04B01-水阀控制转换值*)","LFCU04B01_WVCS          AT%M1158.0     :INT; (*风机盘管04B01-水阀控制转换值*)"]
["1160.0","验证通过","BOOL","风机盘管","L","04B01","程序控制","风机盘管04B01-程序控制",{"$f":"E767&VLOOKUP(D767,list!$D$3:$F$501,2,FALSE)&F767&\"_\"&VLOOKUP(G767,list!$I$2:$K$502,2,FALSE)","v":"LFCU04B01_PC"},"LFCU04B01_PC AT%M1160.0 :BOOL; (*风机盘管04B01-程序控制*)","LFCU04B01_PC            AT%M1160.0     :BOOL; (*风机盘管04B01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C767=\"REAL\",C767=\"DWORD\",C767=\"DINT\"),(IF(OR(C769=\"REAL\",C769=\"DWORD\",C769=\"DINT\"),A767+4+MOD(A767,4),A767+4)),(IF(OR(C769=\"REAL\",C769=\"DWORD\",C769=\"DINT\"),A767+4+MOD(A767,4),A767+2)))&\".0\"","v":"1164.0"},{"$f":"IF((IF(OR(C769=\"INT\",C769=\"WORD\",C769=\"BOOL\"),MOD(A769,2),MOD(A769,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04D01","设定温度值",{"$f":"D769&F769&\"-\"&IF(E769=\"R\",\"新云平台\"&G769,G769)","v":"空调机组04D01-新云平台设定温度值"},{"$f":"E769&VLOOKUP(D769,list!$D$3:$F$501,2,FALSE)&F769&\"_\"&VLOOKUP(G769,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D01_TSET"},{"$f":"I769&\" \"&\"AT%M\"&A769&\" \"&\":\"&C769&\";\"&\" \"&\"(*\"&H769&\"*)\"","v":"RAHU04D01_TSET AT%M1164.0 :REAL; (*空调机组04D01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J769,SEARCH(\"AT%\",J769),,REPT(\" \",25-SEARCH(\"AT%\",J769))),SEARCH(\":\",REPLACE(J769,SEARCH(\"AT%\",J769),,REPT(\" \",25-SEARCH(\"AT%\",J769)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J769,SEARCH(\"AT%\",J769),,REPT(\" \",25-SEARCH(\"AT%\",J769))))))","v":"RAHU04D01_TSET          AT%M1164.0     :REAL; (*空调机组04D01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C769=\"REAL\",C769=\"DWORD\",C769=\"DINT\"),(IF(OR(C770=\"REAL\",C770=\"DWORD\",C770=\"DINT\"),A769+4+MOD(A769,4),A769+4)),(IF(OR(C770=\"REAL\",C770=\"DWORD\",C770=\"DINT\"),A769+4+MOD(A769,4),A769+2)))&\".0\"","v":"1168.0"},"验证通过","INT","空调机组","R",{"$f":"F769","v":"04D01"},"季节模式","空调机组04D01-新云平台季节模式",{"$f":"E770&VLOOKUP(D770,list!$D$3:$F$501,2,FALSE)&F770&\"_\"&VLOOKUP(G770,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D01_SM"},"RAHU04D01_SM AT%M1168.0 :INT; (*空调机组04D01-新云平台季节模式*)","RAHU04D01_SM            AT%M1168.0     :INT; (*空调机组04D01-新云平台季节模式*)"]
["1170.0","验证通过","BOOL","空调机组","R","04D01","程序控制","空调机组04D01-新云平台程序控制",{"$f":"E771&VLOOKUP(D771,list!$D$3:$F$501,2,FALSE)&F771&\"_\"&VLOOKUP(G771,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D01_PC"},"RAHU04D01_PC AT%M1170.0 :BOOL; (*空调机组04D01-新云平台程序控制*)","RAHU04D01_PC            AT%M1170.0     :BOOL; (*空调机组04D01-新云平台程序控制*)"]
["1176.0","验证通过","REAL","空调机组","L","04D01","设定温度值","空调机组04D01-设定温度值",{"$f":"E772&VLOOKUP(D772,list!$D$3:$F$501,2,FALSE)&F772&\"_\"&VLOOKUP(G772,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_TSET"},"LAHU04D01_TSET AT%M1176.0 :REAL; (*空调机组04D01-设定温度值*)","LAHU04D01_TSET          AT%M1176.0     :REAL; (*空调机组04D01-设定温度值*)"]
["1180.0","验证通过","INT","空调机组","L","04D01","季节模式","空调机组04D01-季节模式",{"$f":"E773&VLOOKUP(D773,list!$D$3:$F$501,2,FALSE)&F773&\"_\"&VLOOKUP(G773,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_SM"},"LAHU04D01_SM AT%M1180.0 :INT; (*空调机组04D01-季节模式*)","LAHU04D01_SM            AT%M1180.0     :INT; (*空调机组04D01-季节模式*)"]
["1184.0","验证通过","REAL","空调机组","L","04D01","水阀反馈换算值","空调机组04D01-水阀反馈换算值",{"$f":"E774&VLOOKUP(D774,list!$D$3:$F$501,2,FALSE)&F774&\"_\"&VLOOKUP(G774,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_WVBS"},"LAHU04D01_WVBS AT%M1184.0 :REAL; (*空调机组04D01-水阀反馈换算值*)","LAHU04D01_WVBS          AT%M1184.0     :REAL; (*空调机组04D01-水阀反馈换算值*)"]
["1188.0","验证通过","BOOL","空调机组","L","04D01","水阀手动控制","空调机组04D01-水阀手动控制",{"$f":"E775&VLOOKUP(D775,list!$D$3:$F$501,2,FALSE)&F775&\"_\"&VLOOKUP(G775,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_WVMC"},"LAHU04D01_WVMC AT%M1188.0 :BOOL; (*空调机组04D01-水阀手动控制*)","LAHU04D01_WVMC          AT%M1188.0     :BOOL; (*空调机组04D01-水阀手动控制*)"]
["1192.0","验证通过","REAL","空调机组","L","04D01","水阀手动控制值","空调机组04D01-水阀手动控制值",{"$f":"E776&VLOOKUP(D776,list!$D$3:$F$501,2,FALSE)&F776&\"_\"&VLOOKUP(G776,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_WVMV"},"LAHU04D01_WVMV AT%M1192.0 :REAL; (*空调机组04D01-水阀手动控制值*)","LAHU04D01_WVMV          AT%M1192.0     :REAL; (*空调机组04D01-水阀手动控制值*)"]
["1196.0","验证通过","REAL","空调机组","L","04D01","回风温度换算值","空调机组04D01-回风温度换算值",{"$f":"E777&VLOOKUP(D777,list!$D$3:$F$501,2,FALSE)&F777&\"_\"&VLOOKUP(G777,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_RTS"},"LAHU04D01_RTS AT%M1196.0 :REAL; (*空调机组04D01-回风温度换算值*)","LAHU04D01_RTS           AT%M1196.0     :REAL; (*空调机组04D01-回风温度换算值*)"]
["1200.0","验证通过","BOOL","空调机组","L","04D01","运行时间累积重置","空调机组04D01-运行时间累积重置",{"$f":"E778&VLOOKUP(D778,list!$D$3:$F$501,2,FALSE)&F778&\"_\"&VLOOKUP(G778,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_RST"},"LAHU04D01_RST AT%M1200.0 :BOOL; (*空调机组04D01-运行时间累积重置*)","LAHU04D01_RST           AT%M1200.0     :BOOL; (*空调机组04D01-运行时间累积重置*)"]
["1204.0","验证通过","REAL","空调机组","L","04D01","运行时间累积重置值","空调机组04D01-运行时间累积重置值",{"$f":"E779&VLOOKUP(D779,list!$D$3:$F$501,2,FALSE)&F779&\"_\"&VLOOKUP(G779,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_RSTV"},"LAHU04D01_RSTV AT%M1204.0 :REAL; (*空调机组04D01-运行时间累积重置值*)","LAHU04D01_RSTV          AT%M1204.0     :REAL; (*空调机组04D01-运行时间累积重置值*)"]
["1208.0","验证通过","BOOL","空调机组","L","04D01","隔离开关1","空调机组04D01-隔离开关1",{"$f":"E780&VLOOKUP(D780,list!$D$3:$F$501,2,FALSE)&F780&\"_\"&VLOOKUP(G780,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_ISO1"},"LAHU04D01_ISO1 AT%M1208.0 :BOOL; (*空调机组04D01-隔离开关1*)","LAHU04D01_ISO1          AT%M1208.0     :BOOL; (*空调机组04D01-隔离开关1*)"]
["1210.0","验证通过","BOOL","空调机组","L","04D01","隔离开关2","空调机组04D01-隔离开关2",{"$f":"E781&VLOOKUP(D781,list!$D$3:$F$501,2,FALSE)&F781&\"_\"&VLOOKUP(G781,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_ISO2"},"LAHU04D01_ISO2 AT%M1210.0 :BOOL; (*空调机组04D01-隔离开关2*)","LAHU04D01_ISO2          AT%M1210.0     :BOOL; (*空调机组04D01-隔离开关2*)"]
["1216.0","验证通过","REAL","空调机组","L","04D01","P调节参数","空调机组04D01-P调节参数",{"$f":"E782&VLOOKUP(D782,list!$D$3:$F$501,2,FALSE)&F782&\"_\"&VLOOKUP(G782,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_VP"},"LAHU04D01_VP AT%M1216.0 :REAL; (*空调机组04D01-P调节参数*)","LAHU04D01_VP            AT%M1216.0     :REAL; (*空调机组04D01-P调节参数*)"]
["1220.0","验证通过","REAL","空调机组","L","04D01","I调节参数","空调机组04D01-I调节参数",{"$f":"E783&VLOOKUP(D783,list!$D$3:$F$501,2,FALSE)&F783&\"_\"&VLOOKUP(G783,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_VI"},"LAHU04D01_VI AT%M1220.0 :REAL; (*空调机组04D01-I调节参数*)","LAHU04D01_VI            AT%M1220.0     :REAL; (*空调机组04D01-I调节参数*)"]
["1224.0","验证通过","REAL","空调机组","L","04D01","运行时间累积值","空调机组04D01-运行时间累积值",{"$f":"E784&VLOOKUP(D784,list!$D$3:$F$501,2,FALSE)&F784&\"_\"&VLOOKUP(G784,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_RH"},"LAHU04D01_RH AT%M1224.0 :REAL; (*空调机组04D01-运行时间累积值*)","LAHU04D01_RH            AT%M1224.0     :REAL; (*空调机组04D01-运行时间累积值*)"]
["1228.0","验证通过","INT","空调机组","L","04D01","设备状态代码","空调机组04D01-设备状态代码",{"$f":"E785&VLOOKUP(D785,list!$D$3:$F$501,2,FALSE)&F785&\"_\"&VLOOKUP(G785,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_SN"},"LAHU04D01_SN AT%M1228.0 :INT; (*空调机组04D01-设备状态代码*)","LAHU04D01_SN            AT%M1228.0     :INT; (*空调机组04D01-设备状态代码*)"]
["1230.0","验证通过","INT","空调机组","L","04D01","水阀控制转换值","空调机组04D01-水阀控制转换值",{"$f":"E786&VLOOKUP(D786,list!$D$3:$F$501,2,FALSE)&F786&\"_\"&VLOOKUP(G786,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_WVCS"},"LAHU04D01_WVCS AT%M1230.0 :INT; (*空调机组04D01-水阀控制转换值*)","LAHU04D01_WVCS          AT%M1230.0     :INT; (*空调机组04D01-水阀控制转换值*)"]
["1232.0","验证通过","BOOL","空调机组","L","04D01","程序控制","空调机组04D01-程序控制",{"$f":"E787&VLOOKUP(D787,list!$D$3:$F$501,2,FALSE)&F787&\"_\"&VLOOKUP(G787,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D01_PC"},"LAHU04D01_PC AT%M1232.0 :BOOL; (*空调机组04D01-程序控制*)","LAHU04D01_PC            AT%M1232.0     :BOOL; (*空调机组04D01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C787=\"REAL\",C787=\"DWORD\",C787=\"DINT\"),(IF(OR(C789=\"REAL\",C789=\"DWORD\",C789=\"DINT\"),A787+4+MOD(A787,4),A787+4)),(IF(OR(C789=\"REAL\",C789=\"DWORD\",C789=\"DINT\"),A787+4+MOD(A787,4),A787+2)))&\".0\"","v":"1236.0"},{"$f":"IF((IF(OR(C789=\"INT\",C789=\"WORD\",C789=\"BOOL\"),MOD(A789,2),MOD(A789,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04D02","设定温度值",{"$f":"D789&F789&\"-\"&IF(E789=\"R\",\"新云平台\"&G789,G789)","v":"空调机组04D02-新云平台设定温度值"},{"$f":"E789&VLOOKUP(D789,list!$D$3:$F$501,2,FALSE)&F789&\"_\"&VLOOKUP(G789,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D02_TSET"},{"$f":"I789&\" \"&\"AT%M\"&A789&\" \"&\":\"&C789&\";\"&\" \"&\"(*\"&H789&\"*)\"","v":"RAHU04D02_TSET AT%M1236.0 :REAL; (*空调机组04D02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J789,SEARCH(\"AT%\",J789),,REPT(\" \",25-SEARCH(\"AT%\",J789))),SEARCH(\":\",REPLACE(J789,SEARCH(\"AT%\",J789),,REPT(\" \",25-SEARCH(\"AT%\",J789)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J789,SEARCH(\"AT%\",J789),,REPT(\" \",25-SEARCH(\"AT%\",J789))))))","v":"RAHU04D02_TSET          AT%M1236.0     :REAL; (*空调机组04D02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C789=\"REAL\",C789=\"DWORD\",C789=\"DINT\"),(IF(OR(C790=\"REAL\",C790=\"DWORD\",C790=\"DINT\"),A789+4+MOD(A789,4),A789+4)),(IF(OR(C790=\"REAL\",C790=\"DWORD\",C790=\"DINT\"),A789+4+MOD(A789,4),A789+2)))&\".0\"","v":"1240.0"},"验证通过","INT","空调机组","R",{"$f":"F789","v":"04D02"},"季节模式","空调机组04D02-新云平台季节模式",{"$f":"E790&VLOOKUP(D790,list!$D$3:$F$501,2,FALSE)&F790&\"_\"&VLOOKUP(G790,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D02_SM"},"RAHU04D02_SM AT%M1240.0 :INT; (*空调机组04D02-新云平台季节模式*)","RAHU04D02_SM            AT%M1240.0     :INT; (*空调机组04D02-新云平台季节模式*)"]
["1242.0","验证通过","BOOL","空调机组","R","04D02","程序控制","空调机组04D02-新云平台程序控制",{"$f":"E791&VLOOKUP(D791,list!$D$3:$F$501,2,FALSE)&F791&\"_\"&VLOOKUP(G791,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D02_PC"},"RAHU04D02_PC AT%M1242.0 :BOOL; (*空调机组04D02-新云平台程序控制*)","RAHU04D02_PC            AT%M1242.0     :BOOL; (*空调机组04D02-新云平台程序控制*)"]
["1248.0","验证通过","REAL","空调机组","L","04D02","设定温度值","空调机组04D02-设定温度值",{"$f":"E792&VLOOKUP(D792,list!$D$3:$F$501,2,FALSE)&F792&\"_\"&VLOOKUP(G792,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_TSET"},"LAHU04D02_TSET AT%M1248.0 :REAL; (*空调机组04D02-设定温度值*)","LAHU04D02_TSET          AT%M1248.0     :REAL; (*空调机组04D02-设定温度值*)"]
["1252.0","验证通过","INT","空调机组","L","04D02","季节模式","空调机组04D02-季节模式",{"$f":"E793&VLOOKUP(D793,list!$D$3:$F$501,2,FALSE)&F793&\"_\"&VLOOKUP(G793,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_SM"},"LAHU04D02_SM AT%M1252.0 :INT; (*空调机组04D02-季节模式*)","LAHU04D02_SM            AT%M1252.0     :INT; (*空调机组04D02-季节模式*)"]
["1256.0","验证通过","REAL","空调机组","L","04D02","水阀反馈换算值","空调机组04D02-水阀反馈换算值",{"$f":"E794&VLOOKUP(D794,list!$D$3:$F$501,2,FALSE)&F794&\"_\"&VLOOKUP(G794,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_WVBS"},"LAHU04D02_WVBS AT%M1256.0 :REAL; (*空调机组04D02-水阀反馈换算值*)","LAHU04D02_WVBS          AT%M1256.0     :REAL; (*空调机组04D02-水阀反馈换算值*)"]
["1260.0","验证通过","BOOL","空调机组","L","04D02","水阀手动控制","空调机组04D02-水阀手动控制",{"$f":"E795&VLOOKUP(D795,list!$D$3:$F$501,2,FALSE)&F795&\"_\"&VLOOKUP(G795,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_WVMC"},"LAHU04D02_WVMC AT%M1260.0 :BOOL; (*空调机组04D02-水阀手动控制*)","LAHU04D02_WVMC          AT%M1260.0     :BOOL; (*空调机组04D02-水阀手动控制*)"]
["1264.0","验证通过","REAL","空调机组","L","04D02","水阀手动控制值","空调机组04D02-水阀手动控制值",{"$f":"E796&VLOOKUP(D796,list!$D$3:$F$501,2,FALSE)&F796&\"_\"&VLOOKUP(G796,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_WVMV"},"LAHU04D02_WVMV AT%M1264.0 :REAL; (*空调机组04D02-水阀手动控制值*)","LAHU04D02_WVMV          AT%M1264.0     :REAL; (*空调机组04D02-水阀手动控制值*)"]
["1268.0","验证通过","REAL","空调机组","L","04D02","回风温度换算值","空调机组04D02-回风温度换算值",{"$f":"E797&VLOOKUP(D797,list!$D$3:$F$501,2,FALSE)&F797&\"_\"&VLOOKUP(G797,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_RTS"},"LAHU04D02_RTS AT%M1268.0 :REAL; (*空调机组04D02-回风温度换算值*)","LAHU04D02_RTS           AT%M1268.0     :REAL; (*空调机组04D02-回风温度换算值*)"]
["1272.0","验证通过","BOOL","空调机组","L","04D02","运行时间累积重置","空调机组04D02-运行时间累积重置",{"$f":"E798&VLOOKUP(D798,list!$D$3:$F$501,2,FALSE)&F798&\"_\"&VLOOKUP(G798,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_RST"},"LAHU04D02_RST AT%M1272.0 :BOOL; (*空调机组04D02-运行时间累积重置*)","LAHU04D02_RST           AT%M1272.0     :BOOL; (*空调机组04D02-运行时间累积重置*)"]
["1276.0","验证通过","REAL","空调机组","L","04D02","运行时间累积重置值","空调机组04D02-运行时间累积重置值",{"$f":"E799&VLOOKUP(D799,list!$D$3:$F$501,2,FALSE)&F799&\"_\"&VLOOKUP(G799,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_RSTV"},"LAHU04D02_RSTV AT%M1276.0 :REAL; (*空调机组04D02-运行时间累积重置值*)","LAHU04D02_RSTV          AT%M1276.0     :REAL; (*空调机组04D02-运行时间累积重置值*)"]
["1280.0","验证通过","BOOL","空调机组","L","04D02","隔离开关1","空调机组04D02-隔离开关1",{"$f":"E800&VLOOKUP(D800,list!$D$3:$F$501,2,FALSE)&F800&\"_\"&VLOOKUP(G800,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_ISO1"},"LAHU04D02_ISO1 AT%M1280.0 :BOOL; (*空调机组04D02-隔离开关1*)","LAHU04D02_ISO1          AT%M1280.0     :BOOL; (*空调机组04D02-隔离开关1*)"]
["1282.0","验证通过","BOOL","空调机组","L","04D02","隔离开关2","空调机组04D02-隔离开关2",{"$f":"E801&VLOOKUP(D801,list!$D$3:$F$501,2,FALSE)&F801&\"_\"&VLOOKUP(G801,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_ISO2"},"LAHU04D02_ISO2 AT%M1282.0 :BOOL; (*空调机组04D02-隔离开关2*)","LAHU04D02_ISO2          AT%M1282.0     :BOOL; (*空调机组04D02-隔离开关2*)"]
["1288.0","验证通过","REAL","空调机组","L","04D02","P调节参数","空调机组04D02-P调节参数",{"$f":"E802&VLOOKUP(D802,list!$D$3:$F$501,2,FALSE)&F802&\"_\"&VLOOKUP(G802,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_VP"},"LAHU04D02_VP AT%M1288.0 :REAL; (*空调机组04D02-P调节参数*)","LAHU04D02_VP            AT%M1288.0     :REAL; (*空调机组04D02-P调节参数*)"]
["1292.0","验证通过","REAL","空调机组","L","04D02","I调节参数","空调机组04D02-I调节参数",{"$f":"E803&VLOOKUP(D803,list!$D$3:$F$501,2,FALSE)&F803&\"_\"&VLOOKUP(G803,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_VI"},"LAHU04D02_VI AT%M1292.0 :REAL; (*空调机组04D02-I调节参数*)","LAHU04D02_VI            AT%M1292.0     :REAL; (*空调机组04D02-I调节参数*)"]
["1296.0","验证通过","REAL","空调机组","L","04D02","运行时间累积值","空调机组04D02-运行时间累积值",{"$f":"E804&VLOOKUP(D804,list!$D$3:$F$501,2,FALSE)&F804&\"_\"&VLOOKUP(G804,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_RH"},"LAHU04D02_RH AT%M1296.0 :REAL; (*空调机组04D02-运行时间累积值*)","LAHU04D02_RH            AT%M1296.0     :REAL; (*空调机组04D02-运行时间累积值*)"]
["1300.0","验证通过","INT","空调机组","L","04D02","设备状态代码","空调机组04D02-设备状态代码",{"$f":"E805&VLOOKUP(D805,list!$D$3:$F$501,2,FALSE)&F805&\"_\"&VLOOKUP(G805,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_SN"},"LAHU04D02_SN AT%M1300.0 :INT; (*空调机组04D02-设备状态代码*)","LAHU04D02_SN            AT%M1300.0     :INT; (*空调机组04D02-设备状态代码*)"]
["1302.0","验证通过","INT","空调机组","L","04D02","水阀控制转换值","空调机组04D02-水阀控制转换值",{"$f":"E806&VLOOKUP(D806,list!$D$3:$F$501,2,FALSE)&F806&\"_\"&VLOOKUP(G806,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_WVCS"},"LAHU04D02_WVCS AT%M1302.0 :INT; (*空调机组04D02-水阀控制转换值*)","LAHU04D02_WVCS          AT%M1302.0     :INT; (*空调机组04D02-水阀控制转换值*)"]
["1304.0","验证通过","BOOL","空调机组","L","04D02","程序控制","空调机组04D02-程序控制",{"$f":"E807&VLOOKUP(D807,list!$D$3:$F$501,2,FALSE)&F807&\"_\"&VLOOKUP(G807,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D02_PC"},"LAHU04D02_PC AT%M1304.0 :BOOL; (*空调机组04D02-程序控制*)","LAHU04D02_PC            AT%M1304.0     :BOOL; (*空调机组04D02-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C807=\"REAL\",C807=\"DWORD\",C807=\"DINT\"),(IF(OR(C809=\"REAL\",C809=\"DWORD\",C809=\"DINT\"),A807+4+MOD(A807,4),A807+4)),(IF(OR(C809=\"REAL\",C809=\"DWORD\",C809=\"DINT\"),A807+4+MOD(A807,4),A807+2)))&\".0\"","v":"1308.0"},{"$f":"IF((IF(OR(C809=\"INT\",C809=\"WORD\",C809=\"BOOL\"),MOD(A809,2),MOD(A809,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04D03","设定温度值",{"$f":"D809&F809&\"-\"&IF(E809=\"R\",\"新云平台\"&G809,G809)","v":"空调机组04D03-新云平台设定温度值"},{"$f":"E809&VLOOKUP(D809,list!$D$3:$F$501,2,FALSE)&F809&\"_\"&VLOOKUP(G809,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D03_TSET"},{"$f":"I809&\" \"&\"AT%M\"&A809&\" \"&\":\"&C809&\";\"&\" \"&\"(*\"&H809&\"*)\"","v":"RAHU04D03_TSET AT%M1308.0 :REAL; (*空调机组04D03-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J809,SEARCH(\"AT%\",J809),,REPT(\" \",25-SEARCH(\"AT%\",J809))),SEARCH(\":\",REPLACE(J809,SEARCH(\"AT%\",J809),,REPT(\" \",25-SEARCH(\"AT%\",J809)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J809,SEARCH(\"AT%\",J809),,REPT(\" \",25-SEARCH(\"AT%\",J809))))))","v":"RAHU04D03_TSET          AT%M1308.0     :REAL; (*空调机组04D03-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C809=\"REAL\",C809=\"DWORD\",C809=\"DINT\"),(IF(OR(C810=\"REAL\",C810=\"DWORD\",C810=\"DINT\"),A809+4+MOD(A809,4),A809+4)),(IF(OR(C810=\"REAL\",C810=\"DWORD\",C810=\"DINT\"),A809+4+MOD(A809,4),A809+2)))&\".0\"","v":"1312.0"},"验证通过","INT","空调机组","R",{"$f":"F809","v":"04D03"},"季节模式","空调机组04D03-新云平台季节模式",{"$f":"E810&VLOOKUP(D810,list!$D$3:$F$501,2,FALSE)&F810&\"_\"&VLOOKUP(G810,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D03_SM"},"RAHU04D03_SM AT%M1312.0 :INT; (*空调机组04D03-新云平台季节模式*)","RAHU04D03_SM            AT%M1312.0     :INT; (*空调机组04D03-新云平台季节模式*)"]
["1314.0","验证通过","BOOL","空调机组","R","04D03","程序控制","空调机组04D03-新云平台程序控制",{"$f":"E811&VLOOKUP(D811,list!$D$3:$F$501,2,FALSE)&F811&\"_\"&VLOOKUP(G811,list!$I$2:$K$502,2,FALSE)","v":"RAHU04D03_PC"},"RAHU04D03_PC AT%M1314.0 :BOOL; (*空调机组04D03-新云平台程序控制*)","RAHU04D03_PC            AT%M1314.0     :BOOL; (*空调机组04D03-新云平台程序控制*)"]
["1320.0","验证通过","REAL","空调机组","L","04D03","设定温度值","空调机组04D03-设定温度值",{"$f":"E812&VLOOKUP(D812,list!$D$3:$F$501,2,FALSE)&F812&\"_\"&VLOOKUP(G812,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_TSET"},"LAHU04D03_TSET AT%M1320.0 :REAL; (*空调机组04D03-设定温度值*)","LAHU04D03_TSET          AT%M1320.0     :REAL; (*空调机组04D03-设定温度值*)"]
["1324.0","验证通过","INT","空调机组","L","04D03","季节模式","空调机组04D03-季节模式",{"$f":"E813&VLOOKUP(D813,list!$D$3:$F$501,2,FALSE)&F813&\"_\"&VLOOKUP(G813,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_SM"},"LAHU04D03_SM AT%M1324.0 :INT; (*空调机组04D03-季节模式*)","LAHU04D03_SM            AT%M1324.0     :INT; (*空调机组04D03-季节模式*)"]
["1328.0","验证通过","REAL","空调机组","L","04D03","水阀反馈换算值","空调机组04D03-水阀反馈换算值",{"$f":"E814&VLOOKUP(D814,list!$D$3:$F$501,2,FALSE)&F814&\"_\"&VLOOKUP(G814,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_WVBS"},"LAHU04D03_WVBS AT%M1328.0 :REAL; (*空调机组04D03-水阀反馈换算值*)","LAHU04D03_WVBS          AT%M1328.0     :REAL; (*空调机组04D03-水阀反馈换算值*)"]
["1332.0","验证通过","BOOL","空调机组","L","04D03","水阀手动控制","空调机组04D03-水阀手动控制",{"$f":"E815&VLOOKUP(D815,list!$D$3:$F$501,2,FALSE)&F815&\"_\"&VLOOKUP(G815,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_WVMC"},"LAHU04D03_WVMC AT%M1332.0 :BOOL; (*空调机组04D03-水阀手动控制*)","LAHU04D03_WVMC          AT%M1332.0     :BOOL; (*空调机组04D03-水阀手动控制*)"]
["1336.0","验证通过","REAL","空调机组","L","04D03","水阀手动控制值","空调机组04D03-水阀手动控制值",{"$f":"E816&VLOOKUP(D816,list!$D$3:$F$501,2,FALSE)&F816&\"_\"&VLOOKUP(G816,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_WVMV"},"LAHU04D03_WVMV AT%M1336.0 :REAL; (*空调机组04D03-水阀手动控制值*)","LAHU04D03_WVMV          AT%M1336.0     :REAL; (*空调机组04D03-水阀手动控制值*)"]
["1340.0","验证通过","REAL","空调机组","L","04D03","回风温度换算值","空调机组04D03-回风温度换算值",{"$f":"E817&VLOOKUP(D817,list!$D$3:$F$501,2,FALSE)&F817&\"_\"&VLOOKUP(G817,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_RTS"},"LAHU04D03_RTS AT%M1340.0 :REAL; (*空调机组04D03-回风温度换算值*)","LAHU04D03_RTS           AT%M1340.0     :REAL; (*空调机组04D03-回风温度换算值*)"]
["1344.0","验证通过","BOOL","空调机组","L","04D03","运行时间累积重置","空调机组04D03-运行时间累积重置",{"$f":"E818&VLOOKUP(D818,list!$D$3:$F$501,2,FALSE)&F818&\"_\"&VLOOKUP(G818,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_RST"},"LAHU04D03_RST AT%M1344.0 :BOOL; (*空调机组04D03-运行时间累积重置*)","LAHU04D03_RST           AT%M1344.0     :BOOL; (*空调机组04D03-运行时间累积重置*)"]
["1348.0","验证通过","REAL","空调机组","L","04D03","运行时间累积重置值","空调机组04D03-运行时间累积重置值",{"$f":"E819&VLOOKUP(D819,list!$D$3:$F$501,2,FALSE)&F819&\"_\"&VLOOKUP(G819,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_RSTV"},"LAHU04D03_RSTV AT%M1348.0 :REAL; (*空调机组04D03-运行时间累积重置值*)","LAHU04D03_RSTV          AT%M1348.0     :REAL; (*空调机组04D03-运行时间累积重置值*)"]
["1352.0","验证通过","BOOL","空调机组","L","04D03","隔离开关1","空调机组04D03-隔离开关1",{"$f":"E820&VLOOKUP(D820,list!$D$3:$F$501,2,FALSE)&F820&\"_\"&VLOOKUP(G820,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_ISO1"},"LAHU04D03_ISO1 AT%M1352.0 :BOOL; (*空调机组04D03-隔离开关1*)","LAHU04D03_ISO1          AT%M1352.0     :BOOL; (*空调机组04D03-隔离开关1*)"]
["1354.0","验证通过","BOOL","空调机组","L","04D03","隔离开关2","空调机组04D03-隔离开关2",{"$f":"E821&VLOOKUP(D821,list!$D$3:$F$501,2,FALSE)&F821&\"_\"&VLOOKUP(G821,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_ISO2"},"LAHU04D03_ISO2 AT%M1354.0 :BOOL; (*空调机组04D03-隔离开关2*)","LAHU04D03_ISO2          AT%M1354.0     :BOOL; (*空调机组04D03-隔离开关2*)"]
["1360.0","验证通过","REAL","空调机组","L","04D03","P调节参数","空调机组04D03-P调节参数",{"$f":"E822&VLOOKUP(D822,list!$D$3:$F$501,2,FALSE)&F822&\"_\"&VLOOKUP(G822,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_VP"},"LAHU04D03_VP AT%M1360.0 :REAL; (*空调机组04D03-P调节参数*)","LAHU04D03_VP            AT%M1360.0     :REAL; (*空调机组04D03-P调节参数*)"]
["1364.0","验证通过","REAL","空调机组","L","04D03","I调节参数","空调机组04D03-I调节参数",{"$f":"E823&VLOOKUP(D823,list!$D$3:$F$501,2,FALSE)&F823&\"_\"&VLOOKUP(G823,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_VI"},"LAHU04D03_VI AT%M1364.0 :REAL; (*空调机组04D03-I调节参数*)","LAHU04D03_VI            AT%M1364.0     :REAL; (*空调机组04D03-I调节参数*)"]
["1368.0","验证通过","REAL","空调机组","L","04D03","运行时间累积值","空调机组04D03-运行时间累积值",{"$f":"E824&VLOOKUP(D824,list!$D$3:$F$501,2,FALSE)&F824&\"_\"&VLOOKUP(G824,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_RH"},"LAHU04D03_RH AT%M1368.0 :REAL; (*空调机组04D03-运行时间累积值*)","LAHU04D03_RH            AT%M1368.0     :REAL; (*空调机组04D03-运行时间累积值*)"]
["1372.0","验证通过","INT","空调机组","L","04D03","设备状态代码","空调机组04D03-设备状态代码",{"$f":"E825&VLOOKUP(D825,list!$D$3:$F$501,2,FALSE)&F825&\"_\"&VLOOKUP(G825,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_SN"},"LAHU04D03_SN AT%M1372.0 :INT; (*空调机组04D03-设备状态代码*)","LAHU04D03_SN            AT%M1372.0     :INT; (*空调机组04D03-设备状态代码*)"]
["1374.0","验证通过","INT","空调机组","L","04D03","水阀控制转换值","空调机组04D03-水阀控制转换值",{"$f":"E826&VLOOKUP(D826,list!$D$3:$F$501,2,FALSE)&F826&\"_\"&VLOOKUP(G826,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_WVCS"},"LAHU04D03_WVCS AT%M1374.0 :INT; (*空调机组04D03-水阀控制转换值*)","LAHU04D03_WVCS          AT%M1374.0     :INT; (*空调机组04D03-水阀控制转换值*)"]
["1376.0","验证通过","BOOL","空调机组","L","04D03","程序控制","空调机组04D03-程序控制",{"$f":"E827&VLOOKUP(D827,list!$D$3:$F$501,2,FALSE)&F827&\"_\"&VLOOKUP(G827,list!$I$2:$K$502,2,FALSE)","v":"LAHU04D03_PC"},"LAHU04D03_PC AT%M1376.0 :BOOL; (*空调机组04D03-程序控制*)","LAHU04D03_PC            AT%M1376.0     :BOOL; (*空调机组04D03-程序控制*)"]
["EAF"]
[{"$f":"IF(OR(C827=\"REAL\",C827=\"DWORD\",C827=\"DINT\"),(IF(OR(C829=\"REAL\",C829=\"DWORD\",C829=\"DINT\"),A827+4+MOD(A827,4),A827+4)),(IF(OR(C829=\"REAL\",C829=\"DWORD\",C829=\"DINT\"),A827+4+MOD(A827,4),A827+2)))&\".0\"","v":"1378.0"},{"$f":"IF((IF(OR(C829=\"INT\",C829=\"WORD\",C829=\"BOOL\"),MOD(A829,2),MOD(A829,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","04D01","启停控制",{"$f":"D829&F829&\"-\"&IF(E829=\"R\",\"新云平台\"&G829,G829)","v":"排风机04D01-新云平台启停控制"},{"$f":"E829&VLOOKUP(D829,[1]list!$D$3:$F$501,2,FALSE)&F829&\"_\"&VLOOKUP(G829,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04D01_C"},{"$f":"I829&\" \"&\"AT%M\"&A829&\" \"&\":\"&C829&\";\"&\" \"&\"(*\"&H829&\"*)\"","v":"REAF04D01_C AT%M1378.0 :BOOL; (*排风机04D01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J829,SEARCH(\"AT%\",J829),,REPT(\" \",25-SEARCH(\"AT%\",J829))),SEARCH(\":\",REPLACE(J829,SEARCH(\"AT%\",J829),,REPT(\" \",25-SEARCH(\"AT%\",J829)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J829,SEARCH(\"AT%\",J829),,REPT(\" \",25-SEARCH(\"AT%\",J829))))))","v":"REAF04D01_C             AT%M1378.0     :BOOL; (*排风机04D01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C829=\"REAL\",C829=\"DWORD\",C829=\"DINT\"),(IF(OR(C830=\"REAL\",C830=\"DWORD\",C830=\"DINT\"),A829+4+MOD(A829,4),A829+4)),(IF(OR(C830=\"REAL\",C830=\"DWORD\",C830=\"DINT\"),A829+4+MOD(A829,4),A829+2)))&\".0\"","v":"1380.0"},"验证通过","BOOL","排风机","L","04D01","运行时间累积重置","排风机04D01-运行时间累积重置",{"$f":"E830&VLOOKUP(D830,[1]list!$D$3:$F$501,2,FALSE)&F830&\"_\"&VLOOKUP(G830,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04D01_RST"},"LEAF04D01_RST AT%M1380.0 :BOOL; (*排风机04D01-运行时间累积重置*)","LEAF04D01_RST           AT%M1380.0     :BOOL; (*排风机04D01-运行时间累积重置*)"]
["1384.0","验证通过","REAL","排风机","L","04D01","运行时间累积重置值","排风机04D01-运行时间累积重置值",{"$f":"E831&VLOOKUP(D831,[1]list!$D$3:$F$501,2,FALSE)&F831&\"_\"&VLOOKUP(G831,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04D01_RSTV"},"LEAF04D01_RSTV AT%M1384.0 :REAL; (*排风机04D01-运行时间累积重置值*)","LEAF04D01_RSTV          AT%M1384.0     :REAL; (*排风机04D01-运行时间累积重置值*)"]
["1388.0","验证通过","REAL","排风机","L","04D01","运行时间累积值","排风机04D01-运行时间累积值",{"$f":"E832&VLOOKUP(D832,[1]list!$D$3:$F$501,2,FALSE)&F832&\"_\"&VLOOKUP(G832,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04D01_RH"},"LEAF04D01_RH AT%M1388.0 :REAL; (*排风机04D01-运行时间累积值*)","LEAF04D01_RH            AT%M1388.0     :REAL; (*排风机04D01-运行时间累积值*)"]
["1392.0","验证通过","BOOL","排风机","L","04D01","定时模式","排风机04D01-定时模式",{"$f":"E833&VLOOKUP(D833,[1]list!$D$3:$F$501,2,FALSE)&F833&\"_\"&VLOOKUP(G833,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04D01_TM"},"LEAF04D01_TM AT%M1392.0 :BOOL; (*排风机04D01-定时模式*)","LEAF04D01_TM            AT%M1392.0     :BOOL; (*排风机04D01-定时模式*)"]
["1394.0","验证通过","BOOL","排风机","L","04D01","定时控制","排风机04D01-定时控制",{"$f":"E834&VLOOKUP(D834,[1]list!$D$3:$F$501,2,FALSE)&F834&\"_\"&VLOOKUP(G834,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04D01_TC"},"LEAF04D01_TC AT%M1394.0 :BOOL; (*排风机04D01-定时控制*)","LEAF04D01_TC            AT%M1394.0     :BOOL; (*排风机04D01-定时控制*)"]
["1396.0","验证通过","BOOL","排风机","L","04D01","全天候模式","排风机04D01-全天候模式",{"$f":"E835&VLOOKUP(D835,[1]list!$D$3:$F$501,2,FALSE)&F835&\"_\"&VLOOKUP(G835,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04D01_DM"},"LEAF04D01_DM AT%M1396.0 :BOOL; (*排风机04D01-全天候模式*)","LEAF04D01_DM            AT%M1396.0     :BOOL; (*排风机04D01-全天候模式*)"]
["1400.0","验证通过","REAL","排风机","L","04D01","CO设定值","排风机04D01-CO设定值",{"$f":"E836&VLOOKUP(D836,[1]list!$D$3:$F$501,2,FALSE)&F836&\"_\"&VLOOKUP(G836,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF04D01_COSET"},"LEAF04D01_COSET AT%M1400.0 :REAL; (*排风机04D01-CO设定值*)","LEAF04D01_COSET         AT%M1400.0     :REAL; (*排风机04D01-CO设定值*)"]
["1404.0","验证通过","REAL","排烟机","L","04D01","设定温度值","排烟机04D01-设定温度值",{"$f":"E837&VLOOKUP(D837,[1]list!$D$3:$F$501,2,FALSE)&F837&\"_\"&VLOOKUP(G837,[1]list!$I$2:$K$502,2,FALSE)","v":"LESF04D01_TSET"},"LESF04D01_TSET AT%M1404.0 :REAL; (*排烟机04D01-设定温度值*)","LESF04D01_TSET          AT%M1404.0     :REAL; (*排烟机04D01-设定温度值*)"]
["FCU"]
[{"$f":"IF(OR(C837=\"REAL\",C837=\"DWORD\",C837=\"DINT\"),(IF(OR(C839=\"REAL\",C839=\"DWORD\",C839=\"DINT\"),A837+4+MOD(A837,4),A837+4)),(IF(OR(C839=\"REAL\",C839=\"DWORD\",C839=\"DINT\"),A837+4+MOD(A837,4),A837+2)))&\".0\"","v":"1408.0"},{"$f":"IF((IF(OR(C839=\"INT\",C839=\"WORD\",C839=\"BOOL\"),MOD(A839,2),MOD(A839,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","04D01","设定温度值",{"$f":"D839&F839&\"-\"&IF(E839=\"R\",\"新云平台\"&G839,G839)","v":"风机盘管04D01-新云平台设定温度值"},{"$f":"E839&VLOOKUP(D839,list!$D$3:$F$501,2,FALSE)&F839&\"_\"&VLOOKUP(G839,list!$I$2:$K$502,2,FALSE)","v":"RFCU04D01_TSET"},{"$f":"I839&\" \"&\"AT%M\"&A839&\" \"&\":\"&C839&\";\"&\" \"&\"(*\"&H839&\"*)\"","v":"RFCU04D01_TSET AT%M1408.0 :REAL; (*风机盘管04D01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J839,SEARCH(\"AT%\",J839),,REPT(\" \",25-SEARCH(\"AT%\",J839))),SEARCH(\":\",REPLACE(J839,SEARCH(\"AT%\",J839),,REPT(\" \",25-SEARCH(\"AT%\",J839)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J839,SEARCH(\"AT%\",J839),,REPT(\" \",25-SEARCH(\"AT%\",J839))))))","v":"RFCU04D01_TSET          AT%M1408.0     :REAL; (*风机盘管04D01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C839=\"REAL\",C839=\"DWORD\",C839=\"DINT\"),(IF(OR(C840=\"REAL\",C840=\"DWORD\",C840=\"DINT\"),A839+4+MOD(A839,4),A839+4)),(IF(OR(C840=\"REAL\",C840=\"DWORD\",C840=\"DINT\"),A839+4+MOD(A839,4),A839+2)))&\".0\"","v":"1412.0"},"验证通过","INT","风机盘管","R",{"$f":"F839","v":"04D01"},"季节模式","风机盘管04D01-新云平台季节模式",{"$f":"E840&VLOOKUP(D840,list!$D$3:$F$501,2,FALSE)&F840&\"_\"&VLOOKUP(G840,list!$I$2:$K$502,2,FALSE)","v":"RFCU04D01_SM"},"RFCU04D01_SM AT%M1412.0 :INT; (*风机盘管04D01-新云平台季节模式*)","RFCU04D01_SM            AT%M1412.0     :INT; (*风机盘管04D01-新云平台季节模式*)"]
["1414.0","验证通过","BOOL","风机盘管","R","04D01","程序控制","风机盘管04D01-新云平台程序控制",{"$f":"E841&VLOOKUP(D841,list!$D$3:$F$501,2,FALSE)&F841&\"_\"&VLOOKUP(G841,list!$I$2:$K$502,2,FALSE)","v":"RFCU04D01_PC"},"RFCU04D01_PC AT%M1414.0 :BOOL; (*风机盘管04D01-新云平台程序控制*)","RFCU04D01_PC            AT%M1414.0     :BOOL; (*风机盘管04D01-新云平台程序控制*)"]
["1420.0","验证通过","REAL","风机盘管","L","04D01","设定温度值","风机盘管04D01-设定温度值",{"$f":"E842&VLOOKUP(D842,list!$D$3:$F$501,2,FALSE)&F842&\"_\"&VLOOKUP(G842,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_TSET"},"LFCU04D01_TSET AT%M1420.0 :REAL; (*风机盘管04D01-设定温度值*)","LFCU04D01_TSET          AT%M1420.0     :REAL; (*风机盘管04D01-设定温度值*)"]
["1424.0","验证通过","INT","风机盘管","L","04D01","季节模式","风机盘管04D01-季节模式",{"$f":"E843&VLOOKUP(D843,list!$D$3:$F$501,2,FALSE)&F843&\"_\"&VLOOKUP(G843,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_SM"},"LFCU04D01_SM AT%M1424.0 :INT; (*风机盘管04D01-季节模式*)","LFCU04D01_SM            AT%M1424.0     :INT; (*风机盘管04D01-季节模式*)"]
["1428.0","验证通过","REAL","风机盘管","L","04D01","温度换算值","风机盘管04D01-温度换算值",{"$f":"E844&VLOOKUP(D844,list!$D$3:$F$501,2,FALSE)&F844&\"_\"&VLOOKUP(G844,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_TS"},"LFCU04D01_TS AT%M1428.0 :REAL; (*风机盘管04D01-温度换算值*)","LFCU04D01_TS            AT%M1428.0     :REAL; (*风机盘管04D01-温度换算值*)"]
["1432.0","验证通过","BOOL","风机盘管","L","04D01","电磁阀手动控制","风机盘管04D01-电磁阀手动控制",{"$f":"E845&VLOOKUP(D845,list!$D$3:$F$501,2,FALSE)&F845&\"_\"&VLOOKUP(G845,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_EVMC"},"LFCU04D01_EVMC AT%M1432.0 :BOOL; (*风机盘管04D01-电磁阀手动控制*)","LFCU04D01_EVMC          AT%M1432.0     :BOOL; (*风机盘管04D01-电磁阀手动控制*)"]
["1434.0","验证通过","BOOL","风机盘管","L","04D01","电磁阀手动控制值","风机盘管04D01-电磁阀手动控制值",{"$f":"E846&VLOOKUP(D846,list!$D$3:$F$501,2,FALSE)&F846&\"_\"&VLOOKUP(G846,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_EVMV"},"LFCU04D01_EVMV AT%M1434.0 :BOOL; (*风机盘管04D01-电磁阀手动控制值*)","LFCU04D01_EVMV          AT%M1434.0     :BOOL; (*风机盘管04D01-电磁阀手动控制值*)"]
["1440.0","验证通过","REAL","风机盘管","L","04D01","回风温度换算值","风机盘管04D01-回风温度换算值",{"$f":"E847&VLOOKUP(D847,list!$D$3:$F$501,2,FALSE)&F847&\"_\"&VLOOKUP(G847,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_RTS"},"LFCU04D01_RTS AT%M1440.0 :REAL; (*风机盘管04D01-回风温度换算值*)","LFCU04D01_RTS           AT%M1440.0     :REAL; (*风机盘管04D01-回风温度换算值*)"]
["1444.0","验证通过","BOOL","风机盘管","L","04D01","运行时间累积重置","风机盘管04D01-运行时间累积重置",{"$f":"E848&VLOOKUP(D848,list!$D$3:$F$501,2,FALSE)&F848&\"_\"&VLOOKUP(G848,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_RST"},"LFCU04D01_RST AT%M1444.0 :BOOL; (*风机盘管04D01-运行时间累积重置*)","LFCU04D01_RST           AT%M1444.0     :BOOL; (*风机盘管04D01-运行时间累积重置*)"]
["1448.0","验证通过","REAL","风机盘管","L","04D01","运行时间累积重置值","风机盘管04D01-运行时间累积重置值",{"$f":"E849&VLOOKUP(D849,list!$D$3:$F$501,2,FALSE)&F849&\"_\"&VLOOKUP(G849,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_RSTV"},"LFCU04D01_RSTV AT%M1448.0 :REAL; (*风机盘管04D01-运行时间累积重置值*)","LFCU04D01_RSTV          AT%M1448.0     :REAL; (*风机盘管04D01-运行时间累积重置值*)"]
["1452.0","验证通过","BOOL","风机盘管","L","04D01","隔离开关1","风机盘管04D01-隔离开关1",{"$f":"E850&VLOOKUP(D850,list!$D$3:$F$501,2,FALSE)&F850&\"_\"&VLOOKUP(G850,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_ISO1"},"LFCU04D01_ISO1 AT%M1452.0 :BOOL; (*风机盘管04D01-隔离开关1*)","LFCU04D01_ISO1          AT%M1452.0     :BOOL; (*风机盘管04D01-隔离开关1*)"]
["1456.0","验证通过","REAL","风机盘管","L","04D01","运行时间累积值","风机盘管04D01-运行时间累积值",{"$f":"E851&VLOOKUP(D851,list!$D$3:$F$501,2,FALSE)&F851&\"_\"&VLOOKUP(G851,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_RH"},"LFCU04D01_RH AT%M1456.0 :REAL; (*风机盘管04D01-运行时间累积值*)","LFCU04D01_RH            AT%M1456.0     :REAL; (*风机盘管04D01-运行时间累积值*)"]
["1460.0","验证通过","INT","风机盘管","L","04D01","设备状态代码","风机盘管04D01-设备状态代码",{"$f":"E852&VLOOKUP(D852,list!$D$3:$F$501,2,FALSE)&F852&\"_\"&VLOOKUP(G852,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_SN"},"LFCU04D01_SN AT%M1460.0 :INT; (*风机盘管04D01-设备状态代码*)","LFCU04D01_SN            AT%M1460.0     :INT; (*风机盘管04D01-设备状态代码*)"]
["1462.0","验证通过","INT","风机盘管","L","04D01","水阀控制转换值","风机盘管04D01-水阀控制转换值",{"$f":"E853&VLOOKUP(D853,list!$D$3:$F$501,2,FALSE)&F853&\"_\"&VLOOKUP(G853,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_WVCS"},"LFCU04D01_WVCS AT%M1462.0 :INT; (*风机盘管04D01-水阀控制转换值*)","LFCU04D01_WVCS          AT%M1462.0     :INT; (*风机盘管04D01-水阀控制转换值*)"]
["1464.0","验证通过","BOOL","风机盘管","L","04D01","程序控制","风机盘管04D01-程序控制",{"$f":"E854&VLOOKUP(D854,list!$D$3:$F$501,2,FALSE)&F854&\"_\"&VLOOKUP(G854,list!$I$2:$K$502,2,FALSE)","v":"LFCU04D01_PC"},"LFCU04D01_PC AT%M1464.0 :BOOL; (*风机盘管04D01-程序控制*)","LFCU04D01_PC            AT%M1464.0     :BOOL; (*风机盘管04D01-程序控制*)"]
["PAU"]
[{"$f":"IF(OR(C854=\"REAL\",C854=\"DWORD\",C854=\"DINT\"),(IF(OR(C856=\"REAL\",C856=\"DWORD\",C856=\"DINT\"),A854+4+MOD(A854,4),A854+4)),(IF(OR(C856=\"REAL\",C856=\"DWORD\",C856=\"DINT\"),A854+4+MOD(A854,4),A854+2)))&\".0\"","v":"1468.0"},{"$f":"IF((IF(OR(C856=\"INT\",C856=\"WORD\",C856=\"BOOL\"),MOD(A856,2),MOD(A856,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05G01","设定温度值",{"$f":"D856&F856&\"-\"&IF(E856=\"R\",\"新云平台\"&G856,G856)","v":"P新风机组05G01-新云平台设定温度值"},{"$f":"E856&VLOOKUP(D856,list!$D$3:$F$501,2,FALSE)&F856&\"_\"&VLOOKUP(G856,list!$I$2:$K$502,2,FALSE)","v":"RPAU05G01_TSET"},{"$f":"I856&\" \"&\"AT%M\"&A856&\" \"&\":\"&C856&\";\"&\" \"&\"(*\"&H856&\"*)\"","v":"RPAU05G01_TSET AT%M1468.0 :REAL; (*P新风机组05G01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J856,SEARCH(\"AT%\",J856),,REPT(\" \",25-SEARCH(\"AT%\",J856))),SEARCH(\":\",REPLACE(J856,SEARCH(\"AT%\",J856),,REPT(\" \",25-SEARCH(\"AT%\",J856)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J856,SEARCH(\"AT%\",J856),,REPT(\" \",25-SEARCH(\"AT%\",J856))))))","v":"RPAU05G01_TSET          AT%M1468.0     :REAL; (*P新风机组05G01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C856=\"REAL\",C856=\"DWORD\",C856=\"DINT\"),(IF(OR(C857=\"REAL\",C857=\"DWORD\",C857=\"DINT\"),A856+4+MOD(A856,4),A856+4)),(IF(OR(C857=\"REAL\",C857=\"DWORD\",C857=\"DINT\"),A856+4+MOD(A856,4),A856+2)))&\".0\"","v":"1472.0"},"验证通过","INT","P新风机组","R",{"$f":"F856","v":"05G01"},"季节模式","P新风机组05G01-新云平台季节模式",{"$f":"E857&VLOOKUP(D857,list!$D$3:$F$501,2,FALSE)&F857&\"_\"&VLOOKUP(G857,list!$I$2:$K$502,2,FALSE)","v":"RPAU05G01_SM"},"RPAU05G01_SM AT%M1472.0 :INT; (*P新风机组05G01-新云平台季节模式*)","RPAU05G01_SM            AT%M1472.0     :INT; (*P新风机组05G01-新云平台季节模式*)"]
["1474.0","验证通过","BOOL","P新风机组","R","05G01","程序控制","P新风机组05G01-新云平台程序控制",{"$f":"E858&VLOOKUP(D858,list!$D$3:$F$501,2,FALSE)&F858&\"_\"&VLOOKUP(G858,list!$I$2:$K$502,2,FALSE)","v":"RPAU05G01_PC"},"RPAU05G01_PC AT%M1474.0 :BOOL; (*P新风机组05G01-新云平台程序控制*)","RPAU05G01_PC            AT%M1474.0     :BOOL; (*P新风机组05G01-新云平台程序控制*)"]
["1480.0","验证通过","REAL","P新风机组","L","05G01","设定温度值","P新风机组05G01-设定温度值",{"$f":"E859&VLOOKUP(D859,list!$D$3:$F$501,2,FALSE)&F859&\"_\"&VLOOKUP(G859,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_TSET"},"LPAU05G01_TSET AT%M1480.0 :REAL; (*P新风机组05G01-设定温度值*)","LPAU05G01_TSET          AT%M1480.0     :REAL; (*P新风机组05G01-设定温度值*)"]
["1484.0","验证通过","INT","P新风机组","L","05G01","季节模式","P新风机组05G01-季节模式",{"$f":"E860&VLOOKUP(D860,list!$D$3:$F$501,2,FALSE)&F860&\"_\"&VLOOKUP(G860,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_SM"},"LPAU05G01_SM AT%M1484.0 :INT; (*P新风机组05G01-季节模式*)","LPAU05G01_SM            AT%M1484.0     :INT; (*P新风机组05G01-季节模式*)"]
["1488.0","验证通过","REAL","P新风机组","L","05G01","水阀反馈换算值","P新风机组05G01-水阀反馈换算值",{"$f":"E861&VLOOKUP(D861,list!$D$3:$F$501,2,FALSE)&F861&\"_\"&VLOOKUP(G861,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_WVBS"},"LPAU05G01_WVBS AT%M1488.0 :REAL; (*P新风机组05G01-水阀反馈换算值*)","LPAU05G01_WVBS          AT%M1488.0     :REAL; (*P新风机组05G01-水阀反馈换算值*)"]
["1492.0","验证通过","BOOL","P新风机组","L","05G01","水阀手动控制","P新风机组05G01-水阀手动控制",{"$f":"E862&VLOOKUP(D862,list!$D$3:$F$501,2,FALSE)&F862&\"_\"&VLOOKUP(G862,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_WVMC"},"LPAU05G01_WVMC AT%M1492.0 :BOOL; (*P新风机组05G01-水阀手动控制*)","LPAU05G01_WVMC          AT%M1492.0     :BOOL; (*P新风机组05G01-水阀手动控制*)"]
["1496.0","验证通过","REAL","P新风机组","L","05G01","水阀手动控制值","P新风机组05G01-水阀手动控制值",{"$f":"E863&VLOOKUP(D863,list!$D$3:$F$501,2,FALSE)&F863&\"_\"&VLOOKUP(G863,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_WVMV"},"LPAU05G01_WVMV AT%M1496.0 :REAL; (*P新风机组05G01-水阀手动控制值*)","LPAU05G01_WVMV          AT%M1496.0     :REAL; (*P新风机组05G01-水阀手动控制值*)"]
["1500.0","验证通过","REAL","P新风机组","L","05G01","送风温度换算值","P新风机组05G01-送风温度换算值",{"$f":"E864&VLOOKUP(D864,list!$D$3:$F$501,2,FALSE)&F864&\"_\"&VLOOKUP(G864,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_STS"},"LPAU05G01_STS AT%M1500.0 :REAL; (*P新风机组05G01-送风温度换算值*)","LPAU05G01_STS           AT%M1500.0     :REAL; (*P新风机组05G01-送风温度换算值*)"]
["1504.0","验证通过","BOOL","P新风机组","L","05G01","运行时间累积重置","P新风机组05G01-运行时间累积重置",{"$f":"E865&VLOOKUP(D865,list!$D$3:$F$501,2,FALSE)&F865&\"_\"&VLOOKUP(G865,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_RST"},"LPAU05G01_RST AT%M1504.0 :BOOL; (*P新风机组05G01-运行时间累积重置*)","LPAU05G01_RST           AT%M1504.0     :BOOL; (*P新风机组05G01-运行时间累积重置*)"]
["1508.0","验证通过","REAL","P新风机组","L","05G01","运行时间累积重置值","P新风机组05G01-运行时间累积重置值",{"$f":"E866&VLOOKUP(D866,list!$D$3:$F$501,2,FALSE)&F866&\"_\"&VLOOKUP(G866,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_RSTV"},"LPAU05G01_RSTV AT%M1508.0 :REAL; (*P新风机组05G01-运行时间累积重置值*)","LPAU05G01_RSTV          AT%M1508.0     :REAL; (*P新风机组05G01-运行时间累积重置值*)"]
["1512.0","验证通过","BOOL","P新风机组","L","05G01","隔离开关1","P新风机组05G01-隔离开关1",{"$f":"E867&VLOOKUP(D867,list!$D$3:$F$501,2,FALSE)&F867&\"_\"&VLOOKUP(G867,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_ISO1"},"LPAU05G01_ISO1 AT%M1512.0 :BOOL; (*P新风机组05G01-隔离开关1*)","LPAU05G01_ISO1          AT%M1512.0     :BOOL; (*P新风机组05G01-隔离开关1*)"]
["1514.0","验证通过","BOOL","P新风机组","L","05G01","隔离开关2","P新风机组05G01-隔离开关2",{"$f":"E868&VLOOKUP(D868,list!$D$3:$F$501,2,FALSE)&F868&\"_\"&VLOOKUP(G868,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_ISO2"},"LPAU05G01_ISO2 AT%M1514.0 :BOOL; (*P新风机组05G01-隔离开关2*)","LPAU05G01_ISO2          AT%M1514.0     :BOOL; (*P新风机组05G01-隔离开关2*)"]
["1520.0","验证通过","REAL","P新风机组","L","05G01","P调节参数","P新风机组05G01-P调节参数",{"$f":"E869&VLOOKUP(D869,list!$D$3:$F$501,2,FALSE)&F869&\"_\"&VLOOKUP(G869,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_VP"},"LPAU05G01_VP AT%M1520.0 :REAL; (*P新风机组05G01-P调节参数*)","LPAU05G01_VP            AT%M1520.0     :REAL; (*P新风机组05G01-P调节参数*)"]
["1524.0","验证通过","REAL","P新风机组","L","05G01","I调节参数","P新风机组05G01-I调节参数",{"$f":"E870&VLOOKUP(D870,list!$D$3:$F$501,2,FALSE)&F870&\"_\"&VLOOKUP(G870,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_VI"},"LPAU05G01_VI AT%M1524.0 :REAL; (*P新风机组05G01-I调节参数*)","LPAU05G01_VI            AT%M1524.0     :REAL; (*P新风机组05G01-I调节参数*)"]
["1528.0","验证通过","REAL","P新风机组","L","05G01","运行时间累积值","P新风机组05G01-运行时间累积值",{"$f":"E871&VLOOKUP(D871,list!$D$3:$F$501,2,FALSE)&F871&\"_\"&VLOOKUP(G871,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_RH"},"LPAU05G01_RH AT%M1528.0 :REAL; (*P新风机组05G01-运行时间累积值*)","LPAU05G01_RH            AT%M1528.0     :REAL; (*P新风机组05G01-运行时间累积值*)"]
["1532.0","验证通过","INT","P新风机组","L","05G01","设备状态代码","P新风机组05G01-设备状态代码",{"$f":"E872&VLOOKUP(D872,list!$D$3:$F$501,2,FALSE)&F872&\"_\"&VLOOKUP(G872,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_SN"},"LPAU05G01_SN AT%M1532.0 :INT; (*P新风机组05G01-设备状态代码*)","LPAU05G01_SN            AT%M1532.0     :INT; (*P新风机组05G01-设备状态代码*)"]
["1534.0","验证通过","INT","P新风机组","L","05G01","水阀控制转换值","P新风机组05G01-水阀控制转换值",{"$f":"E873&VLOOKUP(D873,list!$D$3:$F$501,2,FALSE)&F873&\"_\"&VLOOKUP(G873,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_WVCS"},"LPAU05G01_WVCS AT%M1534.0 :INT; (*P新风机组05G01-水阀控制转换值*)","LPAU05G01_WVCS          AT%M1534.0     :INT; (*P新风机组05G01-水阀控制转换值*)"]
["1536.0","验证通过","BOOL","P新风机组","L","05G01","程序控制","P新风机组05G01-程序控制",{"$f":"E874&VLOOKUP(D874,list!$D$3:$F$501,2,FALSE)&F874&\"_\"&VLOOKUP(G874,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_PC"},"LPAU05G01_PC AT%M1536.0 :BOOL; (*P新风机组05G01-程序控制*)","LPAU05G01_PC            AT%M1536.0     :BOOL; (*P新风机组05G01-程序控制*)"]
["1538.0","验证通过","INT","P新风机组","L","05G01","变频手动控制值","P新风机组05G01-变频手动控制值",{"$f":"E875&VLOOKUP(D875,list!$D$3:$F$501,2,FALSE)&F875&\"_\"&VLOOKUP(G875,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_VFMV"},"LPAU05G01_VFMV AT%M1538.0 :INT; (*P新风机组05G01-变频手动控制值*)","LPAU05G01_VFMV          AT%M1538.0     :INT; (*P新风机组05G01-变频手动控制值*)"]
["1540.0","验证通过","BOOL","P新风机组","L","05G01","低温断路报警隔离","P新风机组05G01-低温断路报警隔离",{"$f":"E876&VLOOKUP(D876,list!$D$3:$F$501,2,FALSE)&F876&\"_\"&VLOOKUP(G876,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_ISO3"},"LPAU05G01_ISO3 AT%M1540.0 :BOOL; (*P新风机组05G01-低温断路报警隔离*)","LPAU05G01_ISO3          AT%M1540.0     :BOOL; (*P新风机组05G01-低温断路报警隔离*)"]
["1542.0","验证通过","INT","P新风机组","L","05G01","变频器频率控制值","P新风机组05G01-变频器频率控制值",{"$f":"E877&VLOOKUP(D877,list!$D$3:$F$501,2,FALSE)&F877&\"_\"&VLOOKUP(G877,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_VFCS"},"LPAU05G01_VFCS AT%M1542.0 :INT; (*P新风机组05G01-变频器频率控制值*)","LPAU05G01_VFCS          AT%M1542.0     :INT; (*P新风机组05G01-变频器频率控制值*)"]
["1544.0","验证通过","INT","P新风机组","L","05G01","变频器频率反馈值","P新风机组05G01-变频器频率反馈值",{"$f":"E878&VLOOKUP(D878,list!$D$3:$F$501,2,FALSE)&F878&\"_\"&VLOOKUP(G878,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_VFBS"},"LPAU05G01_VFBS AT%M1544.0 :INT; (*P新风机组05G01-变频器频率反馈值*)","LPAU05G01_VFBS          AT%M1544.0     :INT; (*P新风机组05G01-变频器频率反馈值*)"]
["1546.0","验证通过","BOOL","P新风机组","L","05G01","联动模式","P新风机组05G01-联动模式",{"$f":"E879&VLOOKUP(D879,list!$D$3:$F$501,2,FALSE)&F879&\"_\"&VLOOKUP(G879,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_LM"},"LPAU05G01_LM AT%M1546.0 :BOOL; (*P新风机组05G01-联动模式*)","LPAU05G01_LM            AT%M1546.0     :BOOL; (*P新风机组05G01-联动模式*)"]
["1548.0","验证通过","BOOL","P新风机组","L","05G01","全天候模式","P新风机组05G01-全天候模式",{"$f":"E880&VLOOKUP(D880,list!$D$3:$F$501,2,FALSE)&F880&\"_\"&VLOOKUP(G880,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_DM"},"LPAU05G01_DM AT%M1548.0 :BOOL; (*P新风机组05G01-全天候模式*)","LPAU05G01_DM            AT%M1548.0     :BOOL; (*P新风机组05G01-全天候模式*)"]
["1552.0","验证通过","REAL","P新风机组","L","05G01","CO2设定值","P新风机组05G01-CO2设定值",{"$f":"E881&VLOOKUP(D881,list!$D$3:$F$501,2,FALSE)&F881&\"_\"&VLOOKUP(G881,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_CO2SET"},"LPAU05G01_CO2SET AT%M1552.0 :REAL; (*P新风机组05G01-CO2设定值*)","LPAU05G01_CO2SET        AT%M1552.0     :REAL; (*P新风机组05G01-CO2设定值*)"]
["1556.0","验证通过","BOOL","P新风机组","L","05G01","定时控制","P新风机组05G01-定时控制",{"$f":"E882&VLOOKUP(D882,list!$D$3:$F$501,2,FALSE)&F882&\"_\"&VLOOKUP(G882,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_TC"},"LPAU05G01_TC AT%M1556.0 :BOOL; (*P新风机组05G01-定时控制*)","LPAU05G01_TC            AT%M1556.0     :BOOL; (*P新风机组05G01-定时控制*)"]
["1558.0","验证通过","BOOL","P新风机组","L","05G01","定时模式","P新风机组05G01-定时模式",{"$f":"E883&VLOOKUP(D883,list!$D$3:$F$501,2,FALSE)&F883&\"_\"&VLOOKUP(G883,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G01_TM"},"LPAU05G01_TM AT%M1558.0 :BOOL; (*P新风机组05G01-定时模式*)","LPAU05G01_TM            AT%M1558.0     :BOOL; (*P新风机组05G01-定时模式*)"]
["PAU"]
[{"$f":"IF(OR(C883=\"REAL\",C883=\"DWORD\",C883=\"DINT\"),(IF(OR(C885=\"REAL\",C885=\"DWORD\",C885=\"DINT\"),A883+4+MOD(A883,4),A883+4)),(IF(OR(C885=\"REAL\",C885=\"DWORD\",C885=\"DINT\"),A883+4+MOD(A883,4),A883+2)))&\".0\"","v":"1564.0"},{"$f":"IF((IF(OR(C885=\"INT\",C885=\"WORD\",C885=\"BOOL\"),MOD(A885,2),MOD(A885,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05G02","设定温度值",{"$f":"D885&F885&\"-\"&IF(E885=\"R\",\"新云平台\"&G885,G885)","v":"P新风机组05G02-新云平台设定温度值"},{"$f":"E885&VLOOKUP(D885,list!$D$3:$F$501,2,FALSE)&F885&\"_\"&VLOOKUP(G885,list!$I$2:$K$502,2,FALSE)","v":"RPAU05G02_TSET"},{"$f":"I885&\" \"&\"AT%M\"&A885&\" \"&\":\"&C885&\";\"&\" \"&\"(*\"&H885&\"*)\"","v":"RPAU05G02_TSET AT%M1564.0 :REAL; (*P新风机组05G02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J885,SEARCH(\"AT%\",J885),,REPT(\" \",25-SEARCH(\"AT%\",J885))),SEARCH(\":\",REPLACE(J885,SEARCH(\"AT%\",J885),,REPT(\" \",25-SEARCH(\"AT%\",J885)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J885,SEARCH(\"AT%\",J885),,REPT(\" \",25-SEARCH(\"AT%\",J885))))))","v":"RPAU05G02_TSET          AT%M1564.0     :REAL; (*P新风机组05G02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C885=\"REAL\",C885=\"DWORD\",C885=\"DINT\"),(IF(OR(C886=\"REAL\",C886=\"DWORD\",C886=\"DINT\"),A885+4+MOD(A885,4),A885+4)),(IF(OR(C886=\"REAL\",C886=\"DWORD\",C886=\"DINT\"),A885+4+MOD(A885,4),A885+2)))&\".0\"","v":"1568.0"},"验证通过","INT","P新风机组","R",{"$f":"F885","v":"05G02"},"季节模式","P新风机组05G02-新云平台季节模式",{"$f":"E886&VLOOKUP(D886,list!$D$3:$F$501,2,FALSE)&F886&\"_\"&VLOOKUP(G886,list!$I$2:$K$502,2,FALSE)","v":"RPAU05G02_SM"},"RPAU05G02_SM AT%M1568.0 :INT; (*P新风机组05G02-新云平台季节模式*)","RPAU05G02_SM            AT%M1568.0     :INT; (*P新风机组05G02-新云平台季节模式*)"]
["1570.0","验证通过","BOOL","P新风机组","R","05G02","程序控制","P新风机组05G02-新云平台程序控制",{"$f":"E887&VLOOKUP(D887,list!$D$3:$F$501,2,FALSE)&F887&\"_\"&VLOOKUP(G887,list!$I$2:$K$502,2,FALSE)","v":"RPAU05G02_PC"},"RPAU05G02_PC AT%M1570.0 :BOOL; (*P新风机组05G02-新云平台程序控制*)","RPAU05G02_PC            AT%M1570.0     :BOOL; (*P新风机组05G02-新云平台程序控制*)"]
["1576.0","验证通过","REAL","P新风机组","L","05G02","设定温度值","P新风机组05G02-设定温度值",{"$f":"E888&VLOOKUP(D888,list!$D$3:$F$501,2,FALSE)&F888&\"_\"&VLOOKUP(G888,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_TSET"},"LPAU05G02_TSET AT%M1576.0 :REAL; (*P新风机组05G02-设定温度值*)","LPAU05G02_TSET          AT%M1576.0     :REAL; (*P新风机组05G02-设定温度值*)"]
["1580.0","验证通过","INT","P新风机组","L","05G02","季节模式","P新风机组05G02-季节模式",{"$f":"E889&VLOOKUP(D889,list!$D$3:$F$501,2,FALSE)&F889&\"_\"&VLOOKUP(G889,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_SM"},"LPAU05G02_SM AT%M1580.0 :INT; (*P新风机组05G02-季节模式*)","LPAU05G02_SM            AT%M1580.0     :INT; (*P新风机组05G02-季节模式*)"]
["1584.0","验证通过","REAL","P新风机组","L","05G02","水阀反馈换算值","P新风机组05G02-水阀反馈换算值",{"$f":"E890&VLOOKUP(D890,list!$D$3:$F$501,2,FALSE)&F890&\"_\"&VLOOKUP(G890,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_WVBS"},"LPAU05G02_WVBS AT%M1584.0 :REAL; (*P新风机组05G02-水阀反馈换算值*)","LPAU05G02_WVBS          AT%M1584.0     :REAL; (*P新风机组05G02-水阀反馈换算值*)"]
["1588.0","验证通过","BOOL","P新风机组","L","05G02","水阀手动控制","P新风机组05G02-水阀手动控制",{"$f":"E891&VLOOKUP(D891,list!$D$3:$F$501,2,FALSE)&F891&\"_\"&VLOOKUP(G891,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_WVMC"},"LPAU05G02_WVMC AT%M1588.0 :BOOL; (*P新风机组05G02-水阀手动控制*)","LPAU05G02_WVMC          AT%M1588.0     :BOOL; (*P新风机组05G02-水阀手动控制*)"]
["1592.0","验证通过","REAL","P新风机组","L","05G02","水阀手动控制值","P新风机组05G02-水阀手动控制值",{"$f":"E892&VLOOKUP(D892,list!$D$3:$F$501,2,FALSE)&F892&\"_\"&VLOOKUP(G892,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_WVMV"},"LPAU05G02_WVMV AT%M1592.0 :REAL; (*P新风机组05G02-水阀手动控制值*)","LPAU05G02_WVMV          AT%M1592.0     :REAL; (*P新风机组05G02-水阀手动控制值*)"]
["1596.0","验证通过","REAL","P新风机组","L","05G02","送风温度换算值","P新风机组05G02-送风温度换算值",{"$f":"E893&VLOOKUP(D893,list!$D$3:$F$501,2,FALSE)&F893&\"_\"&VLOOKUP(G893,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_STS"},"LPAU05G02_STS AT%M1596.0 :REAL; (*P新风机组05G02-送风温度换算值*)","LPAU05G02_STS           AT%M1596.0     :REAL; (*P新风机组05G02-送风温度换算值*)"]
["1600.0","验证通过","BOOL","P新风机组","L","05G02","运行时间累积重置","P新风机组05G02-运行时间累积重置",{"$f":"E894&VLOOKUP(D894,list!$D$3:$F$501,2,FALSE)&F894&\"_\"&VLOOKUP(G894,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_RST"},"LPAU05G02_RST AT%M1600.0 :BOOL; (*P新风机组05G02-运行时间累积重置*)","LPAU05G02_RST           AT%M1600.0     :BOOL; (*P新风机组05G02-运行时间累积重置*)"]
["1604.0","验证通过","REAL","P新风机组","L","05G02","运行时间累积重置值","P新风机组05G02-运行时间累积重置值",{"$f":"E895&VLOOKUP(D895,list!$D$3:$F$501,2,FALSE)&F895&\"_\"&VLOOKUP(G895,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_RSTV"},"LPAU05G02_RSTV AT%M1604.0 :REAL; (*P新风机组05G02-运行时间累积重置值*)","LPAU05G02_RSTV          AT%M1604.0     :REAL; (*P新风机组05G02-运行时间累积重置值*)"]
["1608.0","验证通过","BOOL","P新风机组","L","05G02","隔离开关1","P新风机组05G02-隔离开关1",{"$f":"E896&VLOOKUP(D896,list!$D$3:$F$501,2,FALSE)&F896&\"_\"&VLOOKUP(G896,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_ISO1"},"LPAU05G02_ISO1 AT%M1608.0 :BOOL; (*P新风机组05G02-隔离开关1*)","LPAU05G02_ISO1          AT%M1608.0     :BOOL; (*P新风机组05G02-隔离开关1*)"]
["1610.0","验证通过","BOOL","P新风机组","L","05G02","隔离开关2","P新风机组05G02-隔离开关2",{"$f":"E897&VLOOKUP(D897,list!$D$3:$F$501,2,FALSE)&F897&\"_\"&VLOOKUP(G897,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_ISO2"},"LPAU05G02_ISO2 AT%M1610.0 :BOOL; (*P新风机组05G02-隔离开关2*)","LPAU05G02_ISO2          AT%M1610.0     :BOOL; (*P新风机组05G02-隔离开关2*)"]
["1616.0","验证通过","REAL","P新风机组","L","05G02","P调节参数","P新风机组05G02-P调节参数",{"$f":"E898&VLOOKUP(D898,list!$D$3:$F$501,2,FALSE)&F898&\"_\"&VLOOKUP(G898,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_VP"},"LPAU05G02_VP AT%M1616.0 :REAL; (*P新风机组05G02-P调节参数*)","LPAU05G02_VP            AT%M1616.0     :REAL; (*P新风机组05G02-P调节参数*)"]
["1620.0","验证通过","REAL","P新风机组","L","05G02","I调节参数","P新风机组05G02-I调节参数",{"$f":"E899&VLOOKUP(D899,list!$D$3:$F$501,2,FALSE)&F899&\"_\"&VLOOKUP(G899,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_VI"},"LPAU05G02_VI AT%M1620.0 :REAL; (*P新风机组05G02-I调节参数*)","LPAU05G02_VI            AT%M1620.0     :REAL; (*P新风机组05G02-I调节参数*)"]
["1624.0","验证通过","REAL","P新风机组","L","05G02","运行时间累积值","P新风机组05G02-运行时间累积值",{"$f":"E900&VLOOKUP(D900,list!$D$3:$F$501,2,FALSE)&F900&\"_\"&VLOOKUP(G900,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_RH"},"LPAU05G02_RH AT%M1624.0 :REAL; (*P新风机组05G02-运行时间累积值*)","LPAU05G02_RH            AT%M1624.0     :REAL; (*P新风机组05G02-运行时间累积值*)"]
["1628.0","验证通过","INT","P新风机组","L","05G02","设备状态代码","P新风机组05G02-设备状态代码",{"$f":"E901&VLOOKUP(D901,list!$D$3:$F$501,2,FALSE)&F901&\"_\"&VLOOKUP(G901,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_SN"},"LPAU05G02_SN AT%M1628.0 :INT; (*P新风机组05G02-设备状态代码*)","LPAU05G02_SN            AT%M1628.0     :INT; (*P新风机组05G02-设备状态代码*)"]
["1630.0","验证通过","INT","P新风机组","L","05G02","水阀控制转换值","P新风机组05G02-水阀控制转换值",{"$f":"E902&VLOOKUP(D902,list!$D$3:$F$501,2,FALSE)&F902&\"_\"&VLOOKUP(G902,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_WVCS"},"LPAU05G02_WVCS AT%M1630.0 :INT; (*P新风机组05G02-水阀控制转换值*)","LPAU05G02_WVCS          AT%M1630.0     :INT; (*P新风机组05G02-水阀控制转换值*)"]
["1632.0","验证通过","BOOL","P新风机组","L","05G02","程序控制","P新风机组05G02-程序控制",{"$f":"E903&VLOOKUP(D903,list!$D$3:$F$501,2,FALSE)&F903&\"_\"&VLOOKUP(G903,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_PC"},"LPAU05G02_PC AT%M1632.0 :BOOL; (*P新风机组05G02-程序控制*)","LPAU05G02_PC            AT%M1632.0     :BOOL; (*P新风机组05G02-程序控制*)"]
["1634.0","验证通过","INT","P新风机组","L","05G02","变频手动控制值","P新风机组05G02-变频手动控制值",{"$f":"E904&VLOOKUP(D904,list!$D$3:$F$501,2,FALSE)&F904&\"_\"&VLOOKUP(G904,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_VFMV"},"LPAU05G02_VFMV AT%M1634.0 :INT; (*P新风机组05G02-变频手动控制值*)","LPAU05G02_VFMV          AT%M1634.0     :INT; (*P新风机组05G02-变频手动控制值*)"]
["1636.0","验证通过","BOOL","P新风机组","L","05G02","低温断路报警隔离","P新风机组05G02-低温断路报警隔离",{"$f":"E905&VLOOKUP(D905,list!$D$3:$F$501,2,FALSE)&F905&\"_\"&VLOOKUP(G905,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_ISO3"},"LPAU05G02_ISO3 AT%M1636.0 :BOOL; (*P新风机组05G02-低温断路报警隔离*)","LPAU05G02_ISO3          AT%M1636.0     :BOOL; (*P新风机组05G02-低温断路报警隔离*)"]
["1638.0","验证通过","INT","P新风机组","L","05G02","变频器频率控制值","P新风机组05G02-变频器频率控制值",{"$f":"E906&VLOOKUP(D906,list!$D$3:$F$501,2,FALSE)&F906&\"_\"&VLOOKUP(G906,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_VFCS"},"LPAU05G02_VFCS AT%M1638.0 :INT; (*P新风机组05G02-变频器频率控制值*)","LPAU05G02_VFCS          AT%M1638.0     :INT; (*P新风机组05G02-变频器频率控制值*)"]
["1640.0","验证通过","INT","P新风机组","L","05G02","变频器频率反馈值","P新风机组05G02-变频器频率反馈值",{"$f":"E907&VLOOKUP(D907,list!$D$3:$F$501,2,FALSE)&F907&\"_\"&VLOOKUP(G907,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_VFBS"},"LPAU05G02_VFBS AT%M1640.0 :INT; (*P新风机组05G02-变频器频率反馈值*)","LPAU05G02_VFBS          AT%M1640.0     :INT; (*P新风机组05G02-变频器频率反馈值*)"]
["1642.0","验证通过","BOOL","P新风机组","L","05G02","联动模式","P新风机组05G02-联动模式",{"$f":"E908&VLOOKUP(D908,list!$D$3:$F$501,2,FALSE)&F908&\"_\"&VLOOKUP(G908,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_LM"},"LPAU05G02_LM AT%M1642.0 :BOOL; (*P新风机组05G02-联动模式*)","LPAU05G02_LM            AT%M1642.0     :BOOL; (*P新风机组05G02-联动模式*)"]
["1644.0","验证通过","BOOL","P新风机组","L","05G02","全天候模式","P新风机组05G02-全天候模式",{"$f":"E909&VLOOKUP(D909,list!$D$3:$F$501,2,FALSE)&F909&\"_\"&VLOOKUP(G909,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_DM"},"LPAU05G02_DM AT%M1644.0 :BOOL; (*P新风机组05G02-全天候模式*)","LPAU05G02_DM            AT%M1644.0     :BOOL; (*P新风机组05G02-全天候模式*)"]
["1648.0","验证通过","REAL","P新风机组","L","05G02","CO2设定值","P新风机组05G02-CO2设定值",{"$f":"E910&VLOOKUP(D910,list!$D$3:$F$501,2,FALSE)&F910&\"_\"&VLOOKUP(G910,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_CO2SET"},"LPAU05G02_CO2SET AT%M1648.0 :REAL; (*P新风机组05G02-CO2设定值*)","LPAU05G02_CO2SET        AT%M1648.0     :REAL; (*P新风机组05G02-CO2设定值*)"]
["1652.0","验证通过","BOOL","P新风机组","L","05G02","定时控制","P新风机组05G02-定时控制",{"$f":"E911&VLOOKUP(D911,list!$D$3:$F$501,2,FALSE)&F911&\"_\"&VLOOKUP(G911,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_TC"},"LPAU05G02_TC AT%M1652.0 :BOOL; (*P新风机组05G02-定时控制*)","LPAU05G02_TC            AT%M1652.0     :BOOL; (*P新风机组05G02-定时控制*)"]
["1654.0","验证通过","BOOL","P新风机组","L","05G02","定时模式","P新风机组05G02-定时模式",{"$f":"E912&VLOOKUP(D912,list!$D$3:$F$501,2,FALSE)&F912&\"_\"&VLOOKUP(G912,list!$I$2:$K$502,2,FALSE)","v":"LPAU05G02_TM"},"LPAU05G02_TM AT%M1654.0 :BOOL; (*P新风机组05G02-定时模式*)","LPAU05G02_TM            AT%M1654.0     :BOOL; (*P新风机组05G02-定时模式*)"]
["AHU"]
[{"$f":"IF(OR(C827=\"REAL\",C827=\"DWORD\",C827=\"DINT\"),(IF(OR(C914=\"REAL\",C914=\"DWORD\",C914=\"DINT\"),A827+4+MOD(A827,4),A827+4)),(IF(OR(C914=\"REAL\",C914=\"DWORD\",C914=\"DINT\"),A827+4+MOD(A827,4),A827+2)))&\".0\"","v":"1380.0"},{"$f":"IF((IF(OR(C914=\"INT\",C914=\"WORD\",C914=\"BOOL\"),MOD(A914,2),MOD(A914,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04C08","设定温度值",{"$f":"D914&F914&\"-\"&IF(E914=\"R\",\"新云平台\"&G914,G914)","v":"空调机组04C08-新云平台设定温度值"},{"$f":"E914&VLOOKUP(D914,list!$D$3:$F$501,2,FALSE)&F914&\"_\"&VLOOKUP(G914,list!$I$2:$K$502,2,FALSE)","v":"RAHU04C08_TSET"},{"$f":"I914&\" \"&\"AT%M\"&A914&\" \"&\":\"&C914&\";\"&\" \"&\"(*\"&H914&\"*)\"","v":"RAHU04C08_TSET AT%M1380.0 :REAL; (*空调机组04C08-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J914,SEARCH(\"AT%\",J914),,REPT(\" \",25-SEARCH(\"AT%\",J914))),SEARCH(\":\",REPLACE(J914,SEARCH(\"AT%\",J914),,REPT(\" \",25-SEARCH(\"AT%\",J914)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J914,SEARCH(\"AT%\",J914),,REPT(\" \",25-SEARCH(\"AT%\",J914))))))","v":"RAHU04C08_TSET          AT%M1380.0     :REAL; (*空调机组04C08-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C914=\"REAL\",C914=\"DWORD\",C914=\"DINT\"),(IF(OR(C915=\"REAL\",C915=\"DWORD\",C915=\"DINT\"),A914+4+MOD(A914,4),A914+4)),(IF(OR(C915=\"REAL\",C915=\"DWORD\",C915=\"DINT\"),A914+4+MOD(A914,4),A914+2)))&\".0\"","v":"1384.0"},"验证通过","INT","空调机组","R",{"$f":"F914","v":"04C08"},"季节模式","空调机组04C08-新云平台季节模式",{"$f":"E915&VLOOKUP(D915,list!$D$3:$F$501,2,FALSE)&F915&\"_\"&VLOOKUP(G915,list!$I$2:$K$502,2,FALSE)","v":"RAHU04C08_SM"},"RAHU04C08_SM AT%M1384.0 :INT; (*空调机组04C08-新云平台季节模式*)","RAHU04C08_SM            AT%M1384.0     :INT; (*空调机组04C08-新云平台季节模式*)"]
["1386.0","验证通过","BOOL","空调机组","R","04C08","程序控制","空调机组04C08-新云平台程序控制",{"$f":"E916&VLOOKUP(D916,list!$D$3:$F$501,2,FALSE)&F916&\"_\"&VLOOKUP(G916,list!$I$2:$K$502,2,FALSE)","v":"RAHU04C08_PC"},"RAHU04C08_PC AT%M1386.0 :BOOL; (*空调机组04C08-新云平台程序控制*)","RAHU04C08_PC            AT%M1386.0     :BOOL; (*空调机组04C08-新云平台程序控制*)"]
["1392.0","验证通过","REAL","空调机组","L","04C08","设定温度值","空调机组04C08-设定温度值",{"$f":"E917&VLOOKUP(D917,list!$D$3:$F$501,2,FALSE)&F917&\"_\"&VLOOKUP(G917,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_TSET"},"LAHU04C08_TSET AT%M1392.0 :REAL; (*空调机组04C08-设定温度值*)","LAHU04C08_TSET          AT%M1392.0     :REAL; (*空调机组04C08-设定温度值*)"]
["1396.0","验证通过","INT","空调机组","L","04C08","季节模式","空调机组04C08-季节模式",{"$f":"E918&VLOOKUP(D918,list!$D$3:$F$501,2,FALSE)&F918&\"_\"&VLOOKUP(G918,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_SM"},"LAHU04C08_SM AT%M1396.0 :INT; (*空调机组04C08-季节模式*)","LAHU04C08_SM            AT%M1396.0     :INT; (*空调机组04C08-季节模式*)"]
["1400.0","验证通过","REAL","空调机组","L","04C08","水阀反馈换算值","空调机组04C08-水阀反馈换算值",{"$f":"E919&VLOOKUP(D919,list!$D$3:$F$501,2,FALSE)&F919&\"_\"&VLOOKUP(G919,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_WVBS"},"LAHU04C08_WVBS AT%M1400.0 :REAL; (*空调机组04C08-水阀反馈换算值*)","LAHU04C08_WVBS          AT%M1400.0     :REAL; (*空调机组04C08-水阀反馈换算值*)"]
["1404.0","验证通过","BOOL","空调机组","L","04C08","水阀手动控制","空调机组04C08-水阀手动控制",{"$f":"E920&VLOOKUP(D920,list!$D$3:$F$501,2,FALSE)&F920&\"_\"&VLOOKUP(G920,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_WVMC"},"LAHU04C08_WVMC AT%M1404.0 :BOOL; (*空调机组04C08-水阀手动控制*)","LAHU04C08_WVMC          AT%M1404.0     :BOOL; (*空调机组04C08-水阀手动控制*)"]
["1408.0","验证通过","REAL","空调机组","L","04C08","水阀手动控制值","空调机组04C08-水阀手动控制值",{"$f":"E921&VLOOKUP(D921,list!$D$3:$F$501,2,FALSE)&F921&\"_\"&VLOOKUP(G921,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_WVMV"},"LAHU04C08_WVMV AT%M1408.0 :REAL; (*空调机组04C08-水阀手动控制值*)","LAHU04C08_WVMV          AT%M1408.0     :REAL; (*空调机组04C08-水阀手动控制值*)"]
["1412.0","验证通过","REAL","空调机组","L","04C08","回风温度换算值","空调机组04C08-回风温度换算值",{"$f":"E922&VLOOKUP(D922,list!$D$3:$F$501,2,FALSE)&F922&\"_\"&VLOOKUP(G922,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_RTS"},"LAHU04C08_RTS AT%M1412.0 :REAL; (*空调机组04C08-回风温度换算值*)","LAHU04C08_RTS           AT%M1412.0     :REAL; (*空调机组04C08-回风温度换算值*)"]
["1416.0","验证通过","BOOL","空调机组","L","04C08","运行时间累积重置","空调机组04C08-运行时间累积重置",{"$f":"E923&VLOOKUP(D923,list!$D$3:$F$501,2,FALSE)&F923&\"_\"&VLOOKUP(G923,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_RST"},"LAHU04C08_RST AT%M1416.0 :BOOL; (*空调机组04C08-运行时间累积重置*)","LAHU04C08_RST           AT%M1416.0     :BOOL; (*空调机组04C08-运行时间累积重置*)"]
["1420.0","验证通过","REAL","空调机组","L","04C08","运行时间累积重置值","空调机组04C08-运行时间累积重置值",{"$f":"E924&VLOOKUP(D924,list!$D$3:$F$501,2,FALSE)&F924&\"_\"&VLOOKUP(G924,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_RSTV"},"LAHU04C08_RSTV AT%M1420.0 :REAL; (*空调机组04C08-运行时间累积重置值*)","LAHU04C08_RSTV          AT%M1420.0     :REAL; (*空调机组04C08-运行时间累积重置值*)"]
["1424.0","验证通过","BOOL","空调机组","L","04C08","隔离开关1","空调机组04C08-隔离开关1",{"$f":"E925&VLOOKUP(D925,list!$D$3:$F$501,2,FALSE)&F925&\"_\"&VLOOKUP(G925,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_ISO1"},"LAHU04C08_ISO1 AT%M1424.0 :BOOL; (*空调机组04C08-隔离开关1*)","LAHU04C08_ISO1          AT%M1424.0     :BOOL; (*空调机组04C08-隔离开关1*)"]
["1426.0","验证通过","BOOL","空调机组","L","04C08","隔离开关2","空调机组04C08-隔离开关2",{"$f":"E926&VLOOKUP(D926,list!$D$3:$F$501,2,FALSE)&F926&\"_\"&VLOOKUP(G926,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_ISO2"},"LAHU04C08_ISO2 AT%M1426.0 :BOOL; (*空调机组04C08-隔离开关2*)","LAHU04C08_ISO2          AT%M1426.0     :BOOL; (*空调机组04C08-隔离开关2*)"]
["1432.0","验证通过","REAL","空调机组","L","04C08","P调节参数","空调机组04C08-P调节参数",{"$f":"E927&VLOOKUP(D927,list!$D$3:$F$501,2,FALSE)&F927&\"_\"&VLOOKUP(G927,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_VP"},"LAHU04C08_VP AT%M1432.0 :REAL; (*空调机组04C08-P调节参数*)","LAHU04C08_VP            AT%M1432.0     :REAL; (*空调机组04C08-P调节参数*)"]
["1436.0","验证通过","REAL","空调机组","L","04C08","I调节参数","空调机组04C08-I调节参数",{"$f":"E928&VLOOKUP(D928,list!$D$3:$F$501,2,FALSE)&F928&\"_\"&VLOOKUP(G928,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_VI"},"LAHU04C08_VI AT%M1436.0 :REAL; (*空调机组04C08-I调节参数*)","LAHU04C08_VI            AT%M1436.0     :REAL; (*空调机组04C08-I调节参数*)"]
["1440.0","验证通过","REAL","空调机组","L","04C08","运行时间累积值","空调机组04C08-运行时间累积值",{"$f":"E929&VLOOKUP(D929,list!$D$3:$F$501,2,FALSE)&F929&\"_\"&VLOOKUP(G929,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_RH"},"LAHU04C08_RH AT%M1440.0 :REAL; (*空调机组04C08-运行时间累积值*)","LAHU04C08_RH            AT%M1440.0     :REAL; (*空调机组04C08-运行时间累积值*)"]
["1444.0","验证通过","INT","空调机组","L","04C08","设备状态代码","空调机组04C08-设备状态代码",{"$f":"E930&VLOOKUP(D930,list!$D$3:$F$501,2,FALSE)&F930&\"_\"&VLOOKUP(G930,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_SN"},"LAHU04C08_SN AT%M1444.0 :INT; (*空调机组04C08-设备状态代码*)","LAHU04C08_SN            AT%M1444.0     :INT; (*空调机组04C08-设备状态代码*)"]
["1446.0","验证通过","INT","空调机组","L","04C08","水阀控制转换值","空调机组04C08-水阀控制转换值",{"$f":"E931&VLOOKUP(D931,list!$D$3:$F$501,2,FALSE)&F931&\"_\"&VLOOKUP(G931,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_WVCS"},"LAHU04C08_WVCS AT%M1446.0 :INT; (*空调机组04C08-水阀控制转换值*)","LAHU04C08_WVCS          AT%M1446.0     :INT; (*空调机组04C08-水阀控制转换值*)"]
["1448.0","验证通过","BOOL","空调机组","L","04C08","程序控制","空调机组04C08-程序控制",{"$f":"E932&VLOOKUP(D932,list!$D$3:$F$501,2,FALSE)&F932&\"_\"&VLOOKUP(G932,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C08_PC"},"LAHU04C08_PC AT%M1448.0 :BOOL; (*空调机组04C08-程序控制*)","LAHU04C08_PC            AT%M1448.0     :BOOL; (*空调机组04C08-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C932=\"REAL\",C932=\"DWORD\",C932=\"DINT\"),(IF(OR(C934=\"REAL\",C934=\"DWORD\",C934=\"DINT\"),A932+4+MOD(A932,4),A932+4)),(IF(OR(C934=\"REAL\",C934=\"DWORD\",C934=\"DINT\"),A932+4+MOD(A932,4),A932+2)))&\".0\"","v":"1452.0"},{"$f":"IF((IF(OR(C934=\"INT\",C934=\"WORD\",C934=\"BOOL\"),MOD(A934,2),MOD(A934,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","04C09","设定温度值",{"$f":"D934&F934&\"-\"&IF(E934=\"R\",\"新云平台\"&G934,G934)","v":"空调机组04C09-新云平台设定温度值"},{"$f":"E934&VLOOKUP(D934,list!$D$3:$F$501,2,FALSE)&F934&\"_\"&VLOOKUP(G934,list!$I$2:$K$502,2,FALSE)","v":"RAHU04C09_TSET"},{"$f":"I934&\" \"&\"AT%M\"&A934&\" \"&\":\"&C934&\";\"&\" \"&\"(*\"&H934&\"*)\"","v":"RAHU04C09_TSET AT%M1452.0 :REAL; (*空调机组04C09-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J934,SEARCH(\"AT%\",J934),,REPT(\" \",25-SEARCH(\"AT%\",J934))),SEARCH(\":\",REPLACE(J934,SEARCH(\"AT%\",J934),,REPT(\" \",25-SEARCH(\"AT%\",J934)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J934,SEARCH(\"AT%\",J934),,REPT(\" \",25-SEARCH(\"AT%\",J934))))))","v":"RAHU04C09_TSET          AT%M1452.0     :REAL; (*空调机组04C09-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C934=\"REAL\",C934=\"DWORD\",C934=\"DINT\"),(IF(OR(C935=\"REAL\",C935=\"DWORD\",C935=\"DINT\"),A934+4+MOD(A934,4),A934+4)),(IF(OR(C935=\"REAL\",C935=\"DWORD\",C935=\"DINT\"),A934+4+MOD(A934,4),A934+2)))&\".0\"","v":"1456.0"},"验证通过","INT","空调机组","R",{"$f":"F934","v":"04C09"},"季节模式","空调机组04C09-新云平台季节模式",{"$f":"E935&VLOOKUP(D935,list!$D$3:$F$501,2,FALSE)&F935&\"_\"&VLOOKUP(G935,list!$I$2:$K$502,2,FALSE)","v":"RAHU04C09_SM"},"RAHU04C09_SM AT%M1456.0 :INT; (*空调机组04C09-新云平台季节模式*)","RAHU04C09_SM            AT%M1456.0     :INT; (*空调机组04C09-新云平台季节模式*)"]
["1458.0","验证通过","BOOL","空调机组","R","04C09","程序控制","空调机组04C09-新云平台程序控制",{"$f":"E936&VLOOKUP(D936,list!$D$3:$F$501,2,FALSE)&F936&\"_\"&VLOOKUP(G936,list!$I$2:$K$502,2,FALSE)","v":"RAHU04C09_PC"},"RAHU04C09_PC AT%M1458.0 :BOOL; (*空调机组04C09-新云平台程序控制*)","RAHU04C09_PC            AT%M1458.0     :BOOL; (*空调机组04C09-新云平台程序控制*)"]
["1464.0","验证通过","REAL","空调机组","L","04C09","设定温度值","空调机组04C09-设定温度值",{"$f":"E937&VLOOKUP(D937,list!$D$3:$F$501,2,FALSE)&F937&\"_\"&VLOOKUP(G937,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_TSET"},"LAHU04C09_TSET AT%M1464.0 :REAL; (*空调机组04C09-设定温度值*)","LAHU04C09_TSET          AT%M1464.0     :REAL; (*空调机组04C09-设定温度值*)"]
["1468.0","验证通过","INT","空调机组","L","04C09","季节模式","空调机组04C09-季节模式",{"$f":"E938&VLOOKUP(D938,list!$D$3:$F$501,2,FALSE)&F938&\"_\"&VLOOKUP(G938,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_SM"},"LAHU04C09_SM AT%M1468.0 :INT; (*空调机组04C09-季节模式*)","LAHU04C09_SM            AT%M1468.0     :INT; (*空调机组04C09-季节模式*)"]
["1472.0","验证通过","REAL","空调机组","L","04C09","水阀反馈换算值","空调机组04C09-水阀反馈换算值",{"$f":"E939&VLOOKUP(D939,list!$D$3:$F$501,2,FALSE)&F939&\"_\"&VLOOKUP(G939,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_WVBS"},"LAHU04C09_WVBS AT%M1472.0 :REAL; (*空调机组04C09-水阀反馈换算值*)","LAHU04C09_WVBS          AT%M1472.0     :REAL; (*空调机组04C09-水阀反馈换算值*)"]
["1476.0","验证通过","BOOL","空调机组","L","04C09","水阀手动控制","空调机组04C09-水阀手动控制",{"$f":"E940&VLOOKUP(D940,list!$D$3:$F$501,2,FALSE)&F940&\"_\"&VLOOKUP(G940,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_WVMC"},"LAHU04C09_WVMC AT%M1476.0 :BOOL; (*空调机组04C09-水阀手动控制*)","LAHU04C09_WVMC          AT%M1476.0     :BOOL; (*空调机组04C09-水阀手动控制*)"]
["1480.0","验证通过","REAL","空调机组","L","04C09","水阀手动控制值","空调机组04C09-水阀手动控制值",{"$f":"E941&VLOOKUP(D941,list!$D$3:$F$501,2,FALSE)&F941&\"_\"&VLOOKUP(G941,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_WVMV"},"LAHU04C09_WVMV AT%M1480.0 :REAL; (*空调机组04C09-水阀手动控制值*)","LAHU04C09_WVMV          AT%M1480.0     :REAL; (*空调机组04C09-水阀手动控制值*)"]
["1484.0","验证通过","REAL","空调机组","L","04C09","回风温度换算值","空调机组04C09-回风温度换算值",{"$f":"E942&VLOOKUP(D942,list!$D$3:$F$501,2,FALSE)&F942&\"_\"&VLOOKUP(G942,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_RTS"},"LAHU04C09_RTS AT%M1484.0 :REAL; (*空调机组04C09-回风温度换算值*)","LAHU04C09_RTS           AT%M1484.0     :REAL; (*空调机组04C09-回风温度换算值*)"]
["1488.0","验证通过","BOOL","空调机组","L","04C09","运行时间累积重置","空调机组04C09-运行时间累积重置",{"$f":"E943&VLOOKUP(D943,list!$D$3:$F$501,2,FALSE)&F943&\"_\"&VLOOKUP(G943,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_RST"},"LAHU04C09_RST AT%M1488.0 :BOOL; (*空调机组04C09-运行时间累积重置*)","LAHU04C09_RST           AT%M1488.0     :BOOL; (*空调机组04C09-运行时间累积重置*)"]
["1492.0","验证通过","REAL","空调机组","L","04C09","运行时间累积重置值","空调机组04C09-运行时间累积重置值",{"$f":"E944&VLOOKUP(D944,list!$D$3:$F$501,2,FALSE)&F944&\"_\"&VLOOKUP(G944,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_RSTV"},"LAHU04C09_RSTV AT%M1492.0 :REAL; (*空调机组04C09-运行时间累积重置值*)","LAHU04C09_RSTV          AT%M1492.0     :REAL; (*空调机组04C09-运行时间累积重置值*)"]
["1496.0","验证通过","BOOL","空调机组","L","04C09","隔离开关1","空调机组04C09-隔离开关1",{"$f":"E945&VLOOKUP(D945,list!$D$3:$F$501,2,FALSE)&F945&\"_\"&VLOOKUP(G945,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_ISO1"},"LAHU04C09_ISO1 AT%M1496.0 :BOOL; (*空调机组04C09-隔离开关1*)","LAHU04C09_ISO1          AT%M1496.0     :BOOL; (*空调机组04C09-隔离开关1*)"]
["1498.0","验证通过","BOOL","空调机组","L","04C09","隔离开关2","空调机组04C09-隔离开关2",{"$f":"E946&VLOOKUP(D946,list!$D$3:$F$501,2,FALSE)&F946&\"_\"&VLOOKUP(G946,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_ISO2"},"LAHU04C09_ISO2 AT%M1498.0 :BOOL; (*空调机组04C09-隔离开关2*)","LAHU04C09_ISO2          AT%M1498.0     :BOOL; (*空调机组04C09-隔离开关2*)"]
["1504.0","验证通过","REAL","空调机组","L","04C09","P调节参数","空调机组04C09-P调节参数",{"$f":"E947&VLOOKUP(D947,list!$D$3:$F$501,2,FALSE)&F947&\"_\"&VLOOKUP(G947,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_VP"},"LAHU04C09_VP AT%M1504.0 :REAL; (*空调机组04C09-P调节参数*)","LAHU04C09_VP            AT%M1504.0     :REAL; (*空调机组04C09-P调节参数*)"]
["1508.0","验证通过","REAL","空调机组","L","04C09","I调节参数","空调机组04C09-I调节参数",{"$f":"E948&VLOOKUP(D948,list!$D$3:$F$501,2,FALSE)&F948&\"_\"&VLOOKUP(G948,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_VI"},"LAHU04C09_VI AT%M1508.0 :REAL; (*空调机组04C09-I调节参数*)","LAHU04C09_VI            AT%M1508.0     :REAL; (*空调机组04C09-I调节参数*)"]
["1512.0","验证通过","REAL","空调机组","L","04C09","运行时间累积值","空调机组04C09-运行时间累积值",{"$f":"E949&VLOOKUP(D949,list!$D$3:$F$501,2,FALSE)&F949&\"_\"&VLOOKUP(G949,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_RH"},"LAHU04C09_RH AT%M1512.0 :REAL; (*空调机组04C09-运行时间累积值*)","LAHU04C09_RH            AT%M1512.0     :REAL; (*空调机组04C09-运行时间累积值*)"]
["1516.0","验证通过","INT","空调机组","L","04C09","设备状态代码","空调机组04C09-设备状态代码",{"$f":"E950&VLOOKUP(D950,list!$D$3:$F$501,2,FALSE)&F950&\"_\"&VLOOKUP(G950,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_SN"},"LAHU04C09_SN AT%M1516.0 :INT; (*空调机组04C09-设备状态代码*)","LAHU04C09_SN            AT%M1516.0     :INT; (*空调机组04C09-设备状态代码*)"]
["1518.0","验证通过","INT","空调机组","L","04C09","水阀控制转换值","空调机组04C09-水阀控制转换值",{"$f":"E951&VLOOKUP(D951,list!$D$3:$F$501,2,FALSE)&F951&\"_\"&VLOOKUP(G951,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_WVCS"},"LAHU04C09_WVCS AT%M1518.0 :INT; (*空调机组04C09-水阀控制转换值*)","LAHU04C09_WVCS          AT%M1518.0     :INT; (*空调机组04C09-水阀控制转换值*)"]
["1520.0","验证通过","BOOL","空调机组","L","04C09","程序控制","空调机组04C09-程序控制",{"$f":"E952&VLOOKUP(D952,list!$D$3:$F$501,2,FALSE)&F952&\"_\"&VLOOKUP(G952,list!$I$2:$K$502,2,FALSE)","v":"LAHU04C09_PC"},"LAHU04C09_PC AT%M1520.0 :BOOL; (*空调机组04C09-程序控制*)","LAHU04C09_PC            AT%M1520.0     :BOOL; (*空调机组04C09-程序控制*)"]
["EAF"]
[{"$f":"IF(OR(C827=\"REAL\",C827=\"DWORD\",C827=\"DINT\"),(IF(OR(C954=\"REAL\",C954=\"DWORD\",C954=\"DINT\"),A827+4+MOD(A827,4),A827+4)),(IF(OR(C954=\"REAL\",C954=\"DWORD\",C954=\"DINT\"),A827+4+MOD(A827,4),A827+2)))&\".0\"","v":"1378.0"},{"$f":"IF((IF(OR(C954=\"INT\",C954=\"WORD\",C954=\"BOOL\"),MOD(A954,2),MOD(A954,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","04A01","启停控制",{"$f":"D954&F954&\"-\"&IF(E954=\"R\",\"新云平台\"&G954,G954)","v":"排风机04A01-新云平台启停控制"},{"$f":"E954&VLOOKUP(D954,[1]list!$D$3:$F$501,2,FALSE)&F954&\"_\"&VLOOKUP(G954,[1]list!$I$2:$K$502,2,FALSE)","v":"REAF04A01_C"},{"$f":"I954&\" \"&\"AT%M\"&A954&\" \"&\":\"&C954&\";\"&\" \"&\"(*\"&H954&\"*)\"","v":"REAF04A01_C AT%M1378.0 :BOOL; (*排风机04A01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J954,SEARCH(\"AT%\",J954),,REPT(\" \",25-SEARCH(\"AT%\",J954))),SEARCH(\":\",REPLACE(J954,SEARCH(\"AT%\",J954),,REPT(\" \",25-SEARCH(\"AT%\",J954)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J954,SEARCH(\"AT%\",J954),,REPT(\" \",25-SEARCH(\"AT%\",J954))))))","v":"REAF04A01_C             AT%M1378.0     :BOOL; (*排风机04A01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C954=\"REAL\",C954=\"DWORD\",C954=\"DINT\"),(IF(OR(C955=\"REAL\",C955=\"DWORD\",C955=\"DINT\"),A954+4+MOD(A954,4),A954+4)),(IF(OR(C955=\"REAL\",C955=\"DWORD\",C955=\"DINT\"),A954+4+MOD(A954,4),A954+2)))&\".0\"","v":"1380.0"},"验证通过","BOOL","排风机","L","01A01","运行时间累积重置","排风机01A01-运行时间累积重置",{"$f":"E955&VLOOKUP(D955,[1]list!$D$3:$F$501,2,FALSE)&F955&\"_\"&VLOOKUP(G955,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_RST"},"LEAF01A01_RST AT%M1380.0 :BOOL; (*排风机01A01-运行时间累积重置*)","LEAF01A01_RST           AT%M1380.0     :BOOL; (*排风机01A01-运行时间累积重置*)"]
["1384.0","验证通过","REAL","排风机","L","01A01","运行时间累积重置值","排风机01A01-运行时间累积重置值",{"$f":"E956&VLOOKUP(D956,[1]list!$D$3:$F$501,2,FALSE)&F956&\"_\"&VLOOKUP(G956,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_RSTV"},"LEAF01A01_RSTV AT%M1384.0 :REAL; (*排风机01A01-运行时间累积重置值*)","LEAF01A01_RSTV          AT%M1384.0     :REAL; (*排风机01A01-运行时间累积重置值*)"]
["1388.0","验证通过","REAL","排风机","L","01A01","运行时间累积值","排风机01A01-运行时间累积值",{"$f":"E957&VLOOKUP(D957,[1]list!$D$3:$F$501,2,FALSE)&F957&\"_\"&VLOOKUP(G957,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_RH"},"LEAF01A01_RH AT%M1388.0 :REAL; (*排风机01A01-运行时间累积值*)","LEAF01A01_RH            AT%M1388.0     :REAL; (*排风机01A01-运行时间累积值*)"]
["1392.0","验证通过","BOOL","排风机","L","01A01","定时模式","排风机01A01-定时模式",{"$f":"E958&VLOOKUP(D958,[1]list!$D$3:$F$501,2,FALSE)&F958&\"_\"&VLOOKUP(G958,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_TM"},"LEAF01A01_TM AT%M1392.0 :BOOL; (*排风机01A01-定时模式*)","LEAF01A01_TM            AT%M1392.0     :BOOL; (*排风机01A01-定时模式*)"]
["1394.0","验证通过","BOOL","排风机","L","01A01","定时控制","排风机01A01-定时控制",{"$f":"E959&VLOOKUP(D959,[1]list!$D$3:$F$501,2,FALSE)&F959&\"_\"&VLOOKUP(G959,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_TC"},"LEAF01A01_TC AT%M1394.0 :BOOL; (*排风机01A01-定时控制*)","LEAF01A01_TC            AT%M1394.0     :BOOL; (*排风机01A01-定时控制*)"]
["1396.0","验证通过","BOOL","排风机","L","01A01","全天候模式","排风机01A01-全天候模式",{"$f":"E960&VLOOKUP(D960,[1]list!$D$3:$F$501,2,FALSE)&F960&\"_\"&VLOOKUP(G960,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_DM"},"LEAF01A01_DM AT%M1396.0 :BOOL; (*排风机01A01-全天候模式*)","LEAF01A01_DM            AT%M1396.0     :BOOL; (*排风机01A01-全天候模式*)"]
["1400.0","验证通过","REAL","排风机","L","01A01","CO设定值","排风机01A01-CO设定值",{"$f":"E961&VLOOKUP(D961,[1]list!$D$3:$F$501,2,FALSE)&F961&\"_\"&VLOOKUP(G961,[1]list!$I$2:$K$502,2,FALSE)","v":"LEAF01A01_COSET"},"LEAF01A01_COSET AT%M1400.0 :REAL; (*排风机01A01-CO设定值*)","LEAF01A01_COSET         AT%M1400.0     :REAL; (*排风机01A01-CO设定值*)"]
["1404.0","验证通过","REAL","排烟机","L","01A01","设定温度值","排烟机01A01-设定温度值",{"$f":"E962&VLOOKUP(D962,[1]list!$D$3:$F$501,2,FALSE)&F962&\"_\"&VLOOKUP(G962,[1]list!$I$2:$K$502,2,FALSE)","v":"LESF01A01_TSET"},"LESF01A01_TSET AT%M1404.0 :REAL; (*排烟机01A01-设定温度值*)","LESF01A01_TSET          AT%M1404.0     :REAL; (*排烟机01A01-设定温度值*)"]
["PAU"]
[{"$f":"IF(OR(C962=\"REAL\",C962=\"DWORD\",C962=\"DINT\"),(IF(OR(C964=\"REAL\",C964=\"DWORD\",C964=\"DINT\"),A962+4+MOD(A962,4),A962+4)),(IF(OR(C964=\"REAL\",C964=\"DWORD\",C964=\"DINT\"),A962+4+MOD(A962,4),A962+2)))&\".0\"","v":"1408.0"},{"$f":"IF((IF(OR(C964=\"INT\",C964=\"WORD\",C964=\"BOOL\"),MOD(A964,2),MOD(A964,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","P新风机组","R","05H01","设定温度值",{"$f":"D964&F964&\"-\"&IF(E964=\"R\",\"新云平台\"&G964,G964)","v":"P新风机组05H01-新云平台设定温度值"},{"$f":"E964&VLOOKUP(D964,list!$D$3:$F$501,2,FALSE)&F964&\"_\"&VLOOKUP(G964,list!$I$2:$K$502,2,FALSE)","v":"RPAU05H01_TSET"},{"$f":"I964&\" \"&\"AT%M\"&A964&\" \"&\":\"&C964&\";\"&\" \"&\"(*\"&H964&\"*)\"","v":"RPAU05H01_TSET AT%M1408.0 :REAL; (*P新风机组05H01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J964,SEARCH(\"AT%\",J964),,REPT(\" \",25-SEARCH(\"AT%\",J964))),SEARCH(\":\",REPLACE(J964,SEARCH(\"AT%\",J964),,REPT(\" \",25-SEARCH(\"AT%\",J964)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J964,SEARCH(\"AT%\",J964),,REPT(\" \",25-SEARCH(\"AT%\",J964))))))","v":"RPAU05H01_TSET          AT%M1408.0     :REAL; (*P新风机组05H01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C964=\"REAL\",C964=\"DWORD\",C964=\"DINT\"),(IF(OR(C965=\"REAL\",C965=\"DWORD\",C965=\"DINT\"),A964+4+MOD(A964,4),A964+4)),(IF(OR(C965=\"REAL\",C965=\"DWORD\",C965=\"DINT\"),A964+4+MOD(A964,4),A964+2)))&\".0\"","v":"1412.0"},"验证通过","INT","P新风机组","R",{"$f":"F964","v":"05H01"},"季节模式","P新风机组05H01-新云平台季节模式",{"$f":"E965&VLOOKUP(D965,list!$D$3:$F$501,2,FALSE)&F965&\"_\"&VLOOKUP(G965,list!$I$2:$K$502,2,FALSE)","v":"RPAU05H01_SM"},"RPAU05H01_SM AT%M1412.0 :INT; (*P新风机组05H01-新云平台季节模式*)","RPAU05H01_SM            AT%M1412.0     :INT; (*P新风机组05H01-新云平台季节模式*)"]
["1414.0","验证通过","BOOL","P新风机组","R","05H01","程序控制","P新风机组05H01-新云平台程序控制",{"$f":"E966&VLOOKUP(D966,list!$D$3:$F$501,2,FALSE)&F966&\"_\"&VLOOKUP(G966,list!$I$2:$K$502,2,FALSE)","v":"RPAU05H01_PC"},"RPAU05H01_PC AT%M1414.0 :BOOL; (*P新风机组05H01-新云平台程序控制*)","RPAU05H01_PC            AT%M1414.0     :BOOL; (*P新风机组05H01-新云平台程序控制*)"]
["1420.0","验证通过","REAL","P新风机组","L","05H01","设定温度值","P新风机组05H01-设定温度值",{"$f":"E967&VLOOKUP(D967,list!$D$3:$F$501,2,FALSE)&F967&\"_\"&VLOOKUP(G967,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_TSET"},"LPAU05H01_TSET AT%M1420.0 :REAL; (*P新风机组05H01-设定温度值*)","LPAU05H01_TSET          AT%M1420.0     :REAL; (*P新风机组05H01-设定温度值*)"]
["1424.0","验证通过","INT","P新风机组","L","05H01","季节模式","P新风机组05H01-季节模式",{"$f":"E968&VLOOKUP(D968,list!$D$3:$F$501,2,FALSE)&F968&\"_\"&VLOOKUP(G968,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_SM"},"LPAU05H01_SM AT%M1424.0 :INT; (*P新风机组05H01-季节模式*)","LPAU05H01_SM            AT%M1424.0     :INT; (*P新风机组05H01-季节模式*)"]
["1428.0","验证通过","REAL","P新风机组","L","05H01","水阀反馈换算值","P新风机组05H01-水阀反馈换算值",{"$f":"E969&VLOOKUP(D969,list!$D$3:$F$501,2,FALSE)&F969&\"_\"&VLOOKUP(G969,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_WVBS"},"LPAU05H01_WVBS AT%M1428.0 :REAL; (*P新风机组05H01-水阀反馈换算值*)","LPAU05H01_WVBS          AT%M1428.0     :REAL; (*P新风机组05H01-水阀反馈换算值*)"]
["1432.0","验证通过","BOOL","P新风机组","L","05H01","水阀手动控制","P新风机组05H01-水阀手动控制",{"$f":"E970&VLOOKUP(D970,list!$D$3:$F$501,2,FALSE)&F970&\"_\"&VLOOKUP(G970,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_WVMC"},"LPAU05H01_WVMC AT%M1432.0 :BOOL; (*P新风机组05H01-水阀手动控制*)","LPAU05H01_WVMC          AT%M1432.0     :BOOL; (*P新风机组05H01-水阀手动控制*)"]
["1436.0","验证通过","REAL","P新风机组","L","05H01","水阀手动控制值","P新风机组05H01-水阀手动控制值",{"$f":"E971&VLOOKUP(D971,list!$D$3:$F$501,2,FALSE)&F971&\"_\"&VLOOKUP(G971,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_WVMV"},"LPAU05H01_WVMV AT%M1436.0 :REAL; (*P新风机组05H01-水阀手动控制值*)","LPAU05H01_WVMV          AT%M1436.0     :REAL; (*P新风机组05H01-水阀手动控制值*)"]
["1440.0","验证通过","REAL","P新风机组","L","05H01","送风温度换算值","P新风机组05H01-送风温度换算值",{"$f":"E972&VLOOKUP(D972,list!$D$3:$F$501,2,FALSE)&F972&\"_\"&VLOOKUP(G972,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_STS"},"LPAU05H01_STS AT%M1440.0 :REAL; (*P新风机组05H01-送风温度换算值*)","LPAU05H01_STS           AT%M1440.0     :REAL; (*P新风机组05H01-送风温度换算值*)"]
["1444.0","验证通过","BOOL","P新风机组","L","05H01","运行时间累积重置","P新风机组05H01-运行时间累积重置",{"$f":"E973&VLOOKUP(D973,list!$D$3:$F$501,2,FALSE)&F973&\"_\"&VLOOKUP(G973,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_RST"},"LPAU05H01_RST AT%M1444.0 :BOOL; (*P新风机组05H01-运行时间累积重置*)","LPAU05H01_RST           AT%M1444.0     :BOOL; (*P新风机组05H01-运行时间累积重置*)"]
["1448.0","验证通过","REAL","P新风机组","L","05H01","运行时间累积重置值","P新风机组05H01-运行时间累积重置值",{"$f":"E974&VLOOKUP(D974,list!$D$3:$F$501,2,FALSE)&F974&\"_\"&VLOOKUP(G974,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_RSTV"},"LPAU05H01_RSTV AT%M1448.0 :REAL; (*P新风机组05H01-运行时间累积重置值*)","LPAU05H01_RSTV          AT%M1448.0     :REAL; (*P新风机组05H01-运行时间累积重置值*)"]
["1452.0","验证通过","BOOL","P新风机组","L","05H01","隔离开关1","P新风机组05H01-隔离开关1",{"$f":"E975&VLOOKUP(D975,list!$D$3:$F$501,2,FALSE)&F975&\"_\"&VLOOKUP(G975,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_ISO1"},"LPAU05H01_ISO1 AT%M1452.0 :BOOL; (*P新风机组05H01-隔离开关1*)","LPAU05H01_ISO1          AT%M1452.0     :BOOL; (*P新风机组05H01-隔离开关1*)"]
["1454.0","验证通过","BOOL","P新风机组","L","05H01","隔离开关2","P新风机组05H01-隔离开关2",{"$f":"E976&VLOOKUP(D976,list!$D$3:$F$501,2,FALSE)&F976&\"_\"&VLOOKUP(G976,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_ISO2"},"LPAU05H01_ISO2 AT%M1454.0 :BOOL; (*P新风机组05H01-隔离开关2*)","LPAU05H01_ISO2          AT%M1454.0     :BOOL; (*P新风机组05H01-隔离开关2*)"]
["1460.0","验证通过","REAL","P新风机组","L","05H01","P调节参数","P新风机组05H01-P调节参数",{"$f":"E977&VLOOKUP(D977,list!$D$3:$F$501,2,FALSE)&F977&\"_\"&VLOOKUP(G977,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_VP"},"LPAU05H01_VP AT%M1460.0 :REAL; (*P新风机组05H01-P调节参数*)","LPAU05H01_VP            AT%M1460.0     :REAL; (*P新风机组05H01-P调节参数*)"]
["1464.0","验证通过","REAL","P新风机组","L","05H01","I调节参数","P新风机组05H01-I调节参数",{"$f":"E978&VLOOKUP(D978,list!$D$3:$F$501,2,FALSE)&F978&\"_\"&VLOOKUP(G978,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_VI"},"LPAU05H01_VI AT%M1464.0 :REAL; (*P新风机组05H01-I调节参数*)","LPAU05H01_VI            AT%M1464.0     :REAL; (*P新风机组05H01-I调节参数*)"]
["1468.0","验证通过","REAL","P新风机组","L","05H01","运行时间累积值","P新风机组05H01-运行时间累积值",{"$f":"E979&VLOOKUP(D979,list!$D$3:$F$501,2,FALSE)&F979&\"_\"&VLOOKUP(G979,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_RH"},"LPAU05H01_RH AT%M1468.0 :REAL; (*P新风机组05H01-运行时间累积值*)","LPAU05H01_RH            AT%M1468.0     :REAL; (*P新风机组05H01-运行时间累积值*)"]
["1472.0","验证通过","INT","P新风机组","L","05H01","设备状态代码","P新风机组05H01-设备状态代码",{"$f":"E980&VLOOKUP(D980,list!$D$3:$F$501,2,FALSE)&F980&\"_\"&VLOOKUP(G980,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_SN"},"LPAU05H01_SN AT%M1472.0 :INT; (*P新风机组05H01-设备状态代码*)","LPAU05H01_SN            AT%M1472.0     :INT; (*P新风机组05H01-设备状态代码*)"]
["1474.0","验证通过","INT","P新风机组","L","05H01","水阀控制转换值","P新风机组05H01-水阀控制转换值",{"$f":"E981&VLOOKUP(D981,list!$D$3:$F$501,2,FALSE)&F981&\"_\"&VLOOKUP(G981,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_WVCS"},"LPAU05H01_WVCS AT%M1474.0 :INT; (*P新风机组05H01-水阀控制转换值*)","LPAU05H01_WVCS          AT%M1474.0     :INT; (*P新风机组05H01-水阀控制转换值*)"]
["1476.0","验证通过","BOOL","P新风机组","L","05H01","程序控制","P新风机组05H01-程序控制",{"$f":"E982&VLOOKUP(D982,list!$D$3:$F$501,2,FALSE)&F982&\"_\"&VLOOKUP(G982,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_PC"},"LPAU05H01_PC AT%M1476.0 :BOOL; (*P新风机组05H01-程序控制*)","LPAU05H01_PC            AT%M1476.0     :BOOL; (*P新风机组05H01-程序控制*)"]
["1478.0","验证通过","INT","P新风机组","L","05H01","变频手动控制值","P新风机组05H01-变频手动控制值",{"$f":"E983&VLOOKUP(D983,list!$D$3:$F$501,2,FALSE)&F983&\"_\"&VLOOKUP(G983,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_VFMV"},"LPAU05H01_VFMV AT%M1478.0 :INT; (*P新风机组05H01-变频手动控制值*)","LPAU05H01_VFMV          AT%M1478.0     :INT; (*P新风机组05H01-变频手动控制值*)"]
["1480.0","验证通过","BOOL","P新风机组","L","05H01","低温断路报警隔离","P新风机组05H01-低温断路报警隔离",{"$f":"E984&VLOOKUP(D984,list!$D$3:$F$501,2,FALSE)&F984&\"_\"&VLOOKUP(G984,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_ISO3"},"LPAU05H01_ISO3 AT%M1480.0 :BOOL; (*P新风机组05H01-低温断路报警隔离*)","LPAU05H01_ISO3          AT%M1480.0     :BOOL; (*P新风机组05H01-低温断路报警隔离*)"]
["1482.0","验证通过","INT","P新风机组","L","05H01","变频器频率控制值","P新风机组05H01-变频器频率控制值",{"$f":"E985&VLOOKUP(D985,list!$D$3:$F$501,2,FALSE)&F985&\"_\"&VLOOKUP(G985,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_VFCS"},"LPAU05H01_VFCS AT%M1482.0 :INT; (*P新风机组05H01-变频器频率控制值*)","LPAU05H01_VFCS          AT%M1482.0     :INT; (*P新风机组05H01-变频器频率控制值*)"]
["1484.0","验证通过","INT","P新风机组","L","05H01","变频器频率反馈值","P新风机组05H01-变频器频率反馈值",{"$f":"E986&VLOOKUP(D986,list!$D$3:$F$501,2,FALSE)&F986&\"_\"&VLOOKUP(G986,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_VFBS"},"LPAU05H01_VFBS AT%M1484.0 :INT; (*P新风机组05H01-变频器频率反馈值*)","LPAU05H01_VFBS          AT%M1484.0     :INT; (*P新风机组05H01-变频器频率反馈值*)"]
["1486.0","验证通过","BOOL","P新风机组","L","05H01","联动模式","P新风机组05H01-联动模式",{"$f":"E987&VLOOKUP(D987,list!$D$3:$F$501,2,FALSE)&F987&\"_\"&VLOOKUP(G987,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_LM"},"LPAU05H01_LM AT%M1486.0 :BOOL; (*P新风机组05H01-联动模式*)","LPAU05H01_LM            AT%M1486.0     :BOOL; (*P新风机组05H01-联动模式*)"]
["1488.0","验证通过","BOOL","P新风机组","L","05H01","全天候模式","P新风机组05H01-全天候模式",{"$f":"E988&VLOOKUP(D988,list!$D$3:$F$501,2,FALSE)&F988&\"_\"&VLOOKUP(G988,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_DM"},"LPAU05H01_DM AT%M1488.0 :BOOL; (*P新风机组05H01-全天候模式*)","LPAU05H01_DM            AT%M1488.0     :BOOL; (*P新风机组05H01-全天候模式*)"]
["1492.0","验证通过","REAL","P新风机组","L","05H01","CO2设定值","P新风机组05H01-CO2设定值",{"$f":"E989&VLOOKUP(D989,list!$D$3:$F$501,2,FALSE)&F989&\"_\"&VLOOKUP(G989,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_CO2SET"},"LPAU05H01_CO2SET AT%M1492.0 :REAL; (*P新风机组05H01-CO2设定值*)","LPAU05H01_CO2SET        AT%M1492.0     :REAL; (*P新风机组05H01-CO2设定值*)"]
["1496.0","验证通过","BOOL","P新风机组","L","05H01","定时控制","P新风机组05H01-定时控制",{"$f":"E990&VLOOKUP(D990,list!$D$3:$F$501,2,FALSE)&F990&\"_\"&VLOOKUP(G990,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_TC"},"LPAU05H01_TC AT%M1496.0 :BOOL; (*P新风机组05H01-定时控制*)","LPAU05H01_TC            AT%M1496.0     :BOOL; (*P新风机组05H01-定时控制*)"]
["1498.0","验证通过","BOOL","P新风机组","L","05H01","定时模式","P新风机组05H01-定时模式",{"$f":"E991&VLOOKUP(D991,list!$D$3:$F$501,2,FALSE)&F991&\"_\"&VLOOKUP(G991,list!$I$2:$K$502,2,FALSE)","v":"LPAU05H01_TM"},"LPAU05H01_TM AT%M1498.0 :BOOL; (*P新风机组05H01-定时模式*)","LPAU05H01_TM            AT%M1498.0     :BOOL; (*P新风机组05H01-定时模式*)"]
["AHU"]
[{"$f":"IF(OR(C827=\"REAL\",C827=\"DWORD\",C827=\"DINT\"),(IF(OR(C993=\"REAL\",C993=\"DWORD\",C993=\"DINT\"),A827+4+MOD(A827,4),A827+4)),(IF(OR(C993=\"REAL\",C993=\"DWORD\",C993=\"DINT\"),A827+4+MOD(A827,4),A827+2)))&\".0\"","v":"1380.0"},{"$f":"IF((IF(OR(C993=\"INT\",C993=\"WORD\",C993=\"BOOL\"),MOD(A993,2),MOD(A993,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H07","设定温度值",{"$f":"D993&F993&\"-\"&IF(E993=\"R\",\"新云平台\"&G993,G993)","v":"空调机组01H07-新云平台设定温度值"},{"$f":"E993&VLOOKUP(D993,list!$D$3:$F$501,2,FALSE)&F993&\"_\"&VLOOKUP(G993,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_TSET"},{"$f":"I993&\" \"&\"AT%M\"&A993&\" \"&\":\"&C993&\";\"&\" \"&\"(*\"&H993&\"*)\"","v":"RAHU01H07_TSET AT%M1380.0 :REAL; (*空调机组01H07-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J993,SEARCH(\"AT%\",J993),,REPT(\" \",25-SEARCH(\"AT%\",J993))),SEARCH(\":\",REPLACE(J993,SEARCH(\"AT%\",J993),,REPT(\" \",25-SEARCH(\"AT%\",J993)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J993,SEARCH(\"AT%\",J993),,REPT(\" \",25-SEARCH(\"AT%\",J993))))))","v":"RAHU01H07_TSET          AT%M1380.0     :REAL; (*空调机组01H07-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C993=\"REAL\",C993=\"DWORD\",C993=\"DINT\"),(IF(OR(C994=\"REAL\",C994=\"DWORD\",C994=\"DINT\"),A993+4+MOD(A993,4),A993+4)),(IF(OR(C994=\"REAL\",C994=\"DWORD\",C994=\"DINT\"),A993+4+MOD(A993,4),A993+2)))&\".0\"","v":"1384.0"},"验证通过","INT","空调机组","R",{"$f":"F993","v":"01H07"},"季节模式","空调机组01H07-新云平台季节模式",{"$f":"E994&VLOOKUP(D994,list!$D$3:$F$501,2,FALSE)&F994&\"_\"&VLOOKUP(G994,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_SM"},"RAHU01H07_SM AT%M1384.0 :INT; (*空调机组01H07-新云平台季节模式*)","RAHU01H07_SM            AT%M1384.0     :INT; (*空调机组01H07-新云平台季节模式*)"]
["1386.0","验证通过","BOOL","空调机组","R","01H07","程序控制","空调机组01H07-新云平台程序控制",{"$f":"E995&VLOOKUP(D995,list!$D$3:$F$501,2,FALSE)&F995&\"_\"&VLOOKUP(G995,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_PC"},"RAHU01H07_PC AT%M1386.0 :BOOL; (*空调机组01H07-新云平台程序控制*)","RAHU01H07_PC            AT%M1386.0     :BOOL; (*空调机组01H07-新云平台程序控制*)"]
["1392.0","验证通过","REAL","空调机组","L","01H07","设定温度值","空调机组01H07-设定温度值",{"$f":"E996&VLOOKUP(D996,list!$D$3:$F$501,2,FALSE)&F996&\"_\"&VLOOKUP(G996,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_TSET"},"LAHU01H07_TSET AT%M1392.0 :REAL; (*空调机组01H07-设定温度值*)","LAHU01H07_TSET          AT%M1392.0     :REAL; (*空调机组01H07-设定温度值*)"]
["1396.0","验证通过","INT","空调机组","L","01H07","季节模式","空调机组01H07-季节模式",{"$f":"E997&VLOOKUP(D997,list!$D$3:$F$501,2,FALSE)&F997&\"_\"&VLOOKUP(G997,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_SM"},"LAHU01H07_SM AT%M1396.0 :INT; (*空调机组01H07-季节模式*)","LAHU01H07_SM            AT%M1396.0     :INT; (*空调机组01H07-季节模式*)"]
["1400.0","验证通过","REAL","空调机组","L","01H07","水阀反馈换算值","空调机组01H07-水阀反馈换算值",{"$f":"E998&VLOOKUP(D998,list!$D$3:$F$501,2,FALSE)&F998&\"_\"&VLOOKUP(G998,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVBS"},"LAHU01H07_WVBS AT%M1400.0 :REAL; (*空调机组01H07-水阀反馈换算值*)","LAHU01H07_WVBS          AT%M1400.0     :REAL; (*空调机组01H07-水阀反馈换算值*)"]
["1404.0","验证通过","BOOL","空调机组","L","01H07","水阀手动控制","空调机组01H07-水阀手动控制",{"$f":"E999&VLOOKUP(D999,list!$D$3:$F$501,2,FALSE)&F999&\"_\"&VLOOKUP(G999,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVMC"},"LAHU01H07_WVMC AT%M1404.0 :BOOL; (*空调机组01H07-水阀手动控制*)","LAHU01H07_WVMC          AT%M1404.0     :BOOL; (*空调机组01H07-水阀手动控制*)"]
["1408.0","验证通过","REAL","空调机组","L","01H07","水阀手动控制值","空调机组01H07-水阀手动控制值",{"$f":"E1000&VLOOKUP(D1000,list!$D$3:$F$501,2,FALSE)&F1000&\"_\"&VLOOKUP(G1000,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVMV"},"LAHU01H07_WVMV AT%M1408.0 :REAL; (*空调机组01H07-水阀手动控制值*)","LAHU01H07_WVMV          AT%M1408.0     :REAL; (*空调机组01H07-水阀手动控制值*)"]
["1412.0","验证通过","REAL","空调机组","L","01H07","回风温度换算值","空调机组01H07-回风温度换算值",{"$f":"E1001&VLOOKUP(D1001,list!$D$3:$F$501,2,FALSE)&F1001&\"_\"&VLOOKUP(G1001,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RTS"},"LAHU01H07_RTS AT%M1412.0 :REAL; (*空调机组01H07-回风温度换算值*)","LAHU01H07_RTS           AT%M1412.0     :REAL; (*空调机组01H07-回风温度换算值*)"]
["1416.0","验证通过","BOOL","空调机组","L","01H07","运行时间累积重置","空调机组01H07-运行时间累积重置",{"$f":"E1002&VLOOKUP(D1002,list!$D$3:$F$501,2,FALSE)&F1002&\"_\"&VLOOKUP(G1002,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RST"},"LAHU01H07_RST AT%M1416.0 :BOOL; (*空调机组01H07-运行时间累积重置*)","LAHU01H07_RST           AT%M1416.0     :BOOL; (*空调机组01H07-运行时间累积重置*)"]
["1420.0","验证通过","REAL","空调机组","L","01H07","运行时间累积重置值","空调机组01H07-运行时间累积重置值",{"$f":"E1003&VLOOKUP(D1003,list!$D$3:$F$501,2,FALSE)&F1003&\"_\"&VLOOKUP(G1003,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RSTV"},"LAHU01H07_RSTV AT%M1420.0 :REAL; (*空调机组01H07-运行时间累积重置值*)","LAHU01H07_RSTV          AT%M1420.0     :REAL; (*空调机组01H07-运行时间累积重置值*)"]
["1424.0","验证通过","BOOL","空调机组","L","01H07","隔离开关1","空调机组01H07-隔离开关1",{"$f":"E1004&VLOOKUP(D1004,list!$D$3:$F$501,2,FALSE)&F1004&\"_\"&VLOOKUP(G1004,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_ISO1"},"LAHU01H07_ISO1 AT%M1424.0 :BOOL; (*空调机组01H07-隔离开关1*)","LAHU01H07_ISO1          AT%M1424.0     :BOOL; (*空调机组01H07-隔离开关1*)"]
["1426.0","验证通过","BOOL","空调机组","L","01H07","隔离开关2","空调机组01H07-隔离开关2",{"$f":"E1005&VLOOKUP(D1005,list!$D$3:$F$501,2,FALSE)&F1005&\"_\"&VLOOKUP(G1005,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_ISO2"},"LAHU01H07_ISO2 AT%M1426.0 :BOOL; (*空调机组01H07-隔离开关2*)","LAHU01H07_ISO2          AT%M1426.0     :BOOL; (*空调机组01H07-隔离开关2*)"]
["1432.0","验证通过","REAL","空调机组","L","01H07","P调节参数","空调机组01H07-P调节参数",{"$f":"E1006&VLOOKUP(D1006,list!$D$3:$F$501,2,FALSE)&F1006&\"_\"&VLOOKUP(G1006,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_VP"},"LAHU01H07_VP AT%M1432.0 :REAL; (*空调机组01H07-P调节参数*)","LAHU01H07_VP            AT%M1432.0     :REAL; (*空调机组01H07-P调节参数*)"]
["1436.0","验证通过","REAL","空调机组","L","01H07","I调节参数","空调机组01H07-I调节参数",{"$f":"E1007&VLOOKUP(D1007,list!$D$3:$F$501,2,FALSE)&F1007&\"_\"&VLOOKUP(G1007,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_VI"},"LAHU01H07_VI AT%M1436.0 :REAL; (*空调机组01H07-I调节参数*)","LAHU01H07_VI            AT%M1436.0     :REAL; (*空调机组01H07-I调节参数*)"]
["1440.0","验证通过","REAL","空调机组","L","01H07","运行时间累积值","空调机组01H07-运行时间累积值",{"$f":"E1008&VLOOKUP(D1008,list!$D$3:$F$501,2,FALSE)&F1008&\"_\"&VLOOKUP(G1008,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RH"},"LAHU01H07_RH AT%M1440.0 :REAL; (*空调机组01H07-运行时间累积值*)","LAHU01H07_RH            AT%M1440.0     :REAL; (*空调机组01H07-运行时间累积值*)"]
["1444.0","验证通过","INT","空调机组","L","01H07","设备状态代码","空调机组01H07-设备状态代码",{"$f":"E1009&VLOOKUP(D1009,list!$D$3:$F$501,2,FALSE)&F1009&\"_\"&VLOOKUP(G1009,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_SN"},"LAHU01H07_SN AT%M1444.0 :INT; (*空调机组01H07-设备状态代码*)","LAHU01H07_SN            AT%M1444.0     :INT; (*空调机组01H07-设备状态代码*)"]
["1446.0","验证通过","INT","空调机组","L","01H07","水阀控制转换值","空调机组01H07-水阀控制转换值",{"$f":"E1010&VLOOKUP(D1010,list!$D$3:$F$501,2,FALSE)&F1010&\"_\"&VLOOKUP(G1010,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVCS"},"LAHU01H07_WVCS AT%M1446.0 :INT; (*空调机组01H07-水阀控制转换值*)","LAHU01H07_WVCS          AT%M1446.0     :INT; (*空调机组01H07-水阀控制转换值*)"]
["1448.0","验证通过","BOOL","空调机组","L","01H07","程序控制","空调机组01H07-程序控制",{"$f":"E1011&VLOOKUP(D1011,list!$D$3:$F$501,2,FALSE)&F1011&\"_\"&VLOOKUP(G1011,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_PC"},"LAHU01H07_PC AT%M1448.0 :BOOL; (*空调机组01H07-程序控制*)","LAHU01H07_PC            AT%M1448.0     :BOOL; (*空调机组01H07-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1011=\"REAL\",C1011=\"DWORD\",C1011=\"DINT\"),(IF(OR(C1013=\"REAL\",C1013=\"DWORD\",C1013=\"DINT\"),A1011+4+MOD(A1011,4),A1011+4)),(IF(OR(C1013=\"REAL\",C1013=\"DWORD\",C1013=\"DINT\"),A1011+4+MOD(A1011,4),A1011+2)))&\".0\"","v":"1452.0"},{"$f":"IF((IF(OR(C1013=\"INT\",C1013=\"WORD\",C1013=\"BOOL\"),MOD(A1013,2),MOD(A1013,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H08","设定温度值",{"$f":"D1013&F1013&\"-\"&IF(E1013=\"R\",\"新云平台\"&G1013,G1013)","v":"空调机组01H08-新云平台设定温度值"},{"$f":"E1013&VLOOKUP(D1013,list!$D$3:$F$501,2,FALSE)&F1013&\"_\"&VLOOKUP(G1013,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_TSET"},{"$f":"I1013&\" \"&\"AT%M\"&A1013&\" \"&\":\"&C1013&\";\"&\" \"&\"(*\"&H1013&\"*)\"","v":"RAHU01H08_TSET AT%M1452.0 :REAL; (*空调机组01H08-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1013,SEARCH(\"AT%\",J1013),,REPT(\" \",25-SEARCH(\"AT%\",J1013))),SEARCH(\":\",REPLACE(J1013,SEARCH(\"AT%\",J1013),,REPT(\" \",25-SEARCH(\"AT%\",J1013)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1013,SEARCH(\"AT%\",J1013),,REPT(\" \",25-SEARCH(\"AT%\",J1013))))))","v":"RAHU01H08_TSET          AT%M1452.0     :REAL; (*空调机组01H08-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1013=\"REAL\",C1013=\"DWORD\",C1013=\"DINT\"),(IF(OR(C1014=\"REAL\",C1014=\"DWORD\",C1014=\"DINT\"),A1013+4+MOD(A1013,4),A1013+4)),(IF(OR(C1014=\"REAL\",C1014=\"DWORD\",C1014=\"DINT\"),A1013+4+MOD(A1013,4),A1013+2)))&\".0\"","v":"1456.0"},"验证通过","INT","空调机组","R",{"$f":"F1013","v":"01H08"},"季节模式","空调机组01H08-新云平台季节模式",{"$f":"E1014&VLOOKUP(D1014,list!$D$3:$F$501,2,FALSE)&F1014&\"_\"&VLOOKUP(G1014,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_SM"},"RAHU01H08_SM AT%M1456.0 :INT; (*空调机组01H08-新云平台季节模式*)","RAHU01H08_SM            AT%M1456.0     :INT; (*空调机组01H08-新云平台季节模式*)"]
["1458.0","验证通过","BOOL","空调机组","R","01H08","程序控制","空调机组01H08-新云平台程序控制",{"$f":"E1015&VLOOKUP(D1015,list!$D$3:$F$501,2,FALSE)&F1015&\"_\"&VLOOKUP(G1015,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_PC"},"RAHU01H08_PC AT%M1458.0 :BOOL; (*空调机组01H08-新云平台程序控制*)","RAHU01H08_PC            AT%M1458.0     :BOOL; (*空调机组01H08-新云平台程序控制*)"]
["1464.0","验证通过","REAL","空调机组","L","01H08","设定温度值","空调机组01H08-设定温度值",{"$f":"E1016&VLOOKUP(D1016,list!$D$3:$F$501,2,FALSE)&F1016&\"_\"&VLOOKUP(G1016,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_TSET"},"LAHU01H08_TSET AT%M1464.0 :REAL; (*空调机组01H08-设定温度值*)","LAHU01H08_TSET          AT%M1464.0     :REAL; (*空调机组01H08-设定温度值*)"]
["1468.0","验证通过","INT","空调机组","L","01H08","季节模式","空调机组01H08-季节模式",{"$f":"E1017&VLOOKUP(D1017,list!$D$3:$F$501,2,FALSE)&F1017&\"_\"&VLOOKUP(G1017,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_SM"},"LAHU01H08_SM AT%M1468.0 :INT; (*空调机组01H08-季节模式*)","LAHU01H08_SM            AT%M1468.0     :INT; (*空调机组01H08-季节模式*)"]
["1472.0","验证通过","REAL","空调机组","L","01H08","水阀反馈换算值","空调机组01H08-水阀反馈换算值",{"$f":"E1018&VLOOKUP(D1018,list!$D$3:$F$501,2,FALSE)&F1018&\"_\"&VLOOKUP(G1018,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVBS"},"LAHU01H08_WVBS AT%M1472.0 :REAL; (*空调机组01H08-水阀反馈换算值*)","LAHU01H08_WVBS          AT%M1472.0     :REAL; (*空调机组01H08-水阀反馈换算值*)"]
["1476.0","验证通过","BOOL","空调机组","L","01H08","水阀手动控制","空调机组01H08-水阀手动控制",{"$f":"E1019&VLOOKUP(D1019,list!$D$3:$F$501,2,FALSE)&F1019&\"_\"&VLOOKUP(G1019,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVMC"},"LAHU01H08_WVMC AT%M1476.0 :BOOL; (*空调机组01H08-水阀手动控制*)","LAHU01H08_WVMC          AT%M1476.0     :BOOL; (*空调机组01H08-水阀手动控制*)"]
["1480.0","验证通过","REAL","空调机组","L","01H08","水阀手动控制值","空调机组01H08-水阀手动控制值",{"$f":"E1020&VLOOKUP(D1020,list!$D$3:$F$501,2,FALSE)&F1020&\"_\"&VLOOKUP(G1020,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVMV"},"LAHU01H08_WVMV AT%M1480.0 :REAL; (*空调机组01H08-水阀手动控制值*)","LAHU01H08_WVMV          AT%M1480.0     :REAL; (*空调机组01H08-水阀手动控制值*)"]
["1484.0","验证通过","REAL","空调机组","L","01H08","回风温度换算值","空调机组01H08-回风温度换算值",{"$f":"E1021&VLOOKUP(D1021,list!$D$3:$F$501,2,FALSE)&F1021&\"_\"&VLOOKUP(G1021,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RTS"},"LAHU01H08_RTS AT%M1484.0 :REAL; (*空调机组01H08-回风温度换算值*)","LAHU01H08_RTS           AT%M1484.0     :REAL; (*空调机组01H08-回风温度换算值*)"]
["1488.0","验证通过","BOOL","空调机组","L","01H08","运行时间累积重置","空调机组01H08-运行时间累积重置",{"$f":"E1022&VLOOKUP(D1022,list!$D$3:$F$501,2,FALSE)&F1022&\"_\"&VLOOKUP(G1022,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RST"},"LAHU01H08_RST AT%M1488.0 :BOOL; (*空调机组01H08-运行时间累积重置*)","LAHU01H08_RST           AT%M1488.0     :BOOL; (*空调机组01H08-运行时间累积重置*)"]
["1492.0","验证通过","REAL","空调机组","L","01H08","运行时间累积重置值","空调机组01H08-运行时间累积重置值",{"$f":"E1023&VLOOKUP(D1023,list!$D$3:$F$501,2,FALSE)&F1023&\"_\"&VLOOKUP(G1023,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RSTV"},"LAHU01H08_RSTV AT%M1492.0 :REAL; (*空调机组01H08-运行时间累积重置值*)","LAHU01H08_RSTV          AT%M1492.0     :REAL; (*空调机组01H08-运行时间累积重置值*)"]
["1496.0","验证通过","BOOL","空调机组","L","01H08","隔离开关1","空调机组01H08-隔离开关1",{"$f":"E1024&VLOOKUP(D1024,list!$D$3:$F$501,2,FALSE)&F1024&\"_\"&VLOOKUP(G1024,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_ISO1"},"LAHU01H08_ISO1 AT%M1496.0 :BOOL; (*空调机组01H08-隔离开关1*)","LAHU01H08_ISO1          AT%M1496.0     :BOOL; (*空调机组01H08-隔离开关1*)"]
["1498.0","验证通过","BOOL","空调机组","L","01H08","隔离开关2","空调机组01H08-隔离开关2",{"$f":"E1025&VLOOKUP(D1025,list!$D$3:$F$501,2,FALSE)&F1025&\"_\"&VLOOKUP(G1025,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_ISO2"},"LAHU01H08_ISO2 AT%M1498.0 :BOOL; (*空调机组01H08-隔离开关2*)","LAHU01H08_ISO2          AT%M1498.0     :BOOL; (*空调机组01H08-隔离开关2*)"]
["1504.0","验证通过","REAL","空调机组","L","01H08","P调节参数","空调机组01H08-P调节参数",{"$f":"E1026&VLOOKUP(D1026,list!$D$3:$F$501,2,FALSE)&F1026&\"_\"&VLOOKUP(G1026,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_VP"},"LAHU01H08_VP AT%M1504.0 :REAL; (*空调机组01H08-P调节参数*)","LAHU01H08_VP            AT%M1504.0     :REAL; (*空调机组01H08-P调节参数*)"]
["1508.0","验证通过","REAL","空调机组","L","01H08","I调节参数","空调机组01H08-I调节参数",{"$f":"E1027&VLOOKUP(D1027,list!$D$3:$F$501,2,FALSE)&F1027&\"_\"&VLOOKUP(G1027,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_VI"},"LAHU01H08_VI AT%M1508.0 :REAL; (*空调机组01H08-I调节参数*)","LAHU01H08_VI            AT%M1508.0     :REAL; (*空调机组01H08-I调节参数*)"]
["1512.0","验证通过","REAL","空调机组","L","01H08","运行时间累积值","空调机组01H08-运行时间累积值",{"$f":"E1028&VLOOKUP(D1028,list!$D$3:$F$501,2,FALSE)&F1028&\"_\"&VLOOKUP(G1028,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RH"},"LAHU01H08_RH AT%M1512.0 :REAL; (*空调机组01H08-运行时间累积值*)","LAHU01H08_RH            AT%M1512.0     :REAL; (*空调机组01H08-运行时间累积值*)"]
["1516.0","验证通过","INT","空调机组","L","01H08","设备状态代码","空调机组01H08-设备状态代码",{"$f":"E1029&VLOOKUP(D1029,list!$D$3:$F$501,2,FALSE)&F1029&\"_\"&VLOOKUP(G1029,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_SN"},"LAHU01H08_SN AT%M1516.0 :INT; (*空调机组01H08-设备状态代码*)","LAHU01H08_SN            AT%M1516.0     :INT; (*空调机组01H08-设备状态代码*)"]
["1518.0","验证通过","INT","空调机组","L","01H08","水阀控制转换值","空调机组01H08-水阀控制转换值",{"$f":"E1030&VLOOKUP(D1030,list!$D$3:$F$501,2,FALSE)&F1030&\"_\"&VLOOKUP(G1030,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVCS"},"LAHU01H08_WVCS AT%M1518.0 :INT; (*空调机组01H08-水阀控制转换值*)","LAHU01H08_WVCS          AT%M1518.0     :INT; (*空调机组01H08-水阀控制转换值*)"]
["1520.0","验证通过","BOOL","空调机组","L","01H08","程序控制","空调机组01H08-程序控制",{"$f":"E1031&VLOOKUP(D1031,list!$D$3:$F$501,2,FALSE)&F1031&\"_\"&VLOOKUP(G1031,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_PC"},"LAHU01H08_PC AT%M1520.0 :BOOL; (*空调机组01H08-程序控制*)","LAHU01H08_PC            AT%M1520.0     :BOOL; (*空调机组01H08-程序控制*)"]
["FCU"]
[{"$f":"IF(OR(C1031=\"REAL\",C1031=\"DWORD\",C1031=\"DINT\"),(IF(OR(C1033=\"REAL\",C1033=\"DWORD\",C1033=\"DINT\"),A1031+4+MOD(A1031,4),A1031+4)),(IF(OR(C1033=\"REAL\",C1033=\"DWORD\",C1033=\"DINT\"),A1031+4+MOD(A1031,4),A1031+2)))&\".0\"","v":"1524.0"},{"$f":"IF((IF(OR(C1033=\"INT\",C1033=\"WORD\",C1033=\"BOOL\"),MOD(A1033,2),MOD(A1033,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","01H01","设定温度值",{"$f":"D1033&F1033&\"-\"&IF(E1033=\"R\",\"新云平台\"&G1033,G1033)","v":"风机盘管01H01-新云平台设定温度值"},{"$f":"E1033&VLOOKUP(D1033,list!$D$3:$F$501,2,FALSE)&F1033&\"_\"&VLOOKUP(G1033,list!$I$2:$K$502,2,FALSE)","v":"RFCU01H01_TSET"},{"$f":"I1033&\" \"&\"AT%M\"&A1033&\" \"&\":\"&C1033&\";\"&\" \"&\"(*\"&H1033&\"*)\"","v":"RFCU01H01_TSET AT%M1524.0 :REAL; (*风机盘管01H01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1033,SEARCH(\"AT%\",J1033),,REPT(\" \",25-SEARCH(\"AT%\",J1033))),SEARCH(\":\",REPLACE(J1033,SEARCH(\"AT%\",J1033),,REPT(\" \",25-SEARCH(\"AT%\",J1033)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1033,SEARCH(\"AT%\",J1033),,REPT(\" \",25-SEARCH(\"AT%\",J1033))))))","v":"RFCU01H01_TSET          AT%M1524.0     :REAL; (*风机盘管01H01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1033=\"REAL\",C1033=\"DWORD\",C1033=\"DINT\"),(IF(OR(C1034=\"REAL\",C1034=\"DWORD\",C1034=\"DINT\"),A1033+4+MOD(A1033,4),A1033+4)),(IF(OR(C1034=\"REAL\",C1034=\"DWORD\",C1034=\"DINT\"),A1033+4+MOD(A1033,4),A1033+2)))&\".0\"","v":"1528.0"},"验证通过","INT","风机盘管","R",{"$f":"F1033","v":"01H01"},"季节模式","风机盘管01H01-新云平台季节模式",{"$f":"E1034&VLOOKUP(D1034,list!$D$3:$F$501,2,FALSE)&F1034&\"_\"&VLOOKUP(G1034,list!$I$2:$K$502,2,FALSE)","v":"RFCU01H01_SM"},"RFCU01H01_SM AT%M1528.0 :INT; (*风机盘管01H01-新云平台季节模式*)","RFCU01H01_SM            AT%M1528.0     :INT; (*风机盘管01H01-新云平台季节模式*)"]
["1530.0","验证通过","BOOL","风机盘管","R","01H01","程序控制","风机盘管01H01-新云平台程序控制",{"$f":"E1035&VLOOKUP(D1035,list!$D$3:$F$501,2,FALSE)&F1035&\"_\"&VLOOKUP(G1035,list!$I$2:$K$502,2,FALSE)","v":"RFCU01H01_PC"},"RFCU01H01_PC AT%M1530.0 :BOOL; (*风机盘管01H01-新云平台程序控制*)","RFCU01H01_PC            AT%M1530.0     :BOOL; (*风机盘管01H01-新云平台程序控制*)"]
["1536.0","验证通过","REAL","风机盘管","L","01H01","设定温度值","风机盘管01H01-设定温度值",{"$f":"E1036&VLOOKUP(D1036,list!$D$3:$F$501,2,FALSE)&F1036&\"_\"&VLOOKUP(G1036,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_TSET"},"LFCU01H01_TSET AT%M1536.0 :REAL; (*风机盘管01H01-设定温度值*)","LFCU01H01_TSET          AT%M1536.0     :REAL; (*风机盘管01H01-设定温度值*)"]
["1540.0","验证通过","INT","风机盘管","L","01H01","季节模式","风机盘管01H01-季节模式",{"$f":"E1037&VLOOKUP(D1037,list!$D$3:$F$501,2,FALSE)&F1037&\"_\"&VLOOKUP(G1037,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_SM"},"LFCU01H01_SM AT%M1540.0 :INT; (*风机盘管01H01-季节模式*)","LFCU01H01_SM            AT%M1540.0     :INT; (*风机盘管01H01-季节模式*)"]
["1544.0","验证通过","REAL","风机盘管","L","01H01","温度换算值","风机盘管01H01-温度换算值",{"$f":"E1038&VLOOKUP(D1038,list!$D$3:$F$501,2,FALSE)&F1038&\"_\"&VLOOKUP(G1038,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_TS"},"LFCU01H01_TS AT%M1544.0 :REAL; (*风机盘管01H01-温度换算值*)","LFCU01H01_TS            AT%M1544.0     :REAL; (*风机盘管01H01-温度换算值*)"]
["1548.0","验证通过","BOOL","风机盘管","L","01H01","电磁阀手动控制","风机盘管01H01-电磁阀手动控制",{"$f":"E1039&VLOOKUP(D1039,list!$D$3:$F$501,2,FALSE)&F1039&\"_\"&VLOOKUP(G1039,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_EVMC"},"LFCU01H01_EVMC AT%M1548.0 :BOOL; (*风机盘管01H01-电磁阀手动控制*)","LFCU01H01_EVMC          AT%M1548.0     :BOOL; (*风机盘管01H01-电磁阀手动控制*)"]
["1550.0","验证通过","BOOL","风机盘管","L","01H01","电磁阀手动控制值","风机盘管01H01-电磁阀手动控制值",{"$f":"E1040&VLOOKUP(D1040,list!$D$3:$F$501,2,FALSE)&F1040&\"_\"&VLOOKUP(G1040,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_EVMV"},"LFCU01H01_EVMV AT%M1550.0 :BOOL; (*风机盘管01H01-电磁阀手动控制值*)","LFCU01H01_EVMV          AT%M1550.0     :BOOL; (*风机盘管01H01-电磁阀手动控制值*)"]
["1556.0","验证通过","REAL","风机盘管","L","01H01","回风温度换算值","风机盘管01H01-回风温度换算值",{"$f":"E1041&VLOOKUP(D1041,list!$D$3:$F$501,2,FALSE)&F1041&\"_\"&VLOOKUP(G1041,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RTS"},"LFCU01H01_RTS AT%M1556.0 :REAL; (*风机盘管01H01-回风温度换算值*)","LFCU01H01_RTS           AT%M1556.0     :REAL; (*风机盘管01H01-回风温度换算值*)"]
["1560.0","验证通过","BOOL","风机盘管","L","01H01","运行时间累积重置","风机盘管01H01-运行时间累积重置",{"$f":"E1042&VLOOKUP(D1042,list!$D$3:$F$501,2,FALSE)&F1042&\"_\"&VLOOKUP(G1042,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RST"},"LFCU01H01_RST AT%M1560.0 :BOOL; (*风机盘管01H01-运行时间累积重置*)","LFCU01H01_RST           AT%M1560.0     :BOOL; (*风机盘管01H01-运行时间累积重置*)"]
["1564.0","验证通过","REAL","风机盘管","L","01H01","运行时间累积重置值","风机盘管01H01-运行时间累积重置值",{"$f":"E1043&VLOOKUP(D1043,list!$D$3:$F$501,2,FALSE)&F1043&\"_\"&VLOOKUP(G1043,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RSTV"},"LFCU01H01_RSTV AT%M1564.0 :REAL; (*风机盘管01H01-运行时间累积重置值*)","LFCU01H01_RSTV          AT%M1564.0     :REAL; (*风机盘管01H01-运行时间累积重置值*)"]
["1568.0","验证通过","BOOL","风机盘管","L","01H01","隔离开关1","风机盘管01H01-隔离开关1",{"$f":"E1044&VLOOKUP(D1044,list!$D$3:$F$501,2,FALSE)&F1044&\"_\"&VLOOKUP(G1044,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_ISO1"},"LFCU01H01_ISO1 AT%M1568.0 :BOOL; (*风机盘管01H01-隔离开关1*)","LFCU01H01_ISO1          AT%M1568.0     :BOOL; (*风机盘管01H01-隔离开关1*)"]
["1572.0","验证通过","REAL","风机盘管","L","01H01","运行时间累积值","风机盘管01H01-运行时间累积值",{"$f":"E1045&VLOOKUP(D1045,list!$D$3:$F$501,2,FALSE)&F1045&\"_\"&VLOOKUP(G1045,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_RH"},"LFCU01H01_RH AT%M1572.0 :REAL; (*风机盘管01H01-运行时间累积值*)","LFCU01H01_RH            AT%M1572.0     :REAL; (*风机盘管01H01-运行时间累积值*)"]
["1576.0","验证通过","INT","风机盘管","L","01H01","设备状态代码","风机盘管01H01-设备状态代码",{"$f":"E1046&VLOOKUP(D1046,list!$D$3:$F$501,2,FALSE)&F1046&\"_\"&VLOOKUP(G1046,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_SN"},"LFCU01H01_SN AT%M1576.0 :INT; (*风机盘管01H01-设备状态代码*)","LFCU01H01_SN            AT%M1576.0     :INT; (*风机盘管01H01-设备状态代码*)"]
["1578.0","验证通过","INT","风机盘管","L","01H01","水阀控制转换值","风机盘管01H01-水阀控制转换值",{"$f":"E1047&VLOOKUP(D1047,list!$D$3:$F$501,2,FALSE)&F1047&\"_\"&VLOOKUP(G1047,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_WVCS"},"LFCU01H01_WVCS AT%M1578.0 :INT; (*风机盘管01H01-水阀控制转换值*)","LFCU01H01_WVCS          AT%M1578.0     :INT; (*风机盘管01H01-水阀控制转换值*)"]
["1580.0","验证通过","BOOL","风机盘管","L","01H01","程序控制","风机盘管01H01-程序控制",{"$f":"E1048&VLOOKUP(D1048,list!$D$3:$F$501,2,FALSE)&F1048&\"_\"&VLOOKUP(G1048,list!$I$2:$K$502,2,FALSE)","v":"LFCU01H01_PC"},"LFCU01H01_PC AT%M1580.0 :BOOL; (*风机盘管01H01-程序控制*)","LFCU01H01_PC            AT%M1580.0     :BOOL; (*风机盘管01H01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C807=\"REAL\",C807=\"DWORD\",C807=\"DINT\"),(IF(OR(C1050=\"REAL\",C1050=\"DWORD\",C1050=\"DINT\"),A807+4+MOD(A807,4),A807+4)),(IF(OR(C1050=\"REAL\",C1050=\"DWORD\",C1050=\"DINT\"),A807+4+MOD(A807,4),A807+2)))&\".0\"","v":"1308.0"},{"$f":"IF((IF(OR(C1050=\"INT\",C1050=\"WORD\",C1050=\"BOOL\"),MOD(A1050,2),MOD(A1050,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H06","设定温度值",{"$f":"D1050&F1050&\"-\"&IF(E1050=\"R\",\"新云平台\"&G1050,G1050)","v":"空调机组01H06-新云平台设定温度值"},{"$f":"E1050&VLOOKUP(D1050,list!$D$3:$F$501,2,FALSE)&F1050&\"_\"&VLOOKUP(G1050,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H06_TSET"},{"$f":"I1050&\" \"&\"AT%M\"&A1050&\" \"&\":\"&C1050&\";\"&\" \"&\"(*\"&H1050&\"*)\"","v":"RAHU01H06_TSET AT%M1308.0 :REAL; (*空调机组01H06-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1050,SEARCH(\"AT%\",J1050),,REPT(\" \",25-SEARCH(\"AT%\",J1050))),SEARCH(\":\",REPLACE(J1050,SEARCH(\"AT%\",J1050),,REPT(\" \",25-SEARCH(\"AT%\",J1050)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1050,SEARCH(\"AT%\",J1050),,REPT(\" \",25-SEARCH(\"AT%\",J1050))))))","v":"RAHU01H06_TSET          AT%M1308.0     :REAL; (*空调机组01H06-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1050=\"REAL\",C1050=\"DWORD\",C1050=\"DINT\"),(IF(OR(C1051=\"REAL\",C1051=\"DWORD\",C1051=\"DINT\"),A1050+4+MOD(A1050,4),A1050+4)),(IF(OR(C1051=\"REAL\",C1051=\"DWORD\",C1051=\"DINT\"),A1050+4+MOD(A1050,4),A1050+2)))&\".0\"","v":"1312.0"},"验证通过","INT","空调机组","R",{"$f":"F1050","v":"01H06"},"季节模式","空调机组01H06-新云平台季节模式",{"$f":"E1051&VLOOKUP(D1051,list!$D$3:$F$501,2,FALSE)&F1051&\"_\"&VLOOKUP(G1051,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H06_SM"},"RAHU01H06_SM AT%M1312.0 :INT; (*空调机组01H06-新云平台季节模式*)","RAHU01H06_SM            AT%M1312.0     :INT; (*空调机组01H06-新云平台季节模式*)"]
["1314.0","验证通过","BOOL","空调机组","R","01H06","程序控制","空调机组01H06-新云平台程序控制",{"$f":"E1052&VLOOKUP(D1052,list!$D$3:$F$501,2,FALSE)&F1052&\"_\"&VLOOKUP(G1052,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H06_PC"},"RAHU01H06_PC AT%M1314.0 :BOOL; (*空调机组01H06-新云平台程序控制*)","RAHU01H06_PC            AT%M1314.0     :BOOL; (*空调机组01H06-新云平台程序控制*)"]
["1320.0","验证通过","REAL","空调机组","L","01H06","设定温度值","空调机组01H06-设定温度值",{"$f":"E1053&VLOOKUP(D1053,list!$D$3:$F$501,2,FALSE)&F1053&\"_\"&VLOOKUP(G1053,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_TSET"},"LAHU01H06_TSET AT%M1320.0 :REAL; (*空调机组01H06-设定温度值*)","LAHU01H06_TSET          AT%M1320.0     :REAL; (*空调机组01H06-设定温度值*)"]
["1324.0","验证通过","INT","空调机组","L","01H06","季节模式","空调机组01H06-季节模式",{"$f":"E1054&VLOOKUP(D1054,list!$D$3:$F$501,2,FALSE)&F1054&\"_\"&VLOOKUP(G1054,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_SM"},"LAHU01H06_SM AT%M1324.0 :INT; (*空调机组01H06-季节模式*)","LAHU01H06_SM            AT%M1324.0     :INT; (*空调机组01H06-季节模式*)"]
["1328.0","验证通过","REAL","空调机组","L","01H06","水阀反馈换算值","空调机组01H06-水阀反馈换算值",{"$f":"E1055&VLOOKUP(D1055,list!$D$3:$F$501,2,FALSE)&F1055&\"_\"&VLOOKUP(G1055,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVBS"},"LAHU01H06_WVBS AT%M1328.0 :REAL; (*空调机组01H06-水阀反馈换算值*)","LAHU01H06_WVBS          AT%M1328.0     :REAL; (*空调机组01H06-水阀反馈换算值*)"]
["1332.0","验证通过","BOOL","空调机组","L","01H06","水阀手动控制","空调机组01H06-水阀手动控制",{"$f":"E1056&VLOOKUP(D1056,list!$D$3:$F$501,2,FALSE)&F1056&\"_\"&VLOOKUP(G1056,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVMC"},"LAHU01H06_WVMC AT%M1332.0 :BOOL; (*空调机组01H06-水阀手动控制*)","LAHU01H06_WVMC          AT%M1332.0     :BOOL; (*空调机组01H06-水阀手动控制*)"]
["1336.0","验证通过","REAL","空调机组","L","01H06","水阀手动控制值","空调机组01H06-水阀手动控制值",{"$f":"E1057&VLOOKUP(D1057,list!$D$3:$F$501,2,FALSE)&F1057&\"_\"&VLOOKUP(G1057,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVMV"},"LAHU01H06_WVMV AT%M1336.0 :REAL; (*空调机组01H06-水阀手动控制值*)","LAHU01H06_WVMV          AT%M1336.0     :REAL; (*空调机组01H06-水阀手动控制值*)"]
["1340.0","验证通过","REAL","空调机组","L","01H06","回风温度换算值","空调机组01H06-回风温度换算值",{"$f":"E1058&VLOOKUP(D1058,list!$D$3:$F$501,2,FALSE)&F1058&\"_\"&VLOOKUP(G1058,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RTS"},"LAHU01H06_RTS AT%M1340.0 :REAL; (*空调机组01H06-回风温度换算值*)","LAHU01H06_RTS           AT%M1340.0     :REAL; (*空调机组01H06-回风温度换算值*)"]
["1344.0","验证通过","BOOL","空调机组","L","01H06","运行时间累积重置","空调机组01H06-运行时间累积重置",{"$f":"E1059&VLOOKUP(D1059,list!$D$3:$F$501,2,FALSE)&F1059&\"_\"&VLOOKUP(G1059,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RST"},"LAHU01H06_RST AT%M1344.0 :BOOL; (*空调机组01H06-运行时间累积重置*)","LAHU01H06_RST           AT%M1344.0     :BOOL; (*空调机组01H06-运行时间累积重置*)"]
["1348.0","验证通过","REAL","空调机组","L","01H06","运行时间累积重置值","空调机组01H06-运行时间累积重置值",{"$f":"E1060&VLOOKUP(D1060,list!$D$3:$F$501,2,FALSE)&F1060&\"_\"&VLOOKUP(G1060,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RSTV"},"LAHU01H06_RSTV AT%M1348.0 :REAL; (*空调机组01H06-运行时间累积重置值*)","LAHU01H06_RSTV          AT%M1348.0     :REAL; (*空调机组01H06-运行时间累积重置值*)"]
["1352.0","验证通过","BOOL","空调机组","L","01H06","隔离开关1","空调机组01H06-隔离开关1",{"$f":"E1061&VLOOKUP(D1061,list!$D$3:$F$501,2,FALSE)&F1061&\"_\"&VLOOKUP(G1061,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_ISO1"},"LAHU01H06_ISO1 AT%M1352.0 :BOOL; (*空调机组01H06-隔离开关1*)","LAHU01H06_ISO1          AT%M1352.0     :BOOL; (*空调机组01H06-隔离开关1*)"]
["1354.0","验证通过","BOOL","空调机组","L","01H06","隔离开关2","空调机组01H06-隔离开关2",{"$f":"E1062&VLOOKUP(D1062,list!$D$3:$F$501,2,FALSE)&F1062&\"_\"&VLOOKUP(G1062,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_ISO2"},"LAHU01H06_ISO2 AT%M1354.0 :BOOL; (*空调机组01H06-隔离开关2*)","LAHU01H06_ISO2          AT%M1354.0     :BOOL; (*空调机组01H06-隔离开关2*)"]
["1360.0","验证通过","REAL","空调机组","L","01H06","P调节参数","空调机组01H06-P调节参数",{"$f":"E1063&VLOOKUP(D1063,list!$D$3:$F$501,2,FALSE)&F1063&\"_\"&VLOOKUP(G1063,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_VP"},"LAHU01H06_VP AT%M1360.0 :REAL; (*空调机组01H06-P调节参数*)","LAHU01H06_VP            AT%M1360.0     :REAL; (*空调机组01H06-P调节参数*)"]
["1364.0","验证通过","REAL","空调机组","L","01H06","I调节参数","空调机组01H06-I调节参数",{"$f":"E1064&VLOOKUP(D1064,list!$D$3:$F$501,2,FALSE)&F1064&\"_\"&VLOOKUP(G1064,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_VI"},"LAHU01H06_VI AT%M1364.0 :REAL; (*空调机组01H06-I调节参数*)","LAHU01H06_VI            AT%M1364.0     :REAL; (*空调机组01H06-I调节参数*)"]
["1368.0","验证通过","REAL","空调机组","L","01H06","运行时间累积值","空调机组01H06-运行时间累积值",{"$f":"E1065&VLOOKUP(D1065,list!$D$3:$F$501,2,FALSE)&F1065&\"_\"&VLOOKUP(G1065,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_RH"},"LAHU01H06_RH AT%M1368.0 :REAL; (*空调机组01H06-运行时间累积值*)","LAHU01H06_RH            AT%M1368.0     :REAL; (*空调机组01H06-运行时间累积值*)"]
["1372.0","验证通过","INT","空调机组","L","01H06","设备状态代码","空调机组01H06-设备状态代码",{"$f":"E1066&VLOOKUP(D1066,list!$D$3:$F$501,2,FALSE)&F1066&\"_\"&VLOOKUP(G1066,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_SN"},"LAHU01H06_SN AT%M1372.0 :INT; (*空调机组01H06-设备状态代码*)","LAHU01H06_SN            AT%M1372.0     :INT; (*空调机组01H06-设备状态代码*)"]
["1374.0","验证通过","INT","空调机组","L","01H06","水阀控制转换值","空调机组01H06-水阀控制转换值",{"$f":"E1067&VLOOKUP(D1067,list!$D$3:$F$501,2,FALSE)&F1067&\"_\"&VLOOKUP(G1067,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_WVCS"},"LAHU01H06_WVCS AT%M1374.0 :INT; (*空调机组01H06-水阀控制转换值*)","LAHU01H06_WVCS          AT%M1374.0     :INT; (*空调机组01H06-水阀控制转换值*)"]
["1376.0","验证通过","BOOL","空调机组","L","01H06","程序控制","空调机组01H06-程序控制",{"$f":"E1068&VLOOKUP(D1068,list!$D$3:$F$501,2,FALSE)&F1068&\"_\"&VLOOKUP(G1068,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H06_PC"},"LAHU01H06_PC AT%M1376.0 :BOOL; (*空调机组01H06-程序控制*)","LAHU01H06_PC            AT%M1376.0     :BOOL; (*空调机组01H06-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1068=\"REAL\",C1068=\"DWORD\",C1068=\"DINT\"),(IF(OR(C1070=\"REAL\",C1070=\"DWORD\",C1070=\"DINT\"),A1068+4+MOD(A1068,4),A1068+4)),(IF(OR(C1070=\"REAL\",C1070=\"DWORD\",C1070=\"DINT\"),A1068+4+MOD(A1068,4),A1068+2)))&\".0\"","v":"1380.0"},{"$f":"IF((IF(OR(C1070=\"INT\",C1070=\"WORD\",C1070=\"BOOL\"),MOD(A1070,2),MOD(A1070,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H07","设定温度值",{"$f":"D1070&F1070&\"-\"&IF(E1070=\"R\",\"新云平台\"&G1070,G1070)","v":"空调机组01H07-新云平台设定温度值"},{"$f":"E1070&VLOOKUP(D1070,list!$D$3:$F$501,2,FALSE)&F1070&\"_\"&VLOOKUP(G1070,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_TSET"},{"$f":"I1070&\" \"&\"AT%M\"&A1070&\" \"&\":\"&C1070&\";\"&\" \"&\"(*\"&H1070&\"*)\"","v":"RAHU01H07_TSET AT%M1380.0 :REAL; (*空调机组01H07-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1070,SEARCH(\"AT%\",J1070),,REPT(\" \",25-SEARCH(\"AT%\",J1070))),SEARCH(\":\",REPLACE(J1070,SEARCH(\"AT%\",J1070),,REPT(\" \",25-SEARCH(\"AT%\",J1070)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1070,SEARCH(\"AT%\",J1070),,REPT(\" \",25-SEARCH(\"AT%\",J1070))))))","v":"RAHU01H07_TSET          AT%M1380.0     :REAL; (*空调机组01H07-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1070=\"REAL\",C1070=\"DWORD\",C1070=\"DINT\"),(IF(OR(C1071=\"REAL\",C1071=\"DWORD\",C1071=\"DINT\"),A1070+4+MOD(A1070,4),A1070+4)),(IF(OR(C1071=\"REAL\",C1071=\"DWORD\",C1071=\"DINT\"),A1070+4+MOD(A1070,4),A1070+2)))&\".0\"","v":"1384.0"},"验证通过","INT","空调机组","R",{"$f":"F1070","v":"01H07"},"季节模式","空调机组01H07-新云平台季节模式",{"$f":"E1071&VLOOKUP(D1071,list!$D$3:$F$501,2,FALSE)&F1071&\"_\"&VLOOKUP(G1071,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_SM"},"RAHU01H07_SM AT%M1384.0 :INT; (*空调机组01H07-新云平台季节模式*)","RAHU01H07_SM            AT%M1384.0     :INT; (*空调机组01H07-新云平台季节模式*)"]
["1386.0","验证通过","BOOL","空调机组","R","01H07","程序控制","空调机组01H07-新云平台程序控制",{"$f":"E1072&VLOOKUP(D1072,list!$D$3:$F$501,2,FALSE)&F1072&\"_\"&VLOOKUP(G1072,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H07_PC"},"RAHU01H07_PC AT%M1386.0 :BOOL; (*空调机组01H07-新云平台程序控制*)","RAHU01H07_PC            AT%M1386.0     :BOOL; (*空调机组01H07-新云平台程序控制*)"]
["1392.0","验证通过","REAL","空调机组","L","01H07","设定温度值","空调机组01H07-设定温度值",{"$f":"E1073&VLOOKUP(D1073,list!$D$3:$F$501,2,FALSE)&F1073&\"_\"&VLOOKUP(G1073,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_TSET"},"LAHU01H07_TSET AT%M1392.0 :REAL; (*空调机组01H07-设定温度值*)","LAHU01H07_TSET          AT%M1392.0     :REAL; (*空调机组01H07-设定温度值*)"]
["1396.0","验证通过","INT","空调机组","L","01H07","季节模式","空调机组01H07-季节模式",{"$f":"E1074&VLOOKUP(D1074,list!$D$3:$F$501,2,FALSE)&F1074&\"_\"&VLOOKUP(G1074,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_SM"},"LAHU01H07_SM AT%M1396.0 :INT; (*空调机组01H07-季节模式*)","LAHU01H07_SM            AT%M1396.0     :INT; (*空调机组01H07-季节模式*)"]
["1400.0","验证通过","REAL","空调机组","L","01H07","水阀反馈换算值","空调机组01H07-水阀反馈换算值",{"$f":"E1075&VLOOKUP(D1075,list!$D$3:$F$501,2,FALSE)&F1075&\"_\"&VLOOKUP(G1075,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVBS"},"LAHU01H07_WVBS AT%M1400.0 :REAL; (*空调机组01H07-水阀反馈换算值*)","LAHU01H07_WVBS          AT%M1400.0     :REAL; (*空调机组01H07-水阀反馈换算值*)"]
["1404.0","验证通过","BOOL","空调机组","L","01H07","水阀手动控制","空调机组01H07-水阀手动控制",{"$f":"E1076&VLOOKUP(D1076,list!$D$3:$F$501,2,FALSE)&F1076&\"_\"&VLOOKUP(G1076,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVMC"},"LAHU01H07_WVMC AT%M1404.0 :BOOL; (*空调机组01H07-水阀手动控制*)","LAHU01H07_WVMC          AT%M1404.0     :BOOL; (*空调机组01H07-水阀手动控制*)"]
["1408.0","验证通过","REAL","空调机组","L","01H07","水阀手动控制值","空调机组01H07-水阀手动控制值",{"$f":"E1077&VLOOKUP(D1077,list!$D$3:$F$501,2,FALSE)&F1077&\"_\"&VLOOKUP(G1077,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVMV"},"LAHU01H07_WVMV AT%M1408.0 :REAL; (*空调机组01H07-水阀手动控制值*)","LAHU01H07_WVMV          AT%M1408.0     :REAL; (*空调机组01H07-水阀手动控制值*)"]
["1412.0","验证通过","REAL","空调机组","L","01H07","回风温度换算值","空调机组01H07-回风温度换算值",{"$f":"E1078&VLOOKUP(D1078,list!$D$3:$F$501,2,FALSE)&F1078&\"_\"&VLOOKUP(G1078,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RTS"},"LAHU01H07_RTS AT%M1412.0 :REAL; (*空调机组01H07-回风温度换算值*)","LAHU01H07_RTS           AT%M1412.0     :REAL; (*空调机组01H07-回风温度换算值*)"]
["1416.0","验证通过","BOOL","空调机组","L","01H07","运行时间累积重置","空调机组01H07-运行时间累积重置",{"$f":"E1079&VLOOKUP(D1079,list!$D$3:$F$501,2,FALSE)&F1079&\"_\"&VLOOKUP(G1079,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RST"},"LAHU01H07_RST AT%M1416.0 :BOOL; (*空调机组01H07-运行时间累积重置*)","LAHU01H07_RST           AT%M1416.0     :BOOL; (*空调机组01H07-运行时间累积重置*)"]
["1420.0","验证通过","REAL","空调机组","L","01H07","运行时间累积重置值","空调机组01H07-运行时间累积重置值",{"$f":"E1080&VLOOKUP(D1080,list!$D$3:$F$501,2,FALSE)&F1080&\"_\"&VLOOKUP(G1080,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RSTV"},"LAHU01H07_RSTV AT%M1420.0 :REAL; (*空调机组01H07-运行时间累积重置值*)","LAHU01H07_RSTV          AT%M1420.0     :REAL; (*空调机组01H07-运行时间累积重置值*)"]
["1424.0","验证通过","BOOL","空调机组","L","01H07","隔离开关1","空调机组01H07-隔离开关1",{"$f":"E1081&VLOOKUP(D1081,list!$D$3:$F$501,2,FALSE)&F1081&\"_\"&VLOOKUP(G1081,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_ISO1"},"LAHU01H07_ISO1 AT%M1424.0 :BOOL; (*空调机组01H07-隔离开关1*)","LAHU01H07_ISO1          AT%M1424.0     :BOOL; (*空调机组01H07-隔离开关1*)"]
["1426.0","验证通过","BOOL","空调机组","L","01H07","隔离开关2","空调机组01H07-隔离开关2",{"$f":"E1082&VLOOKUP(D1082,list!$D$3:$F$501,2,FALSE)&F1082&\"_\"&VLOOKUP(G1082,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_ISO2"},"LAHU01H07_ISO2 AT%M1426.0 :BOOL; (*空调机组01H07-隔离开关2*)","LAHU01H07_ISO2          AT%M1426.0     :BOOL; (*空调机组01H07-隔离开关2*)"]
["1432.0","验证通过","REAL","空调机组","L","01H07","P调节参数","空调机组01H07-P调节参数",{"$f":"E1083&VLOOKUP(D1083,list!$D$3:$F$501,2,FALSE)&F1083&\"_\"&VLOOKUP(G1083,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_VP"},"LAHU01H07_VP AT%M1432.0 :REAL; (*空调机组01H07-P调节参数*)","LAHU01H07_VP            AT%M1432.0     :REAL; (*空调机组01H07-P调节参数*)"]
["1436.0","验证通过","REAL","空调机组","L","01H07","I调节参数","空调机组01H07-I调节参数",{"$f":"E1084&VLOOKUP(D1084,list!$D$3:$F$501,2,FALSE)&F1084&\"_\"&VLOOKUP(G1084,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_VI"},"LAHU01H07_VI AT%M1436.0 :REAL; (*空调机组01H07-I调节参数*)","LAHU01H07_VI            AT%M1436.0     :REAL; (*空调机组01H07-I调节参数*)"]
["1440.0","验证通过","REAL","空调机组","L","01H07","运行时间累积值","空调机组01H07-运行时间累积值",{"$f":"E1085&VLOOKUP(D1085,list!$D$3:$F$501,2,FALSE)&F1085&\"_\"&VLOOKUP(G1085,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_RH"},"LAHU01H07_RH AT%M1440.0 :REAL; (*空调机组01H07-运行时间累积值*)","LAHU01H07_RH            AT%M1440.0     :REAL; (*空调机组01H07-运行时间累积值*)"]
["1444.0","验证通过","INT","空调机组","L","01H07","设备状态代码","空调机组01H07-设备状态代码",{"$f":"E1086&VLOOKUP(D1086,list!$D$3:$F$501,2,FALSE)&F1086&\"_\"&VLOOKUP(G1086,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_SN"},"LAHU01H07_SN AT%M1444.0 :INT; (*空调机组01H07-设备状态代码*)","LAHU01H07_SN            AT%M1444.0     :INT; (*空调机组01H07-设备状态代码*)"]
["1446.0","验证通过","INT","空调机组","L","01H07","水阀控制转换值","空调机组01H07-水阀控制转换值",{"$f":"E1087&VLOOKUP(D1087,list!$D$3:$F$501,2,FALSE)&F1087&\"_\"&VLOOKUP(G1087,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_WVCS"},"LAHU01H07_WVCS AT%M1446.0 :INT; (*空调机组01H07-水阀控制转换值*)","LAHU01H07_WVCS          AT%M1446.0     :INT; (*空调机组01H07-水阀控制转换值*)"]
["1448.0","验证通过","BOOL","空调机组","L","01H07","程序控制","空调机组01H07-程序控制",{"$f":"E1088&VLOOKUP(D1088,list!$D$3:$F$501,2,FALSE)&F1088&\"_\"&VLOOKUP(G1088,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H07_PC"},"LAHU01H07_PC AT%M1448.0 :BOOL; (*空调机组01H07-程序控制*)","LAHU01H07_PC            AT%M1448.0     :BOOL; (*空调机组01H07-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1088=\"REAL\",C1088=\"DWORD\",C1088=\"DINT\"),(IF(OR(C1090=\"REAL\",C1090=\"DWORD\",C1090=\"DINT\"),A1088+4+MOD(A1088,4),A1088+4)),(IF(OR(C1090=\"REAL\",C1090=\"DWORD\",C1090=\"DINT\"),A1088+4+MOD(A1088,4),A1088+2)))&\".0\"","v":"1452.0"},{"$f":"IF((IF(OR(C1090=\"INT\",C1090=\"WORD\",C1090=\"BOOL\"),MOD(A1090,2),MOD(A1090,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H08","设定温度值",{"$f":"D1090&F1090&\"-\"&IF(E1090=\"R\",\"新云平台\"&G1090,G1090)","v":"空调机组01H08-新云平台设定温度值"},{"$f":"E1090&VLOOKUP(D1090,list!$D$3:$F$501,2,FALSE)&F1090&\"_\"&VLOOKUP(G1090,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_TSET"},{"$f":"I1090&\" \"&\"AT%M\"&A1090&\" \"&\":\"&C1090&\";\"&\" \"&\"(*\"&H1090&\"*)\"","v":"RAHU01H08_TSET AT%M1452.0 :REAL; (*空调机组01H08-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1090,SEARCH(\"AT%\",J1090),,REPT(\" \",25-SEARCH(\"AT%\",J1090))),SEARCH(\":\",REPLACE(J1090,SEARCH(\"AT%\",J1090),,REPT(\" \",25-SEARCH(\"AT%\",J1090)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1090,SEARCH(\"AT%\",J1090),,REPT(\" \",25-SEARCH(\"AT%\",J1090))))))","v":"RAHU01H08_TSET          AT%M1452.0     :REAL; (*空调机组01H08-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1090=\"REAL\",C1090=\"DWORD\",C1090=\"DINT\"),(IF(OR(C1091=\"REAL\",C1091=\"DWORD\",C1091=\"DINT\"),A1090+4+MOD(A1090,4),A1090+4)),(IF(OR(C1091=\"REAL\",C1091=\"DWORD\",C1091=\"DINT\"),A1090+4+MOD(A1090,4),A1090+2)))&\".0\"","v":"1456.0"},"验证通过","INT","空调机组","R",{"$f":"F1090","v":"01H08"},"季节模式","空调机组01H08-新云平台季节模式",{"$f":"E1091&VLOOKUP(D1091,list!$D$3:$F$501,2,FALSE)&F1091&\"_\"&VLOOKUP(G1091,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_SM"},"RAHU01H08_SM AT%M1456.0 :INT; (*空调机组01H08-新云平台季节模式*)","RAHU01H08_SM            AT%M1456.0     :INT; (*空调机组01H08-新云平台季节模式*)"]
["1458.0","验证通过","BOOL","空调机组","R","01H08","程序控制","空调机组01H08-新云平台程序控制",{"$f":"E1092&VLOOKUP(D1092,list!$D$3:$F$501,2,FALSE)&F1092&\"_\"&VLOOKUP(G1092,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H08_PC"},"RAHU01H08_PC AT%M1458.0 :BOOL; (*空调机组01H08-新云平台程序控制*)","RAHU01H08_PC            AT%M1458.0     :BOOL; (*空调机组01H08-新云平台程序控制*)"]
["1464.0","验证通过","REAL","空调机组","L","01H08","设定温度值","空调机组01H08-设定温度值",{"$f":"E1093&VLOOKUP(D1093,list!$D$3:$F$501,2,FALSE)&F1093&\"_\"&VLOOKUP(G1093,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_TSET"},"LAHU01H08_TSET AT%M1464.0 :REAL; (*空调机组01H08-设定温度值*)","LAHU01H08_TSET          AT%M1464.0     :REAL; (*空调机组01H08-设定温度值*)"]
["1468.0","验证通过","INT","空调机组","L","01H08","季节模式","空调机组01H08-季节模式",{"$f":"E1094&VLOOKUP(D1094,list!$D$3:$F$501,2,FALSE)&F1094&\"_\"&VLOOKUP(G1094,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_SM"},"LAHU01H08_SM AT%M1468.0 :INT; (*空调机组01H08-季节模式*)","LAHU01H08_SM            AT%M1468.0     :INT; (*空调机组01H08-季节模式*)"]
["1472.0","验证通过","REAL","空调机组","L","01H08","水阀反馈换算值","空调机组01H08-水阀反馈换算值",{"$f":"E1095&VLOOKUP(D1095,list!$D$3:$F$501,2,FALSE)&F1095&\"_\"&VLOOKUP(G1095,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVBS"},"LAHU01H08_WVBS AT%M1472.0 :REAL; (*空调机组01H08-水阀反馈换算值*)","LAHU01H08_WVBS          AT%M1472.0     :REAL; (*空调机组01H08-水阀反馈换算值*)"]
["1476.0","验证通过","BOOL","空调机组","L","01H08","水阀手动控制","空调机组01H08-水阀手动控制",{"$f":"E1096&VLOOKUP(D1096,list!$D$3:$F$501,2,FALSE)&F1096&\"_\"&VLOOKUP(G1096,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVMC"},"LAHU01H08_WVMC AT%M1476.0 :BOOL; (*空调机组01H08-水阀手动控制*)","LAHU01H08_WVMC          AT%M1476.0     :BOOL; (*空调机组01H08-水阀手动控制*)"]
["1480.0","验证通过","REAL","空调机组","L","01H08","水阀手动控制值","空调机组01H08-水阀手动控制值",{"$f":"E1097&VLOOKUP(D1097,list!$D$3:$F$501,2,FALSE)&F1097&\"_\"&VLOOKUP(G1097,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVMV"},"LAHU01H08_WVMV AT%M1480.0 :REAL; (*空调机组01H08-水阀手动控制值*)","LAHU01H08_WVMV          AT%M1480.0     :REAL; (*空调机组01H08-水阀手动控制值*)"]
["1484.0","验证通过","REAL","空调机组","L","01H08","回风温度换算值","空调机组01H08-回风温度换算值",{"$f":"E1098&VLOOKUP(D1098,list!$D$3:$F$501,2,FALSE)&F1098&\"_\"&VLOOKUP(G1098,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RTS"},"LAHU01H08_RTS AT%M1484.0 :REAL; (*空调机组01H08-回风温度换算值*)","LAHU01H08_RTS           AT%M1484.0     :REAL; (*空调机组01H08-回风温度换算值*)"]
["1488.0","验证通过","BOOL","空调机组","L","01H08","运行时间累积重置","空调机组01H08-运行时间累积重置",{"$f":"E1099&VLOOKUP(D1099,list!$D$3:$F$501,2,FALSE)&F1099&\"_\"&VLOOKUP(G1099,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RST"},"LAHU01H08_RST AT%M1488.0 :BOOL; (*空调机组01H08-运行时间累积重置*)","LAHU01H08_RST           AT%M1488.0     :BOOL; (*空调机组01H08-运行时间累积重置*)"]
["1492.0","验证通过","REAL","空调机组","L","01H08","运行时间累积重置值","空调机组01H08-运行时间累积重置值",{"$f":"E1100&VLOOKUP(D1100,list!$D$3:$F$501,2,FALSE)&F1100&\"_\"&VLOOKUP(G1100,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RSTV"},"LAHU01H08_RSTV AT%M1492.0 :REAL; (*空调机组01H08-运行时间累积重置值*)","LAHU01H08_RSTV          AT%M1492.0     :REAL; (*空调机组01H08-运行时间累积重置值*)"]
["1496.0","验证通过","BOOL","空调机组","L","01H08","隔离开关1","空调机组01H08-隔离开关1",{"$f":"E1101&VLOOKUP(D1101,list!$D$3:$F$501,2,FALSE)&F1101&\"_\"&VLOOKUP(G1101,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_ISO1"},"LAHU01H08_ISO1 AT%M1496.0 :BOOL; (*空调机组01H08-隔离开关1*)","LAHU01H08_ISO1          AT%M1496.0     :BOOL; (*空调机组01H08-隔离开关1*)"]
["1498.0","验证通过","BOOL","空调机组","L","01H08","隔离开关2","空调机组01H08-隔离开关2",{"$f":"E1102&VLOOKUP(D1102,list!$D$3:$F$501,2,FALSE)&F1102&\"_\"&VLOOKUP(G1102,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_ISO2"},"LAHU01H08_ISO2 AT%M1498.0 :BOOL; (*空调机组01H08-隔离开关2*)","LAHU01H08_ISO2          AT%M1498.0     :BOOL; (*空调机组01H08-隔离开关2*)"]
["1504.0","验证通过","REAL","空调机组","L","01H08","P调节参数","空调机组01H08-P调节参数",{"$f":"E1103&VLOOKUP(D1103,list!$D$3:$F$501,2,FALSE)&F1103&\"_\"&VLOOKUP(G1103,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_VP"},"LAHU01H08_VP AT%M1504.0 :REAL; (*空调机组01H08-P调节参数*)","LAHU01H08_VP            AT%M1504.0     :REAL; (*空调机组01H08-P调节参数*)"]
["1508.0","验证通过","REAL","空调机组","L","01H08","I调节参数","空调机组01H08-I调节参数",{"$f":"E1104&VLOOKUP(D1104,list!$D$3:$F$501,2,FALSE)&F1104&\"_\"&VLOOKUP(G1104,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_VI"},"LAHU01H08_VI AT%M1508.0 :REAL; (*空调机组01H08-I调节参数*)","LAHU01H08_VI            AT%M1508.0     :REAL; (*空调机组01H08-I调节参数*)"]
["1512.0","验证通过","REAL","空调机组","L","01H08","运行时间累积值","空调机组01H08-运行时间累积值",{"$f":"E1105&VLOOKUP(D1105,list!$D$3:$F$501,2,FALSE)&F1105&\"_\"&VLOOKUP(G1105,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_RH"},"LAHU01H08_RH AT%M1512.0 :REAL; (*空调机组01H08-运行时间累积值*)","LAHU01H08_RH            AT%M1512.0     :REAL; (*空调机组01H08-运行时间累积值*)"]
["1516.0","验证通过","INT","空调机组","L","01H08","设备状态代码","空调机组01H08-设备状态代码",{"$f":"E1106&VLOOKUP(D1106,list!$D$3:$F$501,2,FALSE)&F1106&\"_\"&VLOOKUP(G1106,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_SN"},"LAHU01H08_SN AT%M1516.0 :INT; (*空调机组01H08-设备状态代码*)","LAHU01H08_SN            AT%M1516.0     :INT; (*空调机组01H08-设备状态代码*)"]
["1518.0","验证通过","INT","空调机组","L","01H08","水阀控制转换值","空调机组01H08-水阀控制转换值",{"$f":"E1107&VLOOKUP(D1107,list!$D$3:$F$501,2,FALSE)&F1107&\"_\"&VLOOKUP(G1107,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_WVCS"},"LAHU01H08_WVCS AT%M1518.0 :INT; (*空调机组01H08-水阀控制转换值*)","LAHU01H08_WVCS          AT%M1518.0     :INT; (*空调机组01H08-水阀控制转换值*)"]
["1520.0","验证通过","BOOL","空调机组","L","01H08","程序控制","空调机组01H08-程序控制",{"$f":"E1108&VLOOKUP(D1108,list!$D$3:$F$501,2,FALSE)&F1108&\"_\"&VLOOKUP(G1108,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H08_PC"},"LAHU01H08_PC AT%M1520.0 :BOOL; (*空调机组01H08-程序控制*)","LAHU01H08_PC            AT%M1520.0     :BOOL; (*空调机组01H08-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1108=\"REAL\",C1108=\"DWORD\",C1108=\"DINT\"),(IF(OR(C1110=\"REAL\",C1110=\"DWORD\",C1110=\"DINT\"),A1108+4+MOD(A1108,4),A1108+4)),(IF(OR(C1110=\"REAL\",C1110=\"DWORD\",C1110=\"DINT\"),A1108+4+MOD(A1108,4),A1108+2)))&\".0\"","v":"1524.0"},{"$f":"IF((IF(OR(C1110=\"INT\",C1110=\"WORD\",C1110=\"BOOL\"),MOD(A1110,2),MOD(A1110,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H09","设定温度值",{"$f":"D1110&F1110&\"-\"&IF(E1110=\"R\",\"新云平台\"&G1110,G1110)","v":"空调机组01H09-新云平台设定温度值"},{"$f":"E1110&VLOOKUP(D1110,list!$D$3:$F$501,2,FALSE)&F1110&\"_\"&VLOOKUP(G1110,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H09_TSET"},{"$f":"I1110&\" \"&\"AT%M\"&A1110&\" \"&\":\"&C1110&\";\"&\" \"&\"(*\"&H1110&\"*)\"","v":"RAHU01H09_TSET AT%M1524.0 :REAL; (*空调机组01H09-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1110,SEARCH(\"AT%\",J1110),,REPT(\" \",25-SEARCH(\"AT%\",J1110))),SEARCH(\":\",REPLACE(J1110,SEARCH(\"AT%\",J1110),,REPT(\" \",25-SEARCH(\"AT%\",J1110)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1110,SEARCH(\"AT%\",J1110),,REPT(\" \",25-SEARCH(\"AT%\",J1110))))))","v":"RAHU01H09_TSET          AT%M1524.0     :REAL; (*空调机组01H09-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1110=\"REAL\",C1110=\"DWORD\",C1110=\"DINT\"),(IF(OR(C1111=\"REAL\",C1111=\"DWORD\",C1111=\"DINT\"),A1110+4+MOD(A1110,4),A1110+4)),(IF(OR(C1111=\"REAL\",C1111=\"DWORD\",C1111=\"DINT\"),A1110+4+MOD(A1110,4),A1110+2)))&\".0\"","v":"1528.0"},"验证通过","INT","空调机组","R",{"$f":"F1110","v":"01H09"},"季节模式","空调机组01H09-新云平台季节模式",{"$f":"E1111&VLOOKUP(D1111,list!$D$3:$F$501,2,FALSE)&F1111&\"_\"&VLOOKUP(G1111,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H09_SM"},"RAHU01H09_SM AT%M1528.0 :INT; (*空调机组01H09-新云平台季节模式*)","RAHU01H09_SM            AT%M1528.0     :INT; (*空调机组01H09-新云平台季节模式*)"]
["1530.0","验证通过","BOOL","空调机组","R","01H09","程序控制","空调机组01H09-新云平台程序控制",{"$f":"E1112&VLOOKUP(D1112,list!$D$3:$F$501,2,FALSE)&F1112&\"_\"&VLOOKUP(G1112,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H09_PC"},"RAHU01H09_PC AT%M1530.0 :BOOL; (*空调机组01H09-新云平台程序控制*)","RAHU01H09_PC            AT%M1530.0     :BOOL; (*空调机组01H09-新云平台程序控制*)"]
["1536.0","验证通过","REAL","空调机组","L","01H09","设定温度值","空调机组01H09-设定温度值",{"$f":"E1113&VLOOKUP(D1113,list!$D$3:$F$501,2,FALSE)&F1113&\"_\"&VLOOKUP(G1113,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_TSET"},"LAHU01H09_TSET AT%M1536.0 :REAL; (*空调机组01H09-设定温度值*)","LAHU01H09_TSET          AT%M1536.0     :REAL; (*空调机组01H09-设定温度值*)"]
["1540.0","验证通过","INT","空调机组","L","01H09","季节模式","空调机组01H09-季节模式",{"$f":"E1114&VLOOKUP(D1114,list!$D$3:$F$501,2,FALSE)&F1114&\"_\"&VLOOKUP(G1114,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_SM"},"LAHU01H09_SM AT%M1540.0 :INT; (*空调机组01H09-季节模式*)","LAHU01H09_SM            AT%M1540.0     :INT; (*空调机组01H09-季节模式*)"]
["1544.0","验证通过","REAL","空调机组","L","01H09","水阀反馈换算值","空调机组01H09-水阀反馈换算值",{"$f":"E1115&VLOOKUP(D1115,list!$D$3:$F$501,2,FALSE)&F1115&\"_\"&VLOOKUP(G1115,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVBS"},"LAHU01H09_WVBS AT%M1544.0 :REAL; (*空调机组01H09-水阀反馈换算值*)","LAHU01H09_WVBS          AT%M1544.0     :REAL; (*空调机组01H09-水阀反馈换算值*)"]
["1548.0","验证通过","BOOL","空调机组","L","01H09","水阀手动控制","空调机组01H09-水阀手动控制",{"$f":"E1116&VLOOKUP(D1116,list!$D$3:$F$501,2,FALSE)&F1116&\"_\"&VLOOKUP(G1116,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVMC"},"LAHU01H09_WVMC AT%M1548.0 :BOOL; (*空调机组01H09-水阀手动控制*)","LAHU01H09_WVMC          AT%M1548.0     :BOOL; (*空调机组01H09-水阀手动控制*)"]
["1552.0","验证通过","REAL","空调机组","L","01H09","水阀手动控制值","空调机组01H09-水阀手动控制值",{"$f":"E1117&VLOOKUP(D1117,list!$D$3:$F$501,2,FALSE)&F1117&\"_\"&VLOOKUP(G1117,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVMV"},"LAHU01H09_WVMV AT%M1552.0 :REAL; (*空调机组01H09-水阀手动控制值*)","LAHU01H09_WVMV          AT%M1552.0     :REAL; (*空调机组01H09-水阀手动控制值*)"]
["1556.0","验证通过","REAL","空调机组","L","01H09","回风温度换算值","空调机组01H09-回风温度换算值",{"$f":"E1118&VLOOKUP(D1118,list!$D$3:$F$501,2,FALSE)&F1118&\"_\"&VLOOKUP(G1118,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RTS"},"LAHU01H09_RTS AT%M1556.0 :REAL; (*空调机组01H09-回风温度换算值*)","LAHU01H09_RTS           AT%M1556.0     :REAL; (*空调机组01H09-回风温度换算值*)"]
["1560.0","验证通过","BOOL","空调机组","L","01H09","运行时间累积重置","空调机组01H09-运行时间累积重置",{"$f":"E1119&VLOOKUP(D1119,list!$D$3:$F$501,2,FALSE)&F1119&\"_\"&VLOOKUP(G1119,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RST"},"LAHU01H09_RST AT%M1560.0 :BOOL; (*空调机组01H09-运行时间累积重置*)","LAHU01H09_RST           AT%M1560.0     :BOOL; (*空调机组01H09-运行时间累积重置*)"]
["1564.0","验证通过","REAL","空调机组","L","01H09","运行时间累积重置值","空调机组01H09-运行时间累积重置值",{"$f":"E1120&VLOOKUP(D1120,list!$D$3:$F$501,2,FALSE)&F1120&\"_\"&VLOOKUP(G1120,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RSTV"},"LAHU01H09_RSTV AT%M1564.0 :REAL; (*空调机组01H09-运行时间累积重置值*)","LAHU01H09_RSTV          AT%M1564.0     :REAL; (*空调机组01H09-运行时间累积重置值*)"]
["1568.0","验证通过","BOOL","空调机组","L","01H09","隔离开关1","空调机组01H09-隔离开关1",{"$f":"E1121&VLOOKUP(D1121,list!$D$3:$F$501,2,FALSE)&F1121&\"_\"&VLOOKUP(G1121,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_ISO1"},"LAHU01H09_ISO1 AT%M1568.0 :BOOL; (*空调机组01H09-隔离开关1*)","LAHU01H09_ISO1          AT%M1568.0     :BOOL; (*空调机组01H09-隔离开关1*)"]
["1570.0","验证通过","BOOL","空调机组","L","01H09","隔离开关2","空调机组01H09-隔离开关2",{"$f":"E1122&VLOOKUP(D1122,list!$D$3:$F$501,2,FALSE)&F1122&\"_\"&VLOOKUP(G1122,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_ISO2"},"LAHU01H09_ISO2 AT%M1570.0 :BOOL; (*空调机组01H09-隔离开关2*)","LAHU01H09_ISO2          AT%M1570.0     :BOOL; (*空调机组01H09-隔离开关2*)"]
["1576.0","验证通过","REAL","空调机组","L","01H09","P调节参数","空调机组01H09-P调节参数",{"$f":"E1123&VLOOKUP(D1123,list!$D$3:$F$501,2,FALSE)&F1123&\"_\"&VLOOKUP(G1123,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_VP"},"LAHU01H09_VP AT%M1576.0 :REAL; (*空调机组01H09-P调节参数*)","LAHU01H09_VP            AT%M1576.0     :REAL; (*空调机组01H09-P调节参数*)"]
["1580.0","验证通过","REAL","空调机组","L","01H09","I调节参数","空调机组01H09-I调节参数",{"$f":"E1124&VLOOKUP(D1124,list!$D$3:$F$501,2,FALSE)&F1124&\"_\"&VLOOKUP(G1124,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_VI"},"LAHU01H09_VI AT%M1580.0 :REAL; (*空调机组01H09-I调节参数*)","LAHU01H09_VI            AT%M1580.0     :REAL; (*空调机组01H09-I调节参数*)"]
["1584.0","验证通过","REAL","空调机组","L","01H09","运行时间累积值","空调机组01H09-运行时间累积值",{"$f":"E1125&VLOOKUP(D1125,list!$D$3:$F$501,2,FALSE)&F1125&\"_\"&VLOOKUP(G1125,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_RH"},"LAHU01H09_RH AT%M1584.0 :REAL; (*空调机组01H09-运行时间累积值*)","LAHU01H09_RH            AT%M1584.0     :REAL; (*空调机组01H09-运行时间累积值*)"]
["1588.0","验证通过","INT","空调机组","L","01H09","设备状态代码","空调机组01H09-设备状态代码",{"$f":"E1126&VLOOKUP(D1126,list!$D$3:$F$501,2,FALSE)&F1126&\"_\"&VLOOKUP(G1126,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_SN"},"LAHU01H09_SN AT%M1588.0 :INT; (*空调机组01H09-设备状态代码*)","LAHU01H09_SN            AT%M1588.0     :INT; (*空调机组01H09-设备状态代码*)"]
["1590.0","验证通过","INT","空调机组","L","01H09","水阀控制转换值","空调机组01H09-水阀控制转换值",{"$f":"E1127&VLOOKUP(D1127,list!$D$3:$F$501,2,FALSE)&F1127&\"_\"&VLOOKUP(G1127,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_WVCS"},"LAHU01H09_WVCS AT%M1590.0 :INT; (*空调机组01H09-水阀控制转换值*)","LAHU01H09_WVCS          AT%M1590.0     :INT; (*空调机组01H09-水阀控制转换值*)"]
["1592.0","验证通过","BOOL","空调机组","L","01H09","程序控制","空调机组01H09-程序控制",{"$f":"E1128&VLOOKUP(D1128,list!$D$3:$F$501,2,FALSE)&F1128&\"_\"&VLOOKUP(G1128,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H09_PC"},"LAHU01H09_PC AT%M1592.0 :BOOL; (*空调机组01H09-程序控制*)","LAHU01H09_PC            AT%M1592.0     :BOOL; (*空调机组01H09-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1128=\"REAL\",C1128=\"DWORD\",C1128=\"DINT\"),(IF(OR(C1130=\"REAL\",C1130=\"DWORD\",C1130=\"DINT\"),A1128+4+MOD(A1128,4),A1128+4)),(IF(OR(C1130=\"REAL\",C1130=\"DWORD\",C1130=\"DINT\"),A1128+4+MOD(A1128,4),A1128+2)))&\".0\"","v":"1596.0"},{"$f":"IF((IF(OR(C1130=\"INT\",C1130=\"WORD\",C1130=\"BOOL\"),MOD(A1130,2),MOD(A1130,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H10","设定温度值",{"$f":"D1130&F1130&\"-\"&IF(E1130=\"R\",\"新云平台\"&G1130,G1130)","v":"空调机组01H10-新云平台设定温度值"},{"$f":"E1130&VLOOKUP(D1130,list!$D$3:$F$501,2,FALSE)&F1130&\"_\"&VLOOKUP(G1130,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H10_TSET"},{"$f":"I1130&\" \"&\"AT%M\"&A1130&\" \"&\":\"&C1130&\";\"&\" \"&\"(*\"&H1130&\"*)\"","v":"RAHU01H10_TSET AT%M1596.0 :REAL; (*空调机组01H10-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1130,SEARCH(\"AT%\",J1130),,REPT(\" \",25-SEARCH(\"AT%\",J1130))),SEARCH(\":\",REPLACE(J1130,SEARCH(\"AT%\",J1130),,REPT(\" \",25-SEARCH(\"AT%\",J1130)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1130,SEARCH(\"AT%\",J1130),,REPT(\" \",25-SEARCH(\"AT%\",J1130))))))","v":"RAHU01H10_TSET          AT%M1596.0     :REAL; (*空调机组01H10-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1130=\"REAL\",C1130=\"DWORD\",C1130=\"DINT\"),(IF(OR(C1131=\"REAL\",C1131=\"DWORD\",C1131=\"DINT\"),A1130+4+MOD(A1130,4),A1130+4)),(IF(OR(C1131=\"REAL\",C1131=\"DWORD\",C1131=\"DINT\"),A1130+4+MOD(A1130,4),A1130+2)))&\".0\"","v":"1600.0"},"验证通过","INT","空调机组","R",{"$f":"F1130","v":"01H10"},"季节模式","空调机组01H10-新云平台季节模式",{"$f":"E1131&VLOOKUP(D1131,list!$D$3:$F$501,2,FALSE)&F1131&\"_\"&VLOOKUP(G1131,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H10_SM"},"RAHU01H10_SM AT%M1600.0 :INT; (*空调机组01H10-新云平台季节模式*)","RAHU01H10_SM            AT%M1600.0     :INT; (*空调机组01H10-新云平台季节模式*)"]
["1602.0","验证通过","BOOL","空调机组","R","01H10","程序控制","空调机组01H10-新云平台程序控制",{"$f":"E1132&VLOOKUP(D1132,list!$D$3:$F$501,2,FALSE)&F1132&\"_\"&VLOOKUP(G1132,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H10_PC"},"RAHU01H10_PC AT%M1602.0 :BOOL; (*空调机组01H10-新云平台程序控制*)","RAHU01H10_PC            AT%M1602.0     :BOOL; (*空调机组01H10-新云平台程序控制*)"]
["1608.0","验证通过","REAL","空调机组","L","01H10","设定温度值","空调机组01H10-设定温度值",{"$f":"E1133&VLOOKUP(D1133,list!$D$3:$F$501,2,FALSE)&F1133&\"_\"&VLOOKUP(G1133,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_TSET"},"LAHU01H10_TSET AT%M1608.0 :REAL; (*空调机组01H10-设定温度值*)","LAHU01H10_TSET          AT%M1608.0     :REAL; (*空调机组01H10-设定温度值*)"]
["1612.0","验证通过","INT","空调机组","L","01H10","季节模式","空调机组01H10-季节模式",{"$f":"E1134&VLOOKUP(D1134,list!$D$3:$F$501,2,FALSE)&F1134&\"_\"&VLOOKUP(G1134,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_SM"},"LAHU01H10_SM AT%M1612.0 :INT; (*空调机组01H10-季节模式*)","LAHU01H10_SM            AT%M1612.0     :INT; (*空调机组01H10-季节模式*)"]
["1616.0","验证通过","REAL","空调机组","L","01H10","水阀反馈换算值","空调机组01H10-水阀反馈换算值",{"$f":"E1135&VLOOKUP(D1135,list!$D$3:$F$501,2,FALSE)&F1135&\"_\"&VLOOKUP(G1135,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVBS"},"LAHU01H10_WVBS AT%M1616.0 :REAL; (*空调机组01H10-水阀反馈换算值*)","LAHU01H10_WVBS          AT%M1616.0     :REAL; (*空调机组01H10-水阀反馈换算值*)"]
["1620.0","验证通过","BOOL","空调机组","L","01H10","水阀手动控制","空调机组01H10-水阀手动控制",{"$f":"E1136&VLOOKUP(D1136,list!$D$3:$F$501,2,FALSE)&F1136&\"_\"&VLOOKUP(G1136,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVMC"},"LAHU01H10_WVMC AT%M1620.0 :BOOL; (*空调机组01H10-水阀手动控制*)","LAHU01H10_WVMC          AT%M1620.0     :BOOL; (*空调机组01H10-水阀手动控制*)"]
["1624.0","验证通过","REAL","空调机组","L","01H10","水阀手动控制值","空调机组01H10-水阀手动控制值",{"$f":"E1137&VLOOKUP(D1137,list!$D$3:$F$501,2,FALSE)&F1137&\"_\"&VLOOKUP(G1137,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVMV"},"LAHU01H10_WVMV AT%M1624.0 :REAL; (*空调机组01H10-水阀手动控制值*)","LAHU01H10_WVMV          AT%M1624.0     :REAL; (*空调机组01H10-水阀手动控制值*)"]
["1628.0","验证通过","REAL","空调机组","L","01H10","回风温度换算值","空调机组01H10-回风温度换算值",{"$f":"E1138&VLOOKUP(D1138,list!$D$3:$F$501,2,FALSE)&F1138&\"_\"&VLOOKUP(G1138,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RTS"},"LAHU01H10_RTS AT%M1628.0 :REAL; (*空调机组01H10-回风温度换算值*)","LAHU01H10_RTS           AT%M1628.0     :REAL; (*空调机组01H10-回风温度换算值*)"]
["1632.0","验证通过","BOOL","空调机组","L","01H10","运行时间累积重置","空调机组01H10-运行时间累积重置",{"$f":"E1139&VLOOKUP(D1139,list!$D$3:$F$501,2,FALSE)&F1139&\"_\"&VLOOKUP(G1139,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RST"},"LAHU01H10_RST AT%M1632.0 :BOOL; (*空调机组01H10-运行时间累积重置*)","LAHU01H10_RST           AT%M1632.0     :BOOL; (*空调机组01H10-运行时间累积重置*)"]
["1636.0","验证通过","REAL","空调机组","L","01H10","运行时间累积重置值","空调机组01H10-运行时间累积重置值",{"$f":"E1140&VLOOKUP(D1140,list!$D$3:$F$501,2,FALSE)&F1140&\"_\"&VLOOKUP(G1140,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RSTV"},"LAHU01H10_RSTV AT%M1636.0 :REAL; (*空调机组01H10-运行时间累积重置值*)","LAHU01H10_RSTV          AT%M1636.0     :REAL; (*空调机组01H10-运行时间累积重置值*)"]
["1640.0","验证通过","BOOL","空调机组","L","01H10","隔离开关1","空调机组01H10-隔离开关1",{"$f":"E1141&VLOOKUP(D1141,list!$D$3:$F$501,2,FALSE)&F1141&\"_\"&VLOOKUP(G1141,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_ISO1"},"LAHU01H10_ISO1 AT%M1640.0 :BOOL; (*空调机组01H10-隔离开关1*)","LAHU01H10_ISO1          AT%M1640.0     :BOOL; (*空调机组01H10-隔离开关1*)"]
["1642.0","验证通过","BOOL","空调机组","L","01H10","隔离开关2","空调机组01H10-隔离开关2",{"$f":"E1142&VLOOKUP(D1142,list!$D$3:$F$501,2,FALSE)&F1142&\"_\"&VLOOKUP(G1142,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_ISO2"},"LAHU01H10_ISO2 AT%M1642.0 :BOOL; (*空调机组01H10-隔离开关2*)","LAHU01H10_ISO2          AT%M1642.0     :BOOL; (*空调机组01H10-隔离开关2*)"]
["1648.0","验证通过","REAL","空调机组","L","01H10","P调节参数","空调机组01H10-P调节参数",{"$f":"E1143&VLOOKUP(D1143,list!$D$3:$F$501,2,FALSE)&F1143&\"_\"&VLOOKUP(G1143,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_VP"},"LAHU01H10_VP AT%M1648.0 :REAL; (*空调机组01H10-P调节参数*)","LAHU01H10_VP            AT%M1648.0     :REAL; (*空调机组01H10-P调节参数*)"]
["1652.0","验证通过","REAL","空调机组","L","01H10","I调节参数","空调机组01H10-I调节参数",{"$f":"E1144&VLOOKUP(D1144,list!$D$3:$F$501,2,FALSE)&F1144&\"_\"&VLOOKUP(G1144,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_VI"},"LAHU01H10_VI AT%M1652.0 :REAL; (*空调机组01H10-I调节参数*)","LAHU01H10_VI            AT%M1652.0     :REAL; (*空调机组01H10-I调节参数*)"]
["1656.0","验证通过","REAL","空调机组","L","01H10","运行时间累积值","空调机组01H10-运行时间累积值",{"$f":"E1145&VLOOKUP(D1145,list!$D$3:$F$501,2,FALSE)&F1145&\"_\"&VLOOKUP(G1145,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_RH"},"LAHU01H10_RH AT%M1656.0 :REAL; (*空调机组01H10-运行时间累积值*)","LAHU01H10_RH            AT%M1656.0     :REAL; (*空调机组01H10-运行时间累积值*)"]
["1660.0","验证通过","INT","空调机组","L","01H10","设备状态代码","空调机组01H10-设备状态代码",{"$f":"E1146&VLOOKUP(D1146,list!$D$3:$F$501,2,FALSE)&F1146&\"_\"&VLOOKUP(G1146,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_SN"},"LAHU01H10_SN AT%M1660.0 :INT; (*空调机组01H10-设备状态代码*)","LAHU01H10_SN            AT%M1660.0     :INT; (*空调机组01H10-设备状态代码*)"]
["1662.0","验证通过","INT","空调机组","L","01H10","水阀控制转换值","空调机组01H10-水阀控制转换值",{"$f":"E1147&VLOOKUP(D1147,list!$D$3:$F$501,2,FALSE)&F1147&\"_\"&VLOOKUP(G1147,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_WVCS"},"LAHU01H10_WVCS AT%M1662.0 :INT; (*空调机组01H10-水阀控制转换值*)","LAHU01H10_WVCS          AT%M1662.0     :INT; (*空调机组01H10-水阀控制转换值*)"]
["1664.0","验证通过","BOOL","空调机组","L","01H10","程序控制","空调机组01H10-程序控制",{"$f":"E1148&VLOOKUP(D1148,list!$D$3:$F$501,2,FALSE)&F1148&\"_\"&VLOOKUP(G1148,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H10_PC"},"LAHU01H10_PC AT%M1664.0 :BOOL; (*空调机组01H10-程序控制*)","LAHU01H10_PC            AT%M1664.0     :BOOL; (*空调机组01H10-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1148=\"REAL\",C1148=\"DWORD\",C1148=\"DINT\"),(IF(OR(C1150=\"REAL\",C1150=\"DWORD\",C1150=\"DINT\"),A1148+4+MOD(A1148,4),A1148+4)),(IF(OR(C1150=\"REAL\",C1150=\"DWORD\",C1150=\"DINT\"),A1148+4+MOD(A1148,4),A1148+2)))&\".0\"","v":"1668.0"},{"$f":"IF((IF(OR(C1150=\"INT\",C1150=\"WORD\",C1150=\"BOOL\"),MOD(A1150,2),MOD(A1150,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H11","设定温度值",{"$f":"D1150&F1150&\"-\"&IF(E1150=\"R\",\"新云平台\"&G1150,G1150)","v":"空调机组01H11-新云平台设定温度值"},{"$f":"E1150&VLOOKUP(D1150,list!$D$3:$F$501,2,FALSE)&F1150&\"_\"&VLOOKUP(G1150,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H11_TSET"},{"$f":"I1150&\" \"&\"AT%M\"&A1150&\" \"&\":\"&C1150&\";\"&\" \"&\"(*\"&H1150&\"*)\"","v":"RAHU01H11_TSET AT%M1668.0 :REAL; (*空调机组01H11-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1150,SEARCH(\"AT%\",J1150),,REPT(\" \",25-SEARCH(\"AT%\",J1150))),SEARCH(\":\",REPLACE(J1150,SEARCH(\"AT%\",J1150),,REPT(\" \",25-SEARCH(\"AT%\",J1150)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1150,SEARCH(\"AT%\",J1150),,REPT(\" \",25-SEARCH(\"AT%\",J1150))))))","v":"RAHU01H11_TSET          AT%M1668.0     :REAL; (*空调机组01H11-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1150=\"REAL\",C1150=\"DWORD\",C1150=\"DINT\"),(IF(OR(C1151=\"REAL\",C1151=\"DWORD\",C1151=\"DINT\"),A1150+4+MOD(A1150,4),A1150+4)),(IF(OR(C1151=\"REAL\",C1151=\"DWORD\",C1151=\"DINT\"),A1150+4+MOD(A1150,4),A1150+2)))&\".0\"","v":"1672.0"},"验证通过","INT","空调机组","R",{"$f":"F1150","v":"01H11"},"季节模式","空调机组01H11-新云平台季节模式",{"$f":"E1151&VLOOKUP(D1151,list!$D$3:$F$501,2,FALSE)&F1151&\"_\"&VLOOKUP(G1151,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H11_SM"},"RAHU01H11_SM AT%M1672.0 :INT; (*空调机组01H11-新云平台季节模式*)","RAHU01H11_SM            AT%M1672.0     :INT; (*空调机组01H11-新云平台季节模式*)"]
["1674.0","验证通过","BOOL","空调机组","R","01H11","程序控制","空调机组01H11-新云平台程序控制",{"$f":"E1152&VLOOKUP(D1152,list!$D$3:$F$501,2,FALSE)&F1152&\"_\"&VLOOKUP(G1152,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H11_PC"},"RAHU01H11_PC AT%M1674.0 :BOOL; (*空调机组01H11-新云平台程序控制*)","RAHU01H11_PC            AT%M1674.0     :BOOL; (*空调机组01H11-新云平台程序控制*)"]
["1680.0","验证通过","REAL","空调机组","L","01H11","设定温度值","空调机组01H11-设定温度值",{"$f":"E1153&VLOOKUP(D1153,list!$D$3:$F$501,2,FALSE)&F1153&\"_\"&VLOOKUP(G1153,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_TSET"},"LAHU01H11_TSET AT%M1680.0 :REAL; (*空调机组01H11-设定温度值*)","LAHU01H11_TSET          AT%M1680.0     :REAL; (*空调机组01H11-设定温度值*)"]
["1684.0","验证通过","INT","空调机组","L","01H11","季节模式","空调机组01H11-季节模式",{"$f":"E1154&VLOOKUP(D1154,list!$D$3:$F$501,2,FALSE)&F1154&\"_\"&VLOOKUP(G1154,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_SM"},"LAHU01H11_SM AT%M1684.0 :INT; (*空调机组01H11-季节模式*)","LAHU01H11_SM            AT%M1684.0     :INT; (*空调机组01H11-季节模式*)"]
["1688.0","验证通过","REAL","空调机组","L","01H11","水阀反馈换算值","空调机组01H11-水阀反馈换算值",{"$f":"E1155&VLOOKUP(D1155,list!$D$3:$F$501,2,FALSE)&F1155&\"_\"&VLOOKUP(G1155,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_WVBS"},"LAHU01H11_WVBS AT%M1688.0 :REAL; (*空调机组01H11-水阀反馈换算值*)","LAHU01H11_WVBS          AT%M1688.0     :REAL; (*空调机组01H11-水阀反馈换算值*)"]
["1692.0","验证通过","BOOL","空调机组","L","01H11","水阀手动控制","空调机组01H11-水阀手动控制",{"$f":"E1156&VLOOKUP(D1156,list!$D$3:$F$501,2,FALSE)&F1156&\"_\"&VLOOKUP(G1156,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_WVMC"},"LAHU01H11_WVMC AT%M1692.0 :BOOL; (*空调机组01H11-水阀手动控制*)","LAHU01H11_WVMC          AT%M1692.0     :BOOL; (*空调机组01H11-水阀手动控制*)"]
["1696.0","验证通过","REAL","空调机组","L","01H11","水阀手动控制值","空调机组01H11-水阀手动控制值",{"$f":"E1157&VLOOKUP(D1157,list!$D$3:$F$501,2,FALSE)&F1157&\"_\"&VLOOKUP(G1157,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_WVMV"},"LAHU01H11_WVMV AT%M1696.0 :REAL; (*空调机组01H11-水阀手动控制值*)","LAHU01H11_WVMV          AT%M1696.0     :REAL; (*空调机组01H11-水阀手动控制值*)"]
["1700.0","验证通过","REAL","空调机组","L","01H11","回风温度换算值","空调机组01H11-回风温度换算值",{"$f":"E1158&VLOOKUP(D1158,list!$D$3:$F$501,2,FALSE)&F1158&\"_\"&VLOOKUP(G1158,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_RTS"},"LAHU01H11_RTS AT%M1700.0 :REAL; (*空调机组01H11-回风温度换算值*)","LAHU01H11_RTS           AT%M1700.0     :REAL; (*空调机组01H11-回风温度换算值*)"]
["1704.0","验证通过","BOOL","空调机组","L","01H11","运行时间累积重置","空调机组01H11-运行时间累积重置",{"$f":"E1159&VLOOKUP(D1159,list!$D$3:$F$501,2,FALSE)&F1159&\"_\"&VLOOKUP(G1159,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_RST"},"LAHU01H11_RST AT%M1704.0 :BOOL; (*空调机组01H11-运行时间累积重置*)","LAHU01H11_RST           AT%M1704.0     :BOOL; (*空调机组01H11-运行时间累积重置*)"]
["1708.0","验证通过","REAL","空调机组","L","01H11","运行时间累积重置值","空调机组01H11-运行时间累积重置值",{"$f":"E1160&VLOOKUP(D1160,list!$D$3:$F$501,2,FALSE)&F1160&\"_\"&VLOOKUP(G1160,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_RSTV"},"LAHU01H11_RSTV AT%M1708.0 :REAL; (*空调机组01H11-运行时间累积重置值*)","LAHU01H11_RSTV          AT%M1708.0     :REAL; (*空调机组01H11-运行时间累积重置值*)"]
["1712.0","验证通过","BOOL","空调机组","L","01H11","隔离开关1","空调机组01H11-隔离开关1",{"$f":"E1161&VLOOKUP(D1161,list!$D$3:$F$501,2,FALSE)&F1161&\"_\"&VLOOKUP(G1161,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_ISO1"},"LAHU01H11_ISO1 AT%M1712.0 :BOOL; (*空调机组01H11-隔离开关1*)","LAHU01H11_ISO1          AT%M1712.0     :BOOL; (*空调机组01H11-隔离开关1*)"]
["1714.0","验证通过","BOOL","空调机组","L","01H11","隔离开关2","空调机组01H11-隔离开关2",{"$f":"E1162&VLOOKUP(D1162,list!$D$3:$F$501,2,FALSE)&F1162&\"_\"&VLOOKUP(G1162,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_ISO2"},"LAHU01H11_ISO2 AT%M1714.0 :BOOL; (*空调机组01H11-隔离开关2*)","LAHU01H11_ISO2          AT%M1714.0     :BOOL; (*空调机组01H11-隔离开关2*)"]
["1720.0","验证通过","REAL","空调机组","L","01H11","P调节参数","空调机组01H11-P调节参数",{"$f":"E1163&VLOOKUP(D1163,list!$D$3:$F$501,2,FALSE)&F1163&\"_\"&VLOOKUP(G1163,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_VP"},"LAHU01H11_VP AT%M1720.0 :REAL; (*空调机组01H11-P调节参数*)","LAHU01H11_VP            AT%M1720.0     :REAL; (*空调机组01H11-P调节参数*)"]
["1724.0","验证通过","REAL","空调机组","L","01H11","I调节参数","空调机组01H11-I调节参数",{"$f":"E1164&VLOOKUP(D1164,list!$D$3:$F$501,2,FALSE)&F1164&\"_\"&VLOOKUP(G1164,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_VI"},"LAHU01H11_VI AT%M1724.0 :REAL; (*空调机组01H11-I调节参数*)","LAHU01H11_VI            AT%M1724.0     :REAL; (*空调机组01H11-I调节参数*)"]
["1728.0","验证通过","REAL","空调机组","L","01H11","运行时间累积值","空调机组01H11-运行时间累积值",{"$f":"E1165&VLOOKUP(D1165,list!$D$3:$F$501,2,FALSE)&F1165&\"_\"&VLOOKUP(G1165,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_RH"},"LAHU01H11_RH AT%M1728.0 :REAL; (*空调机组01H11-运行时间累积值*)","LAHU01H11_RH            AT%M1728.0     :REAL; (*空调机组01H11-运行时间累积值*)"]
["1732.0","验证通过","INT","空调机组","L","01H11","设备状态代码","空调机组01H11-设备状态代码",{"$f":"E1166&VLOOKUP(D1166,list!$D$3:$F$501,2,FALSE)&F1166&\"_\"&VLOOKUP(G1166,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_SN"},"LAHU01H11_SN AT%M1732.0 :INT; (*空调机组01H11-设备状态代码*)","LAHU01H11_SN            AT%M1732.0     :INT; (*空调机组01H11-设备状态代码*)"]
["1734.0","验证通过","INT","空调机组","L","01H11","水阀控制转换值","空调机组01H11-水阀控制转换值",{"$f":"E1167&VLOOKUP(D1167,list!$D$3:$F$501,2,FALSE)&F1167&\"_\"&VLOOKUP(G1167,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_WVCS"},"LAHU01H11_WVCS AT%M1734.0 :INT; (*空调机组01H11-水阀控制转换值*)","LAHU01H11_WVCS          AT%M1734.0     :INT; (*空调机组01H11-水阀控制转换值*)"]
["1736.0","验证通过","BOOL","空调机组","L","01H11","程序控制","空调机组01H11-程序控制",{"$f":"E1168&VLOOKUP(D1168,list!$D$3:$F$501,2,FALSE)&F1168&\"_\"&VLOOKUP(G1168,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H11_PC"},"LAHU01H11_PC AT%M1736.0 :BOOL; (*空调机组01H11-程序控制*)","LAHU01H11_PC            AT%M1736.0     :BOOL; (*空调机组01H11-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1168=\"REAL\",C1168=\"DWORD\",C1168=\"DINT\"),(IF(OR(C1170=\"REAL\",C1170=\"DWORD\",C1170=\"DINT\"),A1168+4+MOD(A1168,4),A1168+4)),(IF(OR(C1170=\"REAL\",C1170=\"DWORD\",C1170=\"DINT\"),A1168+4+MOD(A1168,4),A1168+2)))&\".0\"","v":"1740.0"},{"$f":"IF((IF(OR(C1170=\"INT\",C1170=\"WORD\",C1170=\"BOOL\"),MOD(A1170,2),MOD(A1170,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","01H12","设定温度值",{"$f":"D1170&F1170&\"-\"&IF(E1170=\"R\",\"新云平台\"&G1170,G1170)","v":"空调机组01H12-新云平台设定温度值"},{"$f":"E1170&VLOOKUP(D1170,list!$D$3:$F$501,2,FALSE)&F1170&\"_\"&VLOOKUP(G1170,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H12_TSET"},{"$f":"I1170&\" \"&\"AT%M\"&A1170&\" \"&\":\"&C1170&\";\"&\" \"&\"(*\"&H1170&\"*)\"","v":"RAHU01H12_TSET AT%M1740.0 :REAL; (*空调机组01H12-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1170,SEARCH(\"AT%\",J1170),,REPT(\" \",25-SEARCH(\"AT%\",J1170))),SEARCH(\":\",REPLACE(J1170,SEARCH(\"AT%\",J1170),,REPT(\" \",25-SEARCH(\"AT%\",J1170)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1170,SEARCH(\"AT%\",J1170),,REPT(\" \",25-SEARCH(\"AT%\",J1170))))))","v":"RAHU01H12_TSET          AT%M1740.0     :REAL; (*空调机组01H12-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1170=\"REAL\",C1170=\"DWORD\",C1170=\"DINT\"),(IF(OR(C1171=\"REAL\",C1171=\"DWORD\",C1171=\"DINT\"),A1170+4+MOD(A1170,4),A1170+4)),(IF(OR(C1171=\"REAL\",C1171=\"DWORD\",C1171=\"DINT\"),A1170+4+MOD(A1170,4),A1170+2)))&\".0\"","v":"1744.0"},"验证通过","INT","空调机组","R",{"$f":"F1170","v":"01H12"},"季节模式","空调机组01H12-新云平台季节模式",{"$f":"E1171&VLOOKUP(D1171,list!$D$3:$F$501,2,FALSE)&F1171&\"_\"&VLOOKUP(G1171,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H12_SM"},"RAHU01H12_SM AT%M1744.0 :INT; (*空调机组01H12-新云平台季节模式*)","RAHU01H12_SM            AT%M1744.0     :INT; (*空调机组01H12-新云平台季节模式*)"]
["1746.0","验证通过","BOOL","空调机组","R","01H12","程序控制","空调机组01H12-新云平台程序控制",{"$f":"E1172&VLOOKUP(D1172,list!$D$3:$F$501,2,FALSE)&F1172&\"_\"&VLOOKUP(G1172,list!$I$2:$K$502,2,FALSE)","v":"RAHU01H12_PC"},"RAHU01H12_PC AT%M1746.0 :BOOL; (*空调机组01H12-新云平台程序控制*)","RAHU01H12_PC            AT%M1746.0     :BOOL; (*空调机组01H12-新云平台程序控制*)"]
["1752.0","验证通过","REAL","空调机组","L","01H12","设定温度值","空调机组01H12-设定温度值",{"$f":"E1173&VLOOKUP(D1173,list!$D$3:$F$501,2,FALSE)&F1173&\"_\"&VLOOKUP(G1173,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_TSET"},"LAHU01H12_TSET AT%M1752.0 :REAL; (*空调机组01H12-设定温度值*)","LAHU01H12_TSET          AT%M1752.0     :REAL; (*空调机组01H12-设定温度值*)"]
["1756.0","验证通过","INT","空调机组","L","01H12","季节模式","空调机组01H12-季节模式",{"$f":"E1174&VLOOKUP(D1174,list!$D$3:$F$501,2,FALSE)&F1174&\"_\"&VLOOKUP(G1174,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_SM"},"LAHU01H12_SM AT%M1756.0 :INT; (*空调机组01H12-季节模式*)","LAHU01H12_SM            AT%M1756.0     :INT; (*空调机组01H12-季节模式*)"]
["1760.0","验证通过","REAL","空调机组","L","01H12","水阀反馈换算值","空调机组01H12-水阀反馈换算值",{"$f":"E1175&VLOOKUP(D1175,list!$D$3:$F$501,2,FALSE)&F1175&\"_\"&VLOOKUP(G1175,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_WVBS"},"LAHU01H12_WVBS AT%M1760.0 :REAL; (*空调机组01H12-水阀反馈换算值*)","LAHU01H12_WVBS          AT%M1760.0     :REAL; (*空调机组01H12-水阀反馈换算值*)"]
["1764.0","验证通过","BOOL","空调机组","L","01H12","水阀手动控制","空调机组01H12-水阀手动控制",{"$f":"E1176&VLOOKUP(D1176,list!$D$3:$F$501,2,FALSE)&F1176&\"_\"&VLOOKUP(G1176,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_WVMC"},"LAHU01H12_WVMC AT%M1764.0 :BOOL; (*空调机组01H12-水阀手动控制*)","LAHU01H12_WVMC          AT%M1764.0     :BOOL; (*空调机组01H12-水阀手动控制*)"]
["1768.0","验证通过","REAL","空调机组","L","01H12","水阀手动控制值","空调机组01H12-水阀手动控制值",{"$f":"E1177&VLOOKUP(D1177,list!$D$3:$F$501,2,FALSE)&F1177&\"_\"&VLOOKUP(G1177,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_WVMV"},"LAHU01H12_WVMV AT%M1768.0 :REAL; (*空调机组01H12-水阀手动控制值*)","LAHU01H12_WVMV          AT%M1768.0     :REAL; (*空调机组01H12-水阀手动控制值*)"]
["1772.0","验证通过","REAL","空调机组","L","01H12","回风温度换算值","空调机组01H12-回风温度换算值",{"$f":"E1178&VLOOKUP(D1178,list!$D$3:$F$501,2,FALSE)&F1178&\"_\"&VLOOKUP(G1178,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_RTS"},"LAHU01H12_RTS AT%M1772.0 :REAL; (*空调机组01H12-回风温度换算值*)","LAHU01H12_RTS           AT%M1772.0     :REAL; (*空调机组01H12-回风温度换算值*)"]
["1776.0","验证通过","BOOL","空调机组","L","01H12","运行时间累积重置","空调机组01H12-运行时间累积重置",{"$f":"E1179&VLOOKUP(D1179,list!$D$3:$F$501,2,FALSE)&F1179&\"_\"&VLOOKUP(G1179,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_RST"},"LAHU01H12_RST AT%M1776.0 :BOOL; (*空调机组01H12-运行时间累积重置*)","LAHU01H12_RST           AT%M1776.0     :BOOL; (*空调机组01H12-运行时间累积重置*)"]
["1780.0","验证通过","REAL","空调机组","L","01H12","运行时间累积重置值","空调机组01H12-运行时间累积重置值",{"$f":"E1180&VLOOKUP(D1180,list!$D$3:$F$501,2,FALSE)&F1180&\"_\"&VLOOKUP(G1180,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_RSTV"},"LAHU01H12_RSTV AT%M1780.0 :REAL; (*空调机组01H12-运行时间累积重置值*)","LAHU01H12_RSTV          AT%M1780.0     :REAL; (*空调机组01H12-运行时间累积重置值*)"]
["1784.0","验证通过","BOOL","空调机组","L","01H12","隔离开关1","空调机组01H12-隔离开关1",{"$f":"E1181&VLOOKUP(D1181,list!$D$3:$F$501,2,FALSE)&F1181&\"_\"&VLOOKUP(G1181,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_ISO1"},"LAHU01H12_ISO1 AT%M1784.0 :BOOL; (*空调机组01H12-隔离开关1*)","LAHU01H12_ISO1          AT%M1784.0     :BOOL; (*空调机组01H12-隔离开关1*)"]
["1786.0","验证通过","BOOL","空调机组","L","01H12","隔离开关2","空调机组01H12-隔离开关2",{"$f":"E1182&VLOOKUP(D1182,list!$D$3:$F$501,2,FALSE)&F1182&\"_\"&VLOOKUP(G1182,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_ISO2"},"LAHU01H12_ISO2 AT%M1786.0 :BOOL; (*空调机组01H12-隔离开关2*)","LAHU01H12_ISO2          AT%M1786.0     :BOOL; (*空调机组01H12-隔离开关2*)"]
["1792.0","验证通过","REAL","空调机组","L","01H12","P调节参数","空调机组01H12-P调节参数",{"$f":"E1183&VLOOKUP(D1183,list!$D$3:$F$501,2,FALSE)&F1183&\"_\"&VLOOKUP(G1183,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_VP"},"LAHU01H12_VP AT%M1792.0 :REAL; (*空调机组01H12-P调节参数*)","LAHU01H12_VP            AT%M1792.0     :REAL; (*空调机组01H12-P调节参数*)"]
["1796.0","验证通过","REAL","空调机组","L","01H12","I调节参数","空调机组01H12-I调节参数",{"$f":"E1184&VLOOKUP(D1184,list!$D$3:$F$501,2,FALSE)&F1184&\"_\"&VLOOKUP(G1184,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_VI"},"LAHU01H12_VI AT%M1796.0 :REAL; (*空调机组01H12-I调节参数*)","LAHU01H12_VI            AT%M1796.0     :REAL; (*空调机组01H12-I调节参数*)"]
["1800.0","验证通过","REAL","空调机组","L","01H12","运行时间累积值","空调机组01H12-运行时间累积值",{"$f":"E1185&VLOOKUP(D1185,list!$D$3:$F$501,2,FALSE)&F1185&\"_\"&VLOOKUP(G1185,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_RH"},"LAHU01H12_RH AT%M1800.0 :REAL; (*空调机组01H12-运行时间累积值*)","LAHU01H12_RH            AT%M1800.0     :REAL; (*空调机组01H12-运行时间累积值*)"]
["1804.0","验证通过","INT","空调机组","L","01H12","设备状态代码","空调机组01H12-设备状态代码",{"$f":"E1186&VLOOKUP(D1186,list!$D$3:$F$501,2,FALSE)&F1186&\"_\"&VLOOKUP(G1186,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_SN"},"LAHU01H12_SN AT%M1804.0 :INT; (*空调机组01H12-设备状态代码*)","LAHU01H12_SN            AT%M1804.0     :INT; (*空调机组01H12-设备状态代码*)"]
["1806.0","验证通过","INT","空调机组","L","01H12","水阀控制转换值","空调机组01H12-水阀控制转换值",{"$f":"E1187&VLOOKUP(D1187,list!$D$3:$F$501,2,FALSE)&F1187&\"_\"&VLOOKUP(G1187,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_WVCS"},"LAHU01H12_WVCS AT%M1806.0 :INT; (*空调机组01H12-水阀控制转换值*)","LAHU01H12_WVCS          AT%M1806.0     :INT; (*空调机组01H12-水阀控制转换值*)"]
["1808.0","验证通过","BOOL","空调机组","L","01H12","程序控制","空调机组01H12-程序控制",{"$f":"E1188&VLOOKUP(D1188,list!$D$3:$F$501,2,FALSE)&F1188&\"_\"&VLOOKUP(G1188,list!$I$2:$K$502,2,FALSE)","v":"LAHU01H12_PC"},"LAHU01H12_PC AT%M1808.0 :BOOL; (*空调机组01H12-程序控制*)","LAHU01H12_PC            AT%M1808.0     :BOOL; (*空调机组01H12-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(#REF!=\"REAL\",#REF!=\"DWORD\",#REF!=\"DINT\"),(IF(OR(C1190=\"REAL\",C1190=\"DWORD\",C1190=\"DINT\"),#REF!+4+MOD(#REF!,4),#REF!+4)),(IF(OR(C1190=\"REAL\",C1190=\"DWORD\",C1190=\"DINT\"),#REF!+4+MOD(#REF!,4),#REF!+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1190=\"INT\",C1190=\"WORD\",C1190=\"BOOL\"),MOD(A1190,2),MOD(A1190,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","空调机组","R","01C04","设定温度值",{"$f":"D1190&F1190&\"-\"&IF(E1190=\"R\",\"新云平台\"&G1190,G1190)","v":"空调机组01C04-新云平台设定温度值"},{"$f":"E1190&VLOOKUP(D1190,list!$D$3:$F$501,2,FALSE)&F1190&\"_\"&VLOOKUP(G1190,list!$I$2:$K$502,2,FALSE)","v":"RAHU01C04_TSET"},{"$f":"I1190&\" \"&\"AT%M\"&A1190&\" \"&\":\"&C1190&\";\"&\" \"&\"(*\"&H1190&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J1190,SEARCH(\"AT%\",J1190),,REPT(\" \",25-SEARCH(\"AT%\",J1190))),SEARCH(\":\",REPLACE(J1190,SEARCH(\"AT%\",J1190),,REPT(\" \",25-SEARCH(\"AT%\",J1190)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1190,SEARCH(\"AT%\",J1190),,REPT(\" \",25-SEARCH(\"AT%\",J1190))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C1190=\"REAL\",C1190=\"DWORD\",C1190=\"DINT\"),(IF(OR(C1191=\"REAL\",C1191=\"DWORD\",C1191=\"DINT\"),A1190+4+MOD(A1190,4),A1190+4)),(IF(OR(C1191=\"REAL\",C1191=\"DWORD\",C1191=\"DINT\"),A1190+4+MOD(A1190,4),A1190+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","空调机组","R",{"$f":"F1190","v":"01C04"},"季节模式","空调机组01C04-新云平台季节模式",{"$f":"E1191&VLOOKUP(D1191,list!$D$3:$F$501,2,FALSE)&F1191&\"_\"&VLOOKUP(G1191,list!$I$2:$K$502,2,FALSE)","v":"RAHU01C04_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","R","01C04","程序控制","空调机组01C04-新云平台程序控制",{"$f":"E1192&VLOOKUP(D1192,list!$D$3:$F$501,2,FALSE)&F1192&\"_\"&VLOOKUP(G1192,list!$I$2:$K$502,2,FALSE)","v":"RAHU01C04_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","设定温度值","空调机组01C04-设定温度值",{"$f":"E1193&VLOOKUP(D1193,list!$D$3:$F$501,2,FALSE)&F1193&\"_\"&VLOOKUP(G1193,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01C04","季节模式","空调机组01C04-季节模式",{"$f":"E1194&VLOOKUP(D1194,list!$D$3:$F$501,2,FALSE)&F1194&\"_\"&VLOOKUP(G1194,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","水阀反馈换算值","空调机组01C04-水阀反馈换算值",{"$f":"E1195&VLOOKUP(D1195,list!$D$3:$F$501,2,FALSE)&F1195&\"_\"&VLOOKUP(G1195,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_WVBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01C04","水阀手动控制","空调机组01C04-水阀手动控制",{"$f":"E1196&VLOOKUP(D1196,list!$D$3:$F$501,2,FALSE)&F1196&\"_\"&VLOOKUP(G1196,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_WVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","水阀手动控制值","空调机组01C04-水阀手动控制值",{"$f":"E1197&VLOOKUP(D1197,list!$D$3:$F$501,2,FALSE)&F1197&\"_\"&VLOOKUP(G1197,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_WVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","回风温度换算值","空调机组01C04-回风温度换算值",{"$f":"E1198&VLOOKUP(D1198,list!$D$3:$F$501,2,FALSE)&F1198&\"_\"&VLOOKUP(G1198,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_RTS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01C04","运行时间累积重置","空调机组01C04-运行时间累积重置",{"$f":"E1199&VLOOKUP(D1199,list!$D$3:$F$501,2,FALSE)&F1199&\"_\"&VLOOKUP(G1199,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","运行时间累积重置值","空调机组01C04-运行时间累积重置值",{"$f":"E1200&VLOOKUP(D1200,list!$D$3:$F$501,2,FALSE)&F1200&\"_\"&VLOOKUP(G1200,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01C04","隔离开关1","空调机组01C04-隔离开关1",{"$f":"E1201&VLOOKUP(D1201,list!$D$3:$F$501,2,FALSE)&F1201&\"_\"&VLOOKUP(G1201,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01C04","隔离开关2","空调机组01C04-隔离开关2",{"$f":"E1202&VLOOKUP(D1202,list!$D$3:$F$501,2,FALSE)&F1202&\"_\"&VLOOKUP(G1202,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_ISO2"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","P调节参数","空调机组01C04-P调节参数",{"$f":"E1203&VLOOKUP(D1203,list!$D$3:$F$501,2,FALSE)&F1203&\"_\"&VLOOKUP(G1203,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_VP"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","I调节参数","空调机组01C04-I调节参数",{"$f":"E1204&VLOOKUP(D1204,list!$D$3:$F$501,2,FALSE)&F1204&\"_\"&VLOOKUP(G1204,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_VI"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01C04","运行时间累积值","空调机组01C04-运行时间累积值",{"$f":"E1205&VLOOKUP(D1205,list!$D$3:$F$501,2,FALSE)&F1205&\"_\"&VLOOKUP(G1205,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01C04","设备状态代码","空调机组01C04-设备状态代码",{"$f":"E1206&VLOOKUP(D1206,list!$D$3:$F$501,2,FALSE)&F1206&\"_\"&VLOOKUP(G1206,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01C04","水阀控制转换值","空调机组01C04-水阀控制转换值",{"$f":"E1207&VLOOKUP(D1207,list!$D$3:$F$501,2,FALSE)&F1207&\"_\"&VLOOKUP(G1207,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01C04","程序控制","空调机组01C04-程序控制",{"$f":"E1208&VLOOKUP(D1208,list!$D$3:$F$501,2,FALSE)&F1208&\"_\"&VLOOKUP(G1208,list!$I$2:$K$502,2,FALSE)","v":"LAHU01C04_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
["FCU"]
[{"$f":"IF(OR(C1208=\"REAL\",C1208=\"DWORD\",C1208=\"DINT\"),(IF(OR(C1210=\"REAL\",C1210=\"DWORD\",C1210=\"DINT\"),A1208+4+MOD(A1208,4),A1208+4)),(IF(OR(C1210=\"REAL\",C1210=\"DWORD\",C1210=\"DINT\"),A1208+4+MOD(A1208,4),A1208+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1210=\"INT\",C1210=\"WORD\",C1210=\"BOOL\"),MOD(A1210,2),MOD(A1210,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","风机盘管","R","01C01","设定温度值",{"$f":"D1210&F1210&\"-\"&IF(E1210=\"R\",\"新云平台\"&G1210,G1210)","v":"风机盘管01C01-新云平台设定温度值"},{"$f":"E1210&VLOOKUP(D1210,list!$D$3:$F$501,2,FALSE)&F1210&\"_\"&VLOOKUP(G1210,list!$I$2:$K$502,2,FALSE)","v":"RFCU01C01_TSET"},{"$f":"I1210&\" \"&\"AT%M\"&A1210&\" \"&\":\"&C1210&\";\"&\" \"&\"(*\"&H1210&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J1210,SEARCH(\"AT%\",J1210),,REPT(\" \",25-SEARCH(\"AT%\",J1210))),SEARCH(\":\",REPLACE(J1210,SEARCH(\"AT%\",J1210),,REPT(\" \",25-SEARCH(\"AT%\",J1210)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1210,SEARCH(\"AT%\",J1210),,REPT(\" \",25-SEARCH(\"AT%\",J1210))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C1210=\"REAL\",C1210=\"DWORD\",C1210=\"DINT\"),(IF(OR(C1211=\"REAL\",C1211=\"DWORD\",C1211=\"DINT\"),A1210+4+MOD(A1210,4),A1210+4)),(IF(OR(C1211=\"REAL\",C1211=\"DWORD\",C1211=\"DINT\"),A1210+4+MOD(A1210,4),A1210+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","风机盘管","R",{"$f":"F1210","v":"01C01"},"季节模式","风机盘管01C01-新云平台季节模式",{"$f":"E1211&VLOOKUP(D1211,list!$D$3:$F$501,2,FALSE)&F1211&\"_\"&VLOOKUP(G1211,list!$I$2:$K$502,2,FALSE)","v":"RFCU01C01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","R","01C01","程序控制","风机盘管01C01-新云平台程序控制",{"$f":"E1212&VLOOKUP(D1212,list!$D$3:$F$501,2,FALSE)&F1212&\"_\"&VLOOKUP(G1212,list!$I$2:$K$502,2,FALSE)","v":"RFCU01C01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01C01","设定温度值","风机盘管01C01-设定温度值",{"$f":"E1213&VLOOKUP(D1213,list!$D$3:$F$501,2,FALSE)&F1213&\"_\"&VLOOKUP(G1213,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","01C01","季节模式","风机盘管01C01-季节模式",{"$f":"E1214&VLOOKUP(D1214,list!$D$3:$F$501,2,FALSE)&F1214&\"_\"&VLOOKUP(G1214,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01C01","温度换算值","风机盘管01C01-温度换算值",{"$f":"E1215&VLOOKUP(D1215,list!$D$3:$F$501,2,FALSE)&F1215&\"_\"&VLOOKUP(G1215,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_TS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01C01","电磁阀手动控制","风机盘管01C01-电磁阀手动控制",{"$f":"E1216&VLOOKUP(D1216,list!$D$3:$F$501,2,FALSE)&F1216&\"_\"&VLOOKUP(G1216,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_EVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01C01","电磁阀手动控制值","风机盘管01C01-电磁阀手动控制值",{"$f":"E1217&VLOOKUP(D1217,list!$D$3:$F$501,2,FALSE)&F1217&\"_\"&VLOOKUP(G1217,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_EVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01C01","回风温度换算值","风机盘管01C01-回风温度换算值",{"$f":"E1218&VLOOKUP(D1218,list!$D$3:$F$501,2,FALSE)&F1218&\"_\"&VLOOKUP(G1218,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_RTS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01C01","运行时间累积重置","风机盘管01C01-运行时间累积重置",{"$f":"E1219&VLOOKUP(D1219,list!$D$3:$F$501,2,FALSE)&F1219&\"_\"&VLOOKUP(G1219,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01C01","运行时间累积重置值","风机盘管01C01-运行时间累积重置值",{"$f":"E1220&VLOOKUP(D1220,list!$D$3:$F$501,2,FALSE)&F1220&\"_\"&VLOOKUP(G1220,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01C01","隔离开关1","风机盘管01C01-隔离开关1",{"$f":"E1221&VLOOKUP(D1221,list!$D$3:$F$501,2,FALSE)&F1221&\"_\"&VLOOKUP(G1221,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01C01","运行时间累积值","风机盘管01C01-运行时间累积值",{"$f":"E1222&VLOOKUP(D1222,list!$D$3:$F$501,2,FALSE)&F1222&\"_\"&VLOOKUP(G1222,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","01C01","设备状态代码","风机盘管01C01-设备状态代码",{"$f":"E1223&VLOOKUP(D1223,list!$D$3:$F$501,2,FALSE)&F1223&\"_\"&VLOOKUP(G1223,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","01C01","水阀控制转换值","风机盘管01C01-水阀控制转换值",{"$f":"E1224&VLOOKUP(D1224,list!$D$3:$F$501,2,FALSE)&F1224&\"_\"&VLOOKUP(G1224,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01C01","程序控制","风机盘管01C01-程序控制",{"$f":"E1225&VLOOKUP(D1225,list!$D$3:$F$501,2,FALSE)&F1225&\"_\"&VLOOKUP(G1225,list!$I$2:$K$502,2,FALSE)","v":"LFCU01C01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
["AHU"]
[{"$f":"IF(OR(C1208=\"REAL\",C1208=\"DWORD\",C1208=\"DINT\"),(IF(OR(C1227=\"REAL\",C1227=\"DWORD\",C1227=\"DINT\"),A1208+4+MOD(A1208,4),A1208+4)),(IF(OR(C1227=\"REAL\",C1227=\"DWORD\",C1227=\"DINT\"),A1208+4+MOD(A1208,4),A1208+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1227=\"INT\",C1227=\"WORD\",C1227=\"BOOL\"),MOD(A1227,2),MOD(A1227,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","空调机组","R","01A03","设定温度值",{"$f":"D1227&F1227&\"-\"&IF(E1227=\"R\",\"新云平台\"&G1227,G1227)","v":"空调机组01A03-新云平台设定温度值"},{"$f":"E1227&VLOOKUP(D1227,list!$D$3:$F$501,2,FALSE)&F1227&\"_\"&VLOOKUP(G1227,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A03_TSET"},{"$f":"I1227&\" \"&\"AT%M\"&A1227&\" \"&\":\"&C1227&\";\"&\" \"&\"(*\"&H1227&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J1227,SEARCH(\"AT%\",J1227),,REPT(\" \",25-SEARCH(\"AT%\",J1227))),SEARCH(\":\",REPLACE(J1227,SEARCH(\"AT%\",J1227),,REPT(\" \",25-SEARCH(\"AT%\",J1227)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1227,SEARCH(\"AT%\",J1227),,REPT(\" \",25-SEARCH(\"AT%\",J1227))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C1227=\"REAL\",C1227=\"DWORD\",C1227=\"DINT\"),(IF(OR(C1228=\"REAL\",C1228=\"DWORD\",C1228=\"DINT\"),A1227+4+MOD(A1227,4),A1227+4)),(IF(OR(C1228=\"REAL\",C1228=\"DWORD\",C1228=\"DINT\"),A1227+4+MOD(A1227,4),A1227+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","空调机组","R",{"$f":"F1227","v":"01A03"},"季节模式","空调机组01A03-新云平台季节模式",{"$f":"E1228&VLOOKUP(D1228,list!$D$3:$F$501,2,FALSE)&F1228&\"_\"&VLOOKUP(G1228,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A03_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","R","01A03","程序控制","空调机组01A03-新云平台程序控制",{"$f":"E1229&VLOOKUP(D1229,list!$D$3:$F$501,2,FALSE)&F1229&\"_\"&VLOOKUP(G1229,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A03_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","设定温度值","空调机组01A03-设定温度值",{"$f":"E1230&VLOOKUP(D1230,list!$D$3:$F$501,2,FALSE)&F1230&\"_\"&VLOOKUP(G1230,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A03","季节模式","空调机组01A03-季节模式",{"$f":"E1231&VLOOKUP(D1231,list!$D$3:$F$501,2,FALSE)&F1231&\"_\"&VLOOKUP(G1231,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","水阀反馈换算值","空调机组01A03-水阀反馈换算值",{"$f":"E1232&VLOOKUP(D1232,list!$D$3:$F$501,2,FALSE)&F1232&\"_\"&VLOOKUP(G1232,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_WVBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A03","水阀手动控制","空调机组01A03-水阀手动控制",{"$f":"E1233&VLOOKUP(D1233,list!$D$3:$F$501,2,FALSE)&F1233&\"_\"&VLOOKUP(G1233,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_WVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","水阀手动控制值","空调机组01A03-水阀手动控制值",{"$f":"E1234&VLOOKUP(D1234,list!$D$3:$F$501,2,FALSE)&F1234&\"_\"&VLOOKUP(G1234,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_WVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","回风温度换算值","空调机组01A03-回风温度换算值",{"$f":"E1235&VLOOKUP(D1235,list!$D$3:$F$501,2,FALSE)&F1235&\"_\"&VLOOKUP(G1235,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_RTS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A03","运行时间累积重置","空调机组01A03-运行时间累积重置",{"$f":"E1236&VLOOKUP(D1236,list!$D$3:$F$501,2,FALSE)&F1236&\"_\"&VLOOKUP(G1236,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","运行时间累积重置值","空调机组01A03-运行时间累积重置值",{"$f":"E1237&VLOOKUP(D1237,list!$D$3:$F$501,2,FALSE)&F1237&\"_\"&VLOOKUP(G1237,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A03","隔离开关1","空调机组01A03-隔离开关1",{"$f":"E1238&VLOOKUP(D1238,list!$D$3:$F$501,2,FALSE)&F1238&\"_\"&VLOOKUP(G1238,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A03","隔离开关2","空调机组01A03-隔离开关2",{"$f":"E1239&VLOOKUP(D1239,list!$D$3:$F$501,2,FALSE)&F1239&\"_\"&VLOOKUP(G1239,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_ISO2"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","P调节参数","空调机组01A03-P调节参数",{"$f":"E1240&VLOOKUP(D1240,list!$D$3:$F$501,2,FALSE)&F1240&\"_\"&VLOOKUP(G1240,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_VP"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","I调节参数","空调机组01A03-I调节参数",{"$f":"E1241&VLOOKUP(D1241,list!$D$3:$F$501,2,FALSE)&F1241&\"_\"&VLOOKUP(G1241,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_VI"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A03","运行时间累积值","空调机组01A03-运行时间累积值",{"$f":"E1242&VLOOKUP(D1242,list!$D$3:$F$501,2,FALSE)&F1242&\"_\"&VLOOKUP(G1242,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A03","设备状态代码","空调机组01A03-设备状态代码",{"$f":"E1243&VLOOKUP(D1243,list!$D$3:$F$501,2,FALSE)&F1243&\"_\"&VLOOKUP(G1243,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A03","水阀控制转换值","空调机组01A03-水阀控制转换值",{"$f":"E1244&VLOOKUP(D1244,list!$D$3:$F$501,2,FALSE)&F1244&\"_\"&VLOOKUP(G1244,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A03","程序控制","空调机组01A03-程序控制",{"$f":"E1245&VLOOKUP(D1245,list!$D$3:$F$501,2,FALSE)&F1245&\"_\"&VLOOKUP(G1245,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A03_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
["AHU"]
[{"$f":"IF(OR(C1245=\"REAL\",C1245=\"DWORD\",C1245=\"DINT\"),(IF(OR(C1247=\"REAL\",C1247=\"DWORD\",C1247=\"DINT\"),A1245+4+MOD(A1245,4),A1245+4)),(IF(OR(C1247=\"REAL\",C1247=\"DWORD\",C1247=\"DINT\"),A1245+4+MOD(A1245,4),A1245+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1247=\"INT\",C1247=\"WORD\",C1247=\"BOOL\"),MOD(A1247,2),MOD(A1247,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","空调机组","R","01A04","设定温度值",{"$f":"D1247&F1247&\"-\"&IF(E1247=\"R\",\"新云平台\"&G1247,G1247)","v":"空调机组01A04-新云平台设定温度值"},{"$f":"E1247&VLOOKUP(D1247,list!$D$3:$F$501,2,FALSE)&F1247&\"_\"&VLOOKUP(G1247,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A04_TSET"},{"$f":"I1247&\" \"&\"AT%M\"&A1247&\" \"&\":\"&C1247&\";\"&\" \"&\"(*\"&H1247&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J1247,SEARCH(\"AT%\",J1247),,REPT(\" \",25-SEARCH(\"AT%\",J1247))),SEARCH(\":\",REPLACE(J1247,SEARCH(\"AT%\",J1247),,REPT(\" \",25-SEARCH(\"AT%\",J1247)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1247,SEARCH(\"AT%\",J1247),,REPT(\" \",25-SEARCH(\"AT%\",J1247))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C1247=\"REAL\",C1247=\"DWORD\",C1247=\"DINT\"),(IF(OR(C1248=\"REAL\",C1248=\"DWORD\",C1248=\"DINT\"),A1247+4+MOD(A1247,4),A1247+4)),(IF(OR(C1248=\"REAL\",C1248=\"DWORD\",C1248=\"DINT\"),A1247+4+MOD(A1247,4),A1247+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","空调机组","R",{"$f":"F1247","v":"01A04"},"季节模式","空调机组01A04-新云平台季节模式",{"$f":"E1248&VLOOKUP(D1248,list!$D$3:$F$501,2,FALSE)&F1248&\"_\"&VLOOKUP(G1248,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A04_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","R","01A04","程序控制","空调机组01A04-新云平台程序控制",{"$f":"E1249&VLOOKUP(D1249,list!$D$3:$F$501,2,FALSE)&F1249&\"_\"&VLOOKUP(G1249,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A04_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","设定温度值","空调机组01A04-设定温度值",{"$f":"E1250&VLOOKUP(D1250,list!$D$3:$F$501,2,FALSE)&F1250&\"_\"&VLOOKUP(G1250,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A04","季节模式","空调机组01A04-季节模式",{"$f":"E1251&VLOOKUP(D1251,list!$D$3:$F$501,2,FALSE)&F1251&\"_\"&VLOOKUP(G1251,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","水阀反馈换算值","空调机组01A04-水阀反馈换算值",{"$f":"E1252&VLOOKUP(D1252,list!$D$3:$F$501,2,FALSE)&F1252&\"_\"&VLOOKUP(G1252,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_WVBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A04","水阀手动控制","空调机组01A04-水阀手动控制",{"$f":"E1253&VLOOKUP(D1253,list!$D$3:$F$501,2,FALSE)&F1253&\"_\"&VLOOKUP(G1253,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_WVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","水阀手动控制值","空调机组01A04-水阀手动控制值",{"$f":"E1254&VLOOKUP(D1254,list!$D$3:$F$501,2,FALSE)&F1254&\"_\"&VLOOKUP(G1254,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_WVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","回风温度换算值","空调机组01A04-回风温度换算值",{"$f":"E1255&VLOOKUP(D1255,list!$D$3:$F$501,2,FALSE)&F1255&\"_\"&VLOOKUP(G1255,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_RTS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A04","运行时间累积重置","空调机组01A04-运行时间累积重置",{"$f":"E1256&VLOOKUP(D1256,list!$D$3:$F$501,2,FALSE)&F1256&\"_\"&VLOOKUP(G1256,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","运行时间累积重置值","空调机组01A04-运行时间累积重置值",{"$f":"E1257&VLOOKUP(D1257,list!$D$3:$F$501,2,FALSE)&F1257&\"_\"&VLOOKUP(G1257,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A04","隔离开关1","空调机组01A04-隔离开关1",{"$f":"E1258&VLOOKUP(D1258,list!$D$3:$F$501,2,FALSE)&F1258&\"_\"&VLOOKUP(G1258,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A04","隔离开关2","空调机组01A04-隔离开关2",{"$f":"E1259&VLOOKUP(D1259,list!$D$3:$F$501,2,FALSE)&F1259&\"_\"&VLOOKUP(G1259,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_ISO2"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","P调节参数","空调机组01A04-P调节参数",{"$f":"E1260&VLOOKUP(D1260,list!$D$3:$F$501,2,FALSE)&F1260&\"_\"&VLOOKUP(G1260,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_VP"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","I调节参数","空调机组01A04-I调节参数",{"$f":"E1261&VLOOKUP(D1261,list!$D$3:$F$501,2,FALSE)&F1261&\"_\"&VLOOKUP(G1261,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_VI"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A04","运行时间累积值","空调机组01A04-运行时间累积值",{"$f":"E1262&VLOOKUP(D1262,list!$D$3:$F$501,2,FALSE)&F1262&\"_\"&VLOOKUP(G1262,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A04","设备状态代码","空调机组01A04-设备状态代码",{"$f":"E1263&VLOOKUP(D1263,list!$D$3:$F$501,2,FALSE)&F1263&\"_\"&VLOOKUP(G1263,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A04","水阀控制转换值","空调机组01A04-水阀控制转换值",{"$f":"E1264&VLOOKUP(D1264,list!$D$3:$F$501,2,FALSE)&F1264&\"_\"&VLOOKUP(G1264,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A04","程序控制","空调机组01A04-程序控制",{"$f":"E1265&VLOOKUP(D1265,list!$D$3:$F$501,2,FALSE)&F1265&\"_\"&VLOOKUP(G1265,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A04_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
["AHU"]
[{"$f":"IF(OR(C1265=\"REAL\",C1265=\"DWORD\",C1265=\"DINT\"),(IF(OR(C1267=\"REAL\",C1267=\"DWORD\",C1267=\"DINT\"),A1265+4+MOD(A1265,4),A1265+4)),(IF(OR(C1267=\"REAL\",C1267=\"DWORD\",C1267=\"DINT\"),A1265+4+MOD(A1265,4),A1265+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1267=\"INT\",C1267=\"WORD\",C1267=\"BOOL\"),MOD(A1267,2),MOD(A1267,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","空调机组","R","01A05","设定温度值",{"$f":"D1267&F1267&\"-\"&IF(E1267=\"R\",\"新云平台\"&G1267,G1267)","v":"空调机组01A05-新云平台设定温度值"},{"$f":"E1267&VLOOKUP(D1267,list!$D$3:$F$501,2,FALSE)&F1267&\"_\"&VLOOKUP(G1267,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A05_TSET"},{"$f":"I1267&\" \"&\"AT%M\"&A1267&\" \"&\":\"&C1267&\";\"&\" \"&\"(*\"&H1267&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J1267,SEARCH(\"AT%\",J1267),,REPT(\" \",25-SEARCH(\"AT%\",J1267))),SEARCH(\":\",REPLACE(J1267,SEARCH(\"AT%\",J1267),,REPT(\" \",25-SEARCH(\"AT%\",J1267)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1267,SEARCH(\"AT%\",J1267),,REPT(\" \",25-SEARCH(\"AT%\",J1267))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C1267=\"REAL\",C1267=\"DWORD\",C1267=\"DINT\"),(IF(OR(C1268=\"REAL\",C1268=\"DWORD\",C1268=\"DINT\"),A1267+4+MOD(A1267,4),A1267+4)),(IF(OR(C1268=\"REAL\",C1268=\"DWORD\",C1268=\"DINT\"),A1267+4+MOD(A1267,4),A1267+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","空调机组","R",{"$f":"F1267","v":"01A05"},"季节模式","空调机组01A05-新云平台季节模式",{"$f":"E1268&VLOOKUP(D1268,list!$D$3:$F$501,2,FALSE)&F1268&\"_\"&VLOOKUP(G1268,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A05_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","R","01A05","程序控制","空调机组01A05-新云平台程序控制",{"$f":"E1269&VLOOKUP(D1269,list!$D$3:$F$501,2,FALSE)&F1269&\"_\"&VLOOKUP(G1269,list!$I$2:$K$502,2,FALSE)","v":"RAHU01A05_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","设定温度值","空调机组01A05-设定温度值",{"$f":"E1270&VLOOKUP(D1270,list!$D$3:$F$501,2,FALSE)&F1270&\"_\"&VLOOKUP(G1270,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A05","季节模式","空调机组01A05-季节模式",{"$f":"E1271&VLOOKUP(D1271,list!$D$3:$F$501,2,FALSE)&F1271&\"_\"&VLOOKUP(G1271,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","水阀反馈换算值","空调机组01A05-水阀反馈换算值",{"$f":"E1272&VLOOKUP(D1272,list!$D$3:$F$501,2,FALSE)&F1272&\"_\"&VLOOKUP(G1272,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_WVBS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A05","水阀手动控制","空调机组01A05-水阀手动控制",{"$f":"E1273&VLOOKUP(D1273,list!$D$3:$F$501,2,FALSE)&F1273&\"_\"&VLOOKUP(G1273,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_WVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","水阀手动控制值","空调机组01A05-水阀手动控制值",{"$f":"E1274&VLOOKUP(D1274,list!$D$3:$F$501,2,FALSE)&F1274&\"_\"&VLOOKUP(G1274,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_WVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","回风温度换算值","空调机组01A05-回风温度换算值",{"$f":"E1275&VLOOKUP(D1275,list!$D$3:$F$501,2,FALSE)&F1275&\"_\"&VLOOKUP(G1275,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_RTS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A05","运行时间累积重置","空调机组01A05-运行时间累积重置",{"$f":"E1276&VLOOKUP(D1276,list!$D$3:$F$501,2,FALSE)&F1276&\"_\"&VLOOKUP(G1276,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","运行时间累积重置值","空调机组01A05-运行时间累积重置值",{"$f":"E1277&VLOOKUP(D1277,list!$D$3:$F$501,2,FALSE)&F1277&\"_\"&VLOOKUP(G1277,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A05","隔离开关1","空调机组01A05-隔离开关1",{"$f":"E1278&VLOOKUP(D1278,list!$D$3:$F$501,2,FALSE)&F1278&\"_\"&VLOOKUP(G1278,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A05","隔离开关2","空调机组01A05-隔离开关2",{"$f":"E1279&VLOOKUP(D1279,list!$D$3:$F$501,2,FALSE)&F1279&\"_\"&VLOOKUP(G1279,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_ISO2"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","P调节参数","空调机组01A05-P调节参数",{"$f":"E1280&VLOOKUP(D1280,list!$D$3:$F$501,2,FALSE)&F1280&\"_\"&VLOOKUP(G1280,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_VP"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","I调节参数","空调机组01A05-I调节参数",{"$f":"E1281&VLOOKUP(D1281,list!$D$3:$F$501,2,FALSE)&F1281&\"_\"&VLOOKUP(G1281,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_VI"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","空调机组","L","01A05","运行时间累积值","空调机组01A05-运行时间累积值",{"$f":"E1282&VLOOKUP(D1282,list!$D$3:$F$501,2,FALSE)&F1282&\"_\"&VLOOKUP(G1282,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A05","设备状态代码","空调机组01A05-设备状态代码",{"$f":"E1283&VLOOKUP(D1283,list!$D$3:$F$501,2,FALSE)&F1283&\"_\"&VLOOKUP(G1283,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","空调机组","L","01A05","水阀控制转换值","空调机组01A05-水阀控制转换值",{"$f":"E1284&VLOOKUP(D1284,list!$D$3:$F$501,2,FALSE)&F1284&\"_\"&VLOOKUP(G1284,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","空调机组","L","01A05","程序控制","空调机组01A05-程序控制",{"$f":"E1285&VLOOKUP(D1285,list!$D$3:$F$501,2,FALSE)&F1285&\"_\"&VLOOKUP(G1285,list!$I$2:$K$502,2,FALSE)","v":"LAHU01A05_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
["FCU"]
[{"$f":"IF(OR(C1285=\"REAL\",C1285=\"DWORD\",C1285=\"DINT\"),(IF(OR(C1287=\"REAL\",C1287=\"DWORD\",C1287=\"DINT\"),A1285+4+MOD(A1285,4),A1285+4)),(IF(OR(C1287=\"REAL\",C1287=\"DWORD\",C1287=\"DINT\"),A1285+4+MOD(A1285,4),A1285+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1287=\"INT\",C1287=\"WORD\",C1287=\"BOOL\"),MOD(A1287,2),MOD(A1287,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"REAL","风机盘管","R","01A01","设定温度值",{"$f":"D1287&F1287&\"-\"&IF(E1287=\"R\",\"新云平台\"&G1287,G1287)","v":"风机盘管01A01-新云平台设定温度值"},{"$f":"E1287&VLOOKUP(D1287,list!$D$3:$F$501,2,FALSE)&F1287&\"_\"&VLOOKUP(G1287,list!$I$2:$K$502,2,FALSE)","v":"RFCU01A01_TSET"},{"$f":"I1287&\" \"&\"AT%M\"&A1287&\" \"&\":\"&C1287&\";\"&\" \"&\"(*\"&H1287&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J1287,SEARCH(\"AT%\",J1287),,REPT(\" \",25-SEARCH(\"AT%\",J1287))),SEARCH(\":\",REPLACE(J1287,SEARCH(\"AT%\",J1287),,REPT(\" \",25-SEARCH(\"AT%\",J1287)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1287,SEARCH(\"AT%\",J1287),,REPT(\" \",25-SEARCH(\"AT%\",J1287))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C1287=\"REAL\",C1287=\"DWORD\",C1287=\"DINT\"),(IF(OR(C1288=\"REAL\",C1288=\"DWORD\",C1288=\"DINT\"),A1287+4+MOD(A1287,4),A1287+4)),(IF(OR(C1288=\"REAL\",C1288=\"DWORD\",C1288=\"DINT\"),A1287+4+MOD(A1287,4),A1287+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"INT","风机盘管","R",{"$f":"F1287","v":"01A01"},"季节模式","风机盘管01A01-新云平台季节模式",{"$f":"E1288&VLOOKUP(D1288,list!$D$3:$F$501,2,FALSE)&F1288&\"_\"&VLOOKUP(G1288,list!$I$2:$K$502,2,FALSE)","v":"RFCU01A01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","R","01A01","程序控制","风机盘管01A01-新云平台程序控制",{"$f":"E1289&VLOOKUP(D1289,list!$D$3:$F$501,2,FALSE)&F1289&\"_\"&VLOOKUP(G1289,list!$I$2:$K$502,2,FALSE)","v":"RFCU01A01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01A01","设定温度值","风机盘管01A01-设定温度值",{"$f":"E1290&VLOOKUP(D1290,list!$D$3:$F$501,2,FALSE)&F1290&\"_\"&VLOOKUP(G1290,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_TSET"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","01A01","季节模式","风机盘管01A01-季节模式",{"$f":"E1291&VLOOKUP(D1291,list!$D$3:$F$501,2,FALSE)&F1291&\"_\"&VLOOKUP(G1291,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_SM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01A01","温度换算值","风机盘管01A01-温度换算值",{"$f":"E1292&VLOOKUP(D1292,list!$D$3:$F$501,2,FALSE)&F1292&\"_\"&VLOOKUP(G1292,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_TS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01A01","电磁阀手动控制","风机盘管01A01-电磁阀手动控制",{"$f":"E1293&VLOOKUP(D1293,list!$D$3:$F$501,2,FALSE)&F1293&\"_\"&VLOOKUP(G1293,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_EVMC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01A01","电磁阀手动控制值","风机盘管01A01-电磁阀手动控制值",{"$f":"E1294&VLOOKUP(D1294,list!$D$3:$F$501,2,FALSE)&F1294&\"_\"&VLOOKUP(G1294,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_EVMV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01A01","回风温度换算值","风机盘管01A01-回风温度换算值",{"$f":"E1295&VLOOKUP(D1295,list!$D$3:$F$501,2,FALSE)&F1295&\"_\"&VLOOKUP(G1295,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_RTS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01A01","运行时间累积重置","风机盘管01A01-运行时间累积重置",{"$f":"E1296&VLOOKUP(D1296,list!$D$3:$F$501,2,FALSE)&F1296&\"_\"&VLOOKUP(G1296,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01A01","运行时间累积重置值","风机盘管01A01-运行时间累积重置值",{"$f":"E1297&VLOOKUP(D1297,list!$D$3:$F$501,2,FALSE)&F1297&\"_\"&VLOOKUP(G1297,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01A01","隔离开关1","风机盘管01A01-隔离开关1",{"$f":"E1298&VLOOKUP(D1298,list!$D$3:$F$501,2,FALSE)&F1298&\"_\"&VLOOKUP(G1298,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_ISO1"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风机盘管","L","01A01","运行时间累积值","风机盘管01A01-运行时间累积值",{"$f":"E1299&VLOOKUP(D1299,list!$D$3:$F$501,2,FALSE)&F1299&\"_\"&VLOOKUP(G1299,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","01A01","设备状态代码","风机盘管01A01-设备状态代码",{"$f":"E1300&VLOOKUP(D1300,list!$D$3:$F$501,2,FALSE)&F1300&\"_\"&VLOOKUP(G1300,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_SN"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"INT","风机盘管","L","01A01","水阀控制转换值","风机盘管01A01-水阀控制转换值",{"$f":"E1301&VLOOKUP(D1301,list!$D$3:$F$501,2,FALSE)&F1301&\"_\"&VLOOKUP(G1301,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_WVCS"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风机盘管","L","01A01","程序控制","风机盘管01A01-程序控制",{"$f":"E1302&VLOOKUP(D1302,list!$D$3:$F$501,2,FALSE)&F1302&\"_\"&VLOOKUP(G1302,list!$I$2:$K$502,2,FALSE)","v":"LFCU01A01_PC"},{"$error":"#REF!"},{"$error":"#REF!"}]
["FMJ"]
[{"$f":"IF(OR(C1302=\"REAL\",C1302=\"DWORD\",C1302=\"DINT\"),(IF(OR(C1304=\"REAL\",C1304=\"DWORD\",C1304=\"DINT\"),A1302+4+MOD(A1302,4),A1302+4)),(IF(OR(C1304=\"REAL\",C1304=\"DWORD\",C1304=\"DINT\"),A1302+4+MOD(A1302,4),A1302+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1304=\"INT\",C1304=\"WORD\",C1304=\"BOOL\"),MOD(A1304,2),MOD(A1304,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"BOOL","风幕机","R","01A01","启停控制",{"$f":"D1304&F1304&\"-\"&IF(E1304=\"R\",\"新云平台\"&G1304,G1304)","v":"风幕机01A01-新云平台启停控制"},{"$f":"E1304&VLOOKUP(D1304,list!$D$3:$F$501,2,FALSE)&F1304&\"_\"&VLOOKUP(G1304,list!$I$2:$K$502,2,FALSE)","v":"RFMJ01A01_C"},{"$f":"I1304&\" \"&\"AT%M\"&A1304&\" \"&\":\"&C1304&\";\"&\" \"&\"(*\"&H1304&\"*)\"","v":{"$error":"#REF!"}},{"$f":"REPLACE(REPLACE(J1304,SEARCH(\"AT%\",J1304),,REPT(\" \",25-SEARCH(\"AT%\",J1304))),SEARCH(\":\",REPLACE(J1304,SEARCH(\"AT%\",J1304),,REPT(\" \",25-SEARCH(\"AT%\",J1304)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1304,SEARCH(\"AT%\",J1304),,REPT(\" \",25-SEARCH(\"AT%\",J1304))))))","v":{"$error":"#REF!"}}]
[{"$f":"IF(OR(C1304=\"REAL\",C1304=\"DWORD\",C1304=\"DINT\"),(IF(OR(C1305=\"REAL\",C1305=\"DWORD\",C1305=\"DINT\"),A1304+4+MOD(A1304,4),A1304+4)),(IF(OR(C1305=\"REAL\",C1305=\"DWORD\",C1305=\"DINT\"),A1304+4+MOD(A1304,4),A1304+2)))&\".0\"","v":{"$error":"#REF!"}},{"$error":"#REF!"},"BOOL","风幕机","L","01A01","定时模式","风幕机01A01-定时模式",{"$f":"E1305&VLOOKUP(D1305,list!$D$3:$F$501,2,FALSE)&F1305&\"_\"&VLOOKUP(G1305,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_TM"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风幕机","L","01A01","定时控制","风幕机01A01-定时控制",{"$f":"E1306&VLOOKUP(D1306,list!$D$3:$F$501,2,FALSE)&F1306&\"_\"&VLOOKUP(G1306,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_TC"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"BOOL","风幕机","L","01A01","运行时间累积重置","风幕机01A01-运行时间累积重置",{"$f":"E1307&VLOOKUP(D1307,list!$D$3:$F$501,2,FALSE)&F1307&\"_\"&VLOOKUP(G1307,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_RST"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风幕机","L","01A01","运行时间累积重置值","风幕机01A01-运行时间累积重置值",{"$f":"E1308&VLOOKUP(D1308,list!$D$3:$F$501,2,FALSE)&F1308&\"_\"&VLOOKUP(G1308,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_RSTV"},{"$error":"#REF!"},{"$error":"#REF!"}]
[{"$error":"#REF!"},{"$error":"#REF!"},"REAL","风幕机","L","01A01","运行时间累积值","风幕机01A01-运行时间累积值",{"$f":"E1309&VLOOKUP(D1309,list!$D$3:$F$501,2,FALSE)&F1309&\"_\"&VLOOKUP(G1309,list!$I$2:$K$502,2,FALSE)","v":"LFMJ01A01_RH"},{"$error":"#REF!"},{"$error":"#REF!"}]
["FMJ"]
[{"$f":"IF(OR(C1302=\"REAL\",C1302=\"DWORD\",C1302=\"DINT\"),(IF(OR(C1311=\"REAL\",C1311=\"DWORD\",C1311=\"DINT\"),A1302+4+MOD(A1302,4),A1302+4)),(IF(OR(C1311=\"REAL\",C1311=\"DWORD\",C1311=\"DINT\"),A1302+4+MOD(A1302,4),A1302+2)))&\".0\"","v":{"$error":"#REF!"}},{"$f":"IF((IF(OR(C1311=\"INT\",C1311=\"WORD\",C1311=\"BOOL\"),MOD(A1311,2),MOD(A1311,4)))=0,\"验证通过\",\"验证失败\")","v":{"$error":"#REF!"}},"BOOL","电风幕机","R","01A03","启停控制",{"$f":"D1311&F1311&\"-\"&IF(E1311=\"R\",\"新云平台\"&G1311,G1311)","v":"电风幕机01A03-新云平台启停控制"},{"$f":"E1311&VLOOKUP(D1311,list!$D$3:$F$501,2,FALSE)&F1311&\"_\"&VLOOKUP(G1311,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1311&\" \"&\"AT%M\"&A1311&\" \"&\":\"&C1311&\";\"&\" \"&\"(*\"&H1311&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1311,SEARCH(\"AT%\",J1311),,REPT(\" \",25-SEARCH(\"AT%\",J1311))),SEARCH(\":\",REPLACE(J1311,SEARCH(\"AT%\",J1311),,REPT(\" \",25-SEARCH(\"AT%\",J1311)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1311,SEARCH(\"AT%\",J1311),,REPT(\" \",25-SEARCH(\"AT%\",J1311))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C123=\"REAL\",C123=\"DWORD\",C123=\"DINT\"),(IF(OR(C1313=\"REAL\",C1313=\"DWORD\",C1313=\"DINT\"),A123+4+MOD(A123,4),A123+4)),(IF(OR(C1313=\"REAL\",C1313=\"DWORD\",C1313=\"DINT\"),A123+4+MOD(A123,4),A123+2)))&\".0\"","v":"526.0"},{"$f":"IF((IF(OR(C1313=\"INT\",C1313=\"WORD\",C1313=\"BOOL\"),MOD(A1313,2),MOD(A1313,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A01","启停控制",{"$f":"D1313&F1313&\"-\"&IF(E1313=\"R\",\"新云平台\"&G1313,G1313)","v":"电风幕机01A01-新云平台启停控制"},{"$f":"E1313&VLOOKUP(D1313,list!$D$3:$F$501,2,FALSE)&F1313&\"_\"&VLOOKUP(G1313,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1313&\" \"&\"AT%M\"&A1313&\" \"&\":\"&C1313&\";\"&\" \"&\"(*\"&H1313&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1313,SEARCH(\"AT%\",J1313),,REPT(\" \",25-SEARCH(\"AT%\",J1313))),SEARCH(\":\",REPLACE(J1313,SEARCH(\"AT%\",J1313),,REPT(\" \",25-SEARCH(\"AT%\",J1313)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1313,SEARCH(\"AT%\",J1313),,REPT(\" \",25-SEARCH(\"AT%\",J1313))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1313=\"REAL\",C1313=\"DWORD\",C1313=\"DINT\"),(IF(OR(C1315=\"REAL\",C1315=\"DWORD\",C1315=\"DINT\"),A1313+4+MOD(A1313,4),A1313+4)),(IF(OR(C1315=\"REAL\",C1315=\"DWORD\",C1315=\"DINT\"),A1313+4+MOD(A1313,4),A1313+2)))&\".0\"","v":"528.0"},{"$f":"IF((IF(OR(C1315=\"INT\",C1315=\"WORD\",C1315=\"BOOL\"),MOD(A1315,2),MOD(A1315,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A02","启停控制",{"$f":"D1315&F1315&\"-\"&IF(E1315=\"R\",\"新云平台\"&G1315,G1315)","v":"电风幕机01A02-新云平台启停控制"},{"$f":"E1315&VLOOKUP(D1315,list!$D$3:$F$501,2,FALSE)&F1315&\"_\"&VLOOKUP(G1315,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1315&\" \"&\"AT%M\"&A1315&\" \"&\":\"&C1315&\";\"&\" \"&\"(*\"&H1315&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1315,SEARCH(\"AT%\",J1315),,REPT(\" \",25-SEARCH(\"AT%\",J1315))),SEARCH(\":\",REPLACE(J1315,SEARCH(\"AT%\",J1315),,REPT(\" \",25-SEARCH(\"AT%\",J1315)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1315,SEARCH(\"AT%\",J1315),,REPT(\" \",25-SEARCH(\"AT%\",J1315))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1315=\"REAL\",C1315=\"DWORD\",C1315=\"DINT\"),(IF(OR(C1317=\"REAL\",C1317=\"DWORD\",C1317=\"DINT\"),A1315+4+MOD(A1315,4),A1315+4)),(IF(OR(C1317=\"REAL\",C1317=\"DWORD\",C1317=\"DINT\"),A1315+4+MOD(A1315,4),A1315+2)))&\".0\"","v":"530.0"},{"$f":"IF((IF(OR(C1317=\"INT\",C1317=\"WORD\",C1317=\"BOOL\"),MOD(A1317,2),MOD(A1317,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A03","启停控制",{"$f":"D1317&F1317&\"-\"&IF(E1317=\"R\",\"新云平台\"&G1317,G1317)","v":"电风幕机01A03-新云平台启停控制"},{"$f":"E1317&VLOOKUP(D1317,list!$D$3:$F$501,2,FALSE)&F1317&\"_\"&VLOOKUP(G1317,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1317&\" \"&\"AT%M\"&A1317&\" \"&\":\"&C1317&\";\"&\" \"&\"(*\"&H1317&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1317,SEARCH(\"AT%\",J1317),,REPT(\" \",25-SEARCH(\"AT%\",J1317))),SEARCH(\":\",REPLACE(J1317,SEARCH(\"AT%\",J1317),,REPT(\" \",25-SEARCH(\"AT%\",J1317)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1317,SEARCH(\"AT%\",J1317),,REPT(\" \",25-SEARCH(\"AT%\",J1317))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1317=\"REAL\",C1317=\"DWORD\",C1317=\"DINT\"),(IF(OR(C1319=\"REAL\",C1319=\"DWORD\",C1319=\"DINT\"),A1317+4+MOD(A1317,4),A1317+4)),(IF(OR(C1319=\"REAL\",C1319=\"DWORD\",C1319=\"DINT\"),A1317+4+MOD(A1317,4),A1317+2)))&\".0\"","v":"532.0"},{"$f":"IF((IF(OR(C1319=\"INT\",C1319=\"WORD\",C1319=\"BOOL\"),MOD(A1319,2),MOD(A1319,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A04","启停控制",{"$f":"D1319&F1319&\"-\"&IF(E1319=\"R\",\"新云平台\"&G1319,G1319)","v":"电风幕机01A04-新云平台启停控制"},{"$f":"E1319&VLOOKUP(D1319,list!$D$3:$F$501,2,FALSE)&F1319&\"_\"&VLOOKUP(G1319,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1319&\" \"&\"AT%M\"&A1319&\" \"&\":\"&C1319&\";\"&\" \"&\"(*\"&H1319&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1319,SEARCH(\"AT%\",J1319),,REPT(\" \",25-SEARCH(\"AT%\",J1319))),SEARCH(\":\",REPLACE(J1319,SEARCH(\"AT%\",J1319),,REPT(\" \",25-SEARCH(\"AT%\",J1319)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1319,SEARCH(\"AT%\",J1319),,REPT(\" \",25-SEARCH(\"AT%\",J1319))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1319=\"REAL\",C1319=\"DWORD\",C1319=\"DINT\"),(IF(OR(C1321=\"REAL\",C1321=\"DWORD\",C1321=\"DINT\"),A1319+4+MOD(A1319,4),A1319+4)),(IF(OR(C1321=\"REAL\",C1321=\"DWORD\",C1321=\"DINT\"),A1319+4+MOD(A1319,4),A1319+2)))&\".0\"","v":"534.0"},{"$f":"IF((IF(OR(C1321=\"INT\",C1321=\"WORD\",C1321=\"BOOL\"),MOD(A1321,2),MOD(A1321,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A05","启停控制",{"$f":"D1321&F1321&\"-\"&IF(E1321=\"R\",\"新云平台\"&G1321,G1321)","v":"电风幕机01A05-新云平台启停控制"},{"$f":"E1321&VLOOKUP(D1321,list!$D$3:$F$501,2,FALSE)&F1321&\"_\"&VLOOKUP(G1321,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1321&\" \"&\"AT%M\"&A1321&\" \"&\":\"&C1321&\";\"&\" \"&\"(*\"&H1321&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1321,SEARCH(\"AT%\",J1321),,REPT(\" \",25-SEARCH(\"AT%\",J1321))),SEARCH(\":\",REPLACE(J1321,SEARCH(\"AT%\",J1321),,REPT(\" \",25-SEARCH(\"AT%\",J1321)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1321,SEARCH(\"AT%\",J1321),,REPT(\" \",25-SEARCH(\"AT%\",J1321))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1321=\"REAL\",C1321=\"DWORD\",C1321=\"DINT\"),(IF(OR(C1323=\"REAL\",C1323=\"DWORD\",C1323=\"DINT\"),A1321+4+MOD(A1321,4),A1321+4)),(IF(OR(C1323=\"REAL\",C1323=\"DWORD\",C1323=\"DINT\"),A1321+4+MOD(A1321,4),A1321+2)))&\".0\"","v":"536.0"},{"$f":"IF((IF(OR(C1323=\"INT\",C1323=\"WORD\",C1323=\"BOOL\"),MOD(A1323,2),MOD(A1323,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A06","启停控制",{"$f":"D1323&F1323&\"-\"&IF(E1323=\"R\",\"新云平台\"&G1323,G1323)","v":"电风幕机01A06-新云平台启停控制"},{"$f":"E1323&VLOOKUP(D1323,list!$D$3:$F$501,2,FALSE)&F1323&\"_\"&VLOOKUP(G1323,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1323&\" \"&\"AT%M\"&A1323&\" \"&\":\"&C1323&\";\"&\" \"&\"(*\"&H1323&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1323,SEARCH(\"AT%\",J1323),,REPT(\" \",25-SEARCH(\"AT%\",J1323))),SEARCH(\":\",REPLACE(J1323,SEARCH(\"AT%\",J1323),,REPT(\" \",25-SEARCH(\"AT%\",J1323)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1323,SEARCH(\"AT%\",J1323),,REPT(\" \",25-SEARCH(\"AT%\",J1323))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1323=\"REAL\",C1323=\"DWORD\",C1323=\"DINT\"),(IF(OR(C1325=\"REAL\",C1325=\"DWORD\",C1325=\"DINT\"),A1323+4+MOD(A1323,4),A1323+4)),(IF(OR(C1325=\"REAL\",C1325=\"DWORD\",C1325=\"DINT\"),A1323+4+MOD(A1323,4),A1323+2)))&\".0\"","v":"538.0"},{"$f":"IF((IF(OR(C1325=\"INT\",C1325=\"WORD\",C1325=\"BOOL\"),MOD(A1325,2),MOD(A1325,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A07","启停控制",{"$f":"D1325&F1325&\"-\"&IF(E1325=\"R\",\"新云平台\"&G1325,G1325)","v":"电风幕机01A07-新云平台启停控制"},{"$f":"E1325&VLOOKUP(D1325,list!$D$3:$F$501,2,FALSE)&F1325&\"_\"&VLOOKUP(G1325,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1325&\" \"&\"AT%M\"&A1325&\" \"&\":\"&C1325&\";\"&\" \"&\"(*\"&H1325&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1325,SEARCH(\"AT%\",J1325),,REPT(\" \",25-SEARCH(\"AT%\",J1325))),SEARCH(\":\",REPLACE(J1325,SEARCH(\"AT%\",J1325),,REPT(\" \",25-SEARCH(\"AT%\",J1325)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1325,SEARCH(\"AT%\",J1325),,REPT(\" \",25-SEARCH(\"AT%\",J1325))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1325=\"REAL\",C1325=\"DWORD\",C1325=\"DINT\"),(IF(OR(C1327=\"REAL\",C1327=\"DWORD\",C1327=\"DINT\"),A1325+4+MOD(A1325,4),A1325+4)),(IF(OR(C1327=\"REAL\",C1327=\"DWORD\",C1327=\"DINT\"),A1325+4+MOD(A1325,4),A1325+2)))&\".0\"","v":"540.0"},{"$f":"IF((IF(OR(C1327=\"INT\",C1327=\"WORD\",C1327=\"BOOL\"),MOD(A1327,2),MOD(A1327,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A08","启停控制",{"$f":"D1327&F1327&\"-\"&IF(E1327=\"R\",\"新云平台\"&G1327,G1327)","v":"电风幕机01A08-新云平台启停控制"},{"$f":"E1327&VLOOKUP(D1327,list!$D$3:$F$501,2,FALSE)&F1327&\"_\"&VLOOKUP(G1327,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1327&\" \"&\"AT%M\"&A1327&\" \"&\":\"&C1327&\";\"&\" \"&\"(*\"&H1327&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1327,SEARCH(\"AT%\",J1327),,REPT(\" \",25-SEARCH(\"AT%\",J1327))),SEARCH(\":\",REPLACE(J1327,SEARCH(\"AT%\",J1327),,REPT(\" \",25-SEARCH(\"AT%\",J1327)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1327,SEARCH(\"AT%\",J1327),,REPT(\" \",25-SEARCH(\"AT%\",J1327))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1327=\"REAL\",C1327=\"DWORD\",C1327=\"DINT\"),(IF(OR(C1329=\"REAL\",C1329=\"DWORD\",C1329=\"DINT\"),A1327+4+MOD(A1327,4),A1327+4)),(IF(OR(C1329=\"REAL\",C1329=\"DWORD\",C1329=\"DINT\"),A1327+4+MOD(A1327,4),A1327+2)))&\".0\"","v":"542.0"},{"$f":"IF((IF(OR(C1329=\"INT\",C1329=\"WORD\",C1329=\"BOOL\"),MOD(A1329,2),MOD(A1329,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A09","启停控制",{"$f":"D1329&F1329&\"-\"&IF(E1329=\"R\",\"新云平台\"&G1329,G1329)","v":"电风幕机01A09-新云平台启停控制"},{"$f":"E1329&VLOOKUP(D1329,list!$D$3:$F$501,2,FALSE)&F1329&\"_\"&VLOOKUP(G1329,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1329&\" \"&\"AT%M\"&A1329&\" \"&\":\"&C1329&\";\"&\" \"&\"(*\"&H1329&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1329,SEARCH(\"AT%\",J1329),,REPT(\" \",25-SEARCH(\"AT%\",J1329))),SEARCH(\":\",REPLACE(J1329,SEARCH(\"AT%\",J1329),,REPT(\" \",25-SEARCH(\"AT%\",J1329)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1329,SEARCH(\"AT%\",J1329),,REPT(\" \",25-SEARCH(\"AT%\",J1329))))))","v":{"$error":"#N/A"}}]
["FMJ"]
[{"$f":"IF(OR(C1329=\"REAL\",C1329=\"DWORD\",C1329=\"DINT\"),(IF(OR(C1331=\"REAL\",C1331=\"DWORD\",C1331=\"DINT\"),A1329+4+MOD(A1329,4),A1329+4)),(IF(OR(C1331=\"REAL\",C1331=\"DWORD\",C1331=\"DINT\"),A1329+4+MOD(A1329,4),A1329+2)))&\".0\"","v":"544.0"},{"$f":"IF((IF(OR(C1331=\"INT\",C1331=\"WORD\",C1331=\"BOOL\"),MOD(A1331,2),MOD(A1331,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A10","启停控制",{"$f":"D1331&F1331&\"-\"&IF(E1331=\"R\",\"新云平台\"&G1331,G1331)","v":"电风幕机01A10-新云平台启停控制"},{"$f":"E1331&VLOOKUP(D1331,list!$D$3:$F$501,2,FALSE)&F1331&\"_\"&VLOOKUP(G1331,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1331&\" \"&\"AT%M\"&A1331&\" \"&\":\"&C1331&\";\"&\" \"&\"(*\"&H1331&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1331,SEARCH(\"AT%\",J1331),,REPT(\" \",25-SEARCH(\"AT%\",J1331))),SEARCH(\":\",REPLACE(J1331,SEARCH(\"AT%\",J1331),,REPT(\" \",25-SEARCH(\"AT%\",J1331)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1331,SEARCH(\"AT%\",J1331),,REPT(\" \",25-SEARCH(\"AT%\",J1331))))))","v":{"$error":"#N/A"}}]
["DMJ"]
[{"$f":"IF(OR(C1331=\"REAL\",C1331=\"DWORD\",C1331=\"DINT\"),(IF(OR(C1333=\"REAL\",C1333=\"DWORD\",C1333=\"DINT\"),A1331+4+MOD(A1331,4),A1331+4)),(IF(OR(C1333=\"REAL\",C1333=\"DWORD\",C1333=\"DINT\"),A1331+4+MOD(A1331,4),A1331+2)))&\".0\"","v":"546.0"},{"$f":"IF((IF(OR(C1333=\"INT\",C1333=\"WORD\",C1333=\"BOOL\"),MOD(A1333,2),MOD(A1333,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","电风幕机","R","01A01","水风幕阀控制",{"$f":"D1333&F1333&\"-\"&IF(E1333=\"R\",\"新云平台\"&G1333,G1333)","v":"电风幕机01A01-新云平台水风幕阀控制"},{"$f":"E1333&VLOOKUP(D1333,list!$D$3:$F$501,2,FALSE)&F1333&\"_\"&VLOOKUP(G1333,list!$I$2:$K$502,2,FALSE)","v":{"$error":"#N/A"}},{"$f":"I1333&\" \"&\"AT%M\"&A1333&\" \"&\":\"&C1333&\";\"&\" \"&\"(*\"&H1333&\"*)\"","v":{"$error":"#N/A"}},{"$f":"REPLACE(REPLACE(J1333,SEARCH(\"AT%\",J1333),,REPT(\" \",25-SEARCH(\"AT%\",J1333))),SEARCH(\":\",REPLACE(J1333,SEARCH(\"AT%\",J1333),,REPT(\" \",25-SEARCH(\"AT%\",J1333)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1333,SEARCH(\"AT%\",J1333),,REPT(\" \",25-SEARCH(\"AT%\",J1333))))))","v":{"$error":"#N/A"}}]
["AHU"]
[{"$f":"IF(OR(C1331=\"REAL\",C1331=\"DWORD\",C1331=\"DINT\"),(IF(OR(C1335=\"REAL\",C1335=\"DWORD\",C1335=\"DINT\"),A1331+4+MOD(A1331,4),A1331+4)),(IF(OR(C1335=\"REAL\",C1335=\"DWORD\",C1335=\"DINT\"),A1331+4+MOD(A1331,4),A1331+2)))&\".0\"","v":"548.0"},{"$f":"IF((IF(OR(C1335=\"INT\",C1335=\"WORD\",C1335=\"BOOL\"),MOD(A1335,2),MOD(A1335,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02A01","设定温度值",{"$f":"D1335&F1335&\"-\"&IF(E1335=\"R\",\"新云平台\"&G1335,G1335)","v":"空调机组02A01-新云平台设定温度值"},{"$f":"E1335&VLOOKUP(D1335,list!$D$3:$F$501,2,FALSE)&F1335&\"_\"&VLOOKUP(G1335,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A01_TSET"},{"$f":"I1335&\" \"&\"AT%M\"&A1335&\" \"&\":\"&C1335&\";\"&\" \"&\"(*\"&H1335&\"*)\"","v":"RAHU02A01_TSET AT%M548.0 :REAL; (*空调机组02A01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1335,SEARCH(\"AT%\",J1335),,REPT(\" \",25-SEARCH(\"AT%\",J1335))),SEARCH(\":\",REPLACE(J1335,SEARCH(\"AT%\",J1335),,REPT(\" \",25-SEARCH(\"AT%\",J1335)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1335,SEARCH(\"AT%\",J1335),,REPT(\" \",25-SEARCH(\"AT%\",J1335))))))","v":"RAHU02A01_TSET          AT%M548.0      :REAL; (*空调机组02A01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1335=\"REAL\",C1335=\"DWORD\",C1335=\"DINT\"),(IF(OR(C1336=\"REAL\",C1336=\"DWORD\",C1336=\"DINT\"),A1335+4+MOD(A1335,4),A1335+4)),(IF(OR(C1336=\"REAL\",C1336=\"DWORD\",C1336=\"DINT\"),A1335+4+MOD(A1335,4),A1335+2)))&\".0\"","v":"552.0"},"验证通过","INT","空调机组","R",{"$f":"F1335","v":"02A01"},"季节模式","空调机组02A01-新云平台季节模式",{"$f":"E1336&VLOOKUP(D1336,list!$D$3:$F$501,2,FALSE)&F1336&\"_\"&VLOOKUP(G1336,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A01_SM"},"RAHU02A01_SM AT%M552.0 :INT; (*空调机组02A01-新云平台季节模式*)","RAHU02A01_SM            AT%M552.0      :INT; (*空调机组02A01-新云平台季节模式*)"]
[{"$f":"IF(OR(C1336=\"REAL\",C1336=\"DWORD\",C1336=\"DINT\"),(IF(OR(C1337=\"REAL\",C1337=\"DWORD\",C1337=\"DINT\"),A1336+4+MOD(A1336,4),A1336+4)),(IF(OR(C1337=\"REAL\",C1337=\"DWORD\",C1337=\"DINT\"),A1336+4+MOD(A1336,4),A1336+2)))&\".0\"","v":"554.0"},"验证通过","BOOL","空调机组","R",{"$f":"F1336","v":"02A01"},"程序控制","空调机组02A01-新云平台程序控制",{"$f":"E1337&VLOOKUP(D1337,list!$D$3:$F$501,2,FALSE)&F1337&\"_\"&VLOOKUP(G1337,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A01_PC"},"RAHU02A01_PC AT%M554.0 :BOOL; (*空调机组02A01-新云平台程序控制*)","RAHU02A01_PC            AT%M554.0      :BOOL; (*空调机组02A01-新云平台程序控制*)"]
["560.0","验证通过","REAL","空调机组","L","02A01","设定温度值","空调机组02A01-设定温度值",{"$f":"E1338&VLOOKUP(D1338,list!$D$3:$F$501,2,FALSE)&F1338&\"_\"&VLOOKUP(G1338,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_TSET"},"LAHU02A01_TSET AT%M560.0 :REAL; (*空调机组02A01-设定温度值*)","LAHU02A01_TSET          AT%M560.0      :REAL; (*空调机组02A01-设定温度值*)"]
["564.0","验证通过","INT","空调机组","L","02A01","季节模式","空调机组02A01-季节模式",{"$f":"E1339&VLOOKUP(D1339,list!$D$3:$F$501,2,FALSE)&F1339&\"_\"&VLOOKUP(G1339,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_SM"},"LAHU02A01_SM AT%M564.0 :INT; (*空调机组02A01-季节模式*)","LAHU02A01_SM            AT%M564.0      :INT; (*空调机组02A01-季节模式*)"]
["568.0","验证通过","REAL","空调机组","L","02A01","水阀反馈换算值","空调机组02A01-水阀反馈换算值",{"$f":"E1340&VLOOKUP(D1340,list!$D$3:$F$501,2,FALSE)&F1340&\"_\"&VLOOKUP(G1340,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_WVBS"},"LAHU02A01_WVBS AT%M568.0 :REAL; (*空调机组02A01-水阀反馈换算值*)","LAHU02A01_WVBS          AT%M568.0      :REAL; (*空调机组02A01-水阀反馈换算值*)"]
["572.0","验证通过","BOOL","空调机组","L","02A01","水阀手动控制","空调机组02A01-水阀手动控制",{"$f":"E1341&VLOOKUP(D1341,list!$D$3:$F$501,2,FALSE)&F1341&\"_\"&VLOOKUP(G1341,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_WVMC"},"LAHU02A01_WVMC AT%M572.0 :BOOL; (*空调机组02A01-水阀手动控制*)","LAHU02A01_WVMC          AT%M572.0      :BOOL; (*空调机组02A01-水阀手动控制*)"]
["576.0","验证通过","REAL","空调机组","L","02A01","水阀手动控制值","空调机组02A01-水阀手动控制值",{"$f":"E1342&VLOOKUP(D1342,list!$D$3:$F$501,2,FALSE)&F1342&\"_\"&VLOOKUP(G1342,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_WVMV"},"LAHU02A01_WVMV AT%M576.0 :REAL; (*空调机组02A01-水阀手动控制值*)","LAHU02A01_WVMV          AT%M576.0      :REAL; (*空调机组02A01-水阀手动控制值*)"]
["580.0","验证通过","REAL","空调机组","L","02A01","回风温度换算值","空调机组02A01-回风温度换算值",{"$f":"E1343&VLOOKUP(D1343,list!$D$3:$F$501,2,FALSE)&F1343&\"_\"&VLOOKUP(G1343,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_RTS"},"LAHU02A01_RTS AT%M580.0 :REAL; (*空调机组02A01-回风温度换算值*)","LAHU02A01_RTS           AT%M580.0      :REAL; (*空调机组02A01-回风温度换算值*)"]
["584.0","验证通过","BOOL","空调机组","L","02A01","运行时间累积重置","空调机组02A01-运行时间累积重置",{"$f":"E1344&VLOOKUP(D1344,list!$D$3:$F$501,2,FALSE)&F1344&\"_\"&VLOOKUP(G1344,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_RST"},"LAHU02A01_RST AT%M584.0 :BOOL; (*空调机组02A01-运行时间累积重置*)","LAHU02A01_RST           AT%M584.0      :BOOL; (*空调机组02A01-运行时间累积重置*)"]
["588.0","验证通过","REAL","空调机组","L","02A01","运行时间累积重置值","空调机组02A01-运行时间累积重置值",{"$f":"E1345&VLOOKUP(D1345,list!$D$3:$F$501,2,FALSE)&F1345&\"_\"&VLOOKUP(G1345,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_RSTV"},"LAHU02A01_RSTV AT%M588.0 :REAL; (*空调机组02A01-运行时间累积重置值*)","LAHU02A01_RSTV          AT%M588.0      :REAL; (*空调机组02A01-运行时间累积重置值*)"]
["592.0","验证通过","BOOL","空调机组","L","02A01","隔离开关1","空调机组02A01-隔离开关1",{"$f":"E1346&VLOOKUP(D1346,list!$D$3:$F$501,2,FALSE)&F1346&\"_\"&VLOOKUP(G1346,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_ISO1"},"LAHU02A01_ISO1 AT%M592.0 :BOOL; (*空调机组02A01-隔离开关1*)","LAHU02A01_ISO1          AT%M592.0      :BOOL; (*空调机组02A01-隔离开关1*)"]
["594.0","验证通过","BOOL","空调机组","L","02A01","隔离开关2","空调机组02A01-隔离开关2",{"$f":"E1347&VLOOKUP(D1347,list!$D$3:$F$501,2,FALSE)&F1347&\"_\"&VLOOKUP(G1347,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_ISO2"},"LAHU02A01_ISO2 AT%M594.0 :BOOL; (*空调机组02A01-隔离开关2*)","LAHU02A01_ISO2          AT%M594.0      :BOOL; (*空调机组02A01-隔离开关2*)"]
["600.0","验证通过","REAL","空调机组","L","02A01","P调节参数","空调机组02A01-P调节参数",{"$f":"E1348&VLOOKUP(D1348,list!$D$3:$F$501,2,FALSE)&F1348&\"_\"&VLOOKUP(G1348,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_VP"},"LAHU02A01_VP AT%M600.0 :REAL; (*空调机组02A01-P调节参数*)","LAHU02A01_VP            AT%M600.0      :REAL; (*空调机组02A01-P调节参数*)"]
["604.0","验证通过","REAL","空调机组","L","02A01","I调节参数","空调机组02A01-I调节参数",{"$f":"E1349&VLOOKUP(D1349,list!$D$3:$F$501,2,FALSE)&F1349&\"_\"&VLOOKUP(G1349,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_VI"},"LAHU02A01_VI AT%M604.0 :REAL; (*空调机组02A01-I调节参数*)","LAHU02A01_VI            AT%M604.0      :REAL; (*空调机组02A01-I调节参数*)"]
["608.0","验证通过","REAL","空调机组","L","02A01","运行时间累积值","空调机组02A01-运行时间累积值",{"$f":"E1350&VLOOKUP(D1350,list!$D$3:$F$501,2,FALSE)&F1350&\"_\"&VLOOKUP(G1350,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_RH"},"LAHU02A01_RH AT%M608.0 :REAL; (*空调机组02A01-运行时间累积值*)","LAHU02A01_RH            AT%M608.0      :REAL; (*空调机组02A01-运行时间累积值*)"]
["612.0","验证通过","INT","空调机组","L","02A01","设备状态代码","空调机组02A01-设备状态代码",{"$f":"E1351&VLOOKUP(D1351,list!$D$3:$F$501,2,FALSE)&F1351&\"_\"&VLOOKUP(G1351,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_SN"},"LAHU02A01_SN AT%M612.0 :INT; (*空调机组02A01-设备状态代码*)","LAHU02A01_SN            AT%M612.0      :INT; (*空调机组02A01-设备状态代码*)"]
["614.0","验证通过","INT","空调机组","L","02A01","水阀控制转换值","空调机组02A01-水阀控制转换值",{"$f":"E1352&VLOOKUP(D1352,list!$D$3:$F$501,2,FALSE)&F1352&\"_\"&VLOOKUP(G1352,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_WVCS"},"LAHU02A01_WVCS AT%M614.0 :INT; (*空调机组02A01-水阀控制转换值*)","LAHU02A01_WVCS          AT%M614.0      :INT; (*空调机组02A01-水阀控制转换值*)"]
["616.0","验证通过","BOOL","空调机组","L","02A01","程序控制","空调机组02A01-程序控制",{"$f":"E1353&VLOOKUP(D1353,list!$D$3:$F$501,2,FALSE)&F1353&\"_\"&VLOOKUP(G1353,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A01_PC"},"LAHU02A01_PC AT%M616.0 :BOOL; (*空调机组02A01-程序控制*)","LAHU02A01_PC            AT%M616.0      :BOOL; (*空调机组02A01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1353=\"REAL\",C1353=\"DWORD\",C1353=\"DINT\"),(IF(OR(C1355=\"REAL\",C1355=\"DWORD\",C1355=\"DINT\"),A1353+4+MOD(A1353,4),A1353+4)),(IF(OR(C1355=\"REAL\",C1355=\"DWORD\",C1355=\"DINT\"),A1353+4+MOD(A1353,4),A1353+2)))&\".0\"","v":"620.0"},{"$f":"IF((IF(OR(C1355=\"INT\",C1355=\"WORD\",C1355=\"BOOL\"),MOD(A1355,2),MOD(A1355,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02A02","设定温度值",{"$f":"D1355&F1355&\"-\"&IF(E1355=\"R\",\"新云平台\"&G1355,G1355)","v":"空调机组02A02-新云平台设定温度值"},{"$f":"E1355&VLOOKUP(D1355,list!$D$3:$F$501,2,FALSE)&F1355&\"_\"&VLOOKUP(G1355,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A02_TSET"},{"$f":"I1355&\" \"&\"AT%M\"&A1355&\" \"&\":\"&C1355&\";\"&\" \"&\"(*\"&H1355&\"*)\"","v":"RAHU02A02_TSET AT%M620.0 :REAL; (*空调机组02A02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1355,SEARCH(\"AT%\",J1355),,REPT(\" \",25-SEARCH(\"AT%\",J1355))),SEARCH(\":\",REPLACE(J1355,SEARCH(\"AT%\",J1355),,REPT(\" \",25-SEARCH(\"AT%\",J1355)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1355,SEARCH(\"AT%\",J1355),,REPT(\" \",25-SEARCH(\"AT%\",J1355))))))","v":"RAHU02A02_TSET          AT%M620.0      :REAL; (*空调机组02A02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1355=\"REAL\",C1355=\"DWORD\",C1355=\"DINT\"),(IF(OR(C1356=\"REAL\",C1356=\"DWORD\",C1356=\"DINT\"),A1355+4+MOD(A1355,4),A1355+4)),(IF(OR(C1356=\"REAL\",C1356=\"DWORD\",C1356=\"DINT\"),A1355+4+MOD(A1355,4),A1355+2)))&\".0\"","v":"624.0"},"验证通过","INT","空调机组","R",{"$f":"F1355","v":"02A02"},"季节模式","空调机组02A02-新云平台季节模式",{"$f":"E1356&VLOOKUP(D1356,list!$D$3:$F$501,2,FALSE)&F1356&\"_\"&VLOOKUP(G1356,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A02_SM"},"RAHU02A02_SM AT%M624.0 :INT; (*空调机组02A02-新云平台季节模式*)","RAHU02A02_SM            AT%M624.0      :INT; (*空调机组02A02-新云平台季节模式*)"]
[{"$f":"IF(OR(C1356=\"REAL\",C1356=\"DWORD\",C1356=\"DINT\"),(IF(OR(C1357=\"REAL\",C1357=\"DWORD\",C1357=\"DINT\"),A1356+4+MOD(A1356,4),A1356+4)),(IF(OR(C1357=\"REAL\",C1357=\"DWORD\",C1357=\"DINT\"),A1356+4+MOD(A1356,4),A1356+2)))&\".0\"","v":"626.0"},"验证通过","BOOL","空调机组","R",{"$f":"F1356","v":"02A02"},"程序控制","空调机组02A02-新云平台程序控制",{"$f":"E1357&VLOOKUP(D1357,list!$D$3:$F$501,2,FALSE)&F1357&\"_\"&VLOOKUP(G1357,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A02_PC"},"RAHU02A02_PC AT%M626.0 :BOOL; (*空调机组02A02-新云平台程序控制*)","RAHU02A02_PC            AT%M626.0      :BOOL; (*空调机组02A02-新云平台程序控制*)"]
["632.0","验证通过","REAL","空调机组","L","02A02","设定温度值","空调机组02A02-设定温度值",{"$f":"E1358&VLOOKUP(D1358,list!$D$3:$F$501,2,FALSE)&F1358&\"_\"&VLOOKUP(G1358,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_TSET"},"LAHU02A02_TSET AT%M632.0 :REAL; (*空调机组02A02-设定温度值*)","LAHU02A02_TSET          AT%M632.0      :REAL; (*空调机组02A02-设定温度值*)"]
["636.0","验证通过","INT","空调机组","L","02A02","季节模式","空调机组02A02-季节模式",{"$f":"E1359&VLOOKUP(D1359,list!$D$3:$F$501,2,FALSE)&F1359&\"_\"&VLOOKUP(G1359,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_SM"},"LAHU02A02_SM AT%M636.0 :INT; (*空调机组02A02-季节模式*)","LAHU02A02_SM            AT%M636.0      :INT; (*空调机组02A02-季节模式*)"]
["640.0","验证通过","REAL","空调机组","L","02A02","水阀反馈换算值","空调机组02A02-水阀反馈换算值",{"$f":"E1360&VLOOKUP(D1360,list!$D$3:$F$501,2,FALSE)&F1360&\"_\"&VLOOKUP(G1360,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_WVBS"},"LAHU02A02_WVBS AT%M640.0 :REAL; (*空调机组02A02-水阀反馈换算值*)","LAHU02A02_WVBS          AT%M640.0      :REAL; (*空调机组02A02-水阀反馈换算值*)"]
["644.0","验证通过","BOOL","空调机组","L","02A02","水阀手动控制","空调机组02A02-水阀手动控制",{"$f":"E1361&VLOOKUP(D1361,list!$D$3:$F$501,2,FALSE)&F1361&\"_\"&VLOOKUP(G1361,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_WVMC"},"LAHU02A02_WVMC AT%M644.0 :BOOL; (*空调机组02A02-水阀手动控制*)","LAHU02A02_WVMC          AT%M644.0      :BOOL; (*空调机组02A02-水阀手动控制*)"]
["648.0","验证通过","REAL","空调机组","L","02A02","水阀手动控制值","空调机组02A02-水阀手动控制值",{"$f":"E1362&VLOOKUP(D1362,list!$D$3:$F$501,2,FALSE)&F1362&\"_\"&VLOOKUP(G1362,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_WVMV"},"LAHU02A02_WVMV AT%M648.0 :REAL; (*空调机组02A02-水阀手动控制值*)","LAHU02A02_WVMV          AT%M648.0      :REAL; (*空调机组02A02-水阀手动控制值*)"]
["652.0","验证通过","REAL","空调机组","L","02A02","回风温度换算值","空调机组02A02-回风温度换算值",{"$f":"E1363&VLOOKUP(D1363,list!$D$3:$F$501,2,FALSE)&F1363&\"_\"&VLOOKUP(G1363,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_RTS"},"LAHU02A02_RTS AT%M652.0 :REAL; (*空调机组02A02-回风温度换算值*)","LAHU02A02_RTS           AT%M652.0      :REAL; (*空调机组02A02-回风温度换算值*)"]
["656.0","验证通过","BOOL","空调机组","L","02A02","运行时间累积重置","空调机组02A02-运行时间累积重置",{"$f":"E1364&VLOOKUP(D1364,list!$D$3:$F$501,2,FALSE)&F1364&\"_\"&VLOOKUP(G1364,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_RST"},"LAHU02A02_RST AT%M656.0 :BOOL; (*空调机组02A02-运行时间累积重置*)","LAHU02A02_RST           AT%M656.0      :BOOL; (*空调机组02A02-运行时间累积重置*)"]
["660.0","验证通过","REAL","空调机组","L","02A02","运行时间累积重置值","空调机组02A02-运行时间累积重置值",{"$f":"E1365&VLOOKUP(D1365,list!$D$3:$F$501,2,FALSE)&F1365&\"_\"&VLOOKUP(G1365,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_RSTV"},"LAHU02A02_RSTV AT%M660.0 :REAL; (*空调机组02A02-运行时间累积重置值*)","LAHU02A02_RSTV          AT%M660.0      :REAL; (*空调机组02A02-运行时间累积重置值*)"]
["664.0","验证通过","BOOL","空调机组","L","02A02","隔离开关1","空调机组02A02-隔离开关1",{"$f":"E1366&VLOOKUP(D1366,list!$D$3:$F$501,2,FALSE)&F1366&\"_\"&VLOOKUP(G1366,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_ISO1"},"LAHU02A02_ISO1 AT%M664.0 :BOOL; (*空调机组02A02-隔离开关1*)","LAHU02A02_ISO1          AT%M664.0      :BOOL; (*空调机组02A02-隔离开关1*)"]
["666.0","验证通过","BOOL","空调机组","L","02A02","隔离开关2","空调机组02A02-隔离开关2",{"$f":"E1367&VLOOKUP(D1367,list!$D$3:$F$501,2,FALSE)&F1367&\"_\"&VLOOKUP(G1367,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_ISO2"},"LAHU02A02_ISO2 AT%M666.0 :BOOL; (*空调机组02A02-隔离开关2*)","LAHU02A02_ISO2          AT%M666.0      :BOOL; (*空调机组02A02-隔离开关2*)"]
["672.0","验证通过","REAL","空调机组","L","02A02","P调节参数","空调机组02A02-P调节参数",{"$f":"E1368&VLOOKUP(D1368,list!$D$3:$F$501,2,FALSE)&F1368&\"_\"&VLOOKUP(G1368,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_VP"},"LAHU02A02_VP AT%M672.0 :REAL; (*空调机组02A02-P调节参数*)","LAHU02A02_VP            AT%M672.0      :REAL; (*空调机组02A02-P调节参数*)"]
["676.0","验证通过","REAL","空调机组","L","02A02","I调节参数","空调机组02A02-I调节参数",{"$f":"E1369&VLOOKUP(D1369,list!$D$3:$F$501,2,FALSE)&F1369&\"_\"&VLOOKUP(G1369,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_VI"},"LAHU02A02_VI AT%M676.0 :REAL; (*空调机组02A02-I调节参数*)","LAHU02A02_VI            AT%M676.0      :REAL; (*空调机组02A02-I调节参数*)"]
["680.0","验证通过","REAL","空调机组","L","02A02","运行时间累积值","空调机组02A02-运行时间累积值",{"$f":"E1370&VLOOKUP(D1370,list!$D$3:$F$501,2,FALSE)&F1370&\"_\"&VLOOKUP(G1370,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_RH"},"LAHU02A02_RH AT%M680.0 :REAL; (*空调机组02A02-运行时间累积值*)","LAHU02A02_RH            AT%M680.0      :REAL; (*空调机组02A02-运行时间累积值*)"]
["684.0","验证通过","INT","空调机组","L","02A02","设备状态代码","空调机组02A02-设备状态代码",{"$f":"E1371&VLOOKUP(D1371,list!$D$3:$F$501,2,FALSE)&F1371&\"_\"&VLOOKUP(G1371,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_SN"},"LAHU02A02_SN AT%M684.0 :INT; (*空调机组02A02-设备状态代码*)","LAHU02A02_SN            AT%M684.0      :INT; (*空调机组02A02-设备状态代码*)"]
["686.0","验证通过","INT","空调机组","L","02A02","水阀控制转换值","空调机组02A02-水阀控制转换值",{"$f":"E1372&VLOOKUP(D1372,list!$D$3:$F$501,2,FALSE)&F1372&\"_\"&VLOOKUP(G1372,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_WVCS"},"LAHU02A02_WVCS AT%M686.0 :INT; (*空调机组02A02-水阀控制转换值*)","LAHU02A02_WVCS          AT%M686.0      :INT; (*空调机组02A02-水阀控制转换值*)"]
["688.0","验证通过","BOOL","空调机组","L","02A02","程序控制","空调机组02A02-程序控制",{"$f":"E1373&VLOOKUP(D1373,list!$D$3:$F$501,2,FALSE)&F1373&\"_\"&VLOOKUP(G1373,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A02_PC"},"LAHU02A02_PC AT%M688.0 :BOOL; (*空调机组02A02-程序控制*)","LAHU02A02_PC            AT%M688.0      :BOOL; (*空调机组02A02-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1373=\"REAL\",C1373=\"DWORD\",C1373=\"DINT\"),(IF(OR(C1375=\"REAL\",C1375=\"DWORD\",C1375=\"DINT\"),A1373+4+MOD(A1373,4),A1373+4)),(IF(OR(C1375=\"REAL\",C1375=\"DWORD\",C1375=\"DINT\"),A1373+4+MOD(A1373,4),A1373+2)))&\".0\"","v":"692.0"},{"$f":"IF((IF(OR(C1375=\"INT\",C1375=\"WORD\",C1375=\"BOOL\"),MOD(A1375,2),MOD(A1375,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02A03","设定温度值",{"$f":"D1375&F1375&\"-\"&IF(E1375=\"R\",\"新云平台\"&G1375,G1375)","v":"空调机组02A03-新云平台设定温度值"},{"$f":"E1375&VLOOKUP(D1375,list!$D$3:$F$501,2,FALSE)&F1375&\"_\"&VLOOKUP(G1375,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A03_TSET"},{"$f":"I1375&\" \"&\"AT%M\"&A1375&\" \"&\":\"&C1375&\";\"&\" \"&\"(*\"&H1375&\"*)\"","v":"RAHU02A03_TSET AT%M692.0 :REAL; (*空调机组02A03-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1375,SEARCH(\"AT%\",J1375),,REPT(\" \",25-SEARCH(\"AT%\",J1375))),SEARCH(\":\",REPLACE(J1375,SEARCH(\"AT%\",J1375),,REPT(\" \",25-SEARCH(\"AT%\",J1375)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1375,SEARCH(\"AT%\",J1375),,REPT(\" \",25-SEARCH(\"AT%\",J1375))))))","v":"RAHU02A03_TSET          AT%M692.0      :REAL; (*空调机组02A03-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1375=\"REAL\",C1375=\"DWORD\",C1375=\"DINT\"),(IF(OR(C1376=\"REAL\",C1376=\"DWORD\",C1376=\"DINT\"),A1375+4+MOD(A1375,4),A1375+4)),(IF(OR(C1376=\"REAL\",C1376=\"DWORD\",C1376=\"DINT\"),A1375+4+MOD(A1375,4),A1375+2)))&\".0\"","v":"696.0"},"验证通过","INT","空调机组","R",{"$f":"F1375","v":"02A03"},"季节模式","空调机组02A03-新云平台季节模式",{"$f":"E1376&VLOOKUP(D1376,list!$D$3:$F$501,2,FALSE)&F1376&\"_\"&VLOOKUP(G1376,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A03_SM"},"RAHU02A03_SM AT%M696.0 :INT; (*空调机组02A03-新云平台季节模式*)","RAHU02A03_SM            AT%M696.0      :INT; (*空调机组02A03-新云平台季节模式*)"]
[{"$f":"IF(OR(C1376=\"REAL\",C1376=\"DWORD\",C1376=\"DINT\"),(IF(OR(C1377=\"REAL\",C1377=\"DWORD\",C1377=\"DINT\"),A1376+4+MOD(A1376,4),A1376+4)),(IF(OR(C1377=\"REAL\",C1377=\"DWORD\",C1377=\"DINT\"),A1376+4+MOD(A1376,4),A1376+2)))&\".0\"","v":"698.0"},"验证通过","BOOL","空调机组","R",{"$f":"F1376","v":"02A03"},"程序控制","空调机组02A03-新云平台程序控制",{"$f":"E1377&VLOOKUP(D1377,list!$D$3:$F$501,2,FALSE)&F1377&\"_\"&VLOOKUP(G1377,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A03_PC"},"RAHU02A03_PC AT%M698.0 :BOOL; (*空调机组02A03-新云平台程序控制*)","RAHU02A03_PC            AT%M698.0      :BOOL; (*空调机组02A03-新云平台程序控制*)"]
["704.0","验证通过","REAL","空调机组","L","02A03","设定温度值","空调机组02A03-设定温度值",{"$f":"E1378&VLOOKUP(D1378,list!$D$3:$F$501,2,FALSE)&F1378&\"_\"&VLOOKUP(G1378,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_TSET"},"LAHU02A03_TSET AT%M704.0 :REAL; (*空调机组02A03-设定温度值*)","LAHU02A03_TSET          AT%M704.0      :REAL; (*空调机组02A03-设定温度值*)"]
["708.0","验证通过","INT","空调机组","L","02A03","季节模式","空调机组02A03-季节模式",{"$f":"E1379&VLOOKUP(D1379,list!$D$3:$F$501,2,FALSE)&F1379&\"_\"&VLOOKUP(G1379,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_SM"},"LAHU02A03_SM AT%M708.0 :INT; (*空调机组02A03-季节模式*)","LAHU02A03_SM            AT%M708.0      :INT; (*空调机组02A03-季节模式*)"]
["712.0","验证通过","REAL","空调机组","L","02A03","水阀反馈换算值","空调机组02A03-水阀反馈换算值",{"$f":"E1380&VLOOKUP(D1380,list!$D$3:$F$501,2,FALSE)&F1380&\"_\"&VLOOKUP(G1380,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_WVBS"},"LAHU02A03_WVBS AT%M712.0 :REAL; (*空调机组02A03-水阀反馈换算值*)","LAHU02A03_WVBS          AT%M712.0      :REAL; (*空调机组02A03-水阀反馈换算值*)"]
["716.0","验证通过","BOOL","空调机组","L","02A03","水阀手动控制","空调机组02A03-水阀手动控制",{"$f":"E1381&VLOOKUP(D1381,list!$D$3:$F$501,2,FALSE)&F1381&\"_\"&VLOOKUP(G1381,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_WVMC"},"LAHU02A03_WVMC AT%M716.0 :BOOL; (*空调机组02A03-水阀手动控制*)","LAHU02A03_WVMC          AT%M716.0      :BOOL; (*空调机组02A03-水阀手动控制*)"]
["720.0","验证通过","REAL","空调机组","L","02A03","水阀手动控制值","空调机组02A03-水阀手动控制值",{"$f":"E1382&VLOOKUP(D1382,list!$D$3:$F$501,2,FALSE)&F1382&\"_\"&VLOOKUP(G1382,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_WVMV"},"LAHU02A03_WVMV AT%M720.0 :REAL; (*空调机组02A03-水阀手动控制值*)","LAHU02A03_WVMV          AT%M720.0      :REAL; (*空调机组02A03-水阀手动控制值*)"]
["724.0","验证通过","REAL","空调机组","L","02A03","回风温度换算值","空调机组02A03-回风温度换算值",{"$f":"E1383&VLOOKUP(D1383,list!$D$3:$F$501,2,FALSE)&F1383&\"_\"&VLOOKUP(G1383,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_RTS"},"LAHU02A03_RTS AT%M724.0 :REAL; (*空调机组02A03-回风温度换算值*)","LAHU02A03_RTS           AT%M724.0      :REAL; (*空调机组02A03-回风温度换算值*)"]
["728.0","验证通过","BOOL","空调机组","L","02A03","运行时间累积重置","空调机组02A03-运行时间累积重置",{"$f":"E1384&VLOOKUP(D1384,list!$D$3:$F$501,2,FALSE)&F1384&\"_\"&VLOOKUP(G1384,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_RST"},"LAHU02A03_RST AT%M728.0 :BOOL; (*空调机组02A03-运行时间累积重置*)","LAHU02A03_RST           AT%M728.0      :BOOL; (*空调机组02A03-运行时间累积重置*)"]
["732.0","验证通过","REAL","空调机组","L","02A03","运行时间累积重置值","空调机组02A03-运行时间累积重置值",{"$f":"E1385&VLOOKUP(D1385,list!$D$3:$F$501,2,FALSE)&F1385&\"_\"&VLOOKUP(G1385,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_RSTV"},"LAHU02A03_RSTV AT%M732.0 :REAL; (*空调机组02A03-运行时间累积重置值*)","LAHU02A03_RSTV          AT%M732.0      :REAL; (*空调机组02A03-运行时间累积重置值*)"]
["736.0","验证通过","BOOL","空调机组","L","02A03","隔离开关1","空调机组02A03-隔离开关1",{"$f":"E1386&VLOOKUP(D1386,list!$D$3:$F$501,2,FALSE)&F1386&\"_\"&VLOOKUP(G1386,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_ISO1"},"LAHU02A03_ISO1 AT%M736.0 :BOOL; (*空调机组02A03-隔离开关1*)","LAHU02A03_ISO1          AT%M736.0      :BOOL; (*空调机组02A03-隔离开关1*)"]
["738.0","验证通过","BOOL","空调机组","L","02A03","隔离开关2","空调机组02A03-隔离开关2",{"$f":"E1387&VLOOKUP(D1387,list!$D$3:$F$501,2,FALSE)&F1387&\"_\"&VLOOKUP(G1387,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_ISO2"},"LAHU02A03_ISO2 AT%M738.0 :BOOL; (*空调机组02A03-隔离开关2*)","LAHU02A03_ISO2          AT%M738.0      :BOOL; (*空调机组02A03-隔离开关2*)"]
["744.0","验证通过","REAL","空调机组","L","02A03","P调节参数","空调机组02A03-P调节参数",{"$f":"E1388&VLOOKUP(D1388,list!$D$3:$F$501,2,FALSE)&F1388&\"_\"&VLOOKUP(G1388,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_VP"},"LAHU02A03_VP AT%M744.0 :REAL; (*空调机组02A03-P调节参数*)","LAHU02A03_VP            AT%M744.0      :REAL; (*空调机组02A03-P调节参数*)"]
["748.0","验证通过","REAL","空调机组","L","02A03","I调节参数","空调机组02A03-I调节参数",{"$f":"E1389&VLOOKUP(D1389,list!$D$3:$F$501,2,FALSE)&F1389&\"_\"&VLOOKUP(G1389,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_VI"},"LAHU02A03_VI AT%M748.0 :REAL; (*空调机组02A03-I调节参数*)","LAHU02A03_VI            AT%M748.0      :REAL; (*空调机组02A03-I调节参数*)"]
["752.0","验证通过","REAL","空调机组","L","02A03","运行时间累积值","空调机组02A03-运行时间累积值",{"$f":"E1390&VLOOKUP(D1390,list!$D$3:$F$501,2,FALSE)&F1390&\"_\"&VLOOKUP(G1390,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_RH"},"LAHU02A03_RH AT%M752.0 :REAL; (*空调机组02A03-运行时间累积值*)","LAHU02A03_RH            AT%M752.0      :REAL; (*空调机组02A03-运行时间累积值*)"]
["756.0","验证通过","INT","空调机组","L","02A03","设备状态代码","空调机组02A03-设备状态代码",{"$f":"E1391&VLOOKUP(D1391,list!$D$3:$F$501,2,FALSE)&F1391&\"_\"&VLOOKUP(G1391,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_SN"},"LAHU02A03_SN AT%M756.0 :INT; (*空调机组02A03-设备状态代码*)","LAHU02A03_SN            AT%M756.0      :INT; (*空调机组02A03-设备状态代码*)"]
["758.0","验证通过","INT","空调机组","L","02A03","水阀控制转换值","空调机组02A03-水阀控制转换值",{"$f":"E1392&VLOOKUP(D1392,list!$D$3:$F$501,2,FALSE)&F1392&\"_\"&VLOOKUP(G1392,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_WVCS"},"LAHU02A03_WVCS AT%M758.0 :INT; (*空调机组02A03-水阀控制转换值*)","LAHU02A03_WVCS          AT%M758.0      :INT; (*空调机组02A03-水阀控制转换值*)"]
["760.0","验证通过","BOOL","空调机组","L","02A03","程序控制","空调机组02A03-程序控制",{"$f":"E1393&VLOOKUP(D1393,list!$D$3:$F$501,2,FALSE)&F1393&\"_\"&VLOOKUP(G1393,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A03_PC"},"LAHU02A03_PC AT%M760.0 :BOOL; (*空调机组02A03-程序控制*)","LAHU02A03_PC            AT%M760.0      :BOOL; (*空调机组02A03-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1393=\"REAL\",C1393=\"DWORD\",C1393=\"DINT\"),(IF(OR(C1395=\"REAL\",C1395=\"DWORD\",C1395=\"DINT\"),A1393+4+MOD(A1393,4),A1393+4)),(IF(OR(C1395=\"REAL\",C1395=\"DWORD\",C1395=\"DINT\"),A1393+4+MOD(A1393,4),A1393+2)))&\".0\"","v":"764.0"},{"$f":"IF((IF(OR(C1395=\"INT\",C1395=\"WORD\",C1395=\"BOOL\"),MOD(A1395,2),MOD(A1395,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","02A04","设定温度值",{"$f":"D1395&F1395&\"-\"&IF(E1395=\"R\",\"新云平台\"&G1395,G1395)","v":"空调机组02A04-新云平台设定温度值"},{"$f":"E1395&VLOOKUP(D1395,list!$D$3:$F$501,2,FALSE)&F1395&\"_\"&VLOOKUP(G1395,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A04_TSET"},{"$f":"I1395&\" \"&\"AT%M\"&A1395&\" \"&\":\"&C1395&\";\"&\" \"&\"(*\"&H1395&\"*)\"","v":"RAHU02A04_TSET AT%M764.0 :REAL; (*空调机组02A04-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1395,SEARCH(\"AT%\",J1395),,REPT(\" \",25-SEARCH(\"AT%\",J1395))),SEARCH(\":\",REPLACE(J1395,SEARCH(\"AT%\",J1395),,REPT(\" \",25-SEARCH(\"AT%\",J1395)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1395,SEARCH(\"AT%\",J1395),,REPT(\" \",25-SEARCH(\"AT%\",J1395))))))","v":"RAHU02A04_TSET          AT%M764.0      :REAL; (*空调机组02A04-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1395=\"REAL\",C1395=\"DWORD\",C1395=\"DINT\"),(IF(OR(C1396=\"REAL\",C1396=\"DWORD\",C1396=\"DINT\"),A1395+4+MOD(A1395,4),A1395+4)),(IF(OR(C1396=\"REAL\",C1396=\"DWORD\",C1396=\"DINT\"),A1395+4+MOD(A1395,4),A1395+2)))&\".0\"","v":"768.0"},"验证通过","INT","空调机组","R",{"$f":"F1395","v":"02A04"},"季节模式","空调机组02A04-新云平台季节模式",{"$f":"E1396&VLOOKUP(D1396,list!$D$3:$F$501,2,FALSE)&F1396&\"_\"&VLOOKUP(G1396,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A04_SM"},"RAHU02A04_SM AT%M768.0 :INT; (*空调机组02A04-新云平台季节模式*)","RAHU02A04_SM            AT%M768.0      :INT; (*空调机组02A04-新云平台季节模式*)"]
[{"$f":"IF(OR(C1396=\"REAL\",C1396=\"DWORD\",C1396=\"DINT\"),(IF(OR(C1397=\"REAL\",C1397=\"DWORD\",C1397=\"DINT\"),A1396+4+MOD(A1396,4),A1396+4)),(IF(OR(C1397=\"REAL\",C1397=\"DWORD\",C1397=\"DINT\"),A1396+4+MOD(A1396,4),A1396+2)))&\".0\"","v":"770.0"},"验证通过","BOOL","空调机组","R",{"$f":"F1396","v":"02A04"},"程序控制","空调机组02A04-新云平台程序控制",{"$f":"E1397&VLOOKUP(D1397,list!$D$3:$F$501,2,FALSE)&F1397&\"_\"&VLOOKUP(G1397,list!$I$2:$K$502,2,FALSE)","v":"RAHU02A04_PC"},"RAHU02A04_PC AT%M770.0 :BOOL; (*空调机组02A04-新云平台程序控制*)","RAHU02A04_PC            AT%M770.0      :BOOL; (*空调机组02A04-新云平台程序控制*)"]
["776.0","验证通过","REAL","空调机组","L","02A04","设定温度值","空调机组02A04-设定温度值",{"$f":"E1398&VLOOKUP(D1398,list!$D$3:$F$501,2,FALSE)&F1398&\"_\"&VLOOKUP(G1398,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_TSET"},"LAHU02A04_TSET AT%M776.0 :REAL; (*空调机组02A04-设定温度值*)","LAHU02A04_TSET          AT%M776.0      :REAL; (*空调机组02A04-设定温度值*)"]
["780.0","验证通过","INT","空调机组","L","02A04","季节模式","空调机组02A04-季节模式",{"$f":"E1399&VLOOKUP(D1399,list!$D$3:$F$501,2,FALSE)&F1399&\"_\"&VLOOKUP(G1399,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_SM"},"LAHU02A04_SM AT%M780.0 :INT; (*空调机组02A04-季节模式*)","LAHU02A04_SM            AT%M780.0      :INT; (*空调机组02A04-季节模式*)"]
["784.0","验证通过","REAL","空调机组","L","02A04","水阀反馈换算值","空调机组02A04-水阀反馈换算值",{"$f":"E1400&VLOOKUP(D1400,list!$D$3:$F$501,2,FALSE)&F1400&\"_\"&VLOOKUP(G1400,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_WVBS"},"LAHU02A04_WVBS AT%M784.0 :REAL; (*空调机组02A04-水阀反馈换算值*)","LAHU02A04_WVBS          AT%M784.0      :REAL; (*空调机组02A04-水阀反馈换算值*)"]
["788.0","验证通过","BOOL","空调机组","L","02A04","水阀手动控制","空调机组02A04-水阀手动控制",{"$f":"E1401&VLOOKUP(D1401,list!$D$3:$F$501,2,FALSE)&F1401&\"_\"&VLOOKUP(G1401,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_WVMC"},"LAHU02A04_WVMC AT%M788.0 :BOOL; (*空调机组02A04-水阀手动控制*)","LAHU02A04_WVMC          AT%M788.0      :BOOL; (*空调机组02A04-水阀手动控制*)"]
["792.0","验证通过","REAL","空调机组","L","02A04","水阀手动控制值","空调机组02A04-水阀手动控制值",{"$f":"E1402&VLOOKUP(D1402,list!$D$3:$F$501,2,FALSE)&F1402&\"_\"&VLOOKUP(G1402,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_WVMV"},"LAHU02A04_WVMV AT%M792.0 :REAL; (*空调机组02A04-水阀手动控制值*)","LAHU02A04_WVMV          AT%M792.0      :REAL; (*空调机组02A04-水阀手动控制值*)"]
["796.0","验证通过","REAL","空调机组","L","02A04","回风温度换算值","空调机组02A04-回风温度换算值",{"$f":"E1403&VLOOKUP(D1403,list!$D$3:$F$501,2,FALSE)&F1403&\"_\"&VLOOKUP(G1403,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_RTS"},"LAHU02A04_RTS AT%M796.0 :REAL; (*空调机组02A04-回风温度换算值*)","LAHU02A04_RTS           AT%M796.0      :REAL; (*空调机组02A04-回风温度换算值*)"]
["800.0","验证通过","BOOL","空调机组","L","02A04","运行时间累积重置","空调机组02A04-运行时间累积重置",{"$f":"E1404&VLOOKUP(D1404,list!$D$3:$F$501,2,FALSE)&F1404&\"_\"&VLOOKUP(G1404,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_RST"},"LAHU02A04_RST AT%M800.0 :BOOL; (*空调机组02A04-运行时间累积重置*)","LAHU02A04_RST           AT%M800.0      :BOOL; (*空调机组02A04-运行时间累积重置*)"]
["804.0","验证通过","REAL","空调机组","L","02A04","运行时间累积重置值","空调机组02A04-运行时间累积重置值",{"$f":"E1405&VLOOKUP(D1405,list!$D$3:$F$501,2,FALSE)&F1405&\"_\"&VLOOKUP(G1405,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_RSTV"},"LAHU02A04_RSTV AT%M804.0 :REAL; (*空调机组02A04-运行时间累积重置值*)","LAHU02A04_RSTV          AT%M804.0      :REAL; (*空调机组02A04-运行时间累积重置值*)"]
["808.0","验证通过","BOOL","空调机组","L","02A04","隔离开关1","空调机组02A04-隔离开关1",{"$f":"E1406&VLOOKUP(D1406,list!$D$3:$F$501,2,FALSE)&F1406&\"_\"&VLOOKUP(G1406,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_ISO1"},"LAHU02A04_ISO1 AT%M808.0 :BOOL; (*空调机组02A04-隔离开关1*)","LAHU02A04_ISO1          AT%M808.0      :BOOL; (*空调机组02A04-隔离开关1*)"]
["810.0","验证通过","BOOL","空调机组","L","02A04","隔离开关2","空调机组02A04-隔离开关2",{"$f":"E1407&VLOOKUP(D1407,list!$D$3:$F$501,2,FALSE)&F1407&\"_\"&VLOOKUP(G1407,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_ISO2"},"LAHU02A04_ISO2 AT%M810.0 :BOOL; (*空调机组02A04-隔离开关2*)","LAHU02A04_ISO2          AT%M810.0      :BOOL; (*空调机组02A04-隔离开关2*)"]
["816.0","验证通过","REAL","空调机组","L","02A04","P调节参数","空调机组02A04-P调节参数",{"$f":"E1408&VLOOKUP(D1408,list!$D$3:$F$501,2,FALSE)&F1408&\"_\"&VLOOKUP(G1408,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_VP"},"LAHU02A04_VP AT%M816.0 :REAL; (*空调机组02A04-P调节参数*)","LAHU02A04_VP            AT%M816.0      :REAL; (*空调机组02A04-P调节参数*)"]
["820.0","验证通过","REAL","空调机组","L","02A04","I调节参数","空调机组02A04-I调节参数",{"$f":"E1409&VLOOKUP(D1409,list!$D$3:$F$501,2,FALSE)&F1409&\"_\"&VLOOKUP(G1409,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_VI"},"LAHU02A04_VI AT%M820.0 :REAL; (*空调机组02A04-I调节参数*)","LAHU02A04_VI            AT%M820.0      :REAL; (*空调机组02A04-I调节参数*)"]
["824.0","验证通过","REAL","空调机组","L","02A04","运行时间累积值","空调机组02A04-运行时间累积值",{"$f":"E1410&VLOOKUP(D1410,list!$D$3:$F$501,2,FALSE)&F1410&\"_\"&VLOOKUP(G1410,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_RH"},"LAHU02A04_RH AT%M824.0 :REAL; (*空调机组02A04-运行时间累积值*)","LAHU02A04_RH            AT%M824.0      :REAL; (*空调机组02A04-运行时间累积值*)"]
["828.0","验证通过","INT","空调机组","L","02A04","设备状态代码","空调机组02A04-设备状态代码",{"$f":"E1411&VLOOKUP(D1411,list!$D$3:$F$501,2,FALSE)&F1411&\"_\"&VLOOKUP(G1411,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_SN"},"LAHU02A04_SN AT%M828.0 :INT; (*空调机组02A04-设备状态代码*)","LAHU02A04_SN            AT%M828.0      :INT; (*空调机组02A04-设备状态代码*)"]
["830.0","验证通过","INT","空调机组","L","02A04","水阀控制转换值","空调机组02A04-水阀控制转换值",{"$f":"E1412&VLOOKUP(D1412,list!$D$3:$F$501,2,FALSE)&F1412&\"_\"&VLOOKUP(G1412,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_WVCS"},"LAHU02A04_WVCS AT%M830.0 :INT; (*空调机组02A04-水阀控制转换值*)","LAHU02A04_WVCS          AT%M830.0      :INT; (*空调机组02A04-水阀控制转换值*)"]
["832.0","验证通过","BOOL","空调机组","L","02A04","程序控制","空调机组02A04-程序控制",{"$f":"E1413&VLOOKUP(D1413,list!$D$3:$F$501,2,FALSE)&F1413&\"_\"&VLOOKUP(G1413,list!$I$2:$K$502,2,FALSE)","v":"LAHU02A04_PC"},"LAHU02A04_PC AT%M832.0 :BOOL; (*空调机组02A04-程序控制*)","LAHU02A04_PC            AT%M832.0      :BOOL; (*空调机组02A04-程序控制*)"]
["FCU"]
[{"$f":"IF(OR(C1413=\"REAL\",C1413=\"DWORD\",C1413=\"DINT\"),(IF(OR(C1415=\"REAL\",C1415=\"DWORD\",C1415=\"DINT\"),A1413+4+MOD(A1413,4),A1413+4)),(IF(OR(C1415=\"REAL\",C1415=\"DWORD\",C1415=\"DINT\"),A1413+4+MOD(A1413,4),A1413+2)))&\".0\"","v":"836.0"},{"$f":"IF((IF(OR(C1415=\"INT\",C1415=\"WORD\",C1415=\"BOOL\"),MOD(A1415,2),MOD(A1415,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","02A01","设定温度值",{"$f":"D1415&F1415&\"-\"&IF(E1415=\"R\",\"新云平台\"&G1415,G1415)","v":"风机盘管02A01-新云平台设定温度值"},{"$f":"E1415&VLOOKUP(D1415,list!$D$3:$F$501,2,FALSE)&F1415&\"_\"&VLOOKUP(G1415,list!$I$2:$K$502,2,FALSE)","v":"RFCU02A01_TSET"},{"$f":"I1415&\" \"&\"AT%M\"&A1415&\" \"&\":\"&C1415&\";\"&\" \"&\"(*\"&H1415&\"*)\"","v":"RFCU02A01_TSET AT%M836.0 :REAL; (*风机盘管02A01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1415,SEARCH(\"AT%\",J1415),,REPT(\" \",25-SEARCH(\"AT%\",J1415))),SEARCH(\":\",REPLACE(J1415,SEARCH(\"AT%\",J1415),,REPT(\" \",25-SEARCH(\"AT%\",J1415)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1415,SEARCH(\"AT%\",J1415),,REPT(\" \",25-SEARCH(\"AT%\",J1415))))))","v":"RFCU02A01_TSET          AT%M836.0      :REAL; (*风机盘管02A01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1415=\"REAL\",C1415=\"DWORD\",C1415=\"DINT\"),(IF(OR(C1416=\"REAL\",C1416=\"DWORD\",C1416=\"DINT\"),A1415+4+MOD(A1415,4),A1415+4)),(IF(OR(C1416=\"REAL\",C1416=\"DWORD\",C1416=\"DINT\"),A1415+4+MOD(A1415,4),A1415+2)))&\".0\"","v":"840.0"},"验证通过","INT","风机盘管","R",{"$f":"F1415","v":"02A01"},"季节模式","风机盘管02A01-新云平台季节模式",{"$f":"E1416&VLOOKUP(D1416,list!$D$3:$F$501,2,FALSE)&F1416&\"_\"&VLOOKUP(G1416,list!$I$2:$K$502,2,FALSE)","v":"RFCU02A01_SM"},"RFCU02A01_SM AT%M840.0 :INT; (*风机盘管02A01-新云平台季节模式*)","RFCU02A01_SM            AT%M840.0      :INT; (*风机盘管02A01-新云平台季节模式*)"]
[{"$f":"IF(OR(C1416=\"REAL\",C1416=\"DWORD\",C1416=\"DINT\"),(IF(OR(C1417=\"REAL\",C1417=\"DWORD\",C1417=\"DINT\"),A1416+4+MOD(A1416,4),A1416+4)),(IF(OR(C1417=\"REAL\",C1417=\"DWORD\",C1417=\"DINT\"),A1416+4+MOD(A1416,4),A1416+2)))&\".0\"","v":"842.0"},"验证通过","BOOL","风机盘管","R","02A01","程序控制","风机盘管02A01-新云平台程序控制",{"$f":"E1417&VLOOKUP(D1417,list!$D$3:$F$501,2,FALSE)&F1417&\"_\"&VLOOKUP(G1417,list!$I$2:$K$502,2,FALSE)","v":"RFCU02A01_PC"},"RFCU02A01_PC AT%M842.0 :BOOL; (*风机盘管02A01-新云平台程序控制*)","RFCU02A01_PC            AT%M842.0      :BOOL; (*风机盘管02A01-新云平台程序控制*)"]
["848.0","验证通过","REAL","风机盘管","L","02A01","设定温度值","风机盘管02A01-设定温度值",{"$f":"E1418&VLOOKUP(D1418,list!$D$3:$F$501,2,FALSE)&F1418&\"_\"&VLOOKUP(G1418,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_TSET"},"LFCU02A01_TSET AT%M848.0 :REAL; (*风机盘管02A01-设定温度值*)","LFCU02A01_TSET          AT%M848.0      :REAL; (*风机盘管02A01-设定温度值*)"]
["852.0","验证通过","INT","风机盘管","L","02A01","季节模式","风机盘管02A01-季节模式",{"$f":"E1419&VLOOKUP(D1419,list!$D$3:$F$501,2,FALSE)&F1419&\"_\"&VLOOKUP(G1419,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_SM"},"LFCU02A01_SM AT%M852.0 :INT; (*风机盘管02A01-季节模式*)","LFCU02A01_SM            AT%M852.0      :INT; (*风机盘管02A01-季节模式*)"]
["856.0","验证通过","REAL","风机盘管","L","02A01","温度换算值","风机盘管02A01-温度换算值",{"$f":"E1420&VLOOKUP(D1420,list!$D$3:$F$501,2,FALSE)&F1420&\"_\"&VLOOKUP(G1420,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_TS"},"LFCU02A01_TS AT%M856.0 :REAL; (*风机盘管02A01-温度换算值*)","LFCU02A01_TS            AT%M856.0      :REAL; (*风机盘管02A01-温度换算值*)"]
["860.0","验证通过","BOOL","风机盘管","L","02A01","电磁阀手动控制","风机盘管02A01-电磁阀手动控制",{"$f":"E1421&VLOOKUP(D1421,list!$D$3:$F$501,2,FALSE)&F1421&\"_\"&VLOOKUP(G1421,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_EVMC"},"LFCU02A01_EVMC AT%M860.0 :BOOL; (*风机盘管02A01-电磁阀手动控制*)","LFCU02A01_EVMC          AT%M860.0      :BOOL; (*风机盘管02A01-电磁阀手动控制*)"]
["862.0","验证通过","BOOL","风机盘管","L","02A01","电磁阀手动控制值","风机盘管02A01-电磁阀手动控制值",{"$f":"E1422&VLOOKUP(D1422,list!$D$3:$F$501,2,FALSE)&F1422&\"_\"&VLOOKUP(G1422,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_EVMV"},"LFCU02A01_EVMV AT%M862.0 :BOOL; (*风机盘管02A01-电磁阀手动控制值*)","LFCU02A01_EVMV          AT%M862.0      :BOOL; (*风机盘管02A01-电磁阀手动控制值*)"]
["868.0","验证通过","REAL","风机盘管","L","02A01","回风温度换算值","风机盘管02A01-回风温度换算值",{"$f":"E1423&VLOOKUP(D1423,list!$D$3:$F$501,2,FALSE)&F1423&\"_\"&VLOOKUP(G1423,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_RTS"},"LFCU02A01_RTS AT%M868.0 :REAL; (*风机盘管02A01-回风温度换算值*)","LFCU02A01_RTS           AT%M868.0      :REAL; (*风机盘管02A01-回风温度换算值*)"]
["872.0","验证通过","BOOL","风机盘管","L","02A01","运行时间累积重置","风机盘管02A01-运行时间累积重置",{"$f":"E1424&VLOOKUP(D1424,list!$D$3:$F$501,2,FALSE)&F1424&\"_\"&VLOOKUP(G1424,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_RST"},"LFCU02A01_RST AT%M872.0 :BOOL; (*风机盘管02A01-运行时间累积重置*)","LFCU02A01_RST           AT%M872.0      :BOOL; (*风机盘管02A01-运行时间累积重置*)"]
["876.0","验证通过","REAL","风机盘管","L","02A01","运行时间累积重置值","风机盘管02A01-运行时间累积重置值",{"$f":"E1425&VLOOKUP(D1425,list!$D$3:$F$501,2,FALSE)&F1425&\"_\"&VLOOKUP(G1425,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_RSTV"},"LFCU02A01_RSTV AT%M876.0 :REAL; (*风机盘管02A01-运行时间累积重置值*)","LFCU02A01_RSTV          AT%M876.0      :REAL; (*风机盘管02A01-运行时间累积重置值*)"]
["880.0","验证通过","BOOL","风机盘管","L","02A01","隔离开关1","风机盘管02A01-隔离开关1",{"$f":"E1426&VLOOKUP(D1426,list!$D$3:$F$501,2,FALSE)&F1426&\"_\"&VLOOKUP(G1426,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_ISO1"},"LFCU02A01_ISO1 AT%M880.0 :BOOL; (*风机盘管02A01-隔离开关1*)","LFCU02A01_ISO1          AT%M880.0      :BOOL; (*风机盘管02A01-隔离开关1*)"]
["884.0","验证通过","REAL","风机盘管","L","02A01","运行时间累积值","风机盘管02A01-运行时间累积值",{"$f":"E1427&VLOOKUP(D1427,list!$D$3:$F$501,2,FALSE)&F1427&\"_\"&VLOOKUP(G1427,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_RH"},"LFCU02A01_RH AT%M884.0 :REAL; (*风机盘管02A01-运行时间累积值*)","LFCU02A01_RH            AT%M884.0      :REAL; (*风机盘管02A01-运行时间累积值*)"]
["888.0","验证通过","INT","风机盘管","L","02A01","设备状态代码","风机盘管02A01-设备状态代码",{"$f":"E1428&VLOOKUP(D1428,list!$D$3:$F$501,2,FALSE)&F1428&\"_\"&VLOOKUP(G1428,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_SN"},"LFCU02A01_SN AT%M888.0 :INT; (*风机盘管02A01-设备状态代码*)","LFCU02A01_SN            AT%M888.0      :INT; (*风机盘管02A01-设备状态代码*)"]
["890.0","验证通过","INT","风机盘管","L","02A01","水阀控制转换值","风机盘管02A01-水阀控制转换值",{"$f":"E1429&VLOOKUP(D1429,list!$D$3:$F$501,2,FALSE)&F1429&\"_\"&VLOOKUP(G1429,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_WVCS"},"LFCU02A01_WVCS AT%M890.0 :INT; (*风机盘管02A01-水阀控制转换值*)","LFCU02A01_WVCS          AT%M890.0      :INT; (*风机盘管02A01-水阀控制转换值*)"]
["892.0","验证通过","BOOL","风机盘管","L","02A01","程序控制","风机盘管02A01-程序控制",{"$f":"E1430&VLOOKUP(D1430,list!$D$3:$F$501,2,FALSE)&F1430&\"_\"&VLOOKUP(G1430,list!$I$2:$K$502,2,FALSE)","v":"LFCU02A01_PC"},"LFCU02A01_PC AT%M892.0 :BOOL; (*风机盘管02A01-程序控制*)","LFCU02A01_PC            AT%M892.0      :BOOL; (*风机盘管02A01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1430=\"REAL\",C1430=\"DWORD\",C1430=\"DINT\"),(IF(OR(C1432=\"REAL\",C1432=\"DWORD\",C1432=\"DINT\"),A1430+4+MOD(A1430,4),A1430+4)),(IF(OR(C1432=\"REAL\",C1432=\"DWORD\",C1432=\"DINT\"),A1430+4+MOD(A1430,4),A1430+2)))&\".0\"","v":"896.0"},{"$f":"IF((IF(OR(C1432=\"INT\",C1432=\"WORD\",C1432=\"BOOL\"),MOD(A1432,2),MOD(A1432,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03A01","设定温度值",{"$f":"D1432&F1432&\"-\"&IF(E1432=\"R\",\"新云平台\"&G1432,G1432)","v":"空调机组03A01-新云平台设定温度值"},{"$f":"E1432&VLOOKUP(D1432,list!$D$3:$F$501,2,FALSE)&F1432&\"_\"&VLOOKUP(G1432,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A01_TSET"},{"$f":"I1432&\" \"&\"AT%M\"&A1432&\" \"&\":\"&C1432&\";\"&\" \"&\"(*\"&H1432&\"*)\"","v":"RAHU03A01_TSET AT%M896.0 :REAL; (*空调机组03A01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1432,SEARCH(\"AT%\",J1432),,REPT(\" \",25-SEARCH(\"AT%\",J1432))),SEARCH(\":\",REPLACE(J1432,SEARCH(\"AT%\",J1432),,REPT(\" \",25-SEARCH(\"AT%\",J1432)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1432,SEARCH(\"AT%\",J1432),,REPT(\" \",25-SEARCH(\"AT%\",J1432))))))","v":"RAHU03A01_TSET          AT%M896.0      :REAL; (*空调机组03A01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1432=\"REAL\",C1432=\"DWORD\",C1432=\"DINT\"),(IF(OR(C1433=\"REAL\",C1433=\"DWORD\",C1433=\"DINT\"),A1432+4+MOD(A1432,4),A1432+4)),(IF(OR(C1433=\"REAL\",C1433=\"DWORD\",C1433=\"DINT\"),A1432+4+MOD(A1432,4),A1432+2)))&\".0\"","v":"900.0"},"验证通过","INT","空调机组","R",{"$f":"F1432","v":"03A01"},"季节模式","空调机组03A01-新云平台季节模式",{"$f":"E1433&VLOOKUP(D1433,list!$D$3:$F$501,2,FALSE)&F1433&\"_\"&VLOOKUP(G1433,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A01_SM"},"RAHU03A01_SM AT%M900.0 :INT; (*空调机组03A01-新云平台季节模式*)","RAHU03A01_SM            AT%M900.0      :INT; (*空调机组03A01-新云平台季节模式*)"]
[{"$f":"IF(OR(C1433=\"REAL\",C1433=\"DWORD\",C1433=\"DINT\"),(IF(OR(C1434=\"REAL\",C1434=\"DWORD\",C1434=\"DINT\"),A1433+4+MOD(A1433,4),A1433+4)),(IF(OR(C1434=\"REAL\",C1434=\"DWORD\",C1434=\"DINT\"),A1433+4+MOD(A1433,4),A1433+2)))&\".0\"","v":"902.0"},"验证通过","BOOL","空调机组","R",{"$f":"F1433","v":"03A01"},"程序控制","空调机组03A01-新云平台程序控制",{"$f":"E1434&VLOOKUP(D1434,list!$D$3:$F$501,2,FALSE)&F1434&\"_\"&VLOOKUP(G1434,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A01_PC"},"RAHU03A01_PC AT%M902.0 :BOOL; (*空调机组03A01-新云平台程序控制*)","RAHU03A01_PC            AT%M902.0      :BOOL; (*空调机组03A01-新云平台程序控制*)"]
["908.0","验证通过","REAL","空调机组","L","03A01","设定温度值","空调机组03A01-设定温度值",{"$f":"E1435&VLOOKUP(D1435,list!$D$3:$F$501,2,FALSE)&F1435&\"_\"&VLOOKUP(G1435,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_TSET"},"LAHU03A01_TSET AT%M908.0 :REAL; (*空调机组03A01-设定温度值*)","LAHU03A01_TSET          AT%M908.0      :REAL; (*空调机组03A01-设定温度值*)"]
["912.0","验证通过","INT","空调机组","L","03A01","季节模式","空调机组03A01-季节模式",{"$f":"E1436&VLOOKUP(D1436,list!$D$3:$F$501,2,FALSE)&F1436&\"_\"&VLOOKUP(G1436,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_SM"},"LAHU03A01_SM AT%M912.0 :INT; (*空调机组03A01-季节模式*)","LAHU03A01_SM            AT%M912.0      :INT; (*空调机组03A01-季节模式*)"]
["916.0","验证通过","REAL","空调机组","L","03A01","水阀反馈换算值","空调机组03A01-水阀反馈换算值",{"$f":"E1437&VLOOKUP(D1437,list!$D$3:$F$501,2,FALSE)&F1437&\"_\"&VLOOKUP(G1437,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_WVBS"},"LAHU03A01_WVBS AT%M916.0 :REAL; (*空调机组03A01-水阀反馈换算值*)","LAHU03A01_WVBS          AT%M916.0      :REAL; (*空调机组03A01-水阀反馈换算值*)"]
["920.0","验证通过","BOOL","空调机组","L","03A01","水阀手动控制","空调机组03A01-水阀手动控制",{"$f":"E1438&VLOOKUP(D1438,list!$D$3:$F$501,2,FALSE)&F1438&\"_\"&VLOOKUP(G1438,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_WVMC"},"LAHU03A01_WVMC AT%M920.0 :BOOL; (*空调机组03A01-水阀手动控制*)","LAHU03A01_WVMC          AT%M920.0      :BOOL; (*空调机组03A01-水阀手动控制*)"]
["924.0","验证通过","REAL","空调机组","L","03A01","水阀手动控制值","空调机组03A01-水阀手动控制值",{"$f":"E1439&VLOOKUP(D1439,list!$D$3:$F$501,2,FALSE)&F1439&\"_\"&VLOOKUP(G1439,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_WVMV"},"LAHU03A01_WVMV AT%M924.0 :REAL; (*空调机组03A01-水阀手动控制值*)","LAHU03A01_WVMV          AT%M924.0      :REAL; (*空调机组03A01-水阀手动控制值*)"]
["928.0","验证通过","REAL","空调机组","L","03A01","回风温度换算值","空调机组03A01-回风温度换算值",{"$f":"E1440&VLOOKUP(D1440,list!$D$3:$F$501,2,FALSE)&F1440&\"_\"&VLOOKUP(G1440,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_RTS"},"LAHU03A01_RTS AT%M928.0 :REAL; (*空调机组03A01-回风温度换算值*)","LAHU03A01_RTS           AT%M928.0      :REAL; (*空调机组03A01-回风温度换算值*)"]
["932.0","验证通过","BOOL","空调机组","L","03A01","运行时间累积重置","空调机组03A01-运行时间累积重置",{"$f":"E1441&VLOOKUP(D1441,list!$D$3:$F$501,2,FALSE)&F1441&\"_\"&VLOOKUP(G1441,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_RST"},"LAHU03A01_RST AT%M932.0 :BOOL; (*空调机组03A01-运行时间累积重置*)","LAHU03A01_RST           AT%M932.0      :BOOL; (*空调机组03A01-运行时间累积重置*)"]
["936.0","验证通过","REAL","空调机组","L","03A01","运行时间累积重置值","空调机组03A01-运行时间累积重置值",{"$f":"E1442&VLOOKUP(D1442,list!$D$3:$F$501,2,FALSE)&F1442&\"_\"&VLOOKUP(G1442,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_RSTV"},"LAHU03A01_RSTV AT%M936.0 :REAL; (*空调机组03A01-运行时间累积重置值*)","LAHU03A01_RSTV          AT%M936.0      :REAL; (*空调机组03A01-运行时间累积重置值*)"]
["940.0","验证通过","BOOL","空调机组","L","03A01","隔离开关1","空调机组03A01-隔离开关1",{"$f":"E1443&VLOOKUP(D1443,list!$D$3:$F$501,2,FALSE)&F1443&\"_\"&VLOOKUP(G1443,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_ISO1"},"LAHU03A01_ISO1 AT%M940.0 :BOOL; (*空调机组03A01-隔离开关1*)","LAHU03A01_ISO1          AT%M940.0      :BOOL; (*空调机组03A01-隔离开关1*)"]
["942.0","验证通过","BOOL","空调机组","L","03A01","隔离开关2","空调机组03A01-隔离开关2",{"$f":"E1444&VLOOKUP(D1444,list!$D$3:$F$501,2,FALSE)&F1444&\"_\"&VLOOKUP(G1444,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_ISO2"},"LAHU03A01_ISO2 AT%M942.0 :BOOL; (*空调机组03A01-隔离开关2*)","LAHU03A01_ISO2          AT%M942.0      :BOOL; (*空调机组03A01-隔离开关2*)"]
["948.0","验证通过","REAL","空调机组","L","03A01","P调节参数","空调机组03A01-P调节参数",{"$f":"E1445&VLOOKUP(D1445,list!$D$3:$F$501,2,FALSE)&F1445&\"_\"&VLOOKUP(G1445,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_VP"},"LAHU03A01_VP AT%M948.0 :REAL; (*空调机组03A01-P调节参数*)","LAHU03A01_VP            AT%M948.0      :REAL; (*空调机组03A01-P调节参数*)"]
["952.0","验证通过","REAL","空调机组","L","03A01","I调节参数","空调机组03A01-I调节参数",{"$f":"E1446&VLOOKUP(D1446,list!$D$3:$F$501,2,FALSE)&F1446&\"_\"&VLOOKUP(G1446,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_VI"},"LAHU03A01_VI AT%M952.0 :REAL; (*空调机组03A01-I调节参数*)","LAHU03A01_VI            AT%M952.0      :REAL; (*空调机组03A01-I调节参数*)"]
["956.0","验证通过","REAL","空调机组","L","03A01","运行时间累积值","空调机组03A01-运行时间累积值",{"$f":"E1447&VLOOKUP(D1447,list!$D$3:$F$501,2,FALSE)&F1447&\"_\"&VLOOKUP(G1447,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_RH"},"LAHU03A01_RH AT%M956.0 :REAL; (*空调机组03A01-运行时间累积值*)","LAHU03A01_RH            AT%M956.0      :REAL; (*空调机组03A01-运行时间累积值*)"]
["960.0","验证通过","INT","空调机组","L","03A01","设备状态代码","空调机组03A01-设备状态代码",{"$f":"E1448&VLOOKUP(D1448,list!$D$3:$F$501,2,FALSE)&F1448&\"_\"&VLOOKUP(G1448,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_SN"},"LAHU03A01_SN AT%M960.0 :INT; (*空调机组03A01-设备状态代码*)","LAHU03A01_SN            AT%M960.0      :INT; (*空调机组03A01-设备状态代码*)"]
["962.0","验证通过","INT","空调机组","L","03A01","水阀控制转换值","空调机组03A01-水阀控制转换值",{"$f":"E1449&VLOOKUP(D1449,list!$D$3:$F$501,2,FALSE)&F1449&\"_\"&VLOOKUP(G1449,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_WVCS"},"LAHU03A01_WVCS AT%M962.0 :INT; (*空调机组03A01-水阀控制转换值*)","LAHU03A01_WVCS          AT%M962.0      :INT; (*空调机组03A01-水阀控制转换值*)"]
["964.0","验证通过","BOOL","空调机组","L","03A01","程序控制","空调机组03A01-程序控制",{"$f":"E1450&VLOOKUP(D1450,list!$D$3:$F$501,2,FALSE)&F1450&\"_\"&VLOOKUP(G1450,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A01_PC"},"LAHU03A01_PC AT%M964.0 :BOOL; (*空调机组03A01-程序控制*)","LAHU03A01_PC            AT%M964.0      :BOOL; (*空调机组03A01-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1450=\"REAL\",C1450=\"DWORD\",C1450=\"DINT\"),(IF(OR(C1452=\"REAL\",C1452=\"DWORD\",C1452=\"DINT\"),A1450+4+MOD(A1450,4),A1450+4)),(IF(OR(C1452=\"REAL\",C1452=\"DWORD\",C1452=\"DINT\"),A1450+4+MOD(A1450,4),A1450+2)))&\".0\"","v":"968.0"},{"$f":"IF((IF(OR(C1452=\"INT\",C1452=\"WORD\",C1452=\"BOOL\"),MOD(A1452,2),MOD(A1452,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03A02","设定温度值",{"$f":"D1452&F1452&\"-\"&IF(E1452=\"R\",\"新云平台\"&G1452,G1452)","v":"空调机组03A02-新云平台设定温度值"},{"$f":"E1452&VLOOKUP(D1452,list!$D$3:$F$501,2,FALSE)&F1452&\"_\"&VLOOKUP(G1452,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A02_TSET"},{"$f":"I1452&\" \"&\"AT%M\"&A1452&\" \"&\":\"&C1452&\";\"&\" \"&\"(*\"&H1452&\"*)\"","v":"RAHU03A02_TSET AT%M968.0 :REAL; (*空调机组03A02-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1452,SEARCH(\"AT%\",J1452),,REPT(\" \",25-SEARCH(\"AT%\",J1452))),SEARCH(\":\",REPLACE(J1452,SEARCH(\"AT%\",J1452),,REPT(\" \",25-SEARCH(\"AT%\",J1452)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1452,SEARCH(\"AT%\",J1452),,REPT(\" \",25-SEARCH(\"AT%\",J1452))))))","v":"RAHU03A02_TSET          AT%M968.0      :REAL; (*空调机组03A02-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1452=\"REAL\",C1452=\"DWORD\",C1452=\"DINT\"),(IF(OR(C1453=\"REAL\",C1453=\"DWORD\",C1453=\"DINT\"),A1452+4+MOD(A1452,4),A1452+4)),(IF(OR(C1453=\"REAL\",C1453=\"DWORD\",C1453=\"DINT\"),A1452+4+MOD(A1452,4),A1452+2)))&\".0\"","v":"972.0"},"验证通过","INT","空调机组","R",{"$f":"F1452","v":"03A02"},"季节模式","空调机组03A02-新云平台季节模式",{"$f":"E1453&VLOOKUP(D1453,list!$D$3:$F$501,2,FALSE)&F1453&\"_\"&VLOOKUP(G1453,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A02_SM"},"RAHU03A02_SM AT%M972.0 :INT; (*空调机组03A02-新云平台季节模式*)","RAHU03A02_SM            AT%M972.0      :INT; (*空调机组03A02-新云平台季节模式*)"]
[{"$f":"IF(OR(C1453=\"REAL\",C1453=\"DWORD\",C1453=\"DINT\"),(IF(OR(C1454=\"REAL\",C1454=\"DWORD\",C1454=\"DINT\"),A1453+4+MOD(A1453,4),A1453+4)),(IF(OR(C1454=\"REAL\",C1454=\"DWORD\",C1454=\"DINT\"),A1453+4+MOD(A1453,4),A1453+2)))&\".0\"","v":"974.0"},"验证通过","BOOL","空调机组","R",{"$f":"F1453","v":"03A02"},"程序控制","空调机组03A02-新云平台程序控制",{"$f":"E1454&VLOOKUP(D1454,list!$D$3:$F$501,2,FALSE)&F1454&\"_\"&VLOOKUP(G1454,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A02_PC"},"RAHU03A02_PC AT%M974.0 :BOOL; (*空调机组03A02-新云平台程序控制*)","RAHU03A02_PC            AT%M974.0      :BOOL; (*空调机组03A02-新云平台程序控制*)"]
["980.0","验证通过","REAL","空调机组","L","03A02","设定温度值","空调机组03A02-设定温度值",{"$f":"E1455&VLOOKUP(D1455,list!$D$3:$F$501,2,FALSE)&F1455&\"_\"&VLOOKUP(G1455,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_TSET"},"LAHU03A02_TSET AT%M980.0 :REAL; (*空调机组03A02-设定温度值*)","LAHU03A02_TSET          AT%M980.0      :REAL; (*空调机组03A02-设定温度值*)"]
["984.0","验证通过","INT","空调机组","L","03A02","季节模式","空调机组03A02-季节模式",{"$f":"E1456&VLOOKUP(D1456,list!$D$3:$F$501,2,FALSE)&F1456&\"_\"&VLOOKUP(G1456,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_SM"},"LAHU03A02_SM AT%M984.0 :INT; (*空调机组03A02-季节模式*)","LAHU03A02_SM            AT%M984.0      :INT; (*空调机组03A02-季节模式*)"]
["988.0","验证通过","REAL","空调机组","L","03A02","水阀反馈换算值","空调机组03A02-水阀反馈换算值",{"$f":"E1457&VLOOKUP(D1457,list!$D$3:$F$501,2,FALSE)&F1457&\"_\"&VLOOKUP(G1457,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_WVBS"},"LAHU03A02_WVBS AT%M988.0 :REAL; (*空调机组03A02-水阀反馈换算值*)","LAHU03A02_WVBS          AT%M988.0      :REAL; (*空调机组03A02-水阀反馈换算值*)"]
["992.0","验证通过","BOOL","空调机组","L","03A02","水阀手动控制","空调机组03A02-水阀手动控制",{"$f":"E1458&VLOOKUP(D1458,list!$D$3:$F$501,2,FALSE)&F1458&\"_\"&VLOOKUP(G1458,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_WVMC"},"LAHU03A02_WVMC AT%M992.0 :BOOL; (*空调机组03A02-水阀手动控制*)","LAHU03A02_WVMC          AT%M992.0      :BOOL; (*空调机组03A02-水阀手动控制*)"]
["996.0","验证通过","REAL","空调机组","L","03A02","水阀手动控制值","空调机组03A02-水阀手动控制值",{"$f":"E1459&VLOOKUP(D1459,list!$D$3:$F$501,2,FALSE)&F1459&\"_\"&VLOOKUP(G1459,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_WVMV"},"LAHU03A02_WVMV AT%M996.0 :REAL; (*空调机组03A02-水阀手动控制值*)","LAHU03A02_WVMV          AT%M996.0      :REAL; (*空调机组03A02-水阀手动控制值*)"]
["1000.0","验证通过","REAL","空调机组","L","03A02","回风温度换算值","空调机组03A02-回风温度换算值",{"$f":"E1460&VLOOKUP(D1460,list!$D$3:$F$501,2,FALSE)&F1460&\"_\"&VLOOKUP(G1460,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_RTS"},"LAHU03A02_RTS AT%M1000.0 :REAL; (*空调机组03A02-回风温度换算值*)","LAHU03A02_RTS           AT%M1000.0     :REAL; (*空调机组03A02-回风温度换算值*)"]
["1004.0","验证通过","BOOL","空调机组","L","03A02","运行时间累积重置","空调机组03A02-运行时间累积重置",{"$f":"E1461&VLOOKUP(D1461,list!$D$3:$F$501,2,FALSE)&F1461&\"_\"&VLOOKUP(G1461,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_RST"},"LAHU03A02_RST AT%M1004.0 :BOOL; (*空调机组03A02-运行时间累积重置*)","LAHU03A02_RST           AT%M1004.0     :BOOL; (*空调机组03A02-运行时间累积重置*)"]
["1008.0","验证通过","REAL","空调机组","L","03A02","运行时间累积重置值","空调机组03A02-运行时间累积重置值",{"$f":"E1462&VLOOKUP(D1462,list!$D$3:$F$501,2,FALSE)&F1462&\"_\"&VLOOKUP(G1462,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_RSTV"},"LAHU03A02_RSTV AT%M1008.0 :REAL; (*空调机组03A02-运行时间累积重置值*)","LAHU03A02_RSTV          AT%M1008.0     :REAL; (*空调机组03A02-运行时间累积重置值*)"]
["1012.0","验证通过","BOOL","空调机组","L","03A02","隔离开关1","空调机组03A02-隔离开关1",{"$f":"E1463&VLOOKUP(D1463,list!$D$3:$F$501,2,FALSE)&F1463&\"_\"&VLOOKUP(G1463,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_ISO1"},"LAHU03A02_ISO1 AT%M1012.0 :BOOL; (*空调机组03A02-隔离开关1*)","LAHU03A02_ISO1          AT%M1012.0     :BOOL; (*空调机组03A02-隔离开关1*)"]
["1014.0","验证通过","BOOL","空调机组","L","03A02","隔离开关2","空调机组03A02-隔离开关2",{"$f":"E1464&VLOOKUP(D1464,list!$D$3:$F$501,2,FALSE)&F1464&\"_\"&VLOOKUP(G1464,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_ISO2"},"LAHU03A02_ISO2 AT%M1014.0 :BOOL; (*空调机组03A02-隔离开关2*)","LAHU03A02_ISO2          AT%M1014.0     :BOOL; (*空调机组03A02-隔离开关2*)"]
["1020.0","验证通过","REAL","空调机组","L","03A02","P调节参数","空调机组03A02-P调节参数",{"$f":"E1465&VLOOKUP(D1465,list!$D$3:$F$501,2,FALSE)&F1465&\"_\"&VLOOKUP(G1465,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_VP"},"LAHU03A02_VP AT%M1020.0 :REAL; (*空调机组03A02-P调节参数*)","LAHU03A02_VP            AT%M1020.0     :REAL; (*空调机组03A02-P调节参数*)"]
["1024.0","验证通过","REAL","空调机组","L","03A02","I调节参数","空调机组03A02-I调节参数",{"$f":"E1466&VLOOKUP(D1466,list!$D$3:$F$501,2,FALSE)&F1466&\"_\"&VLOOKUP(G1466,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_VI"},"LAHU03A02_VI AT%M1024.0 :REAL; (*空调机组03A02-I调节参数*)","LAHU03A02_VI            AT%M1024.0     :REAL; (*空调机组03A02-I调节参数*)"]
["1028.0","验证通过","REAL","空调机组","L","03A02","运行时间累积值","空调机组03A02-运行时间累积值",{"$f":"E1467&VLOOKUP(D1467,list!$D$3:$F$501,2,FALSE)&F1467&\"_\"&VLOOKUP(G1467,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_RH"},"LAHU03A02_RH AT%M1028.0 :REAL; (*空调机组03A02-运行时间累积值*)","LAHU03A02_RH            AT%M1028.0     :REAL; (*空调机组03A02-运行时间累积值*)"]
["1032.0","验证通过","INT","空调机组","L","03A02","设备状态代码","空调机组03A02-设备状态代码",{"$f":"E1468&VLOOKUP(D1468,list!$D$3:$F$501,2,FALSE)&F1468&\"_\"&VLOOKUP(G1468,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_SN"},"LAHU03A02_SN AT%M1032.0 :INT; (*空调机组03A02-设备状态代码*)","LAHU03A02_SN            AT%M1032.0     :INT; (*空调机组03A02-设备状态代码*)"]
["1034.0","验证通过","INT","空调机组","L","03A02","水阀控制转换值","空调机组03A02-水阀控制转换值",{"$f":"E1469&VLOOKUP(D1469,list!$D$3:$F$501,2,FALSE)&F1469&\"_\"&VLOOKUP(G1469,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_WVCS"},"LAHU03A02_WVCS AT%M1034.0 :INT; (*空调机组03A02-水阀控制转换值*)","LAHU03A02_WVCS          AT%M1034.0     :INT; (*空调机组03A02-水阀控制转换值*)"]
["1036.0","验证通过","BOOL","空调机组","L","03A02","程序控制","空调机组03A02-程序控制",{"$f":"E1470&VLOOKUP(D1470,list!$D$3:$F$501,2,FALSE)&F1470&\"_\"&VLOOKUP(G1470,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A02_PC"},"LAHU03A02_PC AT%M1036.0 :BOOL; (*空调机组03A02-程序控制*)","LAHU03A02_PC            AT%M1036.0     :BOOL; (*空调机组03A02-程序控制*)"]
["AHU"]
[{"$f":"IF(OR(C1470=\"REAL\",C1470=\"DWORD\",C1470=\"DINT\"),(IF(OR(C1472=\"REAL\",C1472=\"DWORD\",C1472=\"DINT\"),A1470+4+MOD(A1470,4),A1470+4)),(IF(OR(C1472=\"REAL\",C1472=\"DWORD\",C1472=\"DINT\"),A1470+4+MOD(A1470,4),A1470+2)))&\".0\"","v":"1040.0"},{"$f":"IF((IF(OR(C1472=\"INT\",C1472=\"WORD\",C1472=\"BOOL\"),MOD(A1472,2),MOD(A1472,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","空调机组","R","03A03","设定温度值",{"$f":"D1472&F1472&\"-\"&IF(E1472=\"R\",\"新云平台\"&G1472,G1472)","v":"空调机组03A03-新云平台设定温度值"},{"$f":"E1472&VLOOKUP(D1472,list!$D$3:$F$501,2,FALSE)&F1472&\"_\"&VLOOKUP(G1472,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A03_TSET"},{"$f":"I1472&\" \"&\"AT%M\"&A1472&\" \"&\":\"&C1472&\";\"&\" \"&\"(*\"&H1472&\"*)\"","v":"RAHU03A03_TSET AT%M1040.0 :REAL; (*空调机组03A03-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1472,SEARCH(\"AT%\",J1472),,REPT(\" \",25-SEARCH(\"AT%\",J1472))),SEARCH(\":\",REPLACE(J1472,SEARCH(\"AT%\",J1472),,REPT(\" \",25-SEARCH(\"AT%\",J1472)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1472,SEARCH(\"AT%\",J1472),,REPT(\" \",25-SEARCH(\"AT%\",J1472))))))","v":"RAHU03A03_TSET          AT%M1040.0     :REAL; (*空调机组03A03-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1472=\"REAL\",C1472=\"DWORD\",C1472=\"DINT\"),(IF(OR(C1473=\"REAL\",C1473=\"DWORD\",C1473=\"DINT\"),A1472+4+MOD(A1472,4),A1472+4)),(IF(OR(C1473=\"REAL\",C1473=\"DWORD\",C1473=\"DINT\"),A1472+4+MOD(A1472,4),A1472+2)))&\".0\"","v":"1044.0"},"验证通过","INT","空调机组","R",{"$f":"F1472","v":"03A03"},"季节模式","空调机组03A03-新云平台季节模式",{"$f":"E1473&VLOOKUP(D1473,list!$D$3:$F$501,2,FALSE)&F1473&\"_\"&VLOOKUP(G1473,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A03_SM"},"RAHU03A03_SM AT%M1044.0 :INT; (*空调机组03A03-新云平台季节模式*)","RAHU03A03_SM            AT%M1044.0     :INT; (*空调机组03A03-新云平台季节模式*)"]
[{"$f":"IF(OR(C1473=\"REAL\",C1473=\"DWORD\",C1473=\"DINT\"),(IF(OR(C1474=\"REAL\",C1474=\"DWORD\",C1474=\"DINT\"),A1473+4+MOD(A1473,4),A1473+4)),(IF(OR(C1474=\"REAL\",C1474=\"DWORD\",C1474=\"DINT\"),A1473+4+MOD(A1473,4),A1473+2)))&\".0\"","v":"1046.0"},"验证通过","BOOL","空调机组","R",{"$f":"F1473","v":"03A03"},"程序控制","空调机组03A03-新云平台程序控制",{"$f":"E1474&VLOOKUP(D1474,list!$D$3:$F$501,2,FALSE)&F1474&\"_\"&VLOOKUP(G1474,list!$I$2:$K$502,2,FALSE)","v":"RAHU03A03_PC"},"RAHU03A03_PC AT%M1046.0 :BOOL; (*空调机组03A03-新云平台程序控制*)","RAHU03A03_PC            AT%M1046.0     :BOOL; (*空调机组03A03-新云平台程序控制*)"]
["1052.0","验证通过","REAL","空调机组","L","03A03","设定温度值","空调机组03A03-设定温度值",{"$f":"E1475&VLOOKUP(D1475,list!$D$3:$F$501,2,FALSE)&F1475&\"_\"&VLOOKUP(G1475,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_TSET"},"LAHU03A03_TSET AT%M1052.0 :REAL; (*空调机组03A03-设定温度值*)","LAHU03A03_TSET          AT%M1052.0     :REAL; (*空调机组03A03-设定温度值*)"]
["1056.0","验证通过","INT","空调机组","L","03A03","季节模式","空调机组03A03-季节模式",{"$f":"E1476&VLOOKUP(D1476,list!$D$3:$F$501,2,FALSE)&F1476&\"_\"&VLOOKUP(G1476,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_SM"},"LAHU03A03_SM AT%M1056.0 :INT; (*空调机组03A03-季节模式*)","LAHU03A03_SM            AT%M1056.0     :INT; (*空调机组03A03-季节模式*)"]
["1060.0","验证通过","REAL","空调机组","L","03A03","水阀反馈换算值","空调机组03A03-水阀反馈换算值",{"$f":"E1477&VLOOKUP(D1477,list!$D$3:$F$501,2,FALSE)&F1477&\"_\"&VLOOKUP(G1477,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_WVBS"},"LAHU03A03_WVBS AT%M1060.0 :REAL; (*空调机组03A03-水阀反馈换算值*)","LAHU03A03_WVBS          AT%M1060.0     :REAL; (*空调机组03A03-水阀反馈换算值*)"]
["1064.0","验证通过","BOOL","空调机组","L","03A03","水阀手动控制","空调机组03A03-水阀手动控制",{"$f":"E1478&VLOOKUP(D1478,list!$D$3:$F$501,2,FALSE)&F1478&\"_\"&VLOOKUP(G1478,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_WVMC"},"LAHU03A03_WVMC AT%M1064.0 :BOOL; (*空调机组03A03-水阀手动控制*)","LAHU03A03_WVMC          AT%M1064.0     :BOOL; (*空调机组03A03-水阀手动控制*)"]
["1068.0","验证通过","REAL","空调机组","L","03A03","水阀手动控制值","空调机组03A03-水阀手动控制值",{"$f":"E1479&VLOOKUP(D1479,list!$D$3:$F$501,2,FALSE)&F1479&\"_\"&VLOOKUP(G1479,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_WVMV"},"LAHU03A03_WVMV AT%M1068.0 :REAL; (*空调机组03A03-水阀手动控制值*)","LAHU03A03_WVMV          AT%M1068.0     :REAL; (*空调机组03A03-水阀手动控制值*)"]
["1072.0","验证通过","REAL","空调机组","L","03A03","回风温度换算值","空调机组03A03-回风温度换算值",{"$f":"E1480&VLOOKUP(D1480,list!$D$3:$F$501,2,FALSE)&F1480&\"_\"&VLOOKUP(G1480,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_RTS"},"LAHU03A03_RTS AT%M1072.0 :REAL; (*空调机组03A03-回风温度换算值*)","LAHU03A03_RTS           AT%M1072.0     :REAL; (*空调机组03A03-回风温度换算值*)"]
["1076.0","验证通过","BOOL","空调机组","L","03A03","运行时间累积重置","空调机组03A03-运行时间累积重置",{"$f":"E1481&VLOOKUP(D1481,list!$D$3:$F$501,2,FALSE)&F1481&\"_\"&VLOOKUP(G1481,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_RST"},"LAHU03A03_RST AT%M1076.0 :BOOL; (*空调机组03A03-运行时间累积重置*)","LAHU03A03_RST           AT%M1076.0     :BOOL; (*空调机组03A03-运行时间累积重置*)"]
["1080.0","验证通过","REAL","空调机组","L","03A03","运行时间累积重置值","空调机组03A03-运行时间累积重置值",{"$f":"E1482&VLOOKUP(D1482,list!$D$3:$F$501,2,FALSE)&F1482&\"_\"&VLOOKUP(G1482,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_RSTV"},"LAHU03A03_RSTV AT%M1080.0 :REAL; (*空调机组03A03-运行时间累积重置值*)","LAHU03A03_RSTV          AT%M1080.0     :REAL; (*空调机组03A03-运行时间累积重置值*)"]
["1084.0","验证通过","BOOL","空调机组","L","03A03","隔离开关1","空调机组03A03-隔离开关1",{"$f":"E1483&VLOOKUP(D1483,list!$D$3:$F$501,2,FALSE)&F1483&\"_\"&VLOOKUP(G1483,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_ISO1"},"LAHU03A03_ISO1 AT%M1084.0 :BOOL; (*空调机组03A03-隔离开关1*)","LAHU03A03_ISO1          AT%M1084.0     :BOOL; (*空调机组03A03-隔离开关1*)"]
["1086.0","验证通过","BOOL","空调机组","L","03A03","隔离开关2","空调机组03A03-隔离开关2",{"$f":"E1484&VLOOKUP(D1484,list!$D$3:$F$501,2,FALSE)&F1484&\"_\"&VLOOKUP(G1484,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_ISO2"},"LAHU03A03_ISO2 AT%M1086.0 :BOOL; (*空调机组03A03-隔离开关2*)","LAHU03A03_ISO2          AT%M1086.0     :BOOL; (*空调机组03A03-隔离开关2*)"]
["1092.0","验证通过","REAL","空调机组","L","03A03","P调节参数","空调机组03A03-P调节参数",{"$f":"E1485&VLOOKUP(D1485,list!$D$3:$F$501,2,FALSE)&F1485&\"_\"&VLOOKUP(G1485,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_VP"},"LAHU03A03_VP AT%M1092.0 :REAL; (*空调机组03A03-P调节参数*)","LAHU03A03_VP            AT%M1092.0     :REAL; (*空调机组03A03-P调节参数*)"]
["1096.0","验证通过","REAL","空调机组","L","03A03","I调节参数","空调机组03A03-I调节参数",{"$f":"E1486&VLOOKUP(D1486,list!$D$3:$F$501,2,FALSE)&F1486&\"_\"&VLOOKUP(G1486,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_VI"},"LAHU03A03_VI AT%M1096.0 :REAL; (*空调机组03A03-I调节参数*)","LAHU03A03_VI            AT%M1096.0     :REAL; (*空调机组03A03-I调节参数*)"]
["1100.0","验证通过","REAL","空调机组","L","03A03","运行时间累积值","空调机组03A03-运行时间累积值",{"$f":"E1487&VLOOKUP(D1487,list!$D$3:$F$501,2,FALSE)&F1487&\"_\"&VLOOKUP(G1487,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_RH"},"LAHU03A03_RH AT%M1100.0 :REAL; (*空调机组03A03-运行时间累积值*)","LAHU03A03_RH            AT%M1100.0     :REAL; (*空调机组03A03-运行时间累积值*)"]
["1104.0","验证通过","INT","空调机组","L","03A03","设备状态代码","空调机组03A03-设备状态代码",{"$f":"E1488&VLOOKUP(D1488,list!$D$3:$F$501,2,FALSE)&F1488&\"_\"&VLOOKUP(G1488,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_SN"},"LAHU03A03_SN AT%M1104.0 :INT; (*空调机组03A03-设备状态代码*)","LAHU03A03_SN            AT%M1104.0     :INT; (*空调机组03A03-设备状态代码*)"]
["1106.0","验证通过","INT","空调机组","L","03A03","水阀控制转换值","空调机组03A03-水阀控制转换值",{"$f":"E1489&VLOOKUP(D1489,list!$D$3:$F$501,2,FALSE)&F1489&\"_\"&VLOOKUP(G1489,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_WVCS"},"LAHU03A03_WVCS AT%M1106.0 :INT; (*空调机组03A03-水阀控制转换值*)","LAHU03A03_WVCS          AT%M1106.0     :INT; (*空调机组03A03-水阀控制转换值*)"]
["1108.0","验证通过","BOOL","空调机组","L","03A03","程序控制","空调机组03A03-程序控制",{"$f":"E1490&VLOOKUP(D1490,list!$D$3:$F$501,2,FALSE)&F1490&\"_\"&VLOOKUP(G1490,list!$I$2:$K$502,2,FALSE)","v":"LAHU03A03_PC"},"LAHU03A03_PC AT%M1108.0 :BOOL; (*空调机组03A03-程序控制*)","LAHU03A03_PC            AT%M1108.0     :BOOL; (*空调机组03A03-程序控制*)"]
["FCU"]
[{"$f":"IF(OR(C1490=\"REAL\",C1490=\"DWORD\",C1490=\"DINT\"),(IF(OR(C1492=\"REAL\",C1492=\"DWORD\",C1492=\"DINT\"),A1490+4+MOD(A1490,4),A1490+4)),(IF(OR(C1492=\"REAL\",C1492=\"DWORD\",C1492=\"DINT\"),A1490+4+MOD(A1490,4),A1490+2)))&\".0\"","v":"1112.0"},{"$f":"IF((IF(OR(C1492=\"INT\",C1492=\"WORD\",C1492=\"BOOL\"),MOD(A1492,2),MOD(A1492,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","风机盘管","R","03A01","设定温度值",{"$f":"D1492&F1492&\"-\"&IF(E1492=\"R\",\"新云平台\"&G1492,G1492)","v":"风机盘管03A01-新云平台设定温度值"},{"$f":"E1492&VLOOKUP(D1492,list!$D$3:$F$501,2,FALSE)&F1492&\"_\"&VLOOKUP(G1492,list!$I$2:$K$502,2,FALSE)","v":"RFCU03A01_TSET"},{"$f":"I1492&\" \"&\"AT%M\"&A1492&\" \"&\":\"&C1492&\";\"&\" \"&\"(*\"&H1492&\"*)\"","v":"RFCU03A01_TSET AT%M1112.0 :REAL; (*风机盘管03A01-新云平台设定温度值*)"},{"$f":"REPLACE(REPLACE(J1492,SEARCH(\"AT%\",J1492),,REPT(\" \",25-SEARCH(\"AT%\",J1492))),SEARCH(\":\",REPLACE(J1492,SEARCH(\"AT%\",J1492),,REPT(\" \",25-SEARCH(\"AT%\",J1492)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J1492,SEARCH(\"AT%\",J1492),,REPT(\" \",25-SEARCH(\"AT%\",J1492))))))","v":"RFCU03A01_TSET          AT%M1112.0     :REAL; (*风机盘管03A01-新云平台设定温度值*)"}]
[{"$f":"IF(OR(C1492=\"REAL\",C1492=\"DWORD\",C1492=\"DINT\"),(IF(OR(C1493=\"REAL\",C1493=\"DWORD\",C1493=\"DINT\"),A1492+4+MOD(A1492,4),A1492+4)),(IF(OR(C1493=\"REAL\",C1493=\"DWORD\",C1493=\"DINT\"),A1492+4+MOD(A1492,4),A1492+2)))&\".0\"","v":"1116.0"},"验证通过","INT","风机盘管","R",{"$f":"F1492","v":"03A01"},"季节模式","风机盘管03A01-新云平台季节模式",{"$f":"E1493&VLOOKUP(D1493,list!$D$3:$F$501,2,FALSE)&F1493&\"_\"&VLOOKUP(G1493,list!$I$2:$K$502,2,FALSE)","v":"RFCU03A01_SM"},"RFCU03A01_SM AT%M1116.0 :INT; (*风机盘管03A01-新云平台季节模式*)","RFCU03A01_SM            AT%M1116.0     :INT; (*风机盘管03A01-新云平台季节模式*)"]
[{"$f":"IF(OR(C1493=\"REAL\",C1493=\"DWORD\",C1493=\"DINT\"),(IF(OR(C1494=\"REAL\",C1494=\"DWORD\",C1494=\"DINT\"),A1493+4+MOD(A1493,4),A1493+4)),(IF(OR(C1494=\"REAL\",C1494=\"DWORD\",C1494=\"DINT\"),A1493+4+MOD(A1493,4),A1493+2)))&\".0\"","v":"1118.0"},"验证通过","BOOL","风机盘管","R","03A01","程序控制","风机盘管03A01-新云平台程序控制",{"$f":"E1494&VLOOKUP(D1494,list!$D$3:$F$501,2,FALSE)&F1494&\"_\"&VLOOKUP(G1494,list!$I$2:$K$502,2,FALSE)","v":"RFCU03A01_PC"},"RFCU03A01_PC AT%M1118.0 :BOOL; (*风机盘管03A01-新云平台程序控制*)","RFCU03A01_PC            AT%M1118.0     :BOOL; (*风机盘管03A01-新云平台程序控制*)"]
["1124.0","验证通过","REAL","风机盘管","L","03A01","设定温度值","风机盘管03A01-设定温度值",{"$f":"E1495&VLOOKUP(D1495,list!$D$3:$F$501,2,FALSE)&F1495&\"_\"&VLOOKUP(G1495,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_TSET"},"LFCU03A01_TSET AT%M1124.0 :REAL; (*风机盘管03A01-设定温度值*)","LFCU03A01_TSET          AT%M1124.0     :REAL; (*风机盘管03A01-设定温度值*)"]
["1128.0","验证通过","INT","风机盘管","L","03A01","季节模式","风机盘管03A01-季节模式",{"$f":"E1496&VLOOKUP(D1496,list!$D$3:$F$501,2,FALSE)&F1496&\"_\"&VLOOKUP(G1496,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_SM"},"LFCU03A01_SM AT%M1128.0 :INT; (*风机盘管03A01-季节模式*)","LFCU03A01_SM            AT%M1128.0     :INT; (*风机盘管03A01-季节模式*)"]
["1132.0","验证通过","REAL","风机盘管","L","03A01","温度换算值","风机盘管03A01-温度换算值",{"$f":"E1497&VLOOKUP(D1497,list!$D$3:$F$501,2,FALSE)&F1497&\"_\"&VLOOKUP(G1497,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_TS"},"LFCU03A01_TS AT%M1132.0 :REAL; (*风机盘管03A01-温度换算值*)","LFCU03A01_TS            AT%M1132.0     :REAL; (*风机盘管03A01-温度换算值*)"]
["1136.0","验证通过","BOOL","风机盘管","L","03A01","电磁阀手动控制","风机盘管03A01-电磁阀手动控制",{"$f":"E1498&VLOOKUP(D1498,list!$D$3:$F$501,2,FALSE)&F1498&\"_\"&VLOOKUP(G1498,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_EVMC"},"LFCU03A01_EVMC AT%M1136.0 :BOOL; (*风机盘管03A01-电磁阀手动控制*)","LFCU03A01_EVMC          AT%M1136.0     :BOOL; (*风机盘管03A01-电磁阀手动控制*)"]
["1138.0","验证通过","BOOL","风机盘管","L","03A01","电磁阀手动控制值","风机盘管03A01-电磁阀手动控制值",{"$f":"E1499&VLOOKUP(D1499,list!$D$3:$F$501,2,FALSE)&F1499&\"_\"&VLOOKUP(G1499,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_EVMV"},"LFCU03A01_EVMV AT%M1138.0 :BOOL; (*风机盘管03A01-电磁阀手动控制值*)","LFCU03A01_EVMV          AT%M1138.0     :BOOL; (*风机盘管03A01-电磁阀手动控制值*)"]
["1144.0","验证通过","REAL","风机盘管","L","03A01","回风温度换算值","风机盘管03A01-回风温度换算值",{"$f":"E1500&VLOOKUP(D1500,list!$D$3:$F$501,2,FALSE)&F1500&\"_\"&VLOOKUP(G1500,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_RTS"},"LFCU03A01_RTS AT%M1144.0 :REAL; (*风机盘管03A01-回风温度换算值*)","LFCU03A01_RTS           AT%M1144.0     :REAL; (*风机盘管03A01-回风温度换算值*)"]
["1148.0","验证通过","BOOL","风机盘管","L","03A01","运行时间累积重置","风机盘管03A01-运行时间累积重置",{"$f":"E1501&VLOOKUP(D1501,list!$D$3:$F$501,2,FALSE)&F1501&\"_\"&VLOOKUP(G1501,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_RST"},"LFCU03A01_RST AT%M1148.0 :BOOL; (*风机盘管03A01-运行时间累积重置*)","LFCU03A01_RST           AT%M1148.0     :BOOL; (*风机盘管03A01-运行时间累积重置*)"]
["1152.0","验证通过","REAL","风机盘管","L","03A01","运行时间累积重置值","风机盘管03A01-运行时间累积重置值",{"$f":"E1502&VLOOKUP(D1502,list!$D$3:$F$501,2,FALSE)&F1502&\"_\"&VLOOKUP(G1502,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_RSTV"},"LFCU03A01_RSTV AT%M1152.0 :REAL; (*风机盘管03A01-运行时间累积重置值*)","LFCU03A01_RSTV          AT%M1152.0     :REAL; (*风机盘管03A01-运行时间累积重置值*)"]
["1156.0","验证通过","BOOL","风机盘管","L","03A01","隔离开关1","风机盘管03A01-隔离开关1",{"$f":"E1503&VLOOKUP(D1503,list!$D$3:$F$501,2,FALSE)&F1503&\"_\"&VLOOKUP(G1503,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_ISO1"},"LFCU03A01_ISO1 AT%M1156.0 :BOOL; (*风机盘管03A01-隔离开关1*)","LFCU03A01_ISO1          AT%M1156.0     :BOOL; (*风机盘管03A01-隔离开关1*)"]
["1160.0","验证通过","REAL","风机盘管","L","03A01","运行时间累积值","风机盘管03A01-运行时间累积值",{"$f":"E1504&VLOOKUP(D1504,list!$D$3:$F$501,2,FALSE)&F1504&\"_\"&VLOOKUP(G1504,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_RH"},"LFCU03A01_RH AT%M1160.0 :REAL; (*风机盘管03A01-运行时间累积值*)","LFCU03A01_RH            AT%M1160.0     :REAL; (*风机盘管03A01-运行时间累积值*)"]
["1164.0","验证通过","INT","风机盘管","L","03A01","设备状态代码","风机盘管03A01-设备状态代码",{"$f":"E1505&VLOOKUP(D1505,list!$D$3:$F$501,2,FALSE)&F1505&\"_\"&VLOOKUP(G1505,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_SN"},"LFCU03A01_SN AT%M1164.0 :INT; (*风机盘管03A01-设备状态代码*)","LFCU03A01_SN            AT%M1164.0     :INT; (*风机盘管03A01-设备状态代码*)"]
["1166.0","验证通过","INT","风机盘管","L","03A01","水阀控制转换值","风机盘管03A01-水阀控制转换值",{"$f":"E1506&VLOOKUP(D1506,list!$D$3:$F$501,2,FALSE)&F1506&\"_\"&VLOOKUP(G1506,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_WVCS"},"LFCU03A01_WVCS AT%M1166.0 :INT; (*风机盘管03A01-水阀控制转换值*)","LFCU03A01_WVCS          AT%M1166.0     :INT; (*风机盘管03A01-水阀控制转换值*)"]
["1168.0","验证通过","BOOL","风机盘管","L","03A01","程序控制","风机盘管03A01-程序控制",{"$f":"E1507&VLOOKUP(D1507,list!$D$3:$F$501,2,FALSE)&F1507&\"_\"&VLOOKUP(G1507,list!$I$2:$K$502,2,FALSE)","v":"LFCU03A01_PC"},"LFCU03A01_PC AT%M1168.0 :BOOL; (*风机盘管03A01-程序控制*)","LFCU03A01_PC            AT%M1168.0     :BOOL; (*风机盘管03A01-程序控制*)"]

{"sheet":"L19","index":4,"n_rows":148,"n_cols":11,"rows_kept":148,"cut":false,"hidden":false,"merged":[]}
["中间变量"]
["100.0",{"$f":"IF((IF(OR(C2=\"INT\",C2=\"WORD\",C2=\"BOOL\"),MOD(A2,2),MOD(A2,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"INT","命令","L","00000","运行模式","总线程序-运行模式",{"$f":"E2&VLOOKUP(D2,list!$D$3:$F$501,2,FALSE)&F2&\"_\"&VLOOKUP(G2,list!$I$2:$K$502,2,FALSE)","v":"LCMD00000_RM"},{"$f":"I2&\" \"&\"AT%M\"&A2&\" \"&\":\"&C2&\";\"&\" \"&\"(*\"&H2&\"*)\"","v":"LCMD00000_RM AT%M100.0 :INT; (*总线程序-运行模式*)"},{"$f":"REPLACE(REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2))),SEARCH(\":\",REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J2,SEARCH(\"AT%\",J2),,REPT(\" \",25-SEARCH(\"AT%\",J2))))))","v":"LCMD00000_RM            AT%M100.0      :INT; (*总线程序-运行模式*)"}]
[{"$f":"IF(OR(C2=\"REAL\",C2=\"DWORD\",C2=\"DINT\"),(IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),A2+4+MOD(A2,4),A2+4)),(IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),A2+4+MOD(A2,4),A2+2)))&\".0\"","v":"102.0"},{"$f":"IF((IF(OR(C3=\"INT\",C3=\"WORD\",C3=\"BOOL\"),MOD(A3,2),MOD(A3,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","控制箱","L","01","模块地址状态",{"$f":"D3&F3&\"-\"&IF(E3=\"R\",\"新云平台\"&G3,G3)","v":"控制箱01-模块地址状态"},{"$f":"E3&VLOOKUP(D3,list!$D$3:$F$501,2,FALSE)&F3&\"_\"&VLOOKUP(G3,list!$I$2:$K$502,2,FALSE)","v":"LBOX01_DS"},{"$f":"I3&\" \"&\"AT%M\"&A3&\" \"&\":\"&C3&\";\"&\" \"&\"(*\"&H3&\"*)\"","v":"LBOX01_DS AT%M102.0 :BOOL; (*控制箱01-模块地址状态*)"},"LBOX01_DS               AT%M102.0      :BOOL; (*控制箱01-模块地址状态*)"]
[{"$f":"IF(OR(C3=\"REAL\",C3=\"DWORD\",C3=\"DINT\"),(IF(OR(C4=\"REAL\",C4=\"DWORD\",C4=\"DINT\"),A3+4+MOD(A3,4),A3+4)),(IF(OR(C4=\"REAL\",C4=\"DWORD\",C4=\"DINT\"),A3+4+MOD(A3,4),A3+2)))&\".0\"","v":"104.0"},"验证通过","BOOL","控制箱","L","02","模块地址状态",{"$f":"D4&F4&\"-\"&IF(E4=\"R\",\"新云平台\"&G4,G4)","v":"控制箱02-模块地址状态"},{"$f":"E4&VLOOKUP(D4,list!$D$3:$F$501,2,FALSE)&F4&\"_\"&VLOOKUP(G4,list!$I$2:$K$502,2,FALSE)","v":"LBOX02_DS"},"LBOX02_DS AT%M104.0 :BOOL; (*控制箱02-模块地址状态*)","LBOX02_DS               AT%M104.0      :BOOL; (*控制箱02-模块地址状态*)"]
["106.0","验证通过","BOOL","控制箱","L","03","模块地址状态","控制箱03-模块地址状态",{"$f":"E5&VLOOKUP(D5,list!$D$3:$F$501,2,FALSE)&F5&\"_\"&VLOOKUP(G5,list!$I$2:$K$502,2,FALSE)","v":"LBOX03_DS"},"LBOX03_DS AT%M106.0 :BOOL; (*控制箱03-模块地址状态*)","LBOX03_DS               AT%M106.0      :BOOL; (*控制箱03-模块地址状态*)"]
["108.0","验证通过","BOOL","控制箱","L","04","模块地址状态","控制箱04-模块地址状态",{"$f":"E6&VLOOKUP(D6,list!$D$3:$F$501,2,FALSE)&F6&\"_\"&VLOOKUP(G6,list!$I$2:$K$502,2,FALSE)","v":"LBOX04_DS"},"LBOX04_DS AT%M108.0 :BOOL; (*控制箱04-模块地址状态*)","LBOX04_DS               AT%M108.0      :BOOL; (*控制箱04-模块地址状态*)"]
["110.0","验证通过","BOOL","控制箱","L","05","模块地址状态","控制箱05-模块地址状态",{"$f":"E7&VLOOKUP(D7,list!$D$3:$F$501,2,FALSE)&F7&\"_\"&VLOOKUP(G7,list!$I$2:$K$502,2,FALSE)","v":"LBOX05_DS"},"LBOX05_DS AT%M110.0 :BOOL; (*控制箱05-模块地址状态*)","LBOX05_DS               AT%M110.0      :BOOL; (*控制箱05-模块地址状态*)"]
["112.0","验证通过","BOOL","控制箱","L","06","模块地址状态","控制箱06-模块地址状态",{"$f":"E8&VLOOKUP(D8,list!$D$3:$F$501,2,FALSE)&F8&\"_\"&VLOOKUP(G8,list!$I$2:$K$502,2,FALSE)","v":"LBOX06_DS"},"LBOX06_DS AT%M112.0 :BOOL; (*控制箱06-模块地址状态*)","LBOX06_DS               AT%M112.0      :BOOL; (*控制箱06-模块地址状态*)"]
["114.0","验证通过","BOOL","控制箱","L","07","模块地址状态","控制箱07-模块地址状态",{"$f":"E9&VLOOKUP(D9,list!$D$3:$F$501,2,FALSE)&F9&\"_\"&VLOOKUP(G9,list!$I$2:$K$502,2,FALSE)","v":"LBOX07_DS"},"LBOX07_DS AT%M114.0 :BOOL; (*控制箱07-模块地址状态*)","LBOX07_DS               AT%M114.0      :BOOL; (*控制箱07-模块地址状态*)"]
["116.0","验证通过","BOOL","控制箱","L","08","模块地址状态","控制箱08-模块地址状态",{"$f":"E10&VLOOKUP(D10,list!$D$3:$F$501,2,FALSE)&F10&\"_\"&VLOOKUP(G10,list!$I$2:$K$502,2,FALSE)","v":"LBOX08_DS"},"LBOX08_DS AT%M116.0 :BOOL; (*控制箱08-模块地址状态*)","LBOX08_DS               AT%M116.0      :BOOL; (*控制箱08-模块地址状态*)"]
["118.0","验证通过","BOOL","控制箱","L","09","模块地址状态","控制箱09-模块地址状态",{"$f":"E11&VLOOKUP(D11,list!$D$3:$F$501,2,FALSE)&F11&\"_\"&VLOOKUP(G11,list!$I$2:$K$502,2,FALSE)","v":"LBOX09_DS"},"LBOX09_DS AT%M118.0 :BOOL; (*控制箱09-模块地址状态*)","LBOX09_DS               AT%M118.0      :BOOL; (*控制箱09-模块地址状态*)"]
["120.0","验证通过","BOOL","控制箱","L","10","模块地址状态","控制箱10-模块地址状态",{"$f":"E12&VLOOKUP(D12,list!$D$3:$F$501,2,FALSE)&F12&\"_\"&VLOOKUP(G12,list!$I$2:$K$502,2,FALSE)","v":"LBOX10_DS"},"LBOX10_DS AT%M120.0 :BOOL; (*控制箱10-模块地址状态*)","LBOX10_DS               AT%M120.0      :BOOL; (*控制箱10-模块地址状态*)"]
["124.0","验证通过","REAL","控制箱","L","00","模块在线比例","控制箱00-模块在线比例",{"$f":"E13&VLOOKUP(D13,list!$D$3:$F$501,2,FALSE)&F13&\"_\"&VLOOKUP(G13,list!$I$2:$K$502,2,FALSE)","v":"LBOX00_OR"},"LBOX00_OR AT%M124.0 :REAL; (*控制箱00-模块在线比例*)","LBOX00_OR               AT%M124.0      :REAL; (*控制箱00-模块在线比例*)"]
["128.0","验证通过","REAL","控制箱","L","01","模块在线比例","控制箱01-模块在线比例",{"$f":"E14&VLOOKUP(D14,list!$D$3:$F$501,2,FALSE)&F14&\"_\"&VLOOKUP(G14,list!$I$2:$K$502,2,FALSE)","v":"LBOX01_OR"},"LBOX01_OR AT%M128.0 :REAL; (*控制箱01-模块在线比例*)","LBOX01_OR               AT%M128.0      :REAL; (*控制箱01-模块在线比例*)"]
["132.0","验证通过","REAL","控制箱","L","02","模块在线比例","控制箱02-模块在线比例",{"$f":"E15&VLOOKUP(D15,list!$D$3:$F$501,2,FALSE)&F15&\"_\"&VLOOKUP(G15,list!$I$2:$K$502,2,FALSE)","v":"LBOX02_OR"},"LBOX02_OR AT%M132.0 :REAL; (*控制箱02-模块在线比例*)","LBOX02_OR               AT%M132.0      :REAL; (*控制箱02-模块在线比例*)"]
["136.0","验证通过","REAL","控制箱","L","03","模块在线比例","控制箱03-模块在线比例",{"$f":"E16&VLOOKUP(D16,list!$D$3:$F$501,2,FALSE)&F16&\"_\"&VLOOKUP(G16,list!$I$2:$K$502,2,FALSE)","v":"LBOX03_OR"},"LBOX03_OR AT%M136.0 :REAL; (*控制箱03-模块在线比例*)","LBOX03_OR               AT%M136.0      :REAL; (*控制箱03-模块在线比例*)"]
["140.0","验证通过","REAL","控制箱","L","04","模块在线比例","控制箱04-模块在线比例",{"$f":"E17&VLOOKUP(D17,list!$D$3:$F$501,2,FALSE)&F17&\"_\"&VLOOKUP(G17,list!$I$2:$K$502,2,FALSE)","v":"LBOX04_OR"},"LBOX04_OR AT%M140.0 :REAL; (*控制箱04-模块在线比例*)","LBOX04_OR               AT%M140.0      :REAL; (*控制箱04-模块在线比例*)"]
["144.0","验证通过","REAL","控制箱","L","05","模块在线比例","控制箱05-模块在线比例",{"$f":"E18&VLOOKUP(D18,list!$D$3:$F$501,2,FALSE)&F18&\"_\"&VLOOKUP(G18,list!$I$2:$K$502,2,FALSE)","v":"LBOX05_OR"},"LBOX05_OR AT%M144.0 :REAL; (*控制箱05-模块在线比例*)","LBOX05_OR               AT%M144.0      :REAL; (*控制箱05-模块在线比例*)"]
["148.0","验证通过","REAL","控制箱","L","06","模块在线比例","控制箱06-模块在线比例",{"$f":"E19&VLOOKUP(D19,list!$D$3:$F$501,2,FALSE)&F19&\"_\"&VLOOKUP(G19,list!$I$2:$K$502,2,FALSE)","v":"LBOX06_OR"},"LBOX06_OR AT%M148.0 :REAL; (*控制箱06-模块在线比例*)","LBOX06_OR               AT%M148.0      :REAL; (*控制箱06-模块在线比例*)"]
["152.0","验证通过","REAL","控制箱","L","07","模块在线比例","控制箱07-模块在线比例",{"$f":"E20&VLOOKUP(D20,list!$D$3:$F$501,2,FALSE)&F20&\"_\"&VLOOKUP(G20,list!$I$2:$K$502,2,FALSE)","v":"LBOX07_OR"},"LBOX07_OR AT%M152.0 :REAL; (*控制箱07-模块在线比例*)","LBOX07_OR               AT%M152.0      :REAL; (*控制箱07-模块在线比例*)"]
["156.0","验证通过","REAL","控制箱","L","08","模块在线比例","控制箱08-模块在线比例",{"$f":"E21&VLOOKUP(D21,list!$D$3:$F$501,2,FALSE)&F21&\"_\"&VLOOKUP(G21,list!$I$2:$K$502,2,FALSE)","v":"LBOX08_OR"},"LBOX08_OR AT%M156.0 :REAL; (*控制箱08-模块在线比例*)","LBOX08_OR               AT%M156.0      :REAL; (*控制箱08-模块在线比例*)"]
["160.0","验证通过","REAL","控制箱","L","09","模块在线比例","控制箱09-模块在线比例",{"$f":"E22&VLOOKUP(D22,list!$D$3:$F$501,2,FALSE)&F22&\"_\"&VLOOKUP(G22,list!$I$2:$K$502,2,FALSE)","v":"LBOX09_OR"},"LBOX09_OR AT%M160.0 :REAL; (*控制箱09-模块在线比例*)","LBOX09_OR               AT%M160.0      :REAL; (*控制箱09-模块在线比例*)"]
["164.0","验证通过","REAL","控制箱","L","10","模块在线比例","控制箱10-模块在线比例",{"$f":"E23&VLOOKUP(D23,list!$D$3:$F$501,2,FALSE)&F23&\"_\"&VLOOKUP(G23,list!$I$2:$K$502,2,FALSE)","v":"LBOX10_OR"},"LBOX10_OR AT%M164.0 :REAL; (*控制箱10-模块在线比例*)","LBOX10_OR               AT%M164.0      :REAL; (*控制箱10-模块在线比例*)"]
["SWP"]
[{"$f":"IF(OR(C23=\"REAL\",C23=\"DWORD\",C23=\"DINT\"),(IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),A23+4+MOD(A23,4),A23+4)),(IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),A23+4+MOD(A23,4),A23+2)))&\".0\"","v":"168.0"},{"$f":"IF((IF(OR(C25=\"INT\",C25=\"WORD\",C25=\"BOOL\"),MOD(A25,2),MOD(A25,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","潜污泵井","L","B1D01","运行时间累积重置1",{"$f":"D25&F25&\"-\"&IF(E25=\"R\",\"新云平台\"&G25,G25)","v":"潜污泵井B1D01-运行时间累积重置1"},{"$f":"E25&VLOOKUP(D25,list!$D$3:$F$501,2,FALSE)&F25&\"_\"&VLOOKUP(G25,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D01_RST1"},{"$f":"I25&\" \"&\"AT%M\"&A25&\" \"&\":\"&C25&\";\"&\" \"&\"(*\"&H25&\"*)\"","v":"LSWPB1D01_RST1 AT%M168.0 :BOOL; (*潜污泵井B1D01-运行时间累积重置1*)"},{"$f":"REPLACE(REPLACE(J25,SEARCH(\"AT%\",J25),,REPT(\" \",25-SEARCH(\"AT%\",J25))),SEARCH(\":\",REPLACE(J25,SEARCH(\"AT%\",J25),,REPT(\" \",25-SEARCH(\"AT%\",J25)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J25,SEARCH(\"AT%\",J25),,REPT(\" \",25-SEARCH(\"AT%\",J25))))))","v":"LSWPB1D01_RST1          AT%M168.0      :BOOL; (*潜污泵井B1D01-运行时间累积重置1*)"}]
[{"$f":"IF(OR(C25=\"REAL\",C25=\"DWORD\",C25=\"DINT\"),(IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),A25+4+MOD(A25,4),A25+4)),(IF(OR(C26=\"REAL\",C26=\"DWORD\",C26=\"DINT\"),A25+4+MOD(A25,4),A25+2)))&\".0\"","v":"172.0"},"验证通过","REAL","潜污泵井","L",{"$f":"F25","v":"B1D01"},"运行时间累积重置值1","潜污泵井B1D01-运行时间累积重置值1",{"$f":"E26&VLOOKUP(D26,list!$D$3:$F$501,2,FALSE)&F26&\"_\"&VLOOKUP(G26,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D01_RSTV1"},"LSWPB1D01_RSTV1 AT%M172.0 :REAL; (*潜污泵井B1D01-运行时间累积重置值1*)","LSWPB1D01_RSTV1         AT%M172.0      :REAL; (*潜污泵井B1D01-运行时间累积重置值1*)"]
["176.0","验证通过","REAL","潜污泵井","L","B1D01","运行时间累积值1","潜污泵井B1D01-运行时间累积值1",{"$f":"E27&VLOOKUP(D27,list!$D$3:$F$501,2,FALSE)&F27&\"_\"&VLOOKUP(G27,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D01_RH1"},"LSWPB1D01_RH1 AT%M176.0 :REAL; (*潜污泵井B1D01-运行时间累积值1*)","LSWPB1D01_RH1           AT%M176.0      :REAL; (*潜污泵井B1D01-运行时间累积值1*)"]
["180.0","验证通过","BOOL","潜污泵井","L","B1D01","运行时间累积重置2","潜污泵井B1D01-运行时间累积重置2",{"$f":"E28&VLOOKUP(D28,list!$D$3:$F$501,2,FALSE)&F28&\"_\"&VLOOKUP(G28,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D01_RST2"},"LSWPB1D01_RST2 AT%M180.0 :BOOL; (*潜污泵井B1D01-运行时间累积重置2*)","LSWPB1D01_RST2          AT%M180.0      :BOOL; (*潜污泵井B1D01-运行时间累积重置2*)"]
["184.0","验证通过","REAL","潜污泵井","L","B1D01","运行时间累积重置值2","潜污泵井B1D01-运行时间累积重置值2",{"$f":"E29&VLOOKUP(D29,list!$D$3:$F$501,2,FALSE)&F29&\"_\"&VLOOKUP(G29,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D01_RSTV2"},"LSWPB1D01_RSTV2 AT%M184.0 :REAL; (*潜污泵井B1D01-运行时间累积重置值2*)","LSWPB1D01_RSTV2         AT%M184.0      :REAL; (*潜污泵井B1D01-运行时间累积重置值2*)"]
["188.0","验证通过","REAL","潜污泵井","L","B1D01","运行时间累积值2","潜污泵井B1D01-运行时间累积值2",{"$f":"E30&VLOOKUP(D30,list!$D$3:$F$501,2,FALSE)&F30&\"_\"&VLOOKUP(G30,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D01_RH2"},"LSWPB1D01_RH2 AT%M188.0 :REAL; (*潜污泵井B1D01-运行时间累积值2*)","LSWPB1D01_RH2           AT%M188.0      :REAL; (*潜污泵井B1D01-运行时间累积值2*)"]
["SWP"]
[{"$f":"IF(OR(C30=\"REAL\",C30=\"DWORD\",C30=\"DINT\"),(IF(OR(C32=\"REAL\",C32=\"DWORD\",C32=\"DINT\"),A30+4+MOD(A30,4),A30+4)),(IF(OR(C32=\"REAL\",C32=\"DWORD\",C32=\"DINT\"),A30+4+MOD(A30,4),A30+2)))&\".0\"","v":"192.0"},{"$f":"IF((IF(OR(C32=\"INT\",C32=\"WORD\",C32=\"BOOL\"),MOD(A32,2),MOD(A32,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","潜污泵井","L","B1D02","运行时间累积重置1",{"$f":"D32&F32&\"-\"&IF(E32=\"R\",\"新云平台\"&G32,G32)","v":"潜污泵井B1D02-运行时间累积重置1"},{"$f":"E32&VLOOKUP(D32,list!$D$3:$F$501,2,FALSE)&F32&\"_\"&VLOOKUP(G32,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D02_RST1"},{"$f":"I32&\" \"&\"AT%M\"&A32&\" \"&\":\"&C32&\";\"&\" \"&\"(*\"&H32&\"*)\"","v":"LSWPB1D02_RST1 AT%M192.0 :BOOL; (*潜污泵井B1D02-运行时间累积重置1*)"},{"$f":"REPLACE(REPLACE(J32,SEARCH(\"AT%\",J32),,REPT(\" \",25-SEARCH(\"AT%\",J32))),SEARCH(\":\",REPLACE(J32,SEARCH(\"AT%\",J32),,REPT(\" \",25-SEARCH(\"AT%\",J32)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J32,SEARCH(\"AT%\",J32),,REPT(\" \",25-SEARCH(\"AT%\",J32))))))","v":"LSWPB1D02_RST1          AT%M192.0      :BOOL; (*潜污泵井B1D02-运行时间累积重置1*)"}]
[{"$f":"IF(OR(C32=\"REAL\",C32=\"DWORD\",C32=\"DINT\"),(IF(OR(C33=\"REAL\",C33=\"DWORD\",C33=\"DINT\"),A32+4+MOD(A32,4),A32+4)),(IF(OR(C33=\"REAL\",C33=\"DWORD\",C33=\"DINT\"),A32+4+MOD(A32,4),A32+2)))&\".0\"","v":"196.0"},"验证通过","REAL","潜污泵井","L",{"$f":"F32","v":"B1D02"},"运行时间累积重置值1","潜污泵井B1D02-运行时间累积重置值1",{"$f":"E33&VLOOKUP(D33,list!$D$3:$F$501,2,FALSE)&F33&\"_\"&VLOOKUP(G33,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D02_RSTV1"},"LSWPB1D02_RSTV1 AT%M196.0 :REAL; (*潜污泵井B1D02-运行时间累积重置值1*)","LSWPB1D02_RSTV1         AT%M196.0      :REAL; (*潜污泵井B1D02-运行时间累积重置值1*)"]
["200.0","验证通过","REAL","潜污泵井","L","B1D02","运行时间累积值1","潜污泵井B1D02-运行时间累积值1",{"$f":"E34&VLOOKUP(D34,list!$D$3:$F$501,2,FALSE)&F34&\"_\"&VLOOKUP(G34,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D02_RH1"},"LSWPB1D02_RH1 AT%M200.0 :REAL; (*潜污泵井B1D02-运行时间累积值1*)","LSWPB1D02_RH1           AT%M200.0      :REAL; (*潜污泵井B1D02-运行时间累积值1*)"]
["204.0","验证通过","BOOL","潜污泵井","L","B1D02","运行时间累积重置2","潜污泵井B1D02-运行时间累积重置2",{"$f":"E35&VLOOKUP(D35,list!$D$3:$F$501,2,FALSE)&F35&\"_\"&VLOOKUP(G35,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D02_RST2"},"LSWPB1D02_RST2 AT%M204.0 :BOOL; (*潜污泵井B1D02-运行时间累积重置2*)","LSWPB1D02_RST2          AT%M204.0      :BOOL; (*潜污泵井B1D02-运行时间累积重置2*)"]
["208.0","验证通过","REAL","潜污泵井","L","B1D02","运行时间累积重置值2","潜污泵井B1D02-运行时间累积重置值2",{"$f":"E36&VLOOKUP(D36,list!$D$3:$F$501,2,FALSE)&F36&\"_\"&VLOOKUP(G36,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D02_RSTV2"},"LSWPB1D02_RSTV2 AT%M208.0 :REAL; (*潜污泵井B1D02-运行时间累积重置值2*)","LSWPB1D02_RSTV2         AT%M208.0      :REAL; (*潜污泵井B1D02-运行时间累积重置值2*)"]
["212.0","验证通过","REAL","潜污泵井","L","B1D02","运行时间累积值2","潜污泵井B1D02-运行时间累积值2",{"$f":"E37&VLOOKUP(D37,list!$D$3:$F$501,2,FALSE)&F37&\"_\"&VLOOKUP(G37,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D02_RH2"},"LSWPB1D02_RH2 AT%M212.0 :REAL; (*潜污泵井B1D02-运行时间累积值2*)","LSWPB1D02_RH2           AT%M212.0      :REAL; (*潜污泵井B1D02-运行时间累积值2*)"]
["SWP"]
[{"$f":"IF(OR(C37=\"REAL\",C37=\"DWORD\",C37=\"DINT\"),(IF(OR(C39=\"REAL\",C39=\"DWORD\",C39=\"DINT\"),A37+4+MOD(A37,4),A37+4)),(IF(OR(C39=\"REAL\",C39=\"DWORD\",C39=\"DINT\"),A37+4+MOD(A37,4),A37+2)))&\".0\"","v":"216.0"},{"$f":"IF((IF(OR(C39=\"INT\",C39=\"WORD\",C39=\"BOOL\"),MOD(A39,2),MOD(A39,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","潜污泵井","L","B1D03","运行时间累积重置1",{"$f":"D39&F39&\"-\"&IF(E39=\"R\",\"新云平台\"&G39,G39)","v":"潜污泵井B1D03-运行时间累积重置1"},{"$f":"E39&VLOOKUP(D39,list!$D$3:$F$501,2,FALSE)&F39&\"_\"&VLOOKUP(G39,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D03_RST1"},{"$f":"I39&\" \"&\"AT%M\"&A39&\" \"&\":\"&C39&\";\"&\" \"&\"(*\"&H39&\"*)\"","v":"LSWPB1D03_RST1 AT%M216.0 :BOOL; (*潜污泵井B1D03-运行时间累积重置1*)"},{"$f":"REPLACE(REPLACE(J39,SEARCH(\"AT%\",J39),,REPT(\" \",25-SEARCH(\"AT%\",J39))),SEARCH(\":\",REPLACE(J39,SEARCH(\"AT%\",J39),,REPT(\" \",25-SEARCH(\"AT%\",J39)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J39,SEARCH(\"AT%\",J39),,REPT(\" \",25-SEARCH(\"AT%\",J39))))))","v":"LSWPB1D03_RST1          AT%M216.0      :BOOL; (*潜污泵井B1D03-运行时间累积重置1*)"}]
[{"$f":"IF(OR(C39=\"REAL\",C39=\"DWORD\",C39=\"DINT\"),(IF(OR(C40=\"REAL\",C40=\"DWORD\",C40=\"DINT\"),A39+4+MOD(A39,4),A39+4)),(IF(OR(C40=\"REAL\",C40=\"DWORD\",C40=\"DINT\"),A39+4+MOD(A39,4),A39+2)))&\".0\"","v":"220.0"},"验证通过","REAL","潜污泵井","L",{"$f":"F39","v":"B1D03"},"运行时间累积重置值1","潜污泵井B1D03-运行时间累积重置值1",{"$f":"E40&VLOOKUP(D40,list!$D$3:$F$501,2,FALSE)&F40&\"_\"&VLOOKUP(G40,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D03_RSTV1"},"LSWPB1D03_RSTV1 AT%M220.0 :REAL; (*潜污泵井B1D03-运行时间累积重置值1*)","LSWPB1D03_RSTV1         AT%M220.0      :REAL; (*潜污泵井B1D03-运行时间累积重置值1*)"]
["224.0","验证通过","REAL","潜污泵井","L","B1D03","运行时间累积值1","潜污泵井B1D03-运行时间累积值1",{"$f":"E41&VLOOKUP(D41,list!$D$3:$F$501,2,FALSE)&F41&\"_\"&VLOOKUP(G41,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D03_RH1"},"LSWPB1D03_RH1 AT%M224.0 :REAL; (*潜污泵井B1D03-运行时间累积值1*)","LSWPB1D03_RH1           AT%M224.0      :REAL; (*潜污泵井B1D03-运行时间累积值1*)"]
["228.0","验证通过","BOOL","潜污泵井","L","B1D03","运行时间累积重置2","潜污泵井B1D03-运行时间累积重置2",{"$f":"E42&VLOOKUP(D42,list!$D$3:$F$501,2,FALSE)&F42&\"_\"&VLOOKUP(G42,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D03_RST2"},"LSWPB1D03_RST2 AT%M228.0 :BOOL; (*潜污泵井B1D03-运行时间累积重置2*)","LSWPB1D03_RST2          AT%M228.0      :BOOL; (*潜污泵井B1D03-运行时间累积重置2*)"]
["232.0","验证通过","REAL","潜污泵井","L","B1D03","运行时间累积重置值2","潜污泵井B1D03-运行时间累积重置值2",{"$f":"E43&VLOOKUP(D43,list!$D$3:$F$501,2,FALSE)&F43&\"_\"&VLOOKUP(G43,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D03_RSTV2"},"LSWPB1D03_RSTV2 AT%M232.0 :REAL; (*潜污泵井B1D03-运行时间累积重置值2*)","LSWPB1D03_RSTV2         AT%M232.0      :REAL; (*潜污泵井B1D03-运行时间累积重置值2*)"]
["236.0","验证通过","REAL","潜污泵井","L","B1D03","运行时间累积值2","潜污泵井B1D03-运行时间累积值2",{"$f":"E44&VLOOKUP(D44,list!$D$3:$F$501,2,FALSE)&F44&\"_\"&VLOOKUP(G44,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1D03_RH2"},"LSWPB1D03_RH2 AT%M236.0 :REAL; (*潜污泵井B1D03-运行时间累积值2*)","LSWPB1D03_RH2           AT%M236.0      :REAL; (*潜污泵井B1D03-运行时间累积值2*)"]
["EAF"]
[{"$f":"IF(OR(C44=\"REAL\",C44=\"DWORD\",C44=\"DINT\"),(IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),A44+4+MOD(A44,4),A44+4)),(IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),A44+4+MOD(A44,4),A44+2)))&\".0\"","v":"240.0"},{"$f":"IF((IF(OR(C46=\"INT\",C46=\"WORD\",C46=\"BOOL\"),MOD(A46,2),MOD(A46,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排烟机","R","B1D01","启停控制",{"$f":"D46&F46&\"-\"&IF(E46=\"R\",\"新云平台\"&G46,G46)","v":"排烟机B1D01-新云平台启停控制"},{"$f":"E46&VLOOKUP(D46,list!$D$3:$F$501,2,FALSE)&F46&\"_\"&VLOOKUP(G46,list!$I$2:$K$502,2,FALSE)","v":"RESFB1D01_C"},{"$f":"I46&\" \"&\"AT%M\"&A46&\" \"&\":\"&C46&\";\"&\" \"&\"(*\"&H46&\"*)\"","v":"RESFB1D01_C AT%M240.0 :BOOL; (*排烟机B1D01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J46,SEARCH(\"AT%\",J46),,REPT(\" \",25-SEARCH(\"AT%\",J46))),SEARCH(\":\",REPLACE(J46,SEARCH(\"AT%\",J46),,REPT(\" \",25-SEARCH(\"AT%\",J46)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J46,SEARCH(\"AT%\",J46),,REPT(\" \",25-SEARCH(\"AT%\",J46))))))","v":"RESFB1D01_C             AT%M240.0      :BOOL; (*排烟机B1D01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C46=\"REAL\",C46=\"DWORD\",C46=\"DINT\"),(IF(OR(C47=\"REAL\",C47=\"DWORD\",C47=\"DINT\"),A46+4+MOD(A46,4),A46+4)),(IF(OR(C47=\"REAL\",C47=\"DWORD\",C47=\"DINT\"),A46+4+MOD(A46,4),A46+2)))&\".0\"","v":"242.0"},"验证通过","BOOL","排烟机","L",{"$f":"F46","v":"B1D01"},"运行时间累积重置","排烟机B1D01-运行时间累积重置",{"$f":"E47&VLOOKUP(D47,list!$D$3:$F$501,2,FALSE)&F47&\"_\"&VLOOKUP(G47,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D01_RST"},"LESFB1D01_RST AT%M242.0 :BOOL; (*排烟机B1D01-运行时间累积重置*)","LESFB1D01_RST           AT%M242.0      :BOOL; (*排烟机B1D01-运行时间累积重置*)"]
["248.0","验证通过","REAL","排烟机","L","B1D01","运行时间累积重置值","排烟机B1D01-运行时间累积重置值",{"$f":"E48&VLOOKUP(D48,list!$D$3:$F$501,2,FALSE)&F48&\"_\"&VLOOKUP(G48,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D01_RSTV"},"LESFB1D01_RSTV AT%M248.0 :REAL; (*排烟机B1D01-运行时间累积重置值*)","LESFB1D01_RSTV          AT%M248.0      :REAL; (*排烟机B1D01-运行时间累积重置值*)"]
["252.0","验证通过","REAL","排烟机","L","B1D01","运行时间累积值","排烟机B1D01-运行时间累积值",{"$f":"E49&VLOOKUP(D49,list!$D$3:$F$501,2,FALSE)&F49&\"_\"&VLOOKUP(G49,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D01_RH"},"LESFB1D01_RH AT%M252.0 :REAL; (*排烟机B1D01-运行时间累积值*)","LESFB1D01_RH            AT%M252.0      :REAL; (*排烟机B1D01-运行时间累积值*)"]
["256.0","验证通过","BOOL","排烟机","L","B1D01","定时模式","排烟机B1D01-定时模式",{"$f":"E50&VLOOKUP(D50,list!$D$3:$F$501,2,FALSE)&F50&\"_\"&VLOOKUP(G50,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D01_TM"},"LESFB1D01_TM AT%M256.0 :BOOL; (*排烟机B1D01-定时模式*)","LESFB1D01_TM            AT%M256.0      :BOOL; (*排烟机B1D01-定时模式*)"]
["258.0","验证通过","BOOL","排烟机","L","B1D01","定时控制","排烟机B1D01-定时控制",{"$f":"E51&VLOOKUP(D51,list!$D$3:$F$501,2,FALSE)&F51&\"_\"&VLOOKUP(G51,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D01_TC"},"LESFB1D01_TC AT%M258.0 :BOOL; (*排烟机B1D01-定时控制*)","LESFB1D01_TC            AT%M258.0      :BOOL; (*排烟机B1D01-定时控制*)"]
["260.0","验证通过","BOOL","排烟机","L","B1D01","全天候模式","排烟机B1D01-全天候模式",{"$f":"E52&VLOOKUP(D52,list!$D$3:$F$501,2,FALSE)&F52&\"_\"&VLOOKUP(G52,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D01_DM"},"LESFB1D01_DM AT%M260.0 :BOOL; (*排烟机B1D01-全天候模式*)","LESFB1D01_DM            AT%M260.0      :BOOL; (*排烟机B1D01-全天候模式*)"]
["264.0","验证通过","REAL","排烟机","L","B1D01","CO设定值","排烟机B1D01-CO设定值",{"$f":"E53&VLOOKUP(D53,list!$D$3:$F$501,2,FALSE)&F53&\"_\"&VLOOKUP(G53,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D01_COSET"},"LESFB1D01_COSET AT%M264.0 :REAL; (*排烟机B1D01-CO设定值*)","LESFB1D01_COSET         AT%M264.0      :REAL; (*排烟机B1D01-CO设定值*)"]
["EAF"]
[{"$f":"IF(OR(C53=\"REAL\",C53=\"DWORD\",C53=\"DINT\"),(IF(OR(C55=\"REAL\",C55=\"DWORD\",C55=\"DINT\"),A53+4+MOD(A53,4),A53+4)),(IF(OR(C55=\"REAL\",C55=\"DWORD\",C55=\"DINT\"),A53+4+MOD(A53,4),A53+2)))&\".0\"","v":"268.0"},{"$f":"IF((IF(OR(C55=\"INT\",C55=\"WORD\",C55=\"BOOL\"),MOD(A55,2),MOD(A55,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排烟机","R","B1D02","启停控制",{"$f":"D55&F55&\"-\"&IF(E55=\"R\",\"新云平台\"&G55,G55)","v":"排烟机B1D02-新云平台启停控制"},{"$f":"E55&VLOOKUP(D55,list!$D$3:$F$501,2,FALSE)&F55&\"_\"&VLOOKUP(G55,list!$I$2:$K$502,2,FALSE)","v":"RESFB1D02_C"},{"$f":"I55&\" \"&\"AT%M\"&A55&\" \"&\":\"&C55&\";\"&\" \"&\"(*\"&H55&\"*)\"","v":"RESFB1D02_C AT%M268.0 :BOOL; (*排烟机B1D02-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J55,SEARCH(\"AT%\",J55),,REPT(\" \",25-SEARCH(\"AT%\",J55))),SEARCH(\":\",REPLACE(J55,SEARCH(\"AT%\",J55),,REPT(\" \",25-SEARCH(\"AT%\",J55)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J55,SEARCH(\"AT%\",J55),,REPT(\" \",25-SEARCH(\"AT%\",J55))))))","v":"RESFB1D02_C             AT%M268.0      :BOOL; (*排烟机B1D02-新云平台启停控制*)"}]
[{"$f":"IF(OR(C55=\"REAL\",C55=\"DWORD\",C55=\"DINT\"),(IF(OR(C56=\"REAL\",C56=\"DWORD\",C56=\"DINT\"),A55+4+MOD(A55,4),A55+4)),(IF(OR(C56=\"REAL\",C56=\"DWORD\",C56=\"DINT\"),A55+4+MOD(A55,4),A55+2)))&\".0\"","v":"270.0"},"验证通过","BOOL","排烟机","L",{"$f":"F55","v":"B1D02"},"运行时间累积重置","排烟机B1D02-运行时间累积重置",{"$f":"E56&VLOOKUP(D56,list!$D$3:$F$501,2,FALSE)&F56&\"_\"&VLOOKUP(G56,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D02_RST"},"LESFB1D02_RST AT%M270.0 :BOOL; (*排烟机B1D02-运行时间累积重置*)","LESFB1D02_RST           AT%M270.0      :BOOL; (*排烟机B1D02-运行时间累积重置*)"]
["276.0","验证通过","REAL","排烟机","L","B1D02","运行时间累积重置值","排烟机B1D02-运行时间累积重置值",{"$f":"E57&VLOOKUP(D57,list!$D$3:$F$501,2,FALSE)&F57&\"_\"&VLOOKUP(G57,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D02_RSTV"},"LESFB1D02_RSTV AT%M276.0 :REAL; (*排烟机B1D02-运行时间累积重置值*)","LESFB1D02_RSTV          AT%M276.0      :REAL; (*排烟机B1D02-运行时间累积重置值*)"]
["280.0","验证通过","REAL","排烟机","L","B1D02","运行时间累积值","排烟机B1D02-运行时间累积值",{"$f":"E58&VLOOKUP(D58,list!$D$3:$F$501,2,FALSE)&F58&\"_\"&VLOOKUP(G58,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D02_RH"},"LESFB1D02_RH AT%M280.0 :REAL; (*排烟机B1D02-运行时间累积值*)","LESFB1D02_RH            AT%M280.0      :REAL; (*排烟机B1D02-运行时间累积值*)"]
["284.0","验证通过","BOOL","排烟机","L","B1D02","定时模式","排烟机B1D02-定时模式",{"$f":"E59&VLOOKUP(D59,list!$D$3:$F$501,2,FALSE)&F59&\"_\"&VLOOKUP(G59,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D02_TM"},"LESFB1D02_TM AT%M284.0 :BOOL; (*排烟机B1D02-定时模式*)","LESFB1D02_TM            AT%M284.0      :BOOL; (*排烟机B1D02-定时模式*)"]
["286.0","验证通过","BOOL","排烟机","L","B1D02","定时控制","排烟机B1D02-定时控制",{"$f":"E60&VLOOKUP(D60,list!$D$3:$F$501,2,FALSE)&F60&\"_\"&VLOOKUP(G60,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D02_TC"},"LESFB1D02_TC AT%M286.0 :BOOL; (*排烟机B1D02-定时控制*)","LESFB1D02_TC            AT%M286.0      :BOOL; (*排烟机B1D02-定时控制*)"]
["288.0","验证通过","BOOL","排烟机","L","B1D02","全天候模式","排烟机B1D02-全天候模式",{"$f":"E61&VLOOKUP(D61,list!$D$3:$F$501,2,FALSE)&F61&\"_\"&VLOOKUP(G61,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D02_DM"},"LESFB1D02_DM AT%M288.0 :BOOL; (*排烟机B1D02-全天候模式*)","LESFB1D02_DM            AT%M288.0      :BOOL; (*排烟机B1D02-全天候模式*)"]
["292.0","验证通过","REAL","排烟机","L","B1D02","CO设定值","排烟机B1D02-CO设定值",{"$f":"E62&VLOOKUP(D62,list!$D$3:$F$501,2,FALSE)&F62&\"_\"&VLOOKUP(G62,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D02_COSET"},"LESFB1D02_COSET AT%M292.0 :REAL; (*排烟机B1D02-CO设定值*)","LESFB1D02_COSET         AT%M292.0      :REAL; (*排烟机B1D02-CO设定值*)"]
["EAF"]
[{"$f":"IF(OR(C62=\"REAL\",C62=\"DWORD\",C62=\"DINT\"),(IF(OR(C64=\"REAL\",C64=\"DWORD\",C64=\"DINT\"),A62+4+MOD(A62,4),A62+4)),(IF(OR(C64=\"REAL\",C64=\"DWORD\",C64=\"DINT\"),A62+4+MOD(A62,4),A62+2)))&\".0\"","v":"296.0"},{"$f":"IF((IF(OR(C64=\"INT\",C64=\"WORD\",C64=\"BOOL\"),MOD(A64,2),MOD(A64,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排烟机","R","B1D03","启停控制",{"$f":"D64&F64&\"-\"&IF(E64=\"R\",\"新云平台\"&G64,G64)","v":"排烟机B1D03-新云平台启停控制"},{"$f":"E64&VLOOKUP(D64,list!$D$3:$F$501,2,FALSE)&F64&\"_\"&VLOOKUP(G64,list!$I$2:$K$502,2,FALSE)","v":"RESFB1D03_C"},{"$f":"I64&\" \"&\"AT%M\"&A64&\" \"&\":\"&C64&\";\"&\" \"&\"(*\"&H64&\"*)\"","v":"RESFB1D03_C AT%M296.0 :BOOL; (*排烟机B1D03-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J64,SEARCH(\"AT%\",J64),,REPT(\" \",25-SEARCH(\"AT%\",J64))),SEARCH(\":\",REPLACE(J64,SEARCH(\"AT%\",J64),,REPT(\" \",25-SEARCH(\"AT%\",J64)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J64,SEARCH(\"AT%\",J64),,REPT(\" \",25-SEARCH(\"AT%\",J64))))))","v":"RESFB1D03_C             AT%M296.0      :BOOL; (*排烟机B1D03-新云平台启停控制*)"}]
[{"$f":"IF(OR(C64=\"REAL\",C64=\"DWORD\",C64=\"DINT\"),(IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),A64+4+MOD(A64,4),A64+4)),(IF(OR(C65=\"REAL\",C65=\"DWORD\",C65=\"DINT\"),A64+4+MOD(A64,4),A64+2)))&\".0\"","v":"298.0"},"验证通过","BOOL","排烟机","L",{"$f":"F64","v":"B1D03"},"运行时间累积重置","排烟机B1D03-运行时间累积重置",{"$f":"E65&VLOOKUP(D65,list!$D$3:$F$501,2,FALSE)&F65&\"_\"&VLOOKUP(G65,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D03_RST"},"LESFB1D03_RST AT%M298.0 :BOOL; (*排烟机B1D03-运行时间累积重置*)","LESFB1D03_RST           AT%M298.0      :BOOL; (*排烟机B1D03-运行时间累积重置*)"]
["304.0","验证通过","REAL","排烟机","L","B1D03","运行时间累积重置值","排烟机B1D03-运行时间累积重置值",{"$f":"E66&VLOOKUP(D66,list!$D$3:$F$501,2,FALSE)&F66&\"_\"&VLOOKUP(G66,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D03_RSTV"},"LESFB1D03_RSTV AT%M304.0 :REAL; (*排烟机B1D03-运行时间累积重置值*)","LESFB1D03_RSTV          AT%M304.0      :REAL; (*排烟机B1D03-运行时间累积重置值*)"]
["308.0","验证通过","REAL","排烟机","L","B1D03","运行时间累积值","排烟机B1D03-运行时间累积值",{"$f":"E67&VLOOKUP(D67,list!$D$3:$F$501,2,FALSE)&F67&\"_\"&VLOOKUP(G67,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D03_RH"},"LESFB1D03_RH AT%M308.0 :REAL; (*排烟机B1D03-运行时间累积值*)","LESFB1D03_RH            AT%M308.0      :REAL; (*排烟机B1D03-运行时间累积值*)"]
["312.0","验证通过","BOOL","排烟机","L","B1D03","定时模式","排烟机B1D03-定时模式",{"$f":"E68&VLOOKUP(D68,list!$D$3:$F$501,2,FALSE)&F68&\"_\"&VLOOKUP(G68,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D03_TM"},"LESFB1D03_TM AT%M312.0 :BOOL; (*排烟机B1D03-定时模式*)","LESFB1D03_TM            AT%M312.0      :BOOL; (*排烟机B1D03-定时模式*)"]
["314.0","验证通过","BOOL","排烟机","L","B1D03","定时控制","排烟机B1D03-定时控制",{"$f":"E69&VLOOKUP(D69,list!$D$3:$F$501,2,FALSE)&F69&\"_\"&VLOOKUP(G69,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D03_TC"},"LESFB1D03_TC AT%M314.0 :BOOL; (*排烟机B1D03-定时控制*)","LESFB1D03_TC            AT%M314.0      :BOOL; (*排烟机B1D03-定时控制*)"]
["316.0","验证通过","BOOL","排烟机","L","B1D03","全天候模式","排烟机B1D03-全天候模式",{"$f":"E70&VLOOKUP(D70,list!$D$3:$F$501,2,FALSE)&F70&\"_\"&VLOOKUP(G70,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D03_DM"},"LESFB1D03_DM AT%M316.0 :BOOL; (*排烟机B1D03-全天候模式*)","LESFB1D03_DM            AT%M316.0      :BOOL; (*排烟机B1D03-全天候模式*)"]
["320.0","验证通过","REAL","排烟机","L","B1D03","CO设定值","排烟机B1D03-CO设定值",{"$f":"E71&VLOOKUP(D71,list!$D$3:$F$501,2,FALSE)&F71&\"_\"&VLOOKUP(G71,list!$I$2:$K$502,2,FALSE)","v":"LESFB1D03_COSET"},"LESFB1D03_COSET AT%M320.0 :REAL; (*排烟机B1D03-CO设定值*)","LESFB1D03_COSET         AT%M320.0      :REAL; (*排烟机B1D03-CO设定值*)"]
["CO"]
[{"$f":"IF(OR(C71=\"REAL\",C71=\"DWORD\",C71=\"DINT\"),(IF(OR(C73=\"REAL\",C73=\"DWORD\",C73=\"DINT\"),A71+4+MOD(A71,4),A71+4)),(IF(OR(C73=\"REAL\",C73=\"DWORD\",C73=\"DINT\"),A71+4+MOD(A71,4),A71+2)))&\".0\"","v":"324.0"},{"$f":"IF((IF(OR(C73=\"INT\",C73=\"WORD\",C73=\"BOOL\"),MOD(A73,2),MOD(A73,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","室内环境状态","L","B1D01","一氧化碳浓度换算值",{"$f":"D73&F73&\"-\"&IF(E73=\"R\",\"新云平台\"&G73,G73)","v":"室内环境状态B1D01-一氧化碳浓度换算值"},{"$f":"E73&VLOOKUP(D73,list!$D$3:$F$501,2,FALSE)&F73&\"_\"&VLOOKUP(G73,list!$I$2:$K$502,2,FALSE)","v":"LIESB1D01_COS"},{"$f":"I73&\" \"&\"AT%M\"&A73&\" \"&\":\"&C73&\";\"&\" \"&\"(*\"&H73&\"*)\"","v":"LIESB1D01_COS AT%M324.0 :REAL; (*室内环境状态B1D01-一氧化碳浓度换算值*)"},{"$f":"REPLACE(REPLACE(J73,SEARCH(\"AT%\",J73),,REPT(\" \",25-SEARCH(\"AT%\",J73))),SEARCH(\":\",REPLACE(J73,SEARCH(\"AT%\",J73),,REPT(\" \",25-SEARCH(\"AT%\",J73)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J73,SEARCH(\"AT%\",J73),,REPT(\" \",25-SEARCH(\"AT%\",J73))))))","v":"LIESB1D01_COS           AT%M324.0      :REAL; (*室内环境状态B1D01-一氧化碳浓度换算值*)"}]
[{"$f":"IF(OR(C73=\"REAL\",C73=\"DWORD\",C73=\"DINT\"),(IF(OR(C74=\"REAL\",C74=\"DWORD\",C74=\"DINT\"),A73+4+MOD(A73,4),A73+4)),(IF(OR(C74=\"REAL\",C74=\"DWORD\",C74=\"DINT\"),A73+4+MOD(A73,4),A73+2)))&\".0\"","v":"328.0"},{"$f":"IF((IF(OR(C74=\"INT\",C74=\"WORD\",C74=\"BOOL\"),MOD(A74,2),MOD(A74,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","室内环境状态","L","B1D02","一氧化碳浓度换算值",{"$f":"D74&F74&\"-\"&IF(E74=\"R\",\"新云平台\"&G74,G74)","v":"室内环境状态B1D02-一氧化碳浓度换算值"},{"$f":"E74&VLOOKUP(D74,list!$D$3:$F$501,2,FALSE)&F74&\"_\"&VLOOKUP(G74,list!$I$2:$K$502,2,FALSE)","v":"LIESB1D02_COS"},{"$f":"I74&\" \"&\"AT%M\"&A74&\" \"&\":\"&C74&\";\"&\" \"&\"(*\"&H74&\"*)\"","v":"LIESB1D02_COS AT%M328.0 :REAL; (*室内环境状态B1D02-一氧化碳浓度换算值*)"},{"$f":"REPLACE(REPLACE(J74,SEARCH(\"AT%\",J74),,REPT(\" \",25-SEARCH(\"AT%\",J74))),SEARCH(\":\",REPLACE(J74,SEARCH(\"AT%\",J74),,REPT(\" \",25-SEARCH(\"AT%\",J74)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J74,SEARCH(\"AT%\",J74),,REPT(\" \",25-SEARCH(\"AT%\",J74))))))","v":"LIESB1D02_COS           AT%M328.0      :REAL; (*室内环境状态B1D02-一氧化碳浓度换算值*)"}]
["SWP"]
[{"$f":"IF(OR(C74=\"REAL\",C74=\"DWORD\",C74=\"DINT\"),(IF(OR(C76=\"REAL\",C76=\"DWORD\",C76=\"DINT\"),A74+4+MOD(A74,4),A74+4)),(IF(OR(C76=\"REAL\",C76=\"DWORD\",C76=\"DINT\"),A74+4+MOD(A74,4),A74+2)))&\".0\"","v":"332.0"},{"$f":"IF((IF(OR(C76=\"INT\",C76=\"WORD\",C76=\"BOOL\"),MOD(A76,2),MOD(A76,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","潜污泵井","L","B1A01","运行时间累积重置1",{"$f":"D76&F76&\"-\"&IF(E76=\"R\",\"新云平台\"&G76,G76)","v":"潜污泵井B1A01-运行时间累积重置1"},{"$f":"E76&VLOOKUP(D76,list!$D$3:$F$501,2,FALSE)&F76&\"_\"&VLOOKUP(G76,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1A01_RST1"},{"$f":"I76&\" \"&\"AT%M\"&A76&\" \"&\":\"&C76&\";\"&\" \"&\"(*\"&H76&\"*)\"","v":"LSWPB1A01_RST1 AT%M332.0 :BOOL; (*潜污泵井B1A01-运行时间累积重置1*)"},{"$f":"REPLACE(REPLACE(J76,SEARCH(\"AT%\",J76),,REPT(\" \",25-SEARCH(\"AT%\",J76))),SEARCH(\":\",REPLACE(J76,SEARCH(\"AT%\",J76),,REPT(\" \",25-SEARCH(\"AT%\",J76)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J76,SEARCH(\"AT%\",J76),,REPT(\" \",25-SEARCH(\"AT%\",J76))))))","v":"LSWPB1A01_RST1          AT%M332.0      :BOOL; (*潜污泵井B1A01-运行时间累积重置1*)"}]
[{"$f":"IF(OR(C76=\"REAL\",C76=\"DWORD\",C76=\"DINT\"),(IF(OR(C77=\"REAL\",C77=\"DWORD\",C77=\"DINT\"),A76+4+MOD(A76,4),A76+4)),(IF(OR(C77=\"REAL\",C77=\"DWORD\",C77=\"DINT\"),A76+4+MOD(A76,4),A76+2)))&\".0\"","v":"336.0"},"验证通过","REAL","潜污泵井","L",{"$f":"F76","v":"B1A01"},"运行时间累积重置值1","潜污泵井B1A01-运行时间累积重置值1",{"$f":"E77&VLOOKUP(D77,list!$D$3:$F$501,2,FALSE)&F77&\"_\"&VLOOKUP(G77,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1A01_RSTV1"},"LSWPB1A01_RSTV1 AT%M336.0 :REAL; (*潜污泵井B1A01-运行时间累积重置值1*)","LSWPB1A01_RSTV1         AT%M336.0      :REAL; (*潜污泵井B1A01-运行时间累积重置值1*)"]
["340.0","验证通过","REAL","潜污泵井","L","B1A01","运行时间累积值1","潜污泵井B1A01-运行时间累积值1",{"$f":"E78&VLOOKUP(D78,list!$D$3:$F$501,2,FALSE)&F78&\"_\"&VLOOKUP(G78,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1A01_RH1"},"LSWPB1A01_RH1 AT%M340.0 :REAL; (*潜污泵井B1A01-运行时间累积值1*)","LSWPB1A01_RH1           AT%M340.0      :REAL; (*潜污泵井B1A01-运行时间累积值1*)"]
["344.0","验证通过","BOOL","潜污泵井","L","B1A01","运行时间累积重置2","潜污泵井B1A01-运行时间累积重置2",{"$f":"E79&VLOOKUP(D79,list!$D$3:$F$501,2,FALSE)&F79&\"_\"&VLOOKUP(G79,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1A01_RST2"},"LSWPB1A01_RST2 AT%M344.0 :BOOL; (*潜污泵井B1A01-运行时间累积重置2*)","LSWPB1A01_RST2          AT%M344.0      :BOOL; (*潜污泵井B1A01-运行时间累积重置2*)"]
["348.0","验证通过","REAL","潜污泵井","L","B1A01","运行时间累积重置值2","潜污泵井B1A01-运行时间累积重置值2",{"$f":"E80&VLOOKUP(D80,list!$D$3:$F$501,2,FALSE)&F80&\"_\"&VLOOKUP(G80,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1A01_RSTV2"},"LSWPB1A01_RSTV2 AT%M348.0 :REAL; (*潜污泵井B1A01-运行时间累积重置值2*)","LSWPB1A01_RSTV2         AT%M348.0      :REAL; (*潜污泵井B1A01-运行时间累积重置值2*)"]
["352.0","验证通过","REAL","潜污泵井","L","B1A01","运行时间累积值2","潜污泵井B1A01-运行时间累积值2",{"$f":"E81&VLOOKUP(D81,list!$D$3:$F$501,2,FALSE)&F81&\"_\"&VLOOKUP(G81,list!$I$2:$K$502,2,FALSE)","v":"LSWPB1A01_RH2"},"LSWPB1A01_RH2 AT%M352.0 :REAL; (*潜污泵井B1A01-运行时间累积值2*)","LSWPB1A01_RH2           AT%M352.0      :REAL; (*潜污泵井B1A01-运行时间累积值2*)"]
["EAF"]
[{"$f":"IF(OR(C81=\"REAL\",C81=\"DWORD\",C81=\"DINT\"),(IF(OR(C83=\"REAL\",C83=\"DWORD\",C83=\"DINT\"),A81+4+MOD(A81,4),A81+4)),(IF(OR(C83=\"REAL\",C83=\"DWORD\",C83=\"DINT\"),A81+4+MOD(A81,4),A81+2)))&\".0\"","v":"356.0"},{"$f":"IF((IF(OR(C83=\"INT\",C83=\"WORD\",C83=\"BOOL\"),MOD(A83,2),MOD(A83,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","B1A01","启停控制",{"$f":"D83&F83&\"-\"&IF(E83=\"R\",\"新云平台\"&G83,G83)","v":"排风机B1A01-新云平台启停控制"},{"$f":"E83&VLOOKUP(D83,list!$D$3:$F$501,2,FALSE)&F83&\"_\"&VLOOKUP(G83,list!$I$2:$K$502,2,FALSE)","v":"REAFB1A01_C"},{"$f":"I83&\" \"&\"AT%M\"&A83&\" \"&\":\"&C83&\";\"&\" \"&\"(*\"&H83&\"*)\"","v":"REAFB1A01_C AT%M356.0 :BOOL; (*排风机B1A01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J83,SEARCH(\"AT%\",J83),,REPT(\" \",25-SEARCH(\"AT%\",J83))),SEARCH(\":\",REPLACE(J83,SEARCH(\"AT%\",J83),,REPT(\" \",25-SEARCH(\"AT%\",J83)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J83,SEARCH(\"AT%\",J83),,REPT(\" \",25-SEARCH(\"AT%\",J83))))))","v":"REAFB1A01_C             AT%M356.0      :BOOL; (*排风机B1A01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C83=\"REAL\",C83=\"DWORD\",C83=\"DINT\"),(IF(OR(C84=\"REAL\",C84=\"DWORD\",C84=\"DINT\"),A83+4+MOD(A83,4),A83+4)),(IF(OR(C84=\"REAL\",C84=\"DWORD\",C84=\"DINT\"),A83+4+MOD(A83,4),A83+2)))&\".0\"","v":"358.0"},"验证通过","BOOL","排风机","L",{"$f":"F83","v":"B1A01"},"运行时间累积重置","排风机B1A01-运行时间累积重置",{"$f":"E84&VLOOKUP(D84,list!$D$3:$F$501,2,FALSE)&F84&\"_\"&VLOOKUP(G84,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A01_RST"},"LEAFB1A01_RST AT%M358.0 :BOOL; (*排风机B1A01-运行时间累积重置*)","LEAFB1A01_RST           AT%M358.0      :BOOL; (*排风机B1A01-运行时间累积重置*)"]
["364.0","验证通过","REAL","排风机","L","B1A01","运行时间累积重置值","排风机B1A01-运行时间累积重置值",{"$f":"E85&VLOOKUP(D85,list!$D$3:$F$501,2,FALSE)&F85&\"_\"&VLOOKUP(G85,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A01_RSTV"},"LEAFB1A01_RSTV AT%M364.0 :REAL; (*排风机B1A01-运行时间累积重置值*)","LEAFB1A01_RSTV          AT%M364.0      :REAL; (*排风机B1A01-运行时间累积重置值*)"]
["368.0","验证通过","REAL","排风机","L","B1A01","运行时间累积值","排风机B1A01-运行时间累积值",{"$f":"E86&VLOOKUP(D86,list!$D$3:$F$501,2,FALSE)&F86&\"_\"&VLOOKUP(G86,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A01_RH"},"LEAFB1A01_RH AT%M368.0 :REAL; (*排风机B1A01-运行时间累积值*)","LEAFB1A01_RH            AT%M368.0      :REAL; (*排风机B1A01-运行时间累积值*)"]
["372.0","验证通过","BOOL","排风机","L","B1A01","定时模式","排风机B1A01-定时模式",{"$f":"E87&VLOOKUP(D87,list!$D$3:$F$501,2,FALSE)&F87&\"_\"&VLOOKUP(G87,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A01_TM"},"LEAFB1A01_TM AT%M372.0 :BOOL; (*排风机B1A01-定时模式*)","LEAFB1A01_TM            AT%M372.0      :BOOL; (*排风机B1A01-定时模式*)"]
["374.0","验证通过","BOOL","排风机","L","B1A01","定时控制","排风机B1A01-定时控制",{"$f":"E88&VLOOKUP(D88,list!$D$3:$F$501,2,FALSE)&F88&\"_\"&VLOOKUP(G88,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A01_TC"},"LEAFB1A01_TC AT%M374.0 :BOOL; (*排风机B1A01-定时控制*)","LEAFB1A01_TC            AT%M374.0      :BOOL; (*排风机B1A01-定时控制*)"]
["376.0","验证通过","BOOL","排风机","L","B1A01","全天候模式","排风机B1A01-全天候模式",{"$f":"E89&VLOOKUP(D89,list!$D$3:$F$501,2,FALSE)&F89&\"_\"&VLOOKUP(G89,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A01_DM"},"LEAFB1A01_DM AT%M376.0 :BOOL; (*排风机B1A01-全天候模式*)","LEAFB1A01_DM            AT%M376.0      :BOOL; (*排风机B1A01-全天候模式*)"]
["380.0","验证通过","REAL","排风机","L","B1A01","CO设定值","排风机B1A01-CO设定值",{"$f":"E90&VLOOKUP(D90,list!$D$3:$F$501,2,FALSE)&F90&\"_\"&VLOOKUP(G90,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A01_COSET"},"LEAFB1A01_COSET AT%M380.0 :REAL; (*排风机B1A01-CO设定值*)","LEAFB1A01_COSET         AT%M380.0      :REAL; (*排风机B1A01-CO设定值*)"]
["EAF"]
[{"$f":"IF(OR(C90=\"REAL\",C90=\"DWORD\",C90=\"DINT\"),(IF(OR(C92=\"REAL\",C92=\"DWORD\",C92=\"DINT\"),A90+4+MOD(A90,4),A90+4)),(IF(OR(C92=\"REAL\",C92=\"DWORD\",C92=\"DINT\"),A90+4+MOD(A90,4),A90+2)))&\".0\"","v":"384.0"},{"$f":"IF((IF(OR(C92=\"INT\",C92=\"WORD\",C92=\"BOOL\"),MOD(A92,2),MOD(A92,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","B1A02","启停控制",{"$f":"D92&F92&\"-\"&IF(E92=\"R\",\"新云平台\"&G92,G92)","v":"排风机B1A02-新云平台启停控制"},{"$f":"E92&VLOOKUP(D92,list!$D$3:$F$501,2,FALSE)&F92&\"_\"&VLOOKUP(G92,list!$I$2:$K$502,2,FALSE)","v":"REAFB1A02_C"},{"$f":"I92&\" \"&\"AT%M\"&A92&\" \"&\":\"&C92&\";\"&\" \"&\"(*\"&H92&\"*)\"","v":"REAFB1A02_C AT%M384.0 :BOOL; (*排风机B1A02-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J92,SEARCH(\"AT%\",J92),,REPT(\" \",25-SEARCH(\"AT%\",J92))),SEARCH(\":\",REPLACE(J92,SEARCH(\"AT%\",J92),,REPT(\" \",25-SEARCH(\"AT%\",J92)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J92,SEARCH(\"AT%\",J92),,REPT(\" \",25-SEARCH(\"AT%\",J92))))))","v":"REAFB1A02_C             AT%M384.0      :BOOL; (*排风机B1A02-新云平台启停控制*)"}]
[{"$f":"IF(OR(C92=\"REAL\",C92=\"DWORD\",C92=\"DINT\"),(IF(OR(C93=\"REAL\",C93=\"DWORD\",C93=\"DINT\"),A92+4+MOD(A92,4),A92+4)),(IF(OR(C93=\"REAL\",C93=\"DWORD\",C93=\"DINT\"),A92+4+MOD(A92,4),A92+2)))&\".0\"","v":"386.0"},"验证通过","BOOL","排风机","L",{"$f":"F92","v":"B1A02"},"运行时间累积重置","排风机B1A02-运行时间累积重置",{"$f":"E93&VLOOKUP(D93,list!$D$3:$F$501,2,FALSE)&F93&\"_\"&VLOOKUP(G93,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A02_RST"},"LEAFB1A02_RST AT%M386.0 :BOOL; (*排风机B1A02-运行时间累积重置*)","LEAFB1A02_RST           AT%M386.0      :BOOL; (*排风机B1A02-运行时间累积重置*)"]
["392.0","验证通过","REAL","排风机","L","B1A02","运行时间累积重置值","排风机B1A02-运行时间累积重置值",{"$f":"E94&VLOOKUP(D94,list!$D$3:$F$501,2,FALSE)&F94&\"_\"&VLOOKUP(G94,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A02_RSTV"},"LEAFB1A02_RSTV AT%M392.0 :REAL; (*排风机B1A02-运行时间累积重置值*)","LEAFB1A02_RSTV          AT%M392.0      :REAL; (*排风机B1A02-运行时间累积重置值*)"]
["396.0","验证通过","REAL","排风机","L","B1A02","运行时间累积值","排风机B1A02-运行时间累积值",{"$f":"E95&VLOOKUP(D95,list!$D$3:$F$501,2,FALSE)&F95&\"_\"&VLOOKUP(G95,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A02_RH"},"LEAFB1A02_RH AT%M396.0 :REAL; (*排风机B1A02-运行时间累积值*)","LEAFB1A02_RH            AT%M396.0      :REAL; (*排风机B1A02-运行时间累积值*)"]
["400.0","验证通过","BOOL","排风机","L","B1A02","定时模式","排风机B1A02-定时模式",{"$f":"E96&VLOOKUP(D96,list!$D$3:$F$501,2,FALSE)&F96&\"_\"&VLOOKUP(G96,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A02_TM"},"LEAFB1A02_TM AT%M400.0 :BOOL; (*排风机B1A02-定时模式*)","LEAFB1A02_TM            AT%M400.0      :BOOL; (*排风机B1A02-定时模式*)"]
["402.0","验证通过","BOOL","排风机","L","B1A02","定时控制","排风机B1A02-定时控制",{"$f":"E97&VLOOKUP(D97,list!$D$3:$F$501,2,FALSE)&F97&\"_\"&VLOOKUP(G97,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A02_TC"},"LEAFB1A02_TC AT%M402.0 :BOOL; (*排风机B1A02-定时控制*)","LEAFB1A02_TC            AT%M402.0      :BOOL; (*排风机B1A02-定时控制*)"]
["404.0","验证通过","BOOL","排风机","L","B1A02","全天候模式","排风机B1A02-全天候模式",{"$f":"E98&VLOOKUP(D98,list!$D$3:$F$501,2,FALSE)&F98&\"_\"&VLOOKUP(G98,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A02_DM"},"LEAFB1A02_DM AT%M404.0 :BOOL; (*排风机B1A02-全天候模式*)","LEAFB1A02_DM            AT%M404.0      :BOOL; (*排风机B1A02-全天候模式*)"]
["408.0","验证通过","REAL","排风机","L","B1A02","CO设定值","排风机B1A02-CO设定值",{"$f":"E99&VLOOKUP(D99,list!$D$3:$F$501,2,FALSE)&F99&\"_\"&VLOOKUP(G99,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A02_COSET"},"LEAFB1A02_COSET AT%M408.0 :REAL; (*排风机B1A02-CO设定值*)","LEAFB1A02_COSET         AT%M408.0      :REAL; (*排风机B1A02-CO设定值*)"]
["EAF"]
[{"$f":"IF(OR(C99=\"REAL\",C99=\"DWORD\",C99=\"DINT\"),(IF(OR(C101=\"REAL\",C101=\"DWORD\",C101=\"DINT\"),A99+4+MOD(A99,4),A99+4)),(IF(OR(C101=\"REAL\",C101=\"DWORD\",C101=\"DINT\"),A99+4+MOD(A99,4),A99+2)))&\".0\"","v":"412.0"},{"$f":"IF((IF(OR(C101=\"INT\",C101=\"WORD\",C101=\"BOOL\"),MOD(A101,2),MOD(A101,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","B1A03","启停控制",{"$f":"D101&F101&\"-\"&IF(E101=\"R\",\"新云平台\"&G101,G101)","v":"排风机B1A03-新云平台启停控制"},{"$f":"E101&VLOOKUP(D101,list!$D$3:$F$501,2,FALSE)&F101&\"_\"&VLOOKUP(G101,list!$I$2:$K$502,2,FALSE)","v":"REAFB1A03_C"},{"$f":"I101&\" \"&\"AT%M\"&A101&\" \"&\":\"&C101&\";\"&\" \"&\"(*\"&H101&\"*)\"","v":"REAFB1A03_C AT%M412.0 :BOOL; (*排风机B1A03-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J101,SEARCH(\"AT%\",J101),,REPT(\" \",25-SEARCH(\"AT%\",J101))),SEARCH(\":\",REPLACE(J101,SEARCH(\"AT%\",J101),,REPT(\" \",25-SEARCH(\"AT%\",J101)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J101,SEARCH(\"AT%\",J101),,REPT(\" \",25-SEARCH(\"AT%\",J101))))))","v":"REAFB1A03_C             AT%M412.0      :BOOL; (*排风机B1A03-新云平台启停控制*)"}]
[{"$f":"IF(OR(C101=\"REAL\",C101=\"DWORD\",C101=\"DINT\"),(IF(OR(C102=\"REAL\",C102=\"DWORD\",C102=\"DINT\"),A101+4+MOD(A101,4),A101+4)),(IF(OR(C102=\"REAL\",C102=\"DWORD\",C102=\"DINT\"),A101+4+MOD(A101,4),A101+2)))&\".0\"","v":"414.0"},"验证通过","BOOL","排风机","L",{"$f":"F101","v":"B1A03"},"运行时间累积重置","排风机B1A03-运行时间累积重置",{"$f":"E102&VLOOKUP(D102,list!$D$3:$F$501,2,FALSE)&F102&\"_\"&VLOOKUP(G102,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A03_RST"},"LEAFB1A03_RST AT%M414.0 :BOOL; (*排风机B1A03-运行时间累积重置*)","LEAFB1A03_RST           AT%M414.0      :BOOL; (*排风机B1A03-运行时间累积重置*)"]
["420.0","验证通过","REAL","排风机","L","B1A03","运行时间累积重置值","排风机B1A03-运行时间累积重置值",{"$f":"E103&VLOOKUP(D103,list!$D$3:$F$501,2,FALSE)&F103&\"_\"&VLOOKUP(G103,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A03_RSTV"},"LEAFB1A03_RSTV AT%M420.0 :REAL; (*排风机B1A03-运行时间累积重置值*)","LEAFB1A03_RSTV          AT%M420.0      :REAL; (*排风机B1A03-运行时间累积重置值*)"]
["424.0","验证通过","REAL","排风机","L","B1A03","运行时间累积值","排风机B1A03-运行时间累积值",{"$f":"E104&VLOOKUP(D104,list!$D$3:$F$501,2,FALSE)&F104&\"_\"&VLOOKUP(G104,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A03_RH"},"LEAFB1A03_RH AT%M424.0 :REAL; (*排风机B1A03-运行时间累积值*)","LEAFB1A03_RH            AT%M424.0      :REAL; (*排风机B1A03-运行时间累积值*)"]
["428.0","验证通过","BOOL","排风机","L","B1A03","定时模式","排风机B1A03-定时模式",{"$f":"E105&VLOOKUP(D105,list!$D$3:$F$501,2,FALSE)&F105&\"_\"&VLOOKUP(G105,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A03_TM"},"LEAFB1A03_TM AT%M428.0 :BOOL; (*排风机B1A03-定时模式*)","LEAFB1A03_TM            AT%M428.0      :BOOL; (*排风机B1A03-定时模式*)"]
["430.0","验证通过","BOOL","排风机","L","B1A03","定时控制","排风机B1A03-定时控制",{"$f":"E106&VLOOKUP(D106,list!$D$3:$F$501,2,FALSE)&F106&\"_\"&VLOOKUP(G106,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A03_TC"},"LEAFB1A03_TC AT%M430.0 :BOOL; (*排风机B1A03-定时控制*)","LEAFB1A03_TC            AT%M430.0      :BOOL; (*排风机B1A03-定时控制*)"]
["432.0","验证通过","BOOL","排风机","L","B1A03","全天候模式","排风机B1A03-全天候模式",{"$f":"E107&VLOOKUP(D107,list!$D$3:$F$501,2,FALSE)&F107&\"_\"&VLOOKUP(G107,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A03_DM"},"LEAFB1A03_DM AT%M432.0 :BOOL; (*排风机B1A03-全天候模式*)","LEAFB1A03_DM            AT%M432.0      :BOOL; (*排风机B1A03-全天候模式*)"]
["436.0","验证通过","REAL","排风机","L","B1A03","CO设定值","排风机B1A03-CO设定值",{"$f":"E108&VLOOKUP(D108,list!$D$3:$F$501,2,FALSE)&F108&\"_\"&VLOOKUP(G108,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A03_COSET"},"LEAFB1A03_COSET AT%M436.0 :REAL; (*排风机B1A03-CO设定值*)","LEAFB1A03_COSET         AT%M436.0      :REAL; (*排风机B1A03-CO设定值*)"]
["EAF"]
[{"$f":"IF(OR(C108=\"REAL\",C108=\"DWORD\",C108=\"DINT\"),(IF(OR(C110=\"REAL\",C110=\"DWORD\",C110=\"DINT\"),A108+4+MOD(A108,4),A108+4)),(IF(OR(C110=\"REAL\",C110=\"DWORD\",C110=\"DINT\"),A108+4+MOD(A108,4),A108+2)))&\".0\"","v":"440.0"},{"$f":"IF((IF(OR(C110=\"INT\",C110=\"WORD\",C110=\"BOOL\"),MOD(A110,2),MOD(A110,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","B1A04","启停控制",{"$f":"D110&F110&\"-\"&IF(E110=\"R\",\"新云平台\"&G110,G110)","v":"排风机B1A04-新云平台启停控制"},{"$f":"E110&VLOOKUP(D110,list!$D$3:$F$501,2,FALSE)&F110&\"_\"&VLOOKUP(G110,list!$I$2:$K$502,2,FALSE)","v":"REAFB1A04_C"},{"$f":"I110&\" \"&\"AT%M\"&A110&\" \"&\":\"&C110&\";\"&\" \"&\"(*\"&H110&\"*)\"","v":"REAFB1A04_C AT%M440.0 :BOOL; (*排风机B1A04-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J110,SEARCH(\"AT%\",J110),,REPT(\" \",25-SEARCH(\"AT%\",J110))),SEARCH(\":\",REPLACE(J110,SEARCH(\"AT%\",J110),,REPT(\" \",25-SEARCH(\"AT%\",J110)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J110,SEARCH(\"AT%\",J110),,REPT(\" \",25-SEARCH(\"AT%\",J110))))))","v":"REAFB1A04_C             AT%M440.0      :BOOL; (*排风机B1A04-新云平台启停控制*)"}]
[{"$f":"IF(OR(C110=\"REAL\",C110=\"DWORD\",C110=\"DINT\"),(IF(OR(C111=\"REAL\",C111=\"DWORD\",C111=\"DINT\"),A110+4+MOD(A110,4),A110+4)),(IF(OR(C111=\"REAL\",C111=\"DWORD\",C111=\"DINT\"),A110+4+MOD(A110,4),A110+2)))&\".0\"","v":"442.0"},"验证通过","BOOL","排风机","L",{"$f":"F110","v":"B1A04"},"运行时间累积重置","排风机B1A04-运行时间累积重置",{"$f":"E111&VLOOKUP(D111,list!$D$3:$F$501,2,FALSE)&F111&\"_\"&VLOOKUP(G111,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A04_RST"},"LEAFB1A04_RST AT%M442.0 :BOOL; (*排风机B1A04-运行时间累积重置*)","LEAFB1A04_RST           AT%M442.0      :BOOL; (*排风机B1A04-运行时间累积重置*)"]
["448.0","验证通过","REAL","排风机","L","B1A04","运行时间累积重置值","排风机B1A04-运行时间累积重置值",{"$f":"E112&VLOOKUP(D112,list!$D$3:$F$501,2,FALSE)&F112&\"_\"&VLOOKUP(G112,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A04_RSTV"},"LEAFB1A04_RSTV AT%M448.0 :REAL; (*排风机B1A04-运行时间累积重置值*)","LEAFB1A04_RSTV          AT%M448.0      :REAL; (*排风机B1A04-运行时间累积重置值*)"]
["452.0","验证通过","REAL","排风机","L","B1A04","运行时间累积值","排风机B1A04-运行时间累积值",{"$f":"E113&VLOOKUP(D113,list!$D$3:$F$501,2,FALSE)&F113&\"_\"&VLOOKUP(G113,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A04_RH"},"LEAFB1A04_RH AT%M452.0 :REAL; (*排风机B1A04-运行时间累积值*)","LEAFB1A04_RH            AT%M452.0      :REAL; (*排风机B1A04-运行时间累积值*)"]
["456.0","验证通过","BOOL","排风机","L","B1A04","定时模式","排风机B1A04-定时模式",{"$f":"E114&VLOOKUP(D114,list!$D$3:$F$501,2,FALSE)&F114&\"_\"&VLOOKUP(G114,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A04_TM"},"LEAFB1A04_TM AT%M456.0 :BOOL; (*排风机B1A04-定时模式*)","LEAFB1A04_TM            AT%M456.0      :BOOL; (*排风机B1A04-定时模式*)"]
["458.0","验证通过","BOOL","排风机","L","B1A04","定时控制","排风机B1A04-定时控制",{"$f":"E115&VLOOKUP(D115,list!$D$3:$F$501,2,FALSE)&F115&\"_\"&VLOOKUP(G115,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A04_TC"},"LEAFB1A04_TC AT%M458.0 :BOOL; (*排风机B1A04-定时控制*)","LEAFB1A04_TC            AT%M458.0      :BOOL; (*排风机B1A04-定时控制*)"]
["460.0","验证通过","BOOL","排风机","L","B1A04","全天候模式","排风机B1A04-全天候模式",{"$f":"E116&VLOOKUP(D116,list!$D$3:$F$501,2,FALSE)&F116&\"_\"&VLOOKUP(G116,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A04_DM"},"LEAFB1A04_DM AT%M460.0 :BOOL; (*排风机B1A04-全天候模式*)","LEAFB1A04_DM            AT%M460.0      :BOOL; (*排风机B1A04-全天候模式*)"]
["464.0","验证通过","REAL","排风机","L","B1A04","CO设定值","排风机B1A04-CO设定值",{"$f":"E117&VLOOKUP(D117,list!$D$3:$F$501,2,FALSE)&F117&\"_\"&VLOOKUP(G117,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1A04_COSET"},"LEAFB1A04_COSET AT%M464.0 :REAL; (*排风机B1A04-CO设定值*)","LEAFB1A04_COSET         AT%M464.0      :REAL; (*排风机B1A04-CO设定值*)"]
["CO"]
[{"$f":"IF(OR(C117=\"REAL\",C117=\"DWORD\",C117=\"DINT\"),(IF(OR(C119=\"REAL\",C119=\"DWORD\",C119=\"DINT\"),A117+4+MOD(A117,4),A117+4)),(IF(OR(C119=\"REAL\",C119=\"DWORD\",C119=\"DINT\"),A117+4+MOD(A117,4),A117+2)))&\".0\"","v":"468.0"},{"$f":"IF((IF(OR(C119=\"INT\",C119=\"WORD\",C119=\"BOOL\"),MOD(A119,2),MOD(A119,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","室内环境状态","L","B1A01","一氧化碳浓度换算值",{"$f":"D119&F119&\"-\"&IF(E119=\"R\",\"新云平台\"&G119,G119)","v":"室内环境状态B1A01-一氧化碳浓度换算值"},{"$f":"E119&VLOOKUP(D119,list!$D$3:$F$501,2,FALSE)&F119&\"_\"&VLOOKUP(G119,list!$I$2:$K$502,2,FALSE)","v":"LIESB1A01_COS"},{"$f":"I119&\" \"&\"AT%M\"&A119&\" \"&\":\"&C119&\";\"&\" \"&\"(*\"&H119&\"*)\"","v":"LIESB1A01_COS AT%M468.0 :REAL; (*室内环境状态B1A01-一氧化碳浓度换算值*)"},{"$f":"REPLACE(REPLACE(J119,SEARCH(\"AT%\",J119),,REPT(\" \",25-SEARCH(\"AT%\",J119))),SEARCH(\":\",REPLACE(J119,SEARCH(\"AT%\",J119),,REPT(\" \",25-SEARCH(\"AT%\",J119)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J119,SEARCH(\"AT%\",J119),,REPT(\" \",25-SEARCH(\"AT%\",J119))))))","v":"LIESB1A01_COS           AT%M468.0      :REAL; (*室内环境状态B1A01-一氧化碳浓度换算值*)"}]
["EAF"]
[{"$f":"IF(OR(C119=\"REAL\",C119=\"DWORD\",C119=\"DINT\"),(IF(OR(C121=\"REAL\",C121=\"DWORD\",C121=\"DINT\"),A119+4+MOD(A119,4),A119+4)),(IF(OR(C121=\"REAL\",C121=\"DWORD\",C121=\"DINT\"),A119+4+MOD(A119,4),A119+2)))&\".0\"","v":"472.0"},{"$f":"IF((IF(OR(C121=\"INT\",C121=\"WORD\",C121=\"BOOL\"),MOD(A121,2),MOD(A121,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","B1F01","启停控制",{"$f":"D121&F121&\"-\"&IF(E121=\"R\",\"新云平台\"&G121,G121)","v":"排风机B1F01-新云平台启停控制"},{"$f":"E121&VLOOKUP(D121,list!$D$3:$F$501,2,FALSE)&F121&\"_\"&VLOOKUP(G121,list!$I$2:$K$502,2,FALSE)","v":"REAFB1F01_C"},{"$f":"I121&\" \"&\"AT%M\"&A121&\" \"&\":\"&C121&\";\"&\" \"&\"(*\"&H121&\"*)\"","v":"REAFB1F01_C AT%M472.0 :BOOL; (*排风机B1F01-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J121,SEARCH(\"AT%\",J121),,REPT(\" \",25-SEARCH(\"AT%\",J121))),SEARCH(\":\",REPLACE(J121,SEARCH(\"AT%\",J121),,REPT(\" \",25-SEARCH(\"AT%\",J121)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J121,SEARCH(\"AT%\",J121),,REPT(\" \",25-SEARCH(\"AT%\",J121))))))","v":"REAFB1F01_C             AT%M472.0      :BOOL; (*排风机B1F01-新云平台启停控制*)"}]
[{"$f":"IF(OR(C121=\"REAL\",C121=\"DWORD\",C121=\"DINT\"),(IF(OR(C122=\"REAL\",C122=\"DWORD\",C122=\"DINT\"),A121+4+MOD(A121,4),A121+4)),(IF(OR(C122=\"REAL\",C122=\"DWORD\",C122=\"DINT\"),A121+4+MOD(A121,4),A121+2)))&\".0\"","v":"474.0"},"验证通过","BOOL","排风机","L",{"$f":"F121","v":"B1F01"},"运行时间累积重置","排风机B1F01-运行时间累积重置",{"$f":"E122&VLOOKUP(D122,list!$D$3:$F$501,2,FALSE)&F122&\"_\"&VLOOKUP(G122,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F01_RST"},"LEAFB1F01_RST AT%M474.0 :BOOL; (*排风机B1F01-运行时间累积重置*)","LEAFB1F01_RST           AT%M474.0      :BOOL; (*排风机B1F01-运行时间累积重置*)"]
["480.0","验证通过","REAL","排风机","L","B1F01","运行时间累积重置值","排风机B1F01-运行时间累积重置值",{"$f":"E123&VLOOKUP(D123,list!$D$3:$F$501,2,FALSE)&F123&\"_\"&VLOOKUP(G123,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F01_RSTV"},"LEAFB1F01_RSTV AT%M480.0 :REAL; (*排风机B1F01-运行时间累积重置值*)","LEAFB1F01_RSTV          AT%M480.0      :REAL; (*排风机B1F01-运行时间累积重置值*)"]
["484.0","验证通过","REAL","排风机","L","B1F01","运行时间累积值","排风机B1F01-运行时间累积值",{"$f":"E124&VLOOKUP(D124,list!$D$3:$F$501,2,FALSE)&F124&\"_\"&VLOOKUP(G124,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F01_RH"},"LEAFB1F01_RH AT%M484.0 :REAL; (*排风机B1F01-运行时间累积值*)","LEAFB1F01_RH            AT%M484.0      :REAL; (*排风机B1F01-运行时间累积值*)"]
["488.0","验证通过","BOOL","排风机","L","B1F01","定时模式","排风机B1F01-定时模式",{"$f":"E125&VLOOKUP(D125,list!$D$3:$F$501,2,FALSE)&F125&\"_\"&VLOOKUP(G125,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F01_TM"},"LEAFB1F01_TM AT%M488.0 :BOOL; (*排风机B1F01-定时模式*)","LEAFB1F01_TM            AT%M488.0      :BOOL; (*排风机B1F01-定时模式*)"]
["490.0","验证通过","BOOL","排风机","L","B1F01","定时控制","排风机B1F01-定时控制",{"$f":"E126&VLOOKUP(D126,list!$D$3:$F$501,2,FALSE)&F126&\"_\"&VLOOKUP(G126,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F01_TC"},"LEAFB1F01_TC AT%M490.0 :BOOL; (*排风机B1F01-定时控制*)","LEAFB1F01_TC            AT%M490.0      :BOOL; (*排风机B1F01-定时控制*)"]
["492.0","验证通过","BOOL","排风机","L","B1F01","全天候模式","排风机B1F01-全天候模式",{"$f":"E127&VLOOKUP(D127,list!$D$3:$F$501,2,FALSE)&F127&\"_\"&VLOOKUP(G127,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F01_DM"},"LEAFB1F01_DM AT%M492.0 :BOOL; (*排风机B1F01-全天候模式*)","LEAFB1F01_DM            AT%M492.0      :BOOL; (*排风机B1F01-全天候模式*)"]
["496.0","验证通过","REAL","排风机","L","B1F01","CO设定值","排风机B1F01-CO设定值",{"$f":"E128&VLOOKUP(D128,list!$D$3:$F$501,2,FALSE)&F128&\"_\"&VLOOKUP(G128,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F01_COSET"},"LEAFB1F01_COSET AT%M496.0 :REAL; (*排风机B1F01-CO设定值*)","LEAFB1F01_COSET         AT%M496.0      :REAL; (*排风机B1F01-CO设定值*)"]
["EAF"]
[{"$f":"IF(OR(C128=\"REAL\",C128=\"DWORD\",C128=\"DINT\"),(IF(OR(C130=\"REAL\",C130=\"DWORD\",C130=\"DINT\"),A128+4+MOD(A128,4),A128+4)),(IF(OR(C130=\"REAL\",C130=\"DWORD\",C130=\"DINT\"),A128+4+MOD(A128,4),A128+2)))&\".0\"","v":"500.0"},{"$f":"IF((IF(OR(C130=\"INT\",C130=\"WORD\",C130=\"BOOL\"),MOD(A130,2),MOD(A130,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","B1F02","启停控制",{"$f":"D130&F130&\"-\"&IF(E130=\"R\",\"新云平台\"&G130,G130)","v":"排风机B1F02-新云平台启停控制"},{"$f":"E130&VLOOKUP(D130,list!$D$3:$F$501,2,FALSE)&F130&\"_\"&VLOOKUP(G130,list!$I$2:$K$502,2,FALSE)","v":"REAFB1F02_C"},{"$f":"I130&\" \"&\"AT%M\"&A130&\" \"&\":\"&C130&\";\"&\" \"&\"(*\"&H130&\"*)\"","v":"REAFB1F02_C AT%M500.0 :BOOL; (*排风机B1F02-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J130,SEARCH(\"AT%\",J130),,REPT(\" \",25-SEARCH(\"AT%\",J130))),SEARCH(\":\",REPLACE(J130,SEARCH(\"AT%\",J130),,REPT(\" \",25-SEARCH(\"AT%\",J130)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J130,SEARCH(\"AT%\",J130),,REPT(\" \",25-SEARCH(\"AT%\",J130))))))","v":"REAFB1F02_C             AT%M500.0      :BOOL; (*排风机B1F02-新云平台启停控制*)"}]
[{"$f":"IF(OR(C130=\"REAL\",C130=\"DWORD\",C130=\"DINT\"),(IF(OR(C131=\"REAL\",C131=\"DWORD\",C131=\"DINT\"),A130+4+MOD(A130,4),A130+4)),(IF(OR(C131=\"REAL\",C131=\"DWORD\",C131=\"DINT\"),A130+4+MOD(A130,4),A130+2)))&\".0\"","v":"502.0"},"验证通过","BOOL","排风机","L",{"$f":"F130","v":"B1F02"},"运行时间累积重置","排风机B1F02-运行时间累积重置",{"$f":"E131&VLOOKUP(D131,list!$D$3:$F$501,2,FALSE)&F131&\"_\"&VLOOKUP(G131,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F02_RST"},"LEAFB1F02_RST AT%M502.0 :BOOL; (*排风机B1F02-运行时间累积重置*)","LEAFB1F02_RST           AT%M502.0      :BOOL; (*排风机B1F02-运行时间累积重置*)"]
["508.0","验证通过","REAL","排风机","L","B1F02","运行时间累积重置值","排风机B1F02-运行时间累积重置值",{"$f":"E132&VLOOKUP(D132,list!$D$3:$F$501,2,FALSE)&F132&\"_\"&VLOOKUP(G132,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F02_RSTV"},"LEAFB1F02_RSTV AT%M508.0 :REAL; (*排风机B1F02-运行时间累积重置值*)","LEAFB1F02_RSTV          AT%M508.0      :REAL; (*排风机B1F02-运行时间累积重置值*)"]
["512.0","验证通过","REAL","排风机","L","B1F02","运行时间累积值","排风机B1F02-运行时间累积值",{"$f":"E133&VLOOKUP(D133,list!$D$3:$F$501,2,FALSE)&F133&\"_\"&VLOOKUP(G133,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F02_RH"},"LEAFB1F02_RH AT%M512.0 :REAL; (*排风机B1F02-运行时间累积值*)","LEAFB1F02_RH            AT%M512.0      :REAL; (*排风机B1F02-运行时间累积值*)"]
["516.0","验证通过","BOOL","排风机","L","B1F02","定时模式","排风机B1F02-定时模式",{"$f":"E134&VLOOKUP(D134,list!$D$3:$F$501,2,FALSE)&F134&\"_\"&VLOOKUP(G134,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F02_TM"},"LEAFB1F02_TM AT%M516.0 :BOOL; (*排风机B1F02-定时模式*)","LEAFB1F02_TM            AT%M516.0      :BOOL; (*排风机B1F02-定时模式*)"]
["518.0","验证通过","BOOL","排风机","L","B1F02","定时控制","排风机B1F02-定时控制",{"$f":"E135&VLOOKUP(D135,list!$D$3:$F$501,2,FALSE)&F135&\"_\"&VLOOKUP(G135,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F02_TC"},"LEAFB1F02_TC AT%M518.0 :BOOL; (*排风机B1F02-定时控制*)","LEAFB1F02_TC            AT%M518.0      :BOOL; (*排风机B1F02-定时控制*)"]
["520.0","验证通过","BOOL","排风机","L","B1F02","全天候模式","排风机B1F02-全天候模式",{"$f":"E136&VLOOKUP(D136,list!$D$3:$F$501,2,FALSE)&F136&\"_\"&VLOOKUP(G136,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F02_DM"},"LEAFB1F02_DM AT%M520.0 :BOOL; (*排风机B1F02-全天候模式*)","LEAFB1F02_DM            AT%M520.0      :BOOL; (*排风机B1F02-全天候模式*)"]
["524.0","验证通过","REAL","排风机","L","B1F02","CO设定值","排风机B1F02-CO设定值",{"$f":"E137&VLOOKUP(D137,list!$D$3:$F$501,2,FALSE)&F137&\"_\"&VLOOKUP(G137,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F02_COSET"},"LEAFB1F02_COSET AT%M524.0 :REAL; (*排风机B1F02-CO设定值*)","LEAFB1F02_COSET         AT%M524.0      :REAL; (*排风机B1F02-CO设定值*)"]
["EAF"]
[{"$f":"IF(OR(C137=\"REAL\",C137=\"DWORD\",C137=\"DINT\"),(IF(OR(C139=\"REAL\",C139=\"DWORD\",C139=\"DINT\"),A137+4+MOD(A137,4),A137+4)),(IF(OR(C139=\"REAL\",C139=\"DWORD\",C139=\"DINT\"),A137+4+MOD(A137,4),A137+2)))&\".0\"","v":"528.0"},{"$f":"IF((IF(OR(C139=\"INT\",C139=\"WORD\",C139=\"BOOL\"),MOD(A139,2),MOD(A139,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"BOOL","排风机","R","B1F03","启停控制",{"$f":"D139&F139&\"-\"&IF(E139=\"R\",\"新云平台\"&G139,G139)","v":"排风机B1F03-新云平台启停控制"},{"$f":"E139&VLOOKUP(D139,list!$D$3:$F$501,2,FALSE)&F139&\"_\"&VLOOKUP(G139,list!$I$2:$K$502,2,FALSE)","v":"REAFB1F03_C"},{"$f":"I139&\" \"&\"AT%M\"&A139&\" \"&\":\"&C139&\";\"&\" \"&\"(*\"&H139&\"*)\"","v":"REAFB1F03_C AT%M528.0 :BOOL; (*排风机B1F03-新云平台启停控制*)"},{"$f":"REPLACE(REPLACE(J139,SEARCH(\"AT%\",J139),,REPT(\" \",25-SEARCH(\"AT%\",J139))),SEARCH(\":\",REPLACE(J139,SEARCH(\"AT%\",J139),,REPT(\" \",25-SEARCH(\"AT%\",J139)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J139,SEARCH(\"AT%\",J139),,REPT(\" \",25-SEARCH(\"AT%\",J139))))))","v":"REAFB1F03_C             AT%M528.0      :BOOL; (*排风机B1F03-新云平台启停控制*)"}]
[{"$f":"IF(OR(C139=\"REAL\",C139=\"DWORD\",C139=\"DINT\"),(IF(OR(C140=\"REAL\",C140=\"DWORD\",C140=\"DINT\"),A139+4+MOD(A139,4),A139+4)),(IF(OR(C140=\"REAL\",C140=\"DWORD\",C140=\"DINT\"),A139+4+MOD(A139,4),A139+2)))&\".0\"","v":"530.0"},"验证通过","BOOL","排风机","L",{"$f":"F139","v":"B1F03"},"运行时间累积重置","排风机B1F03-运行时间累积重置",{"$f":"E140&VLOOKUP(D140,list!$D$3:$F$501,2,FALSE)&F140&\"_\"&VLOOKUP(G140,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F03_RST"},"LEAFB1F03_RST AT%M530.0 :BOOL; (*排风机B1F03-运行时间累积重置*)","LEAFB1F03_RST           AT%M530.0      :BOOL; (*排风机B1F03-运行时间累积重置*)"]
["536.0","验证通过","REAL","排风机","L","B1F03","运行时间累积重置值","排风机B1F03-运行时间累积重置值",{"$f":"E141&VLOOKUP(D141,list!$D$3:$F$501,2,FALSE)&F141&\"_\"&VLOOKUP(G141,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F03_RSTV"},"LEAFB1F03_RSTV AT%M536.0 :REAL; (*排风机B1F03-运行时间累积重置值*)","LEAFB1F03_RSTV          AT%M536.0      :REAL; (*排风机B1F03-运行时间累积重置值*)"]
["540.0","验证通过","REAL","排风机","L","B1F03","运行时间累积值","排风机B1F03-运行时间累积值",{"$f":"E142&VLOOKUP(D142,list!$D$3:$F$501,2,FALSE)&F142&\"_\"&VLOOKUP(G142,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F03_RH"},"LEAFB1F03_RH AT%M540.0 :REAL; (*排风机B1F03-运行时间累积值*)","LEAFB1F03_RH            AT%M540.0      :REAL; (*排风机B1F03-运行时间累积值*)"]
["544.0","验证通过","BOOL","排风机","L","B1F03","定时模式","排风机B1F03-定时模式",{"$f":"E143&VLOOKUP(D143,list!$D$3:$F$501,2,FALSE)&F143&\"_\"&VLOOKUP(G143,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F03_TM"},"LEAFB1F03_TM AT%M544.0 :BOOL; (*排风机B1F03-定时模式*)","LEAFB1F03_TM            AT%M544.0      :BOOL; (*排风机B1F03-定时模式*)"]
["546.0","验证通过","BOOL","排风机","L","B1F03","定时控制","排风机B1F03-定时控制",{"$f":"E144&VLOOKUP(D144,list!$D$3:$F$501,2,FALSE)&F144&\"_\"&VLOOKUP(G144,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F03_TC"},"LEAFB1F03_TC AT%M546.0 :BOOL; (*排风机B1F03-定时控制*)","LEAFB1F03_TC            AT%M546.0      :BOOL; (*排风机B1F03-定时控制*)"]
["548.0","验证通过","BOOL","排风机","L","B1F03","全天候模式","排风机B1F03-全天候模式",{"$f":"E145&VLOOKUP(D145,list!$D$3:$F$501,2,FALSE)&F145&\"_\"&VLOOKUP(G145,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F03_DM"},"LEAFB1F03_DM AT%M548.0 :BOOL; (*排风机B1F03-全天候模式*)","LEAFB1F03_DM            AT%M548.0      :BOOL; (*排风机B1F03-全天候模式*)"]
["552.0","验证通过","REAL","排风机","L","B1F03","CO设定值","排风机B1F03-CO设定值",{"$f":"E146&VLOOKUP(D146,list!$D$3:$F$501,2,FALSE)&F146&\"_\"&VLOOKUP(G146,list!$I$2:$K$502,2,FALSE)","v":"LEAFB1F03_COSET"},"LEAFB1F03_COSET AT%M552.0 :REAL; (*排风机B1F03-CO设定值*)","LEAFB1F03_COSET         AT%M552.0      :REAL; (*排风机B1F03-CO设定值*)"]
["CO"]
[{"$f":"IF(OR(C146=\"REAL\",C146=\"DWORD\",C146=\"DINT\"),(IF(OR(C148=\"REAL\",C148=\"DWORD\",C148=\"DINT\"),A146+4+MOD(A146,4),A146+4)),(IF(OR(C148=\"REAL\",C148=\"DWORD\",C148=\"DINT\"),A146+4+MOD(A146,4),A146+2)))&\".0\"","v":"556.0"},{"$f":"IF((IF(OR(C148=\"INT\",C148=\"WORD\",C148=\"BOOL\"),MOD(A148,2),MOD(A148,4)))=0,\"验证通过\",\"验证失败\")","v":"验证通过"},"REAL","室内环境状态","L","B1F01","一氧化碳浓度换算值",{"$f":"D148&F148&\"-\"&IF(E148=\"R\",\"新云平台\"&G148,G148)","v":"室内环境状态B1F01-一氧化碳浓度换算值"},{"$f":"E148&VLOOKUP(D148,list!$D$3:$F$501,2,FALSE)&F148&\"_\"&VLOOKUP(G148,list!$I$2:$K$502,2,FALSE)","v":"LIESB1F01_COS"},{"$f":"I148&\" \"&\"AT%M\"&A148&\" \"&\":\"&C148&\";\"&\" \"&\"(*\"&H148&\"*)\"","v":"LIESB1F01_COS AT%M556.0 :REAL; (*室内环境状态B1F01-一氧化碳浓度换算值*)"},{"$f":"REPLACE(REPLACE(J148,SEARCH(\"AT%\",J148),,REPT(\" \",25-SEARCH(\"AT%\",J148))),SEARCH(\":\",REPLACE(J148,SEARCH(\"AT%\",J148),,REPT(\" \",25-SEARCH(\"AT%\",J148)))),,REPT(\" \",40-SEARCH(\":\",REPLACE(J148,SEARCH(\"AT%\",J148),,REPT(\" \",25-SEARCH(\"AT%\",J148))))))","v":"LIESB1F01_COS           AT%M556.0      :REAL; (*室内环境状态B1F01-一氧化碳浓度换算值*)"}]

{"sheet":"新风机","index":5,"n_rows":66,"n_cols":18,"rows_kept":66,"cut":false,"hidden":false,"merged":[[2,1,6,1]]}
["编号","楼层","程序端声明",null,null,null,"    (********************************************PAU05I01********************************************)"]
["PAU05G01","PAU05X00",{"$f":"\"\"&A2&\"_IN :FAU_IN;\"","v":"PAU05G01_IN :FAU_IN;"},null,null,null,"    (*输入，类型，示值上限，示值下限，基准补偿，输出补偿*)"]
["LIES04C01_CO2S","CO2数量",{"$f":"\"\"&A2&\"_OUT:FAU_OUT;\"","v":"PAU05G01_OUT:FAU_OUT;"},null,null,null,"    PAU05I01_WVB_AVE(INPUT:=LPAU05I01_WVB);"]
["LIES05J02_CO2S",null,{"$f":"\"\"&A2&\"_SyncControl:IJ_LSyncControl;\"","v":"PAU05G01_SyncControl:IJ_LSyncControl;"},null,null,null,"    PAU05I01_ST_AVE (INPUT:=LPAU05I01_ST );"]
[null,null,{"$f":"\"\"&A2&\"_FAU:IJ_FAU;\"","v":"PAU05G01_FAU:IJ_FAU;"},null,null,null,"    LPAU05I01_STS :=            BS_Scale(PAU05I01_ST_AVE.Output ,1,0,100,0,0.0);"]
[null,null,{"$f":"\"\"&A2&\"_ST_AVE :BS_Average;\"","v":"PAU05G01_ST_AVE :BS_Average;"},null,null,null,"    LPAU05I01_WVBS:=            BS_Scale(PAU05I01_WVB_AVE.Output,2,0,100,0,0.0);"]
[null,null,{"$f":"\"\"&A2&\"_WVB_AVE:BS_Average;\"","v":"PAU05G01_WVB_AVE:BS_Average;"},null,null,null,"    LPAU05I01_WVC :=REAL_TO_INT(BS_Scale(LPAU05I01_WVCS         ,4,0,100,0,0.0));"]
[null,null,{"$f":"\"\"&A2&\"_SLG    :BS_SLG;\"","v":"PAU05G01_SLG    :BS_SLG;"},null,null,null,"    LPAU05I01_VFBS:=REAL_TO_INT(BS_Scale(LPAU05I01_VFB          ,2,0,50 ,0,0.0));"]
[null,null,{"$f":"\"L\"&A2&\"_CO2S:ARRAY[0..10] OF REAL;\"","v":"LPAU05G01_CO2S:ARRAY[0..10] OF REAL;"},null,null,null,"    LPAU05I01_VFC :=REAL_TO_INT(BS_Scale((LPAU05I01_VFCS*100)   ,4,0,50 ,0,0.0));"]
[null,null,{"$f":"\"L\"&A2&\"_LC  :ARRAY[0..10] OF BOOL;\"","v":"LPAU05G01_LC  :ARRAY[0..10] OF BOOL;"},null,null,null,"    (*主程序*)"]
[null,null,"程序",null,null,null,"    PAU05I01_FAU(FAU_STRUCT_IN:=PAU05I01_IN | PAU05I01_OUT:=FAU_STRUCT_OUT);"]
[null,null,{"$f":"\"    (********************************************\"&A2&\"********************************************)\"","v":"(********************************************PAU05G01********************************************)"},null,null,null,"    (*FAU_INSTRUCT*)"]
[null,null,"    (*输入，类型，示值上限，示值下限，基准补偿，输出补偿*)",null,null,null,"    PAU05I01_IN.SM     :=LPAU05I01_SM        ;"]
[null,null,{"$f":"\"    \"&A2&\"_WVB_AVE(INPUT:=L\"&A2&\"_WVB);\"","v":"PAU05G01_WVB_AVE(INPUT:=LPAU05G01_WVB);"},null,null,null,"    PAU05I01_IN.LM     :=LPAU05I01_LM        ;"]
[null,null,{"$f":"\"    \"&A2&\"_ST_AVE (INPUT:=L\"&A2&\"_ST );\"","v":"PAU05G01_ST_AVE (INPUT:=LPAU05G01_ST );"},null,null,null,"    PAU05I01_IN.Run    :=LPAU05I01_R         ;",{"$nulls":10},"   "]
[null,null,{"$f":"\"    L\"&A2&\"_STS :=            BS_Scale(\"&A2&\"_ST_AVE.Output ,1,0,100,0,0.0);\"","v":"LPAU05G01_STS :=            BS_Scale(PAU05G01_ST_AVE.Output ,1,0,100,0,0.0);"},null," ",null,"    PAU05I01_IN.Fault  :=LPAU05I01_F         ;"]
[null,null,{"$f":"\"    L\"&A2&\"_WVBS:=            BS_Scale(\"&A2&\"_WVB_AVE.Output,2,0,100,0,0.0);\"","v":"LPAU05G01_WVBS:=            BS_Scale(PAU05G01_WVB_AVE.Output,2,0,100,0,0.0);"}," ",null,null,"    PAU05I01_IN.Auto   :=LPAU05I01_A         ;"]
[null,null,{"$f":"\"    L\"&A2&\"_WVC :=REAL_TO_INT(BS_Scale(L\"&A2&\"_WVCS         ,4,0,100,0,0.0));\"","v":"LPAU05G01_WVC :=REAL_TO_INT(BS_Scale(LPAU05G01_WVCS         ,4,0,100,0,0.0));"}," ",null,null,"    PAU05I01_IN.ContRol:=LPAU05I01_PC        ;"]
[null,null,{"$f":"\"    L\"&A2&\"_VFBS:=REAL_TO_INT(BS_Scale(L\"&A2&\"_VFB          ,2,0,50 ,0,0.0));\"","v":"LPAU05G01_VFBS:=REAL_TO_INT(BS_Scale(LPAU05G01_VFB          ,2,0,50 ,0,0.0));"}," ",null,null,"    PAU05I01_IN.FDOB   :=LPAU05I01_FDOB       ;"]
[null,null,{"$f":"\"    L\"&A2&\"_VFC :=REAL_TO_INT(BS_Scale((L\"&A2&\"_VFCS*100)   ,4,0,50 ,0,0.0));\"","v":"LPAU05G01_VFC :=REAL_TO_INT(BS_Scale((LPAU05G01_VFCS*100)   ,4,0,50 ,0,0.0));"}," ",null,null,"    PAU05I01_IN.FDSB   :=LPAU05I01_FDSB       ;"]
[null,null,"    (*主程序*)",null,null,null,"    PAU05I01_IN.TSET   :=LPAU05I01_TSET      ;"]
[null,null,{"$f":"\"    \"&A2&\"_FAU(FAU_STRUCT_IN:=\"&A2&\"_IN | \"&A2&\"_OUT:=FAU_STRUCT_OUT);\"","v":"PAU05G01_FAU(FAU_STRUCT_IN:=PAU05G01_IN | PAU05G01_OUT:=FAU_STRUCT_OUT);"},null,null,null,"    PAU05I01_IN.WVMC   :=LPAU05I01_WVMC      ;"]
[null,null,"    (*FAU_INSTRUCT*)",null,null,null,"    PAU05I01_IN.WVMV   :=LPAU05I01_WVMV      ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.SM     :=L\"&A2&\"_SM        ;\"","v":"PAU05G01_IN.SM     :=LPAU05G01_SM        ;"},null,null,null,"    PAU05I01_IN.VFMV   :=LPAU05I01_VFMV      ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.LM     :=L\"&A2&\"_LM        ;\"","v":"PAU05G01_IN.LM     :=LPAU05G01_LM        ;"},null,null,null,"    PAU05I01_IN.STS    :=LPAU05I01_STS       ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.Run    :=L\"&A2&\"_R         ;\"","v":"PAU05G01_IN.Run    :=LPAU05G01_R         ;"},null,null,null,"    PAU05I01_IN.RST    :=LPAU05I01_RST       ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.Fault  :=L\"&A2&\"_F         ;\"","v":"PAU05G01_IN.Fault  :=LPAU05G01_F         ;"},null,null,null,"    PAU05I01_IN.RSTV   :=LPAU05I01_RSTV      ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.Auto   :=L\"&A2&\"_A         ;\"","v":"PAU05G01_IN.Auto   :=LPAU05G01_A         ;"},null,null,null,"    PAU05I01_IN.FPS    :=LPAU05I01_FPS       ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.ContRol:=L\"&A2&\"_PC        ;\"","v":"PAU05G01_IN.ContRol:=LPAU05G01_PC        ;"},null,null,null,"    PAU05I01_IN.IPS    :=LPAU05I01_IPS       ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.FDOB   :=L\"&A2&\"_FDOB       ;\"","v":"PAU05G01_IN.FDOB   :=LPAU05G01_FDOB       ;"},null,null,null,"    PAU05I01_IN.AFS    :=LPAU05I01_AFS       ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.FDSB   :=L\"&A2&\"_FDSB       ;\"","v":"PAU05G01_IN.FDSB   :=LPAU05G01_FDSB       ;"},null,null,null,"    PAU05I01_IN.ISO1   :=LPAU05I01_ISO1      ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.TSET   :=L\"&A2&\"_TSET      ;\"","v":"PAU05G01_IN.TSET   :=LPAU05G01_TSET      ;"},null,null,null,"    PAU05I01_IN.ISO2   :=LPAU05I01_ISO2      ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.WVMC   :=L\"&A2&\"_WVMC      ;\"","v":"PAU05G01_IN.WVMC   :=LPAU05G01_WVMC      ;"}," ",null,null,"    PAU05I01_IN.ISO3   :=LPAU05I01_ISO3      ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.WVMV   :=L\"&A2&\"_WVMV      ;\"","v":"PAU05G01_IN.WVMV   :=LPAU05G01_WVMV      ;"},null,null,null,"    PAU05I01_IN.VP     :=LPAU05I01_VP        ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.VFMV   :=L\"&A2&\"_VFMV      ;\"","v":"PAU05G01_IN.VFMV   :=LPAU05G01_VFMV      ;"},null,null,null,"    PAU05I01_IN.VI     :=LPAU05I01_VI        ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.STS    :=L\"&A2&\"_STS       ;\"","v":"PAU05G01_IN.STS    :=LPAU05G01_STS       ;"},null,null,null,"    PAU05I01_IN.FDELAY :=t#30s               ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.RST    :=L\"&A2&\"_RST       ;\"","v":"PAU05G01_IN.RST    :=LPAU05G01_RST       ;"},null,null,null,"    PAU05I01_IN.VDELAY :=t#120s              ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.RSTV   :=L\"&A2&\"_RSTV      ;\"","v":"PAU05G01_IN.RSTV   :=LPAU05G01_RSTV      ;"},null,null,null,"    (*FAU_OUTSTRUCT*)"]
[null,null,{"$f":"\"    \"&A2&\"_IN.FPS    :=L\"&A2&\"_FPS       ;\"","v":"PAU05G01_IN.FPS    :=LPAU05G01_FPS       ;"},null,null,null,"    LPAU05I01_WVCS     :=PAU05I01_OUT.WVCS   ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.IPS    :=L\"&A2&\"_IPS       ;\"","v":"PAU05G01_IN.IPS    :=LPAU05G01_IPS       ;"},null,null,null,"    LPAU05I01_VFCS     :=PAU05I01_OUT.VFCS   ;"]
["注：部分地区无防冻开关",null,{"$f":"\"    \"&A2&\"_IN.AFS    :=L\"&A2&\"_AFS       ;\"","v":"PAU05G01_IN.AFS    :=LPAU05G01_AFS       ;"},null,null,null,"    LPAU05I01_FDOC     :=PAU05I01_OUT.FDO    ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.ISO1   :=L\"&A2&\"_ISO1      ;\"","v":"PAU05G01_IN.ISO1   :=LPAU05G01_ISO1      ;"},null,null,null,"    LPAU05I01_FDSC     :=PAU05I01_OUT.FDS    ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.ISO2   :=L\"&A2&\"_ISO2      ;\"","v":"PAU05G01_IN.ISO2   :=LPAU05G01_ISO2      ;"},null,null,null,"    LPAU05I01_C        :=PAU05I01_OUT.ContRol;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.ISO3   :=L\"&A2&\"_ISO3      ;\"","v":"PAU05G01_IN.ISO3   :=LPAU05G01_ISO3      ;"},null,null,null,"    LPAU05I01_RH       :=PAU05I01_OUT.RH     ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.VP     :=L\"&A2&\"_VP        ;\"","v":"PAU05G01_IN.VP     :=LPAU05G01_VP        ;"}," ",null,null,"    LPAU05I01_SN       :=PAU05I01_OUT.SN     ;"]
[null,null,{"$f":"\"    \"&A2&\"_IN.VI     :=L\"&A2&\"_VI        ;\"","v":"PAU05G01_IN.VI     :=LPAU05G01_VI        ;"}," ",null,null,"    (*同步程序*)"]
[null,null,{"$f":"\"    \"&A2&\"_IN.FDELAY :=t#30s               ;\"","v":"PAU05G01_IN.FDELAY :=t#30s               ;"}," ",null,null,"    PAU05I01_SyncContRol(CM:=RNIPAU00000_CM,RM:=LCMD00000_RM,"]
[null,null,{"$f":"\"    \"&A2&\"_IN.VDELAY :=t#120s              ;\"","v":"PAU05G01_IN.VDELAY :=t#120s              ;"}," ",null,null,"                     BOOL_IN0:=RNIPAU05X00_PC  ,BOOL_IN1:=LPAU05I01_PC  ,BOOL_IN2      :=RPAU05I01_PC  ,BOOL_IN3:=LPAU05I01_TC,"]
[null,null,"    (*FAU_OUTSTRUCT*)",null,null,null,"                     REAL_IN0:=RNIPAU05X00_TSET,REAL_IN1:=LPAU05I01_TSET,REAL_IN2      :=RPAU05I01_TSET,"]
[null,null,{"$f":"\"    L\"&A2&\"_WVCS     :=\"&A2&\"_OUT.WVCS   ;\"","v":"LPAU05G01_WVCS     :=PAU05G01_OUT.WVCS   ;"},null,null,"    ","                     INT_IN0 :=RNIPAU05X00_SM  ,INT_IN1 :=LPAU05I01_SM  ,INT_IN2       :=RPAU05I01_SM  |"]
[null,null,{"$f":"\"    L\"&A2&\"_VFCS     :=\"&A2&\"_OUT.VFCS   ;\"","v":"LPAU05G01_VFCS     :=PAU05G01_OUT.VFCS   ;"},null,null,null,"                                          LPAU05I01_PC  :=BOOL_OUT1     ,RPAU05I01_PC  :=BOOL_OUT2     ,"]
[null,null,{"$f":"\"    L\"&A2&\"_FDOC     :=\"&A2&\"_OUT.FDO    ;\"","v":"LPAU05G01_FDOC     :=PAU05G01_OUT.FDO    ;"},null,null,null,"                                          LPAU05I01_TSET:=REAL_OUT1     ,RPAU05I01_TSET:=REAL_OUT2     ,"]
[null,null,{"$f":"\"    L\"&A2&\"_FDSC     :=\"&A2&\"_OUT.FDS    ;\"","v":"LPAU05G01_FDSC     :=PAU05G01_OUT.FDS    ;"},null,null,null,"                                          LPAU05I01_SM  :=INT_OUT1      ,RPAU05I01_SM  :=INT_OUT2     );"]
[null,null,{"$f":"\"    L\"&A2&\"_C        :=\"&A2&\"_OUT.ContRol;\"","v":"LPAU05G01_C        :=PAU05G01_OUT.ContRol;"},null,null,null,"    (*新风机CO2联动程序*)"]
[null,null,{"$f":"\"    L\"&A2&\"_RH       :=\"&A2&\"_OUT.RH     ;\"","v":"LPAU05G01_RH       :=PAU05G01_OUT.RH     ;"},null,"  ",null,"    LPAU05I01_TC:=LPAU05I01_LC[1];"]
[null,null,{"$f":"\"    L\"&A2&\"_SN       :=\"&A2&\"_OUT.SN     ;\"","v":"LPAU05G01_SN       :=PAU05G01_OUT.SN     ;"},null,null,null,"    LPAU05I01_CO2S[1]:=LIES04B01_CO2S;"]
[null,null,"    (*同步程序*)"]
[null,null,{"$f":"\"    \"&A2&\"_SyncContRol(CM:=RNIPAU00000_CM,RM:=LCMD00000_RM,\n                     BOOL_IN0:=RNI\"&B2&\"_PC  ,BOOL_IN1:=L\"&A2&\"_PC  ,BOOL_IN2      :=R\"&A2&\"_PC  ,BOOL_IN3:=L\"&A2&\"_TC,\n                     REAL_IN0:=RNI\"&B2&\"_TSET,REAL_IN1:=L\"&A2&\"_TSET,REAL_IN2      :=R\"&A2&\"_TSET,\n                     INT_IN0 :=RNI\"&B2&\"_SM  ,INT_IN1 :=L\"&A2&\"_SM  ,INT_IN2       :=R\"&A2&\"_SM  |\n                                          L\"&A2&\"_PC  :=BOOL_OUT1     ,R\"&A2&\"_PC  :=BOOL_OUT2     ,\n                                          L\"&A2&\"_TSET:=REAL_OUT1     ,R\"&A2&\"_TSET:=REAL_OUT2     ,\n                                          L\"&A2&\"_SM  :=INT_OUT1      ,R\"&A2&\"_SM  :=INT_OUT2     );\"","v":"PAU05G01_SyncContRol(CM:=RNIPAU00000_CM,RM:=LCMD00000_RM,\n                     BOOL_IN0:=RNIPAU05X00_PC  ,BOOL_IN1:=LPAU05G01_PC  ,BOOL_IN2      :=RPAU05G01_PC  ,BOOL_IN3:=LPAU05G01_TC,\n                     REAL_IN0:=RNIPAU05X00_TSET,REAL_IN1:=LPAU05G01_TSET,REAL_IN2      :=RPAU05G01_TSET,\n                     INT_IN0 :=RNIPAU05X00_SM  ,INT_IN1 :=LPAU05G01_SM  ,INT_IN2       :=RPAU05G01_SM  |\n                                          LPAU05G01_PC  :=BOOL_OUT1     ,RPAU05G01_PC  :=BOOL_OUT2     ,\n                                          LPAU05G01_TSET:=REAL_OUT1     ,RPAU05G01_TSET:=REAL_OUT2     ,\n                                          LPAU05G01_SM  :=INT_OUT1      ,RPAU05G01_SM  :=INT_OUT2     );"},null,null,null,"    PAU05I01_SLG(ENABLE:=LPAU05I01_TM,LINKAGEVALUE:=LPAU05I01_CO2S,DEAD_BAND:=10.0,MAXRANGE:=2000.0,MINRANGE:=10.0,"]
[null,null,"    (*新风机CO2联动程序*)",null,null,null,"             LINKAGESET:=LPAU05I01_CO2SET,HOLDDELAY:=t#60s,ENABLENUM:=4,SCH_STR:=LPAU05I01_TSTR,ALLDAY:=LPAU05I01_DM | LPAU05I01_LC:=LINKAGEOUT);"]
[null,null,{"$f":"\"    L\"&A2&\"_TC:=L\"&A2&\"_LC[1];\"","v":"LPAU05G01_TC:=LPAU05G01_LC[1];"}]
[null,null,{"$f":"\"    L\"&$A$2&\"_CO2S[1]:=\"&A3&\";\"","v":"LPAU05G01_CO2S[1]:=LIES04C01_CO2S;"}]
[null,null,{"$f":"\"    L\"&$A$2&\"_CO2S[2]:=\"&A4&\";\"","v":"LPAU05G01_CO2S[2]:=LIES05J02_CO2S;"}]
[null,null,{"$f":"\"    L\"&$A$2&\"_CO2S[3]:=\"&A5&\";\"","v":"LPAU05G01_CO2S[3]:=;"}]
[null,null,{"$f":"\"    L\"&$A$2&\"_CO2S[4]:=\"&A6&\";\"","v":"LPAU05G01_CO2S[4]:=;"}]
[null,null,{"$f":"\"    L\"&$A$2&\"_CO2S[5]:=\"&A7&\";\"","v":"LPAU05G01_CO2S[5]:=;"}]
[null,null,{"$f":"\"    \"&A2&\"_SLG(ENABLE:=L\"&A2&\"_TM,LINKAGEVALUE:=L\"&A2&\"_CO2S,DEAD_BAND:=10.0,MAXRANGE:=2000.0,MINRANGE:=10.0,\n             LINKAGESET:=L\"&A2&\"_CO2SET,HOLDDELAY:=t#60s,ENABLENUM:=4,SCH_STR:=L\"&A2&\"_TSTR,ALLDAY:=L\"&A2&\"_DM | L\"&A2&\"_LC:=LINKAGEOUT);\"","v":"PAU05G01_SLG(ENABLE:=LPAU05G01_TM,LINKAGEVALUE:=LPAU05G01_CO2S,DEAD_BAND:=10.0,MAXRANGE:=2000.0,MINRANGE:=10.0,\n             LINKAGESET:=LPAU05G01_CO2SET,HOLDDELAY:=t#60s,ENABLENUM:=4,SCH_STR:=LPAU05G01_TSTR,ALLDAY:=LPAU05G01_DM | LPAU05G01_LC:=LINKAGEOUT);"}]

{"sheet":"吊顶空调","index":6,"n_rows":79,"n_cols":17,"rows_kept":79,"cut":false,"hidden":false,"merged":[[42,0,42,2]]}
["编号","楼层","程序端声明"]
["AHU01A05","AHU01X00",{"$f":"\"D\"&A2&\"_IN :DAHU_IN;\"","v":"DAHU01A05_IN :DAHU_IN;"}]
[null,null,{"$f":"\"D\"&A2&\"_OUT:DAHU_OUT;\"","v":"DAHU01A05_OUT:DAHU_OUT;"}]
[null,null,{"$f":"\"\"&A2&\"_SyncControl:IJ_SyncControl;\"","v":"AHU01A05_SyncControl:IJ_SyncControl;"}]
[null,null,{"$f":"\"\"&A2&\"_DAHU:IJ_DAHU;\"","v":"AHU01A05_DAHU:IJ_DAHU;"}]
[null,null,{"$f":"\"\"&A2&\"_RT_AVE :BS_Average;\"","v":"AHU01A05_RT_AVE :BS_Average;"}]
[null,null,{"$f":"\"\"&A2&\"_WVB_AVE:BS_Average;\"","v":"AHU01A05_WVB_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    (********************************************\"&A2&\"********************************************)\"","v":"(********************************************AHU01A05********************************************)"}]
[null,null,"    (*输入，类型，示值上限，示值下限，基准补偿，输出补偿*)"]
[null,null,{"$f":"\"    \"&A2&\"_WVB_AVE(INPUT:=L\"&A2&\"_WVB);\"","v":"AHU01A05_WVB_AVE(INPUT:=LAHU01A05_WVB);"}]
[null,null,{"$f":"\"    \"&A2&\"_RT_AVE (INPUT:=L\"&A2&\"_RT) ;\"","v":"AHU01A05_RT_AVE (INPUT:=LAHU01A05_RT) ;"},{"$nulls":13},"   "]
[null,null,{"$f":"\"    L\"&A2&\"_RTS :=            BS_Scale(\"&A2&\"_RT_AVE.Output ,1,0,100,0,0.0) ;\"","v":"LAHU01A05_RTS :=            BS_Scale(AHU01A05_RT_AVE.Output ,1,0,100,0,0.0) ;"}]
[null,null,{"$f":"\"    L\"&A2&\"_WVBS:=            BS_Scale(\"&A2&\"_WVB_AVE.Output,2,0,100,0,0.0) ;\"","v":"LAHU01A05_WVBS:=            BS_Scale(AHU01A05_WVB_AVE.Output,2,0,100,0,0.0) ;"}]
[null,null,{"$f":"\"    L\"&A2&\"_WVC :=REAL_TO_INT(BS_Scale(L\"&A2&\"_WVCS         ,4,0,100,0,0.0));\"","v":"LAHU01A05_WVC :=REAL_TO_INT(BS_Scale(LAHU01A05_WVCS         ,4,0,100,0,0.0));"}]
[null,null,"    (*主程序*)"]
[null,null,{"$f":"\"    \"&A2&\"_DAHU(DAHU_STRUCT_IN:=D\"&A2&\"_IN | D\"&A2&\"_OUT:=DAHU_STRUCT_OUT);\"","v":"AHU01A05_DAHU(DAHU_STRUCT_IN:=DAHU01A05_IN | DAHU01A05_OUT:=DAHU_STRUCT_OUT);"}]
[null,null,"    (*AHU_INSTRUCT*)"]
[null,null,{"$f":"\"    D\"&A2&\"_IN.SM     :=L\"&A2&\"_SM         ;\"","v":"DAHU01A05_IN.SM     :=LAHU01A05_SM         ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.Run    :=L\"&A2&\"_R          ;\"","v":"DAHU01A05_IN.Run    :=LAHU01A05_R          ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.Fault  :=L\"&A2&\"_F          ;\"","v":"DAHU01A05_IN.Fault  :=LAHU01A05_F          ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.Auto   :=L\"&A2&\"_A          ;\"","v":"DAHU01A05_IN.Auto   :=LAHU01A05_A          ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.ContRol:=L\"&A2&\"_PC         ;\"","v":"DAHU01A05_IN.ContRol:=LAHU01A05_PC         ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.TSET   :=L\"&A2&\"_TSET       ;\"","v":"DAHU01A05_IN.TSET   :=LAHU01A05_TSET       ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.WVMC   :=L\"&A2&\"_WVMC       ;\"","v":"DAHU01A05_IN.WVMC   :=LAHU01A05_WVMC       ;"}]
["    ",null,{"$f":"\"    D\"&A2&\"_IN.WVMV   :=L\"&A2&\"_WVMV       ;\"","v":"DAHU01A05_IN.WVMV   :=LAHU01A05_WVMV       ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.RTS    :=L\"&A2&\"_RTS        ;\"","v":"DAHU01A05_IN.RTS    :=LAHU01A05_RTS        ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.RST    :=L\"&A2&\"_RST        ;\"","v":"DAHU01A05_IN.RST    :=LAHU01A05_RST        ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.RSTV   :=L\"&A2&\"_RSTV       ;\"","v":"DAHU01A05_IN.RSTV   :=LAHU01A05_RSTV       ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.FPS    :=L\"&A2&\"_FPS        ;\"","v":"DAHU01A05_IN.FPS    :=LAHU01A05_FPS        ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.ISO1   :=L\"&A2&\"_ISO1       ;\"","v":"DAHU01A05_IN.ISO1   :=LAHU01A05_ISO1       ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.ISO2   :=L\"&A2&\"_ISO2       ;\"","v":"DAHU01A05_IN.ISO2   :=LAHU01A05_ISO2       ;"}]
[null,null,{"$f":"\"    D\"&A2&\"_IN.VP     :=L\"&A2&\"_VP         ;\"","v":"DAHU01A05_IN.VP     :=LAHU01A05_VP         ;"}]
["    ",null,{"$f":"\"    D\"&A2&\"_IN.VI     :=L\"&A2&\"_VI         ;\"","v":"DAHU01A05_IN.VI     :=LAHU01A05_VI         ;"}]
[null,null,"    (*AHU_OUTSTRUCT*)"]
[null,null,{"$f":"\"    L\"&A2&\"_WVCS      :=D\"&A2&\"_OUT.WVCS   ;\"","v":"LAHU01A05_WVCS      :=DAHU01A05_OUT.WVCS   ;"}]
[null,null,{"$f":"\"    L\"&A2&\"_C         :=D\"&A2&\"_OUT.ContRol;\"","v":"LAHU01A05_C         :=DAHU01A05_OUT.ContRol;"}]
[null,null,{"$f":"\"    L\"&A2&\"_RH        :=D\"&A2&\"_OUT.RH     ;\"","v":"LAHU01A05_RH        :=DAHU01A05_OUT.RH     ;"}]
[null,null,{"$f":"\"    L\"&A2&\"_SN        :=D\"&A2&\"_OUT.SN     ;\"","v":"LAHU01A05_SN        :=DAHU01A05_OUT.SN     ;"}]
[null,null,"    (*同步程序*)"]
[null,null,{"$f":"\"    \"&A2&\"_SyncContRol(CM:=RNIAHU00000_CM,RM:=LCMD00000_RM,\n                         BOOL_IN0:=RNI\"&B2&\"_PC  ,BOOL_IN1:=L\"&A2&\"_PC  ,BOOL_IN2      :=R\"&A2&\"_PC  ,\n                         REAL_IN0:=RNI\"&B2&\"_TSET,REAL_IN1:=L\"&A2&\"_TSET,REAL_IN2      :=R\"&A2&\"_TSET,\n                         INT_IN0 :=RNI\"&B2&\"_SM  ,INT_IN1 :=L\"&A2&\"_SM  ,INT_IN2       :=R\"&A2&\"_SM  |\n                                              L\"&A2&\"_PC  :=BOOL_OUT1     ,R\"&A2&\"_PC  :=BOOL_OUT2     ,\n                                              L\"&A2&\"_TSET:=REAL_OUT1     ,R\"&A2&\"_TSET:=REAL_OUT2     ,\n                                              L\"&A2&\"_SM  :=INT_OUT1      ,R\"&A2&\"_SM  :=INT_OUT2)     ;\"","v":"AHU01A05_SyncContRol(CM:=RNIAHU00000_CM,RM:=LCMD00000_RM,\n                         BOOL_IN0:=RNIAHU01X00_PC  ,BOOL_IN1:=LAHU01A05_PC  ,BOOL_IN2      :=RAHU01A05_PC  ,\n                         REAL_IN0:=RNIAHU01X00_TSET,REAL_IN1:=LAHU01A05_TSET,REAL_IN2      :=RAHU01A05_TSET,\n                         INT_IN0 :=RNIAHU01X00_SM  ,INT_IN1 :=LAHU01A05_SM  ,INT_IN2       :=RAHU01A05_SM  |\n                                              LAHU01A05_PC  :=BOOL_OUT1     ,RAHU01A05_PC  :=BOOL_OUT2     ,\n                                              LAHU01A05_TSET:=REAL_OUT1     ,RAHU01A05_TSET:=REAL_OUT2     ,\n                                              LAHU01A05_SM  :=INT_OUT1      ,RAHU01A05_SM  :=INT_OUT2)     ;"}]
[]
["0803模块"]
["编号","楼层","程序端声明"]
["AHU","AHU01X00",{"$f":"\"D\"&A45&\"_IN :DAHU_IN;\"","v":"DAHU_IN :DAHU_IN;"}]
[null,null,{"$f":"\"D\"&A45&\"_OUT:DAHU_OUT;\"","v":"DAHU_OUT:DAHU_OUT;"}]
[null,null,{"$f":"\"\"&A45&\"_SyncControl:IJ_SyncControl;\"","v":"AHU_SyncControl:IJ_SyncControl;"}]
[null,null,{"$f":"\"\"&A45&\"_SyncControl:IJ_SyncControl;\"","v":"AHU_SyncControl:IJ_SyncControl;"}]
[null,null,{"$f":"\"\"&A45&\"_SyncControl:IJ_SyncControl;\"","v":"AHU_SyncControl:IJ_SyncControl;"}]
[null,null,{"$f":"\"\"&A45&\"_DAHU:IJ_DAHU;\"","v":"AHU_DAHU:IJ_DAHU;"}]
[null,null,{"$f":"\"\"&A45&\"_RT_AVE :BS_Average;\"","v":"AHU_RT_AVE :BS_Average;"}]
[null,null,{"$f":"\"\"&A45&\"_WVB_AVE:BS_Average;\"","v":"AHU_WVB_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    (********************************************\"&A45&\"********************************************)\"","v":"(********************************************AHU********************************************)"}]
[null,null," (*输入，类型，示值上限，示值下限，基准补偿，输出补偿*)"]
[null,null,"    AHU_WVB_AVE(INPUT:=Device_AI001);"]
[null,null,"    AHU_RT_AVE (INPUT:=Device_AI003) ;"]
[null,null,"    LAHU_RTS :=           BS_Scale(AHU_RT_AVE.Output ,1,0,100,0,0.0) ;"]
[null,null,"    LAHU_WVBS:=           BS_Scale(AHU_WVB_AVE.Output,2,0,100,0,0.0) ;"]
[null,null,"    LAHU_WVC :=           REAL_TO_INT(BS_Scale(LAHU_WVCS,4,0,100,0,0.0));"]
[null,null,"    (*主程序*)"]
[null,null,"    AHU_DAHU(DAHU_STRUCT_IN:=LDAHU_IN | LDAHU_OUT:=DAHU_STRUCT_OUT);"]
[null,null,"    (*AHU_INSTRUCT*)"]
[null,null,"    LDAHU_IN.SM     :=LAHU_SM         ;"]
[null,null,"    LDAHU_IN.ContRol:=LAHU_PC         ;"]
[null,null,"    LDAHU_IN.TSET   :=LAHU_TSET       ;"]
[null,null,"    LDAHU_IN.WVMC   :=LAHU_WVMC       ;"]
[null,null,"    LDAHU_IN.WVMV   :=LAHU_WVMV       ;"]
[null,null,"    LDAHU_IN.RTS    :=LAHU_RTS        ;"]
[null,null,"    LDAHU_IN.FPS    :=LAHU_FPS        ;"]
["    ",null,"    LDAHU_IN.ISO1   :=LAHU_ISO1       ;"]
[null,null,"    LDAHU_IN.ISO2   :=LAHU_ISO2       ;"]
[null,null,"    LDAHU_IN.CTV    :=LAHU_CTV        ;"]
[null,null,"    LDAHU_IN.RunMode:=LAHU_RunMode    ;"]
[null,null,"    (*AHU_OUTSTRUCT*)"]
[null,null,"    LAHU_WVCS      :=LDAHU_OUT.WVCS   ;"]
[null,null,"    LAHU_FPSSIM    :=LDAHU_OUT.FPSSIM ;"]
[null,null," (*同步程序*)"]
["    ",null,"LAHU_SyncContRol(CM:=RNIAHU00000_CM,RM:=0,\n                         REAL_IN0:=RNIAHU01X00_TSET,REAL_IN1:=LAHU_TSET,REAL_IN2      :=RAHU_TSET,\n                         INT_IN0 :=RNIAHU01X00_SM  ,INT_IN1 :=LAHU_SM  ,INT_IN2       :=RAHU_SM  |\n                                              LAHU_TSET:=REAL_OUT1     ,RAHU_TSET:=REAL_OUT2     ,\n                                              LAHU_SM  :=INT_OUT1      ,RAHU_SM  :=INT_OUT2)     ;\n\tLAHU_SyncContRol2(CM:=RNIAHU00000_CM,RM:=0,\n                         INT_IN0 :=RNIAHU00000_RunMode  ,INT_IN1 :=LAHU_RunMode    |\n                                              LAHU_RunMode  :=INT_OUT1      )     ;\n\tLAHU_SyncContRol3(CM:=RNIAHU00000_CM,RM:=0,\n                         INT_IN0 :=RNIAHU00000_WVMC  ,INT_IN1 :=LAHU_WVMC    |\n                                              LAHU_WVMC  :=INT_OUT1      )     ;"]

{"sheet":"风机盘管","index":7,"n_rows":34,"n_cols":3,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["编号","楼层","程序端声明"]
["FCU04H01","FCU04X00",{"$f":"\"\"&A2&\"_IN :FCU_IN;\"","v":"FCU04H01_IN :FCU_IN;"}]
[null,null,{"$f":"\"\"&A2&\"_OUT:FCU_OUT;\"","v":"FCU04H01_OUT:FCU_OUT;"}]
[null,null,{"$f":"\"\"&A2&\"_SyncControl:IJ_SyncControl;\"","v":"FCU04H01_SyncControl:IJ_SyncControl;"}]
[null,null,{"$f":"\"\"&A2&\"_FCU:IJ_FCU;\"","v":"FCU04H01_FCU:IJ_FCU;"}]
[null,null,{"$f":"\"\"&A2&\"_T_AVE:BS_Average;\"","v":"FCU04H01_T_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    (********************************************\"&A2&\"********************************************)\"","v":"(********************************************FCU04H01********************************************)"}]
[null,null,"    (*输入，类型，示值上限，示值下限，基准补偿，输出补偿*)"]
[null,null,{"$f":"\"    \"&A2&\"_T_AVE(INPUT:=L\"&A2&\"_T);\"","v":"FCU04H01_T_AVE(INPUT:=LFCU04H01_T);"}]
[null,null,{"$f":"\"    L\"&A2&\"_TS        :=BS_Scale(\"&A2&\"_T_AVE.Output,1,0,100,0,0.0);\"","v":"LFCU04H01_TS        :=BS_Scale(FCU04H01_T_AVE.Output,1,0,100,0,0.0);"}]
[null,null,"    (*主程序*)"]
[null,null,{"$f":"\"    \"&A2&\"_FCU(FCU_STRUCT_IN:=\"&A2&\"_IN | \"&A2&\"_OUT:=FCU_STRUCT_OUT);\"","v":"FCU04H01_FCU(FCU_STRUCT_IN:=FCU04H01_IN | FCU04H01_OUT:=FCU_STRUCT_OUT);"}]
[null,null,"    (*AHU_INSTRUCT*)"]
[null,null,{"$f":"\"    \"&A2&\"_IN.SM      :=L\"&A2&\"_SM         ;\"","v":"FCU04H01_IN.SM      :=LFCU04H01_SM         ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.Run     :=L\"&A2&\"_R          ;\"","v":"FCU04H01_IN.Run     :=LFCU04H01_R          ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.Auto    :=L\"&A2&\"_A          ;\"","v":"FCU04H01_IN.Auto    :=LFCU04H01_A          ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.Control :=L\"&A2&\"_PC         ;\"","v":"FCU04H01_IN.Control :=LFCU04H01_PC         ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.TSET    :=L\"&A2&\"_TSET       ;\"","v":"FCU04H01_IN.TSET    :=LFCU04H01_TSET       ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.EVA     :=L\"&A2&\"_EVA        ;\"","v":"FCU04H01_IN.EVA     :=LFCU04H01_EVA        ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.EVR     :=L\"&A2&\"_EVR        ;\"","v":"FCU04H01_IN.EVR     :=LFCU04H01_EVR        ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.EVMC    :=L\"&A2&\"_EVMC       ;\"","v":"FCU04H01_IN.EVMC    :=LFCU04H01_EVMC       ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.EVMV    :=L\"&A2&\"_EVMV       ;\"","v":"FCU04H01_IN.EVMV    :=LFCU04H01_EVMV       ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.TS      :=L\"&A2&\"_TS         ;\"","v":"FCU04H01_IN.TS      :=LFCU04H01_TS         ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.RST     :=L\"&A2&\"_RST        ;\"","v":"FCU04H01_IN.RST     :=LFCU04H01_RST        ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.RSTV    :=L\"&A2&\"_RSTV       ;\"","v":"FCU04H01_IN.RSTV    :=LFCU04H01_RSTV       ;"}]
[null,null,{"$f":"\"    \"&A2&\"_IN.ISO1    :=L\"&A2&\"_ISO1       ;\"","v":"FCU04H01_IN.ISO1    :=LFCU04H01_ISO1       ;"}]
[null,null,"    (*FCU_OUTSTRUCT*)"]
[null,null,{"$f":"\"    L\"&A2&\"_EVC       :=\"&A2&\"_OUT.EVC     ;\"","v":"LFCU04H01_EVC       :=FCU04H01_OUT.EVC     ;"}]
[null,null,{"$f":"\"    L\"&A2&\"_C         :=\"&A2&\"_OUT.Control ;\"","v":"LFCU04H01_C         :=FCU04H01_OUT.Control ;"}]
[null,null,{"$f":"\"    L\"&A2&\"_RH        :=\"&A2&\"_OUT.RH      ;\"","v":"LFCU04H01_RH        :=FCU04H01_OUT.RH      ;"}]
[null,null,{"$f":"\"    L\"&A2&\"_SN        :=\"&A2&\"_OUT.SN      ;\"","v":"LFCU04H01_SN        :=FCU04H01_OUT.SN      ;"}]
[null,null,"    (*同步程序*)"]
[null,null,{"$f":"\"    \"&A2&\"_SyncControl(CM:=RNIFCU00000_CM,RM:=LCMD00000_RM,\n                         BOOL_IN0 :=RNI\"&B2&\"_PC  ,BOOL_IN1      :=L\"&A2&\"_PC    ,BOOL_IN2      :=R\"&A2&\"_PC   ,\n                         INT_IN0  :=RNI\"&B2&\"_SM  ,INT_IN1       :=L\"&A2&\"_SM    ,INT_IN2       :=R\"&A2&\"_SM   ,\n                         REAL_IN0 :=RNI\"&B2&\"_TSET,REAL_IN1      :=L\"&A2&\"_TSET  ,REAL_IN2      :=R\"&A2&\"_TSET |\n                                                     L\"&A2&\"_PC  :=BOOL_OUT1       ,R\"&A2&\"_PC  :=BOOL_OUT2      ,\n                                                     L\"&A2&\"_TSET:=REAL_OUT1       ,R\"&A2&\"_TSET:=REAL_OUT2      ,\n                                                     L\"&A2&\"_SM  :=INT_OUT1        ,R\"&A2&\"_SM  :=INT_OUT2)      ;\"","v":"FCU04H01_SyncControl(CM:=RNIFCU00000_CM,RM:=LCMD00000_RM,\n                         BOOL_IN0 :=RNIFCU04X00_PC  ,BOOL_IN1      :=LFCU04H01_PC    ,BOOL_IN2      :=RFCU04H01_PC   ,\n                         INT_IN0  :=RNIFCU04X00_SM  ,INT_IN1       :=LFCU04H01_SM    ,INT_IN2       :=RFCU04H01_SM   ,\n                         REAL_IN0 :=RNIFCU04X00_TSET,REAL_IN1      :=LFCU04H01_TSET  ,REAL_IN2      :=RFCU04H01_TSET |\n                                                     LFCU04H01_PC  :=BOOL_OUT1       ,RFCU04H01_PC  :=BOOL_OUT2      ,\n                                                     LFCU04H01_TSET:=REAL_OUT1       ,RFCU04H01_TSET:=REAL_OUT2      ,\n                                                     LFCU04H01_SM  :=INT_OUT1        ,RFCU04H01_SM  :=INT_OUT2)      ;"}]

{"sheet":"水风幕机","index":8,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["编号","楼层","程序端声明"]
["FMJ01D01","FMJ01X00",{"$f":"\"\"&A2&\"_SyncControl:IJ_SyncControl;\"","v":"FMJ01D01_SyncControl:IJ_SyncControl;"}]
[null,null,"程序"]
[null,null,"    (*同步程序*)"]
[null,null,{"$f":"\"    \"&A2&\"_SyncControl(CM:=RNIFMJ00000_CM,RM:=LCMD00000_RM,\n                         BOOL_IN0 :=RNI\"&B2&\"_PC  ,BOOL_IN1     :=L\"&A2&\"_C     ,BOOL_IN2     :=R\"&A2&\"_C   |\n                                                     L\"&A2&\"_C  :=BOOL_OUT1       ,R\"&A2&\"_C  :=BOOL_OUT2     );\"","v":"FMJ01D01_SyncControl(CM:=RNIFMJ00000_CM,RM:=LCMD00000_RM,\n                         BOOL_IN0 :=RNIFMJ01X00_PC  ,BOOL_IN1     :=LFMJ01D01_C     ,BOOL_IN2     :=RFMJ01D01_C   |\n                                                     LFMJ01D01_C  :=BOOL_OUT1       ,RFMJ01D01_C  :=BOOL_OUT2     );"}]
[null,null,"    (*运行累积时间*)"]
[null,null,{"$f":"\"    \"&A2&\"_RunTime(RUN :=L\"&A2&\"_R , RUNTIMESET :=L\"&A2&\"_RSTV , RUNTIMERST :=L\"&A2&\"_RST , RunTimeRec_In :=L\"&A2&\"_RH |  L\"&A2&\"_RH:= RUNTIME);\"","v":"FMJ01D01_RunTime(RUN :=LFMJ01D01_R , RUNTIMESET :=LFMJ01D01_RSTV , RUNTIMERST :=LFMJ01D01_RST , RunTimeRec_In :=LFMJ01D01_RH |  LFMJ01D01_RH:= RUNTIME);"}]

{"sheet":"排风机","index":9,"n_rows":41,"n_cols":4,"rows_kept":41,"cut":false,"hidden":false,"merged":[[1,0,20,0],[21,0,40,0]]}
["类型","编号","楼层","程序端声明"]
["地下室排风","EAF04A01","EAF01X00",{"$f":"\"\"&B3&\":ARRAY[0..10] OF REAL;\"","v":"LEAFB1A01_COS:ARRAY[0..10] OF REAL;"}]
[null,"LEAFB1A01_COS","CO数组平均值"]
[null,null,null,"程序端声明"]
[null,null,null,{"$f":"\"\"&B2&\"_SyncControl:IJ_LSyncControl;\"","v":"EAF04A01_SyncControl:IJ_LSyncControl;"}]
[null,null,null,{"$f":"\"\"&B2&\"_SLG:IJ_EAFGroup;\"","v":"EAF04A01_SLG:IJ_EAFGroup;"}]
[null,null,null,{"$f":"\"\"&B2&\"_RunTime:BS_RunTime;\"","v":"EAF04A01_RunTime:BS_RunTime;"}]
[null,null,null,{"$f":"\"L\"&B2&\"_LC  :ARRAY[0..10] OF BOOL;\"","v":"LEAF04A01_LC  :ARRAY[0..10] OF BOOL;"}]
[null,null,null,"程序"]
[null,null,null,{"$f":"\"    L\"&B2&\"_TC    :=L\"&B2&\"_LC[1];\"","v":"LEAF04A01_TC    :=LEAF04A01_LC[1];"}]
[null,null,null,"    (*排风机联动程序*)"]
[null,null,null,{"$f":"\"    \"&B2&\"_SLG(ENABLE :=L\"&B2&\"_TM ,LINKAGEVALUE :=\"&B3&\" , DEAD_BAND :=10.0 , MAXRANGE :=1000.0 , MINRANGE :=0.1 ,LINKAGESET :=L\"&B2&\"_COSET ,  HOLDDELAY :=t#60s , ENABLENUM :=4 , SCH_STR :=L\"&B2&\"_TSTR ,ALLDAY :=L\"&B2&\"_DM  |  L\"&B2&\"_LC:= LINKAGEOUT);\"","v":"EAF04A01_SLG(ENABLE :=LEAF04A01_TM ,LINKAGEVALUE :=LEAFB1A01_COS , DEAD_BAND :=10.0 , MAXRANGE :=1000.0 , MINRANGE :=0.1 ,LINKAGESET :=LEAF04A01_COSET ,  HOLDDELAY :=t#60s , ENABLENUM :=4 , SCH_STR :=LEAF04A01_TSTR ,ALLDAY :=LEAF04A01_DM  |  LEAF04A01_LC:= LINKAGEOUT);"}]
[null,null,null,"    (*同步程序*)"]
[null,null,null,{"$f":"\"    \"&B2&\"_SyncContRol(CM :=RNIEAF00000_CM , RM :=LCMD00000_RM ,BOOL_IN0:= RNI\"&C2&\"_PC,BOOL_IN1:=L\"&B2&\"_C,BOOL_IN2:=R\"&B2&\"_C,BOOL_IN3:=L\"&B2&\"_TC | L\"&B2&\"_C:= BOOL_OUT1,R\"&B2&\"_C:=BOOL_OUT2);\"","v":"EAF04A01_SyncContRol(CM :=RNIEAF00000_CM , RM :=LCMD00000_RM ,BOOL_IN0:= RNIEAF01X00_PC,BOOL_IN1:=LEAF04A01_C,BOOL_IN2:=REAF04A01_C,BOOL_IN3:=LEAF04A01_TC | LEAF04A01_C:= BOOL_OUT1,REAF04A01_C:=BOOL_OUT2);"}]
[null,null,null,"    (*运行累积时间*)"]
[null,null,null,{"$f":"\"    \"&B2&\"_RunTime(RUN :=L\"&B2&\"_R , RUNTIMESET :=L\"&B2&\"_RSTV , RUNTIMERST :=L\"&B2&\"_RST , RunTimeRec_In :=L\"&B2&\"_RH |  L\"&B2&\"_RH:= RUNTIME);\"","v":"EAF04A01_RunTime(RUN :=LEAF04A01_R , RUNTIMESET :=LEAF04A01_RSTV , RUNTIMERST :=LEAF04A01_RST , RunTimeRec_In :=LEAF04A01_RH |  LEAF04A01_RH:= RUNTIME);"}]
[null,"CO数量",null,"程序"]
[null,"LIESB1A01_COS",null,{"$f":"\"    \"&$B$3&\"[1]:=\"&B18&\";\"","v":"LEAFB1A01_COS[1]:=LIESB1A01_COS;"}]
[null,"LIESB1A02_COS",null,{"$f":"\"    \"&$B$3&\"[2]:=\"&B19&\";\"","v":"LEAFB1A01_COS[2]:=LIESB1A02_COS;"}]
[null,"LIESB1B01_COS",null,{"$f":"\"    \"&$B$3&\"[3]:=\"&B20&\";\"","v":"LEAFB1A01_COS[3]:=LIESB1B01_COS;"}]
[null,"LIESB1E01_COS",null,{"$f":"\"    \"&$B$3&\"[4]:=\"&B21&\";\"","v":"LEAFB1A01_COS[4]:=LIESB1E01_COS;"}]
["中庭排风","EAF04D01","EAF05X00",{"$f":"\"\"&B23&\":ARRAY[0..10] OF REAL;\"","v":"LEAF04D01_TS:ARRAY[0..10] OF REAL;"}]
[null,"LEAF04D01_TS","T数组平均值"]
[null,null,null,"程序端声明"]
[null,null,null,{"$f":"\"\"&B22&\"_SyncControl:IJ_LSyncControl;\"","v":"EAF04D01_SyncControl:IJ_LSyncControl;"}]
[null,null,null,{"$f":"\"\"&B22&\"_SLG:IJ_EAFGroup;\"","v":"EAF04D01_SLG:IJ_EAFGroup;"}]
[null,null,null,{"$f":"\"\"&B22&\"_RunTime:BS_RunTime;\"","v":"EAF04D01_RunTime:BS_RunTime;"}]
[null,null,null,{"$f":"\"L\"&B22&\"_LC  :ARRAY[0..10] OF BOOL;\"","v":"LEAF04D01_LC  :ARRAY[0..10] OF BOOL;"}]
[null,null,null,"程序"]
[null,null,null,{"$f":"\"    L\"&B22&\"_TC    :=L\"&B22&\"_LC[1];\"","v":"LEAF04D01_TC    :=LEAF04D01_LC[1];"}]
[null,null,null,"    (*排风机联动程序*)"]
[null,null,null,{"$f":"\"    \"&B22&\"_SLG(ENABLE :=L\"&B22&\"_TM ,LINKAGEVALUE :=\"&B23&\" , DEAD_BAND :=1.0 , MAXRANGE :=50.0 , MINRANGE :=0.1 ,LINKAGESET :=L\"&B22&\"_TSET ,  HOLDDELAY :=t#60s , ENABLENUM :=4 , SCH_STR :=L\"&B22&\"_TSTR ,ALLDAY :=L\"&B22&\"_DM  |  L\"&B22&\"_LC:= LINKAGEOUT);\"","v":"EAF04D01_SLG(ENABLE :=LEAF04D01_TM ,LINKAGEVALUE :=LEAF04D01_TS , DEAD_BAND :=1.0 , MAXRANGE :=50.0 , MINRANGE :=0.1 ,LINKAGESET :=LEAF04D01_TSET ,  HOLDDELAY :=t#60s , ENABLENUM :=4 , SCH_STR :=LEAF04D01_TSTR ,ALLDAY :=LEAF04D01_DM  |  LEAF04D01_LC:= LINKAGEOUT);"}]
[null,null,null,"    (*同步程序*)"]
[null,null,null,{"$f":"\"    \"&B22&\"_SyncContRol(CM :=RNIEAF00000_CM , RM :=LCMD00000_RM ,BOOL_IN0:= RNI\"&C22&\"_PC,BOOL_IN1:=L\"&B22&\"_C,BOOL_IN2:=R\"&B22&\"_C,BOOL_IN3:=L\"&B22&\"_TC | L\"&B22&\"_C:= BOOL_OUT1,R\"&B22&\"_C:=BOOL_OUT2);\"","v":"EAF04D01_SyncContRol(CM :=RNIEAF00000_CM , RM :=LCMD00000_RM ,BOOL_IN0:= RNIEAF05X00_PC,BOOL_IN1:=LEAF04D01_C,BOOL_IN2:=REAF04D01_C,BOOL_IN3:=LEAF04D01_TC | LEAF04D01_C:= BOOL_OUT1,REAF04D01_C:=BOOL_OUT2);"}]
[null,null,null,"    (*运行累积时间*)"]
[null,null,null,{"$f":"\"    \"&B22&\"_RunTime(RUN :=L\"&B22&\"_R , RUNTIMESET :=L\"&B22&\"_RSTV , RUNTIMERST :=L\"&B22&\"_RST, RunTimeRec_In :=L\"&B22&\"_RH  |  L\"&B22&\"_RH:= RUNTIME);\"","v":"EAF04D01_RunTime(RUN :=LEAF04D01_R , RUNTIMESET :=LEAF04D01_RSTV , RUNTIMERST :=LEAF04D01_RST, RunTimeRec_In :=LEAF04D01_RH  |  LEAF04D01_RH:= RUNTIME);"}]
[null," 温度数量",null,"程序"]
[null,"LIES04D01_TS",null,{"$f":"\"    \"&$B$23&\"[1]:=\"&B38&\";\"","v":"LEAF04D01_TS[1]:=LIES04D01_TS;"}]
[null,"LIES04H02_TS",null,{"$f":"\"    \"&$B$23&\"[2]:=\"&B39&\";\"","v":"LEAF04D01_TS[2]:=LIES04H02_TS;"}]
[null,"LIES04H03_TS",null,{"$f":"\"    \"&$B$23&\"[3]:=\"&B40&\";\"","v":"LEAF04D01_TS[3]:=LIES04H03_TS;"}]
[null,"LIES04B02_TS",null,{"$f":"\"    \"&$B$23&\"[4]:=\"&B41&\";\"","v":"LEAF04D01_TS[4]:=LIES04B02_TS;"}]

{"sheet":"断电保存","index":10,"n_rows":12,"n_cols":4,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
[null,"程序端声明"]
[null,"SYS_SavePower:BS_SavePower;"]
[null,"程序"]
[null,"(*Input_Type :1周期，2变化           Read_Iso     :系统读取隔离开关       Set_Timer    :周期、变化判断周期时间设定"]
[null,"Judge_Num    :变化判断变量           MEM_ADDR     :M区保存起始地址        FLASH_ADDR   :闪存区保存起始地址"]
[null,"SAVE_LEN     :保存地址长度           Write_Flag   :系统闪存写入成功标记    Read_Flag    :系统闪存读取成功标记 "]
[null,"初次下载程序时 Read_Iso :=1  Set_Timer :=t#30s ，下载完后30S后将程序调整回 Read_Iso :=0  Set_Timer :=t#720m*)"]
[]
[null,"SYS_SavePower(Input_Type :=1 ,Read_Iso :=0, Set_Timer :=t#720m , Judge_Num :=SYS_Judge_Num , MEM_ADDR :=0, FLASH_ADDR :=0 ,SAVE_LEN :=1000  ,"]
[null,"WriteNumRec_In:=SYS_WriteNum   | SYS_Write_Flag:= Write_Flag ,  SYS_Read_Flag:= Read_Flag,  SYS_WriteNum:= Write_Num );"]
[null,null,null,"  "]

{"sheet":"集水井","index":11,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["编号","程序端声明"]
["SWPB1A01",{"$f":"\"\"&$A$2&\"_RunTime1:BS_RunTime;\"","v":"SWPB1A01_RunTime1:BS_RunTime;"}]
[null,{"$f":"\"\"&$A$2&\"_RunTime2:BS_RunTime;\"","v":"SWPB1A01_RunTime2:BS_RunTime;"}]
[null,{"$f":"\"\"&$A$2&\"_RunTime3:BS_RunTime;\"","v":"SWPB1A01_RunTime3:BS_RunTime;"}]
[null,"程序"]
[null,"    (*运行累积时间*)"]
[null,{"$f":"\"    \"&$A$2&\"_RunTime1(RUN :=L\"&$A$2&\"_R1 , RUNTIMESET :=L\"&$A$2&\"_RSTV1 , RUNTIMERST :=L\"&$A$2&\"_RST1 , RunTimeRec_In :=L\"&$A$2&\"_RH1  |  L\"&$A$2&\"_RH1:= RUNTIME);\"","v":"SWPB1A01_RunTime1(RUN :=LSWPB1A01_R1 , RUNTIMESET :=LSWPB1A01_RSTV1 , RUNTIMERST :=LSWPB1A01_RST1 , RunTimeRec_In :=LSWPB1A01_RH1  |  LSWPB1A01_RH1:= RUNTIME);"}]
[null,{"$f":"\"    \"&$A$2&\"_RunTime2(RUN :=L\"&$A$2&\"_R2 , RUNTIMESET :=L\"&$A$2&\"_RSTV2 , RUNTIMERST :=L\"&$A$2&\"_RST2 , RunTimeRec_In :=L\"&$A$2&\"_RH2  |  L\"&$A$2&\"_RH2:= RUNTIME);\"","v":"SWPB1A01_RunTime2(RUN :=LSWPB1A01_R2 , RUNTIMESET :=LSWPB1A01_RSTV2 , RUNTIMERST :=LSWPB1A01_RST2 , RunTimeRec_In :=LSWPB1A01_RH2  |  LSWPB1A01_RH2:= RUNTIME);"}]
[null,{"$f":"\"    \"&$A$2&\"_RunTime3(RUN :=L\"&$A$2&\"_R3 , RUNTIMESET :=L\"&$A$2&\"_RSTV3 , RUNTIMERST :=L\"&$A$2&\"_RST3 , RunTimeRec_In :=L\"&$A$2&\"_RH3  |  L\"&$A$2&\"_RH3:= RUNTIME);\"","v":"SWPB1A01_RunTime3(RUN :=LSWPB1A01_R3 , RUNTIMESET :=LSWPB1A01_RSTV3 , RUNTIMERST :=LSWPB1A01_RST3 , RunTimeRec_In :=LSWPB1A01_RH3  |  LSWPB1A01_RH3:= RUNTIME);"}]
[]
[null,"BOX01_DevScan( Dev_Array:= Dev_Array , Dev_Scan_Hex:= BOX01_Hex |  LDDCB101BOX_DS:= Dev_Ready, LDDCB101BOX_OR:= Dev_Ratio );"]

{"sheet":"扶梯","index":12,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["编号",null,"程序端声明"]
["LET01A01",null,{"$f":"\"\"&A2&\"_RunTime:BS_RunTime;\"","v":"LET01A01_RunTime:BS_RunTime;"}]
[null,null,"程序"]
[null,null,"    (*运行累积时间*)"]
[null,null,{"$f":"\"    L\"&A2&\"_R := IJ_DT(L\"&A2&\"_US, L\"&A2&\"_DS) ;\"","v":"LLET01A01_R := IJ_DT(LLET01A01_US, LLET01A01_DS) ;"}]
[null,null,{"$f":"\"    \"&A2&\"_RunTime(RUN :=L\"&A2&\"_R , RUNTIMESET :=L\"&A2&\"_RSTV , RUNTIMERST :=L\"&A2&\"_RST, RunTimeRec_In :=L\"&A2&\"_RH  |  L\"&A2&\"_RH:= RUNTIME);\"","v":"LET01A01_RunTime(RUN :=LLET01A01_R , RUNTIMESET :=LLET01A01_RSTV , RUNTIMERST :=LLET01A01_RST, RunTimeRec_In :=LLET01A01_RH  |  LLET01A01_RH:= RUNTIME);"}]

{"sheet":"环境换算","index":13,"n_rows":40,"n_cols":3,"rows_kept":40,"cut":false,"hidden":false,"merged":[[25,1,29,1],[30,1,34,1],[35,1,39,1],[0,1,4,1],[5,1,9,1],[10,1,14,1],[15,1,19,1],[20,1,24,1]]}
["编号","光照度","程序端声明"]
["LIES04C01_I",null,{"$f":"\"\"&A2&\"_AVE:BS_Average;\"","v":"LIES04C01_I_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A2&\"_AVE(INPUT :=\"&A2&\"   );\"","v":"LIES04C01_I_AVE(INPUT :=LIES04C01_I   );"}]
[null,null,{"$f":"\"    \"&A2&\"S          :=     BS_Scale(\"&A2&\"_AVE.Output  , 2, 0, 2000, 0, 0.0);\"","v":"LIES04C01_IS          :=     BS_Scale(LIES04C01_I_AVE.Output  , 2, 0, 2000, 0, 0.0);"}]
["LIES04C01_CO2","二氧化碳","程序端声明"]
[null,null,{"$f":"\"\"&A6&\"_AVE:BS_Average;\"","v":"LIES04C01_CO2_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A6&\"_AVE(INPUT :=\"&A6&\"   );\"","v":"LIES04C01_CO2_AVE(INPUT :=LIES04C01_CO2   );"}]
[null,null,{"$f":"\"    \"&A6&\"S          :=     BS_Scale(\"&A6&\"_AVE.Output  , 2, 0, 2000, 0, 0.0);\"","v":"LIES04C01_CO2S          :=     BS_Scale(LIES04C01_CO2_AVE.Output  , 2, 0, 2000, 0, 0.0);"}]
["LIESB1E01_CO","一氧化碳","程序端声明"]
[null,null,{"$f":"\"\"&A11&\"_AVE:BS_Average;\"","v":"LIESB1E01_CO_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A11&\"_AVE(INPUT :=\"&A11&\"   );\"","v":"LIESB1E01_CO_AVE(INPUT :=LIESB1E01_CO   );"}]
[null,null,{"$f":"\"    \"&A11&\"S          :=     BS_Scale(\"&A11&\"_AVE.Output  , 3, 0, 1000, 0, 0.0);\"","v":"LIESB1E01_COS          :=     BS_Scale(LIESB1E01_CO_AVE.Output  , 3, 0, 1000, 0, 0.0);"}]
["LIES04E01_H","湿度","程序端声明"]
[null,null,{"$f":"\"\"&A16&\"_AVE:BS_Average;\"","v":"LIES04E01_H_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A16&\"_AVE(INPUT :=\"&A16&\"   );\"","v":"LIES04E01_H_AVE(INPUT :=LIES04E01_H   );"}]
[null,null,{"$f":"\"    \"&A16&\"S          :=     BS_Scale(\"&A16&\"_AVE.Output  , 3, 0, 100, 0, 0.0);\"","v":"LIES04E01_HS          :=     BS_Scale(LIES04E01_H_AVE.Output  , 3, 0, 100, 0, 0.0);"}]
["LIES04B01_T","温度","程序端声明"]
[null,null,{"$f":"\"\"&A21&\"_AVE:BS_Average;\"","v":"LIES04B01_T_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A21&\"_AVE(INPUT :=\"&A21&\"   );\"","v":"LIES04B01_T_AVE(INPUT :=LIES04B01_T   );"}]
[null,null,{"$f":"\"    \"&A21&\"S          :=     BS_Scale(\"&A21&\"_AVE.Output  , 1, 0, 100, 0, 0.0);\"","v":"LIES04B01_TS          :=     BS_Scale(LIES04B01_T_AVE.Output  , 1, 0, 100, 0, 0.0);"}]
["LEAF01A01_SPT","压力","程序端声明"]
[null,null,{"$f":"\"\"&A26&\"_AVE:BS_Average;\"","v":"LEAF01A01_SPT_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A26&\"_AVE(INPUT :=\"&A26&\"   );\"","v":"LEAF01A01_SPT_AVE(INPUT :=LEAF01A01_SPT   );"}]
[null,null,{"$f":"\"    \"&A26&\"S          :=     BS_Scale(\"&A26&\"_AVE.Output  , 3, 0, 16, 0, 0.0);\"","v":"LEAF01A01_SPTS          :=     BS_Scale(LEAF01A01_SPT_AVE.Output  , 3, 0, 16, 0, 0.0);"}]
["LCHSB2D01_RF","流量","程序端声明"]
[null,null,{"$f":"\"\"&A31&\"_AVE:BS_Average;\"","v":"LCHSB2D01_RF_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A31&\"_AVE(INPUT :=\"&A31&\"   );\"","v":"LCHSB2D01_RF_AVE(INPUT :=LCHSB2D01_RF   );"}]
[null,null,{"$f":"\"    \"&A31&\"S          :=     BS_Scale(\"&A31&\"_AVE.Output  , 3, 0, 10000, 0, 0.0);\"","v":"LCHSB2D01_RFS          :=     BS_Scale(LCHSB2D01_RF_AVE.Output  , 3, 0, 10000, 0, 0.0);"}]
["LEAF01A01_VFB",null,"程序端声明"]
[null,null,{"$f":"\"\"&A36&\"_AVE:BS_Average;\"","v":"LEAF01A01_VFB_AVE:BS_Average;"}]
[null,null,"程序"]
[null,null,{"$f":"\"    \"&A36&\"_AVE(INPUT :=\"&A36&\"   );\"","v":"LEAF01A01_VFB_AVE(INPUT :=LEAF01A01_VFB   );"}]
[null,null,{"$f":"\"    \"&A36&\"S          :=     BS_Scale(\"&A36&\"_AVE.Output  , 2, 0, 50, 0, 0.0);\"","v":"LEAF01A01_VFBS          :=     BS_Scale(LEAF01A01_VFB_AVE.Output  , 2, 0, 50, 0, 0.0);"}]